board.c:303:0:pwm_init	8	static
board.c:328:0:Set_PWM_Duty	24	static
board.c:355:0:SPI_init	8	static
board.c:361:0:SPI_test	32	static
board.c:388:0:Lin1callback	0	static
board.c:408:0:Lin2callback	0	static
board.c:429:0:Lin_tx_test	24	static
board.c:458:0:i2c0_init	8	static
board.c:480:0:i2c1_init	8	static
board.c:508:0:i2c_test	8	static
board.c:584:0:i2c_delay	8	static
board.c:556:0:sda_in	0	static
board.c:570:0:sda_out	0	static
board.c:596:0:CAN0_Callback	24	static
board.c:653:0:CAN1_Callback	24	static
board.c:710:0:CAN2_Callback	24	static
board.c:764:0:CAN3_Callback	24	static
board.c:818:0:CAN4_Callback	24	static
board.c:872:0:CAN5_Callback	24	static
board.c:926:0:get_can_data	0	static
board.c:936:0:can_main_ECU3	48	static
board.c:1458:0:ECU3_Data_Init	32	static
board.c:2223:0:clear_tx_buf	0	static
board.c:2232:0:clear_tx_ring	8	static
board.c:2254:0:can_send_txring	32	static
board.c:2282:0:can_transmit_txring	40	static
board.c:2241:0:can_tx_check	24	static
board.c:2331:0:DIN_TEST	8	static
board.c:2336:0:Digital_Write	0	static
board.c:2372:0:Digital_Read	0	static
board.c:2415:0:led_onoff	8	static
board.c:2497:0:ADC_Read	0	static
board.c:2538:0:Adc0EndOfChainNoti	8	static
board.c:2546:0:Adc1EndOfChainNoti	8	static
board.c:2553:0:Adc2EndOfChainNoti	8	static
board.c:2566:0:Adc_Read_ch	0	static
board.c:2574:0:tmr_delay	8	static
board.c:2589:0:Pit_Callback	16	static
board.c:2611:0:board_init	0	static
board.c:2621:0:Uart_Init	8	static
board.c:2656:0:UART0_RX_Callback	4	static
board.c:2673:0:UART2_RX_Callback	4	static
board.c:2690:0:UART10_RX_Callback	4	static
board.c:2706:0:UART13_RX_Callback	4	static
board.c:2722:0:UART1_RX_Callback	4	static
board.c:2738:0:UART9_RX_Callback	4	static
board.c:2756:0:Gvar_init	0	static
board.c:2776:0:register_bus_off_callback	8	static
board.c:2786:0:get_char	0	static
board.c:2799:0:put_char	16	static
board.c:2921:0:debug_printf	280	static
board.c:375:0:Lin_init	8	static
board.c:626:0:CAN0_ErrCallback	16	static
board.c:683:0:CAN1_ErrCallback	16	static
board.c:738:0:CAN2_ErrCallback	16	static
board.c:791:0:CAN3_ErrCallback	16	static
board.c:845:0:CAN4_ErrCallback	16	static
board.c:899:0:CAN5_ErrCallback	16	static
board.c:2425:0:Adc_Init	16	static
board.c:2807:0:get_line	16	static
board.c:2850:0:UART0_get_cmd	8	static
board.c:2941:0:setupCanTJA1153	72	static
board.c:1185:0:Can_Init_ECU3	24	static
