
Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:
Symbol table:

CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0) @0740a700
  Type: function definition analyzed
  Visibility: artificial
  References: bufferFreqs/25 (read)configuredCoreClock/29 (write)bufferFreqs/25 (read)configuredAipsPlatClock/30 (write)bufferFreqs/25 (read)configuredAipsSlowClock/31 (write)bufferFreqs/25 (read)configuredHseClock/32 (write)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (26801491 (estimated locally),0.23 per call) 
  Calls: 
NOT_UNDER_MCU_CONTROL_A.part.0/230 (NOT_UNDER_MCU_CONTROL_A.part.0) @0740a9a0
  Type: function definition analyzed
  Visibility: artificial
  References: clkState/27 (write)clkState/27 (write)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: NOT_UNDER_MCU_CONTROL_A/44 (536870912 (estimated locally),0.50 per call) 
  Calls: 
CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (CONFIG_ELEMENTS_MAPPINGS_01.part.0) @0740a000
  Type: function definition analyzed
  Visibility: artificial
  References: freqPointers/26 (write)config_clock/33 (read)freqPointers/26 (write)freqPointers/26 (write)freqPointers/26 (write)
  Referring: 
  Availability: local
  Function flags: count:118111598 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: CONFIG_ELEMENTS_MAPPINGS_01/42 (46707769 (estimated locally),1.00 per call) 
  Calls: 
*.LC1/228 (*.LC1) @068cbc18
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: 
  Referring: PCFS_PLL_PHI0_B/63 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
*.LC0/227 (*.LC0) @068cbb88
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: 
  Referring: PCFS_PLL_PHI0_B/63 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
pcfsCallbacks/226 (pcfsCallbacks) @07160288
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
selectorCallbacks/225 (selectorCallbacks) @071601b0
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
pllCallbacks/224 (pllCallbacks) @07160048
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
intOscCallbacks/223 (intOscCallbacks) @0715ef30
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
gateCallbacks/222 (gateCallbacks) @0715edc8
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
fracDivCallbacks/221 (fracDivCallbacks) @0715ec60
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
extOscCallbacks/220 (extOscCallbacks) @0715eb88
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
dividerTriggerCallbacks/219 (dividerTriggerCallbacks) @0715eab0
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
dividerCallbacks/218 (dividerCallbacks) @0715e9d8
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
cmuCallbacks/217 (cmuCallbacks) @0715e750
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
ClockTimeoutExpired/216 (ClockTimeoutExpired) @07154b60
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: CallbackDelay/77 (1073741824 (estimated locally),9.09 per call) 
  Calls: 
ClockStartTimeout/215 (ClockStartTimeout) @07154a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: CallbackDelay/77 (118111600 (estimated locally),1.00 per call) 
  Calls: 
bufferFreqEntriesCLKOUT_RUN_CLK.5132/214 (bufferFreqEntriesCLKOUT_RUN_CLK) @0715e318
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntriesCLKOUT_RUN_CLK.5131/213 (selectorEntriesCLKOUT_RUN_CLK) @0715e2d0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesQSPI_MEM_CLK.5130/212 (bufferFreqEntriesQSPI_MEM_CLK) @0715e288
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesLBIST_CLK.5129/211 (bufferFreqEntriesLBIST_CLK) @0715e240
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesDCM_CLK.5128/210 (bufferFreqEntriesDCM_CLK) @0715e1f8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesHSE_CLK.5127/209 (bufferFreqEntriesHSE_CLK) @0715e1b0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesAIPS_SLOW_CLK.5126/208 (bufferFreqEntriesAIPS_SLOW_CLK) @0715e168
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesAIPS_PLAT_CLK.5125/207 (bufferFreqEntriesAIPS_PLAT_CLK) @0715e120
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesCORE_CLK.5124/206 (bufferFreqEntriesCORE_CLK) @0715e0d8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesSCS_CLK.5123/205 (bufferFreqEntriesSCS_CLK) @0715e090
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntriesSCS_CLK.5122/204 (selectorEntriesSCS_CLK) @0715e048
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
convertValueToClockState.5133/203 (convertValueToClockState) @0715e000
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
get_TRACE_CLK_Frequency/202 (get_TRACE_CLK_Frequency) @0714ab60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_STM1_CLK_Frequency/201 (get_STM1_CLK_Frequency) @0714a620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_STMB_CLK_Frequency/200 (get_STMB_CLK_Frequency) @0714a0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_STM0_CLK_Frequency/199 (get_STM0_CLK_Frequency) @0714ad20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_STMA_CLK_Frequency/198 (get_STMA_CLK_Frequency) @0714aa80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_RTC0_CLK_Frequency/197 (get_RTC0_CLK_Frequency) @0714a7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_RTC_CLK_Frequency/196 (get_RTC_CLK_Frequency) @0714a540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_QSPI0_SFCK_CLK_Frequency/195 (get_QSPI0_SFCK_CLK_Frequency) @0714a2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_QSPI_SFCK_CLK_Frequency/194 (get_QSPI_SFCK_CLK_Frequency) @0714a000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLEXCAN5_CLK_Frequency/193 (get_FLEXCAN5_CLK_Frequency) @0713db60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLEXCAN4_CLK_Frequency/192 (get_FLEXCAN4_CLK_Frequency) @0713d620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLEXCAN3_CLK_Frequency/191 (get_FLEXCAN3_CLK_Frequency) @0713d0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLEXCANB_CLK_Frequency/190 (get_FLEXCANB_CLK_Frequency) @0713dd20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLEXCAN2_CLK_Frequency/189 (get_FLEXCAN2_CLK_Frequency) @0713da80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLEXCAN1_CLK_Frequency/188 (get_FLEXCAN1_CLK_Frequency) @0713d7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLEXCAN0_CLK_Frequency/187 (get_FLEXCAN0_CLK_Frequency) @0713d540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLEXCANA_CLK_Frequency/186 (get_FLEXCANA_CLK_Frequency) @0713d2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EMAC0_TX_CLK_Frequency/185 (get_EMAC0_TX_CLK_Frequency) @0713d000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EMAC_TX_CLK_Frequency/184 (get_EMAC_TX_CLK_Frequency) @07134b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EMAC0_TS_CLK_Frequency/183 (get_EMAC0_TS_CLK_Frequency) @07134620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EMAC_TS_CLK_Frequency/182 (get_EMAC_TS_CLK_Frequency) @071340e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EMAC0_RX_CLK_Frequency/181 (get_EMAC0_RX_CLK_Frequency) @07134d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EMAC_RX_CLK_Frequency/180 (get_EMAC_RX_CLK_Frequency) @07134a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_CLKOUT_STANDBY_CLK_Frequency/179 (get_CLKOUT_STANDBY_CLK_Frequency) @071347e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SWT1_CLK_Frequency/178 (get_SWT1_CLK_Frequency) @07134540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SWT0_CLK_Frequency/177 (get_SWT0_CLK_Frequency) @071342a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SIUL0_CLK_Frequency/176 (get_SIUL0_CLK_Frequency) @07134000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_QSPI0_TX_MEM_CLK_Frequency/175 (get_QSPI0_TX_MEM_CLK_Frequency) @07131b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_QSPI0_RAM_CLK_Frequency/174 (get_QSPI0_RAM_CLK_Frequency) @07131620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_DCM0_CLK_Frequency/173 (get_DCM0_CLK_Frequency) @071310e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SEMA42_CLK_Frequency/172 (get_SEMA42_CLK_Frequency) @07131d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_MSCM_CLK_Frequency/171 (get_MSCM_CLK_Frequency) @07131a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART8_CLK_Frequency/170 (get_LPUART8_CLK_Frequency) @071317e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART0_CLK_Frequency/169 (get_LPUART0_CLK_Frequency) @07131540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPSPI0_CLK_Frequency/168 (get_LPSPI0_CLK_Frequency) @071312a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_INTM_CLK_Frequency/167 (get_INTM_CLK_Frequency) @07131000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLEXIO0_CLK_Frequency/166 (get_FLEXIO0_CLK_Frequency) @0712eb60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_CRC0_CLK_Frequency/165 (get_CRC0_CLK_Frequency) @0712e620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_WKPU0_CLK_Frequency/164 (get_WKPU0_CLK_Frequency) @0712e0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_TSENSE0_CLK_Frequency/163 (get_TSENSE0_CLK_Frequency) @0712ed20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_TRGMUX0_CLK_Frequency/162 (get_TRGMUX0_CLK_Frequency) @0712ea80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_STCU0_CLK_Frequency/161 (get_STCU0_CLK_Frequency) @0712e7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SAI1_CLK_Frequency/160 (get_SAI1_CLK_Frequency) @0712e540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SAI0_CLK_Frequency/159 (get_SAI0_CLK_Frequency) @0712e2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_PIT2_CLK_Frequency/158 (get_PIT2_CLK_Frequency) @0712e000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_PIT1_CLK_Frequency/157 (get_PIT1_CLK_Frequency) @07127b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_PIT0_CLK_Frequency/156 (get_PIT0_CLK_Frequency) @07127620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_MUB_CLK_Frequency/155 (get_MUB_CLK_Frequency) @071270e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_MUA_CLK_Frequency/154 (get_MUA_CLK_Frequency) @07127d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART9_CLK_Frequency/153 (get_LPUART9_CLK_Frequency) @07127a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART7_CLK_Frequency/152 (get_LPUART7_CLK_Frequency) @071277e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART6_CLK_Frequency/151 (get_LPUART6_CLK_Frequency) @07127540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART5_CLK_Frequency/150 (get_LPUART5_CLK_Frequency) @071272a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART4_CLK_Frequency/149 (get_LPUART4_CLK_Frequency) @07127000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART3_CLK_Frequency/148 (get_LPUART3_CLK_Frequency) @07124b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART2_CLK_Frequency/147 (get_LPUART2_CLK_Frequency) @07124620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART1_CLK_Frequency/146 (get_LPUART1_CLK_Frequency) @071240e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART15_CLK_Frequency/145 (get_LPUART15_CLK_Frequency) @07124d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART14_CLK_Frequency/144 (get_LPUART14_CLK_Frequency) @07124a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART13_CLK_Frequency/143 (get_LPUART13_CLK_Frequency) @071247e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART12_CLK_Frequency/142 (get_LPUART12_CLK_Frequency) @07124540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART11_CLK_Frequency/141 (get_LPUART11_CLK_Frequency) @071242a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPUART10_CLK_Frequency/140 (get_LPUART10_CLK_Frequency) @07124000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPSPI5_CLK_Frequency/139 (get_LPSPI5_CLK_Frequency) @07121b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPSPI4_CLK_Frequency/138 (get_LPSPI4_CLK_Frequency) @07121620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPSPI3_CLK_Frequency/137 (get_LPSPI3_CLK_Frequency) @071210e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPSPI2_CLK_Frequency/136 (get_LPSPI2_CLK_Frequency) @07121d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPSPI1_CLK_Frequency/135 (get_LPSPI1_CLK_Frequency) @07121a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPI2C1_CLK_Frequency/134 (get_LPI2C1_CLK_Frequency) @071217e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LPI2C0_CLK_Frequency/133 (get_LPI2C0_CLK_Frequency) @07121540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_FLASH0_CLK_Frequency/132 (get_FLASH0_CLK_Frequency) @071212a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_ERM0_CLK_Frequency/131 (get_ERM0_CLK_Frequency) @07121000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EIM0_CLK_Frequency/130 (get_EIM0_CLK_Frequency) @0711eb60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_CMP2_CLK_Frequency/129 (get_CMP2_CLK_Frequency) @0711e620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_CMP1_CLK_Frequency/128 (get_CMP1_CLK_Frequency) @0711e0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_CMP0_CLK_Frequency/127 (get_CMP0_CLK_Frequency) @0711ed20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_TEMPSENSE_CLK_Frequency/126 (get_TEMPSENSE_CLK_Frequency) @0711ea80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_TCM_CM7_1_CLK_Frequency/125 (get_TCM_CM7_1_CLK_Frequency) @0711e7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_TCM_CM7_0_CLK_Frequency/124 (get_TCM_CM7_0_CLK_Frequency) @0711e540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LCU1_CLK_Frequency/123 (get_LCU1_CLK_Frequency) @0711e2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_LCU0_CLK_Frequency/122 (get_LCU0_CLK_Frequency) @0711e000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EMIOS2_CLK_Frequency/121 (get_EMIOS2_CLK_Frequency) @07118b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EMIOS1_CLK_Frequency/120 (get_EMIOS1_CLK_Frequency) @07118620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EMIOS0_CLK_Frequency/119 (get_EMIOS0_CLK_Frequency) @071180e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD9_CLK_Frequency/118 (get_EDMA0_TCD9_CLK_Frequency) @07118d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD8_CLK_Frequency/117 (get_EDMA0_TCD8_CLK_Frequency) @07118a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD7_CLK_Frequency/116 (get_EDMA0_TCD7_CLK_Frequency) @071187e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD6_CLK_Frequency/115 (get_EDMA0_TCD6_CLK_Frequency) @07118540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD5_CLK_Frequency/114 (get_EDMA0_TCD5_CLK_Frequency) @071182a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD4_CLK_Frequency/113 (get_EDMA0_TCD4_CLK_Frequency) @07118000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD3_CLK_Frequency/112 (get_EDMA0_TCD3_CLK_Frequency) @07116b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD31_CLK_Frequency/111 (get_EDMA0_TCD31_CLK_Frequency) @07116620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD30_CLK_Frequency/110 (get_EDMA0_TCD30_CLK_Frequency) @071160e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD2_CLK_Frequency/109 (get_EDMA0_TCD2_CLK_Frequency) @07116d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD29_CLK_Frequency/108 (get_EDMA0_TCD29_CLK_Frequency) @07116a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD28_CLK_Frequency/107 (get_EDMA0_TCD28_CLK_Frequency) @071167e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD27_CLK_Frequency/106 (get_EDMA0_TCD27_CLK_Frequency) @07116540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD26_CLK_Frequency/105 (get_EDMA0_TCD26_CLK_Frequency) @071162a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD25_CLK_Frequency/104 (get_EDMA0_TCD25_CLK_Frequency) @07116000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD24_CLK_Frequency/103 (get_EDMA0_TCD24_CLK_Frequency) @07113b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD23_CLK_Frequency/102 (get_EDMA0_TCD23_CLK_Frequency) @07113620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD22_CLK_Frequency/101 (get_EDMA0_TCD22_CLK_Frequency) @071130e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD21_CLK_Frequency/100 (get_EDMA0_TCD21_CLK_Frequency) @07113d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD20_CLK_Frequency/99 (get_EDMA0_TCD20_CLK_Frequency) @07113a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD1_CLK_Frequency/98 (get_EDMA0_TCD1_CLK_Frequency) @071137e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD19_CLK_Frequency/97 (get_EDMA0_TCD19_CLK_Frequency) @07113540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD18_CLK_Frequency/96 (get_EDMA0_TCD18_CLK_Frequency) @071132a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD17_CLK_Frequency/95 (get_EDMA0_TCD17_CLK_Frequency) @07113000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD16_CLK_Frequency/94 (get_EDMA0_TCD16_CLK_Frequency) @0710eb60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD15_CLK_Frequency/93 (get_EDMA0_TCD15_CLK_Frequency) @0710e620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD14_CLK_Frequency/92 (get_EDMA0_TCD14_CLK_Frequency) @0710e0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD13_CLK_Frequency/91 (get_EDMA0_TCD13_CLK_Frequency) @0710ed20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD12_CLK_Frequency/90 (get_EDMA0_TCD12_CLK_Frequency) @0710ea80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD11_CLK_Frequency/89 (get_EDMA0_TCD11_CLK_Frequency) @0710e7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD10_CLK_Frequency/88 (get_EDMA0_TCD10_CLK_Frequency) @0710e540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_TCD0_CLK_Frequency/87 (get_EDMA0_TCD0_CLK_Frequency) @0710e2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_EDMA0_CLK_Frequency/86 (get_EDMA0_CLK_Frequency) @0710e000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_DMAMUX1_CLK_Frequency/85 (get_DMAMUX1_CLK_Frequency) @07108a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_DMAMUX0_CLK_Frequency/84 (get_DMAMUX0_CLK_Frequency) @07108540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_BCTU0_CLK_Frequency/83 (get_BCTU0_CLK_Frequency) @07108ee0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_ADC2_CLK_Frequency/82 (get_ADC2_CLK_Frequency) @07108c40
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_ADC1_CLK_Frequency/81 (get_ADC1_CLK_Frequency) @071089a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_ADC0_CLK_Frequency/80 (get_ADC0_CLK_Frequency) @07108700
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
consumerClockCallbacks/79 (consumerClockCallbacks) @07107240
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: get_ADC0_CLK_Frequency/80 (addr)get_ADC1_CLK_Frequency/81 (addr)get_ADC2_CLK_Frequency/82 (addr)get_BCTU0_CLK_Frequency/83 (addr)get_CLKOUT_STANDBY_CLK_Frequency/179 (addr)get_CMP0_CLK_Frequency/127 (addr)get_CMP1_CLK_Frequency/128 (addr)get_CMP2_CLK_Frequency/129 (addr)get_CRC0_CLK_Frequency/165 (addr)get_DCM0_CLK_Frequency/173 (addr)get_DMAMUX0_CLK_Frequency/84 (addr)get_DMAMUX1_CLK_Frequency/85 (addr)get_EDMA0_CLK_Frequency/86 (addr)get_EDMA0_TCD0_CLK_Frequency/87 (addr)get_EDMA0_TCD10_CLK_Frequency/88 (addr)get_EDMA0_TCD11_CLK_Frequency/89 (addr)get_EDMA0_TCD12_CLK_Frequency/90 (addr)get_EDMA0_TCD13_CLK_Frequency/91 (addr)get_EDMA0_TCD14_CLK_Frequency/92 (addr)get_EDMA0_TCD15_CLK_Frequency/93 (addr)get_EDMA0_TCD16_CLK_Frequency/94 (addr)get_EDMA0_TCD17_CLK_Frequency/95 (addr)get_EDMA0_TCD18_CLK_Frequency/96 (addr)get_EDMA0_TCD19_CLK_Frequency/97 (addr)get_EDMA0_TCD1_CLK_Frequency/98 (addr)get_EDMA0_TCD20_CLK_Frequency/99 (addr)get_EDMA0_TCD21_CLK_Frequency/100 (addr)get_EDMA0_TCD22_CLK_Frequency/101 (addr)get_EDMA0_TCD23_CLK_Frequency/102 (addr)get_EDMA0_TCD24_CLK_Frequency/103 (addr)get_EDMA0_TCD25_CLK_Frequency/104 (addr)get_EDMA0_TCD26_CLK_Frequency/105 (addr)get_EDMA0_TCD27_CLK_Frequency/106 (addr)get_EDMA0_TCD28_CLK_Frequency/107 (addr)get_EDMA0_TCD29_CLK_Frequency/108 (addr)get_EDMA0_TCD2_CLK_Frequency/109 (addr)get_EDMA0_TCD30_CLK_Frequency/110 (addr)get_EDMA0_TCD31_CLK_Frequency/111 (addr)get_EDMA0_TCD3_CLK_Frequency/112 (addr)get_EDMA0_TCD4_CLK_Frequency/113 (addr)get_EDMA0_TCD5_CLK_Frequency/114 (addr)get_EDMA0_TCD6_CLK_Frequency/115 (addr)get_EDMA0_TCD7_CLK_Frequency/116 (addr)get_EDMA0_TCD8_CLK_Frequency/117 (addr)get_EDMA0_TCD9_CLK_Frequency/118 (addr)get_EIM0_CLK_Frequency/130 (addr)get_EMAC_RX_CLK_Frequency/180 (addr)get_EMAC0_RX_CLK_Frequency/181 (addr)get_EMAC_TS_CLK_Frequency/182 (addr)get_EMAC0_TS_CLK_Frequency/183 (addr)get_EMAC_TX_CLK_Frequency/184 (addr)get_EMAC0_TX_CLK_Frequency/185 (addr)get_EMIOS0_CLK_Frequency/119 (addr)get_EMIOS1_CLK_Frequency/120 (addr)get_EMIOS2_CLK_Frequency/121 (addr)get_ERM0_CLK_Frequency/131 (addr)get_FLASH0_CLK_Frequency/132 (addr)get_FLEXCANA_CLK_Frequency/186 (addr)get_FLEXCAN0_CLK_Frequency/187 (addr)get_FLEXCAN1_CLK_Frequency/188 (addr)get_FLEXCAN2_CLK_Frequency/189 (addr)get_FLEXCANB_CLK_Frequency/190 (addr)get_FLEXCAN3_CLK_Frequency/191 (addr)get_FLEXCAN4_CLK_Frequency/192 (addr)get_FLEXCAN5_CLK_Frequency/193 (addr)get_FLEXIO0_CLK_Frequency/166 (addr)get_INTM_CLK_Frequency/167 (addr)get_LCU0_CLK_Frequency/122 (addr)get_LCU1_CLK_Frequency/123 (addr)get_LPI2C0_CLK_Frequency/133 (addr)get_LPI2C1_CLK_Frequency/134 (addr)get_LPSPI0_CLK_Frequency/168 (addr)get_LPSPI1_CLK_Frequency/135 (addr)get_LPSPI2_CLK_Frequency/136 (addr)get_LPSPI3_CLK_Frequency/137 (addr)get_LPSPI4_CLK_Frequency/138 (addr)get_LPSPI5_CLK_Frequency/139 (addr)get_LPUART0_CLK_Frequency/169 (addr)get_LPUART10_CLK_Frequency/140 (addr)get_LPUART11_CLK_Frequency/141 (addr)get_LPUART12_CLK_Frequency/142 (addr)get_LPUART13_CLK_Frequency/143 (addr)get_LPUART14_CLK_Frequency/144 (addr)get_LPUART15_CLK_Frequency/145 (addr)get_LPUART1_CLK_Frequency/146 (addr)get_LPUART2_CLK_Frequency/147 (addr)get_LPUART3_CLK_Frequency/148 (addr)get_LPUART4_CLK_Frequency/149 (addr)get_LPUART5_CLK_Frequency/150 (addr)get_LPUART6_CLK_Frequency/151 (addr)get_LPUART7_CLK_Frequency/152 (addr)get_LPUART8_CLK_Frequency/170 (addr)get_LPUART9_CLK_Frequency/153 (addr)get_MSCM_CLK_Frequency/171 (addr)get_MUA_CLK_Frequency/154 (addr)get_MUB_CLK_Frequency/155 (addr)get_PIT0_CLK_Frequency/156 (addr)get_PIT1_CLK_Frequency/157 (addr)get_PIT2_CLK_Frequency/158 (addr)get_QSPI0_RAM_CLK_Frequency/174 (addr)get_QSPI_SFCK_CLK_Frequency/194 (addr)get_QSPI0_SFCK_CLK_Frequency/195 (addr)get_QSPI0_TX_MEM_CLK_Frequency/175 (addr)get_RTC_CLK_Frequency/196 (addr)get_RTC0_CLK_Frequency/197 (addr)get_SAI0_CLK_Frequency/159 (addr)get_SAI1_CLK_Frequency/160 (addr)get_SEMA42_CLK_Frequency/172 (addr)get_SIUL0_CLK_Frequency/176 (addr)get_STCU0_CLK_Frequency/161 (addr)get_STMA_CLK_Frequency/198 (addr)get_STM0_CLK_Frequency/199 (addr)get_STMB_CLK_Frequency/200 (addr)get_STM1_CLK_Frequency/201 (addr)get_SWT0_CLK_Frequency/177 (addr)get_SWT1_CLK_Frequency/178 (addr)get_TCM_CM7_0_CLK_Frequency/124 (addr)get_TCM_CM7_1_CLK_Frequency/125 (addr)get_TEMPSENSE_CLK_Frequency/126 (addr)get_TRACE_CLK_Frequency/202 (addr)get_TRGMUX0_CLK_Frequency/162 (addr)get_TSENSE0_CLK_Frequency/163 (addr)get_WKPU0_CLK_Frequency/164 (addr)
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
calcFreqCallbacks/78 (calcFreqCallbacks) @07054ea0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: CONFIG_ELEMENTS_MAPPINGS_01/42 (addr)CONFIG_ELEMENTS_MAPPINGS_02/43 (addr)NOT_UNDER_MCU_CONTROL_A/44 (addr)NOT_UNDER_MCU_CONTROL_B/45 (addr)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (addr)PLL_A/47 (addr)PLL_B/48 (addr)PLL_C/49 (addr)IntegerDividers_A/50 (addr)IntegerDividers_B/51 (addr)IntegerDividers_C/52 (addr)IntegerDividers_D/53 (addr)IntegerDividers_E/54 (addr)IntegerDividers_F/55 (addr)IntegerDividers_G/56 (addr)IntegerDividers_H/57 (addr)IntegerDividers_I/58 (addr)IntegerDividers_J/59 (addr)IntegerDividers_K/60 (addr)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (addr)PCFS_PLL_PHI0_A/62 (addr)PCFS_PLL_PHI0_B/63 (addr)PCFS_PLL_PHI0_C/64 (addr)PCFS_PLL_PHI0_D/65 (addr)PCFS_PLL_PHI0_E/66 (addr)CMU_FXOSC_CLK_A/67 (addr)CMU_FXOSC_CLK_B/68 (addr)CMU_CORE_CLK_A/69 (addr)CMU_CORE_CLK_B/70 (addr)CMU_AIPS_PLAT_CLK_A/71 (addr)CMU_AIPS_PLAT_CLK_B/72 (addr)CMU_HSE_CLK_A/73 (addr)CMU_HSE_CLK_B/74 (addr)CallEmptyCallbacks/76 (addr)CallbackDelay/77 (addr)
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
CallbackDelay/77 (CallbackDelay) @070aa460
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:118111600 (estimated locally) body optimize_size
  Called by: 
  Calls: ClockTimeoutExpired/216 (1073741824 (estimated locally),9.09 per call) ClockStartTimeout/215 (118111600 (estimated locally),1.00 per call) 
CallEmptyCallbacks/76 (CallEmptyCallbacks) @070aa1c0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuCallbacks/217 (read)cmuCallbacks/217 (read)cmuCallbacks/217 (read)cmuCallbacks/217 (read)dividerCallbacks/218 (read)dividerTriggerCallbacks/219 (read)extOscCallbacks/220 (read)fracDivCallbacks/221 (read)fracDivCallbacks/221 (read)gateCallbacks/222 (read)gateCallbacks/222 (read)intOscCallbacks/223 (read)pllCallbacks/224 (read)pllCallbacks/224 (read)selectorCallbacks/225 (read)pcfsCallbacks/226 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
McMeEnterKey/75 (McMeEnterKey) @070a2e00
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_HSE_CLK_B/74 (CMU_HSE_CLK_B) @070a2d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_HSE_CLK_A/73 (CMU_HSE_CLK_A) @070a2a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)configuredHseClock/32 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_AIPS_PLAT_CLK_B/72 (CMU_AIPS_PLAT_CLK_B) @070a27e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_AIPS_PLAT_CLK_A/71 (CMU_AIPS_PLAT_CLK_A) @070a2540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)configuredAipsPlatClock/30 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_CORE_CLK_B/70 (CMU_CORE_CLK_B) @070a22a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_CORE_CLK_A/69 (CMU_CORE_CLK_A) @070a2000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)configuredCoreClock/29 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_FXOSC_CLK_B/68 (CMU_FXOSC_CLK_B) @07056d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_FXOSC_CLK_A/67 (CMU_FXOSC_CLK_A) @07056a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_E/66 (PCFS_PLL_PHI0_E) @070567e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)pcfsEntries/34 (write)pcfsEntries/34 (write)pcfsEntries/34 (write)pcfsEntries/34 (write)pcfsEntries/34 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_D/65 (PCFS_PLL_PHI0_D) @07056540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:118111600 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_C/64 (PCFS_PLL_PHI0_C) @070562a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:118111600 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_B/63 (PCFS_PLL_PHI0_B) @07056000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: *.LC0/227 (read)*.LC1/228 (read)tmpData/28 (read)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:357985524 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_A/62 (PCFS_PLL_PHI0_A) @07048d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: pcfsEntries/34 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS) @07048a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: config_clock/33 (read)bufferFreqs/25 (read)configuredCoreClock/29 (write)bufferFreqs/25 (read)configuredAipsPlatClock/30 (write)bufferFreqs/25 (read)configuredAipsSlowClock/31 (write)bufferFreqs/25 (read)configuredHseClock/32 (write)configuredCoreClock/29 (write)configuredAipsPlatClock/30 (write)configuredAipsSlowClock/31 (write)configuredHseClock/32 (write)configuredCoreClock/29 (write)configuredAipsPlatClock/30 (write)configuredAipsSlowClock/31 (write)configuredHseClock/32 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:114863532 (estimated locally) body optimize_size
  Called by: 
  Calls: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (26801491 (estimated locally),0.23 per call) 
IntegerDividers_K/60 (IntegerDividers_K) @070487e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_J/59 (IntegerDividers_J) @07048540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_I/58 (IntegerDividers_I) @070482a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_H/57 (IntegerDividers_H) @07048000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_G/56 (IntegerDividers_G) @06ff0d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_F/55 (IntegerDividers_F) @06ff0a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (read)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_E/54 (IntegerDividers_E) @06ff07e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_D/53 (IntegerDividers_D) @06ff0540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_C/52 (IntegerDividers_C) @06ff02a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_B/51 (IntegerDividers_B) @06ff0000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_A/50 (IntegerDividers_A) @06fe5d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PLL_C/49 (PLL_C) @06fe5a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PLL_B/48 (PLL_B) @06fe57e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (write)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PLL_A/47 (PLL_A) @06fe5540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: bufferFreqs/25 (read)tmpData/28 (write)freqPointers/26 (read)config_clock/33 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS) @06fe52a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (write)freqPointers/26 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (write)freqPointers/26 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
NOT_UNDER_MCU_CONTROL_B/45 (NOT_UNDER_MCU_CONTROL_B) @06fe5000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)clkState/27 (write)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)clkState/27 (write)clkState/27 (write)clkState/27 (write)freqPointers/26 (read)selectorEntryIndex/23 (read)clkState/27 (write)freqPointers/26 (read)selectorEntryIndex/23 (read)clkState/27 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
NOT_UNDER_MCU_CONTROL_A/44 (NOT_UNDER_MCU_CONTROL_A) @06f8cee0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: clkState/27 (write)freqPointers/26 (read)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)freqPointers/26 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: NOT_UNDER_MCU_CONTROL_A.part.0/230 (536870912 (estimated locally),0.50 per call) 
CONFIG_ELEMENTS_MAPPINGS_02/43 (CONFIG_ELEMENTS_MAPPINGS_02) @06f8cc40
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (write)config_clock/33 (read)freqPointers/26 (write)freqPointers/26 (write)pcfsEntries/34 (read)pcfsEntries/34 (write)cmuEntries/35 (read)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:7299031 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CONFIG_ELEMENTS_MAPPINGS_01/42 (CONFIG_ELEMENTS_MAPPINGS_01) @06f8c9a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:46707770 (estimated locally) body optimize_size
  Called by: 
  Calls: CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (46707769 (estimated locally),1.00 per call) 
UpdateFrequencies/41 (UpdateFrequencies) @06f8c700
  Type: function definition analyzed
  Visibility: externally_visible public
  References: clkState/27 (read)freqPointers/26 (write)clkState/27 (read)freqPointers/26 (write)clkState/27 (read)clkState/27 (read)freqPointers/26 (write)clkState/27 (read)freqPointers/26 (write)freqPointers/26 (write)clkState/27 (read)convertValueToClockState.5133/203 (read)clkState/27 (write)clkState/27 (read)convertValueToClockState.5133/203 (read)clkState/27 (write)freqPointers/26 (write)freqPointers/26 (write)clkState/27 (read)selectorEntriesSCS_CLK.5122/204 (read)clkState/27 (read)bufferFreqEntriesSCS_CLK.5123/205 (read)freqPointers/26 (write)bufferFreqEntriesCORE_CLK.5124/206 (read)freqPointers/26 (write)bufferFreqEntriesAIPS_PLAT_CLK.5125/207 (read)freqPointers/26 (write)bufferFreqEntriesAIPS_SLOW_CLK.5126/208 (read)freqPointers/26 (write)bufferFreqEntriesHSE_CLK.5127/209 (read)freqPointers/26 (write)bufferFreqEntriesDCM_CLK.5128/210 (read)freqPointers/26 (write)bufferFreqEntriesLBIST_CLK.5129/211 (read)freqPointers/26 (write)bufferFreqEntriesQSPI_MEM_CLK.5130/212 (read)freqPointers/26 (write)selectorEntryIndex/23 (read)clkState/27 (write)selectorEntriesCLKOUT_RUN_CLK.5131/213 (read)clkState/27 (read)bufferFreqEntriesCLKOUT_RUN_CLK.5132/214 (read)freqPointers/26 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
GetProducerClockFreq/40 (GetProducerClockFreq) @06f8c000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
SpecificPlatformInitClock/39 (SpecificPlatformInitClock) @06f87a80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: config_clock/33 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
SpecificPeripheralClockInitialization/38 (SpecificPeripheralClockInitialization) @06f87ee0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
GetClockState/37 (GetClockState) @06f87c40
  Type: function definition analyzed
  Visibility: externally_visible public
  References: clkState/27 (read)clkState/27 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
UpdateClockState/36 (UpdateClockState) @06f879a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: clkState/27 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
cmuEntries/35 (cmuEntries) @06f84870
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: CMU_FXOSC_CLK_A/67 (write)CMU_AIPS_PLAT_CLK_B/72 (read)CMU_AIPS_PLAT_CLK_B/72 (write)CMU_AIPS_PLAT_CLK_B/72 (write)CMU_HSE_CLK_A/73 (read)CMU_AIPS_PLAT_CLK_A/71 (read)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (read)CMU_CORE_CLK_B/70 (read)CMU_CORE_CLK_B/70 (write)CMU_CORE_CLK_B/70 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CMU_CORE_CLK_A/69 (read)CMU_CORE_CLK_A/69 (write)CMU_CORE_CLK_A/69 (write)CMU_HSE_CLK_A/73 (write)CMU_FXOSC_CLK_B/68 (read)CMU_FXOSC_CLK_B/68 (write)CMU_FXOSC_CLK_B/68 (write)CMU_HSE_CLK_A/73 (write)CMU_FXOSC_CLK_A/67 (read)CMU_FXOSC_CLK_A/67 (write)CMU_HSE_CLK_B/74 (read)CMU_HSE_CLK_B/74 (write)CMU_HSE_CLK_B/74 (write)
  Availability: available
  Varpool flags: initialized
pcfsEntries/34 (pcfsEntries) @06f84708
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (read)PCFS_PLL_PHI0_A/62 (read)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)
  Availability: available
  Varpool flags: initialized
config_clock/33 (config_clock) @06f84678
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CMU_AIPS_PLAT_CLK_A/71 (read)CMU_CORE_CLK_A/69 (read)CMU_FXOSC_CLK_A/67 (read)PCFS_PLL_PHI0_A/62 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)IntegerDividers_K/60 (read)IntegerDividers_J/59 (read)IntegerDividers_J/59 (read)IntegerDividers_J/59 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)IntegerDividers_F/55 (read)IntegerDividers_F/55 (read)IntegerDividers_F/55 (read)IntegerDividers_E/54 (read)IntegerDividers_E/54 (read)IntegerDividers_E/54 (read)IntegerDividers_D/53 (read)IntegerDividers_D/53 (read)IntegerDividers_D/53 (read)IntegerDividers_C/52 (read)IntegerDividers_C/52 (read)IntegerDividers_C/52 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)PLL_A/47 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (read)IntegerDividers_K/60 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)CONFIG_ELEMENTS_MAPPINGS_02/43 (read)IntegerDividers_K/60 (read)CMU_HSE_CLK_A/73 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)SpecificPlatformInitClock/39 (write)
  Availability: available
  Varpool flags: initialized
configuredHseClock/32 (configuredHseClock) @06f84480
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_HSE_CLK_A/73 (read)
  Availability: available
  Varpool flags: initialized
configuredAipsSlowClock/31 (configuredAipsSlowClock) @06f843f0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CMU_CORE_CLK_A/69 (read)CMU_FXOSC_CLK_A/67 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_AIPS_PLAT_CLK_A/71 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_HSE_CLK_A/73 (read)
  Availability: available
  Varpool flags: initialized
configuredAipsPlatClock/30 (configuredAipsPlatClock) @06f84360
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_AIPS_PLAT_CLK_A/71 (read)
  Availability: available
  Varpool flags: initialized
configuredCoreClock/29 (configuredCoreClock) @06f842d0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_CORE_CLK_A/69 (read)
  Availability: available
  Varpool flags: initialized
tmpData/28 (tmpData) @06f84240
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CMU_AIPS_PLAT_CLK_B/72 (read)CMU_AIPS_PLAT_CLK_B/72 (read)CMU_CORE_CLK_A/69 (write)CMU_CORE_CLK_A/69 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_CORE_CLK_B/70 (read)CMU_CORE_CLK_B/70 (read)CMU_FXOSC_CLK_A/67 (write)CMU_FXOSC_CLK_A/67 (write)CMU_CORE_CLK_A/69 (write)CMU_CORE_CLK_A/69 (write)CMU_FXOSC_CLK_B/68 (read)CMU_FXOSC_CLK_B/68 (read)PCFS_PLL_PHI0_E/66 (read)PCFS_PLL_PHI0_E/66 (read)CMU_FXOSC_CLK_A/67 (write)CMU_FXOSC_CLK_A/67 (write)PCFS_PLL_PHI0_E/66 (read)PCFS_PLL_PHI0_E/66 (read)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_D/65 (write)PCFS_PLL_PHI0_D/65 (write)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_C/64 (read)PCFS_PLL_PHI0_C/64 (write)PCFS_PLL_PHI0_C/64 (write)PCFS_PLL_PHI0_C/64 (write)PCFS_PLL_PHI0_C/64 (read)PLL_A/47 (write)PCFS_PLL_PHI0_C/64 (read)PCFS_PLL_PHI0_C/64 (read)PCFS_PLL_PHI0_D/65 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_AIPS_PLAT_CLK_A/71 (write)PLL_C/49 (read)PLL_C/49 (read)PLL_C/49 (read)PLL_C/49 (read)PLL_C/49 (read)PCFS_PLL_PHI0_A/62 (write)PCFS_PLL_PHI0_A/62 (write)PCFS_PLL_PHI0_B/63 (read)PCFS_PLL_PHI0_B/63 (write)CMU_HSE_CLK_A/73 (write)CMU_HSE_CLK_A/73 (write)PLL_B/48 (read)PLL_B/48 (write)PLL_B/48 (read)PLL_C/49 (read)PLL_C/49 (read)PCFS_PLL_PHI0_A/62 (write)PCFS_PLL_PHI0_A/62 (write)PLL_C/49 (read)PLL_C/49 (write)PLL_B/48 (write)PLL_B/48 (write)PLL_B/48 (read)PLL_B/48 (write)PLL_A/47 (read)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (read)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_D/65 (write)PCFS_PLL_PHI0_E/66 (read)CMU_HSE_CLK_A/73 (write)CMU_HSE_CLK_A/73 (write)CMU_HSE_CLK_B/74 (read)CMU_HSE_CLK_B/74 (read)
  Availability: available
  Varpool flags:
clkState/27 (clkState) @06f841b0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_A.part.0/230 (write)NOT_UNDER_MCU_CONTROL_A.part.0/230 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)UpdateClockState/36 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)GetClockState/37 (read)GetClockState/37 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags:
freqPointers/26 (freqPointers) @06f84120
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: get_STM1_CLK_Frequency/201 (read)get_EDMA0_TCD0_CLK_Frequency/87 (read)get_EDMA0_CLK_Frequency/86 (read)get_DMAMUX1_CLK_Frequency/85 (read)get_DMAMUX0_CLK_Frequency/84 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_EMAC0_TX_CLK_Frequency/185 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_EIM0_CLK_Frequency/130 (read)get_CMP2_CLK_Frequency/129 (read)get_EMIOS0_CLK_Frequency/119 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)get_SWT1_CLK_Frequency/178 (read)get_CMP1_CLK_Frequency/128 (read)get_EDMA0_TCD7_CLK_Frequency/116 (read)get_TRACE_CLK_Frequency/202 (read)get_EDMA0_TCD6_CLK_Frequency/115 (read)get_EDMA0_TCD5_CLK_Frequency/114 (read)get_EDMA0_TCD4_CLK_Frequency/113 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)get_EDMA0_TCD3_CLK_Frequency/112 (read)get_EDMA0_TCD31_CLK_Frequency/111 (read)get_EDMA0_TCD30_CLK_Frequency/110 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)get_EDMA0_TCD2_CLK_Frequency/109 (read)get_EDMA0_TCD29_CLK_Frequency/108 (read)get_EDMA0_TCD28_CLK_Frequency/107 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)get_EDMA0_TCD27_CLK_Frequency/106 (read)get_EDMA0_TCD26_CLK_Frequency/105 (read)get_EDMA0_TCD25_CLK_Frequency/104 (read)get_EDMA0_TCD24_CLK_Frequency/103 (read)IntegerDividers_F/55 (read)IntegerDividers_F/55 (read)get_EDMA0_TCD23_CLK_Frequency/102 (read)get_EDMA0_TCD22_CLK_Frequency/101 (read)get_EDMA0_TCD21_CLK_Frequency/100 (read)get_EDMA0_TCD20_CLK_Frequency/99 (read)get_EDMA0_TCD1_CLK_Frequency/98 (read)IntegerDividers_E/54 (read)get_EDMA0_TCD19_CLK_Frequency/97 (read)get_EDMA0_TCD18_CLK_Frequency/96 (read)get_EDMA0_TCD17_CLK_Frequency/95 (read)get_EDMA0_TCD16_CLK_Frequency/94 (read)get_EDMA0_TCD15_CLK_Frequency/93 (read)IntegerDividers_D/53 (read)get_EDMA0_TCD14_CLK_Frequency/92 (read)get_EDMA0_TCD13_CLK_Frequency/91 (read)get_EDMA0_TCD12_CLK_Frequency/90 (read)get_EDMA0_TCD11_CLK_Frequency/89 (read)IntegerDividers_C/52 (read)IntegerDividers_C/52 (read)get_EDMA0_TCD10_CLK_Frequency/88 (read)get_FLEXCANB_CLK_Frequency/190 (read)get_FLEXCAN2_CLK_Frequency/189 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)get_FLEXCAN1_CLK_Frequency/188 (read)get_FLEXCAN0_CLK_Frequency/187 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)PLL_A/47 (read)get_EDMA0_TCD9_CLK_Frequency/118 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)NOT_UNDER_MCU_CONTROL_B/45 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)get_BCTU0_CLK_Frequency/83 (read)get_ADC2_CLK_Frequency/82 (read)get_MSCM_CLK_Frequency/171 (read)get_TSENSE0_CLK_Frequency/163 (read)get_CMP0_CLK_Frequency/127 (read)get_TEMPSENSE_CLK_Frequency/126 (read)get_TCM_CM7_1_CLK_Frequency/125 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)NOT_UNDER_MCU_CONTROL_A/44 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)get_EDMA0_TCD8_CLK_Frequency/117 (read)get_EMAC0_TS_CLK_Frequency/183 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)CONFIG_ELEMENTS_MAPPINGS_01/42 (write)get_EMAC_TS_CLK_Frequency/182 (read)get_EMAC0_RX_CLK_Frequency/181 (read)GetProducerClockFreq/40 (read)get_SWT0_CLK_Frequency/177 (read)get_ADC1_CLK_Frequency/81 (read)get_ADC0_CLK_Frequency/80 (read)IntegerDividers_K/60 (read)IntegerDividers_J/59 (read)get_TRGMUX0_CLK_Frequency/162 (read)get_STCU0_CLK_Frequency/161 (read)get_SAI1_CLK_Frequency/160 (read)get_STMB_CLK_Frequency/200 (read)get_TCM_CM7_0_CLK_Frequency/124 (read)get_LCU1_CLK_Frequency/123 (read)get_LCU0_CLK_Frequency/122 (read)get_SIUL0_CLK_Frequency/176 (read)get_QSPI0_TX_MEM_CLK_Frequency/175 (read)get_STM0_CLK_Frequency/199 (read)get_STMA_CLK_Frequency/198 (read)get_QSPI0_SFCK_CLK_Frequency/195 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_SAI0_CLK_Frequency/159 (read)get_QSPI0_RAM_CLK_Frequency/174 (read)get_LPUART8_CLK_Frequency/170 (read)get_PIT2_CLK_Frequency/158 (read)get_PIT1_CLK_Frequency/157 (read)get_DCM0_CLK_Frequency/173 (read)get_FLEXCAN5_CLK_Frequency/193 (read)get_FLEXCAN4_CLK_Frequency/192 (read)get_SEMA42_CLK_Frequency/172 (read)get_PIT0_CLK_Frequency/156 (read)get_MUB_CLK_Frequency/155 (read)get_MUA_CLK_Frequency/154 (read)get_LPUART9_CLK_Frequency/153 (read)get_LPUART7_CLK_Frequency/152 (read)get_LPUART0_CLK_Frequency/169 (read)get_LPUART6_CLK_Frequency/151 (read)get_LPSPI0_CLK_Frequency/168 (read)get_LPUART5_CLK_Frequency/150 (read)get_LPUART4_CLK_Frequency/149 (read)get_LPUART3_CLK_Frequency/148 (read)get_LPUART2_CLK_Frequency/147 (read)get_LPUART1_CLK_Frequency/146 (read)get_LPUART15_CLK_Frequency/145 (read)get_LPUART14_CLK_Frequency/144 (read)get_LPUART13_CLK_Frequency/143 (read)get_LPUART12_CLK_Frequency/142 (read)get_LPUART11_CLK_Frequency/141 (read)get_LPUART10_CLK_Frequency/140 (read)get_LPSPI5_CLK_Frequency/139 (read)get_LPSPI4_CLK_Frequency/138 (read)get_INTM_CLK_Frequency/167 (read)get_LPSPI3_CLK_Frequency/137 (read)get_LPSPI2_CLK_Frequency/136 (read)get_LPSPI1_CLK_Frequency/135 (read)get_LPI2C1_CLK_Frequency/134 (read)get_LPI2C0_CLK_Frequency/133 (read)get_FLEXIO0_CLK_Frequency/166 (read)get_FLASH0_CLK_Frequency/132 (read)get_ERM0_CLK_Frequency/131 (read)get_EMIOS2_CLK_Frequency/121 (read)get_EMIOS1_CLK_Frequency/120 (read)get_CRC0_CLK_Frequency/165 (read)get_WKPU0_CLK_Frequency/164 (read)get_FLEXCAN3_CLK_Frequency/191 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)
  Availability: available
  Varpool flags:
bufferFreqs/25 (bufferFreqs) @06f84090
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: get_STM1_CLK_Frequency/201 (read)CMU_CORE_CLK_A/69 (read)CMU_FXOSC_CLK_A/67 (read)PCFS_PLL_PHI0_A/62 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)IntegerDividers_K/60 (write)IntegerDividers_K/60 (write)IntegerDividers_J/59 (write)IntegerDividers_J/59 (write)IntegerDividers_J/59 (read)IntegerDividers_J/59 (write)IntegerDividers_J/59 (write)IntegerDividers_J/59 (read)IntegerDividers_J/59 (write)IntegerDividers_J/59 (write)IntegerDividers_I/58 (read)IntegerDividers_I/58 (write)IntegerDividers_I/58 (write)IntegerDividers_I/58 (read)IntegerDividers_I/58 (write)IntegerDividers_I/58 (write)IntegerDividers_I/58 (read)IntegerDividers_I/58 (write)IntegerDividers_I/58 (write)IntegerDividers_H/57 (read)IntegerDividers_H/57 (write)IntegerDividers_H/57 (write)IntegerDividers_H/57 (read)IntegerDividers_H/57 (write)IntegerDividers_H/57 (write)IntegerDividers_H/57 (read)IntegerDividers_H/57 (write)IntegerDividers_H/57 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (write)IntegerDividers_G/56 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (write)IntegerDividers_G/56 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (write)IntegerDividers_G/56 (write)IntegerDividers_F/55 (write)IntegerDividers_F/55 (write)IntegerDividers_F/55 (read)IntegerDividers_F/55 (write)IntegerDividers_F/55 (write)IntegerDividers_F/55 (read)IntegerDividers_F/55 (write)IntegerDividers_F/55 (read)IntegerDividers_F/55 (write)IntegerDividers_E/54 (read)IntegerDividers_E/54 (write)IntegerDividers_E/54 (write)IntegerDividers_E/54 (read)IntegerDividers_E/54 (write)IntegerDividers_E/54 (write)IntegerDividers_E/54 (read)IntegerDividers_E/54 (write)IntegerDividers_E/54 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IntegerDividers_D/53 (read)IntegerDividers_D/53 (write)IntegerDividers_D/53 (write)IntegerDividers_D/53 (read)IntegerDividers_D/53 (write)IntegerDividers_D/53 (write)IntegerDividers_D/53 (read)IntegerDividers_D/53 (write)IntegerDividers_D/53 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (write)IntegerDividers_C/52 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (write)IntegerDividers_C/52 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (write)IntegerDividers_C/52 (write)IntegerDividers_B/51 (read)IntegerDividers_B/51 (write)IntegerDividers_B/51 (write)IntegerDividers_B/51 (read)IntegerDividers_B/51 (write)IntegerDividers_B/51 (write)IntegerDividers_B/51 (read)IntegerDividers_B/51 (write)IntegerDividers_B/51 (write)IntegerDividers_A/50 (read)IntegerDividers_A/50 (write)IntegerDividers_A/50 (write)IntegerDividers_A/50 (read)IntegerDividers_A/50 (write)IntegerDividers_A/50 (write)IntegerDividers_A/50 (read)IntegerDividers_A/50 (write)IntegerDividers_A/50 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)PLL_C/49 (write)IntegerDividers_J/59 (read)IntegerDividers_K/60 (write)IntegerDividers_K/60 (write)IntegerDividers_K/60 (read)IntegerDividers_K/60 (write)IntegerDividers_K/60 (write)IntegerDividers_K/60 (read)PCFS_PLL_PHI0_A/62 (read)PLL_A/47 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)get_TRACE_CLK_Frequency/202 (read)get_MSCM_CLK_Frequency/171 (read)get_TSENSE0_CLK_Frequency/163 (read)get_CMP0_CLK_Frequency/127 (read)get_TEMPSENSE_CLK_Frequency/126 (read)get_TCM_CM7_1_CLK_Frequency/125 (read)get_SWT0_CLK_Frequency/177 (read)get_ADC1_CLK_Frequency/81 (read)get_ADC0_CLK_Frequency/80 (read)CMU_HSE_CLK_A/73 (read)CMU_AIPS_PLAT_CLK_A/71 (read)get_TRGMUX0_CLK_Frequency/162 (read)get_STCU0_CLK_Frequency/161 (read)get_SAI1_CLK_Frequency/160 (read)get_STMB_CLK_Frequency/200 (read)get_TCM_CM7_0_CLK_Frequency/124 (read)get_LCU1_CLK_Frequency/123 (read)get_LCU0_CLK_Frequency/122 (read)get_SIUL0_CLK_Frequency/176 (read)get_QSPI0_TX_MEM_CLK_Frequency/175 (read)get_STM0_CLK_Frequency/199 (read)get_STMA_CLK_Frequency/198 (read)get_QSPI0_SFCK_CLK_Frequency/195 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_SAI0_CLK_Frequency/159 (read)get_QSPI0_RAM_CLK_Frequency/174 (read)get_LPUART8_CLK_Frequency/170 (read)get_PIT2_CLK_Frequency/158 (read)get_PIT1_CLK_Frequency/157 (read)get_DCM0_CLK_Frequency/173 (read)get_FLEXCAN5_CLK_Frequency/193 (read)get_FLEXCAN4_CLK_Frequency/192 (read)get_SEMA42_CLK_Frequency/172 (read)get_PIT0_CLK_Frequency/156 (read)get_MUB_CLK_Frequency/155 (read)get_MUA_CLK_Frequency/154 (read)get_LPUART9_CLK_Frequency/153 (read)get_LPUART7_CLK_Frequency/152 (read)get_LPUART0_CLK_Frequency/169 (read)get_LPUART6_CLK_Frequency/151 (read)get_LPSPI0_CLK_Frequency/168 (read)get_LPUART5_CLK_Frequency/150 (read)get_LPUART4_CLK_Frequency/149 (read)get_LPUART3_CLK_Frequency/148 (read)get_LPUART2_CLK_Frequency/147 (read)get_LPUART1_CLK_Frequency/146 (read)get_LPUART15_CLK_Frequency/145 (read)get_LPUART14_CLK_Frequency/144 (read)get_LPUART13_CLK_Frequency/143 (read)get_LPUART12_CLK_Frequency/142 (read)get_LPUART11_CLK_Frequency/141 (read)get_LPUART10_CLK_Frequency/140 (read)get_LPSPI5_CLK_Frequency/139 (read)get_LPSPI4_CLK_Frequency/138 (read)get_INTM_CLK_Frequency/167 (read)get_LPSPI3_CLK_Frequency/137 (read)get_LPSPI2_CLK_Frequency/136 (read)get_LPSPI1_CLK_Frequency/135 (read)get_LPI2C1_CLK_Frequency/134 (read)get_LPI2C0_CLK_Frequency/133 (read)get_FLEXIO0_CLK_Frequency/166 (read)get_FLASH0_CLK_Frequency/132 (read)get_ERM0_CLK_Frequency/131 (read)get_EMIOS2_CLK_Frequency/121 (read)get_EMIOS1_CLK_Frequency/120 (read)get_CRC0_CLK_Frequency/165 (read)get_WKPU0_CLK_Frequency/164 (read)get_FLEXCAN3_CLK_Frequency/191 (read)get_FLEXCANB_CLK_Frequency/190 (read)get_FLEXCAN2_CLK_Frequency/189 (read)get_FLEXCAN1_CLK_Frequency/188 (read)get_FLEXCAN0_CLK_Frequency/187 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_EMAC0_TX_CLK_Frequency/185 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_EIM0_CLK_Frequency/130 (read)get_CMP2_CLK_Frequency/129 (read)get_EMIOS0_CLK_Frequency/119 (read)get_EDMA0_TCD9_CLK_Frequency/118 (read)get_EDMA0_TCD8_CLK_Frequency/117 (read)get_EMAC0_TS_CLK_Frequency/183 (read)get_EMAC_TS_CLK_Frequency/182 (read)get_EMAC0_RX_CLK_Frequency/181 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)get_SWT1_CLK_Frequency/178 (read)get_CMP1_CLK_Frequency/128 (read)get_EDMA0_TCD7_CLK_Frequency/116 (read)get_EDMA0_TCD6_CLK_Frequency/115 (read)get_EDMA0_TCD5_CLK_Frequency/114 (read)get_EDMA0_TCD4_CLK_Frequency/113 (read)get_EDMA0_TCD3_CLK_Frequency/112 (read)get_EDMA0_TCD31_CLK_Frequency/111 (read)get_EDMA0_TCD30_CLK_Frequency/110 (read)get_EDMA0_TCD2_CLK_Frequency/109 (read)get_EDMA0_TCD29_CLK_Frequency/108 (read)get_EDMA0_TCD28_CLK_Frequency/107 (read)get_EDMA0_TCD27_CLK_Frequency/106 (read)get_EDMA0_TCD26_CLK_Frequency/105 (read)get_EDMA0_TCD25_CLK_Frequency/104 (read)get_EDMA0_TCD24_CLK_Frequency/103 (read)get_EDMA0_TCD23_CLK_Frequency/102 (read)get_EDMA0_TCD22_CLK_Frequency/101 (read)get_EDMA0_TCD21_CLK_Frequency/100 (read)get_EDMA0_TCD20_CLK_Frequency/99 (read)get_EDMA0_TCD1_CLK_Frequency/98 (read)get_EDMA0_TCD19_CLK_Frequency/97 (read)get_EDMA0_TCD18_CLK_Frequency/96 (read)get_EDMA0_TCD17_CLK_Frequency/95 (read)get_EDMA0_TCD16_CLK_Frequency/94 (read)get_EDMA0_TCD15_CLK_Frequency/93 (read)get_EDMA0_TCD14_CLK_Frequency/92 (read)get_EDMA0_TCD13_CLK_Frequency/91 (read)get_EDMA0_TCD12_CLK_Frequency/90 (read)get_EDMA0_TCD11_CLK_Frequency/89 (read)get_EDMA0_TCD10_CLK_Frequency/88 (read)get_EDMA0_TCD0_CLK_Frequency/87 (read)get_EDMA0_CLK_Frequency/86 (read)get_DMAMUX1_CLK_Frequency/85 (read)get_DMAMUX0_CLK_Frequency/84 (read)get_BCTU0_CLK_Frequency/83 (read)get_ADC2_CLK_Frequency/82 (read)IntegerDividers_F/55 (read)IntegerDividers_K/60 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)CMU_FXOSC_CLK_A/67 (read)GetProducerClockFreq/40 (read)
  Availability: available
  Varpool flags:
HwPllName/24 (HwPllName) @06f84000
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntryIndex/23 (selectorEntryIndex) @06f59f30
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: NOT_UNDER_MCU_CONTROL_B/45 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
hardwareValue_selectorEntry/22 (hardwareValue_selectorEntry) @06f59ca8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: get_STMB_CLK_Frequency/200 (read)get_STM0_CLK_Frequency/199 (read)get_STMA_CLK_Frequency/198 (read)get_QSPI0_SFCK_CLK_Frequency/195 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_FLEXCAN5_CLK_Frequency/193 (read)get_FLEXCAN4_CLK_Frequency/192 (read)get_FLEXCAN3_CLK_Frequency/191 (read)get_FLEXCANB_CLK_Frequency/190 (read)get_FLEXCAN2_CLK_Frequency/189 (read)get_FLEXCAN1_CLK_Frequency/188 (read)get_FLEXCAN0_CLK_Frequency/187 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_EMAC0_TX_CLK_Frequency/185 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_EMAC0_TS_CLK_Frequency/183 (read)get_EMAC_TS_CLK_Frequency/182 (read)get_EMAC0_RX_CLK_Frequency/181 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)get_STM1_CLK_Frequency/201 (read)get_TRACE_CLK_Frequency/202 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
clockName_sourceType/21 (clockName_sourceType) @06f59f78
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
mcmeTriggerPartitions/20 (mcmeTriggerPartitions) @06f59ee8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
mcmeGetPartitions/19 (mcmeGetPartitions) @06f59ea0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
mcmeSetPartitions/18 (mcmeSetPartitions) @06f59e58
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cmu/17 (cmu) @06f59e10
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
pll/16 (pll) @06f59dc8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
xosc/15 (xosc) @06f59d80
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cgmPcfs/14 (cgmPcfs) @06f59d38
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cgm/13 (cgm) @06f59cf0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
enableDisableMask/12 (enableDisableMask) @06f59c60
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: get_STMB_CLK_Frequency/200 (read)get_STM0_CLK_Frequency/199 (read)get_STMA_CLK_Frequency/198 (read)get_QSPI0_SFCK_CLK_Frequency/195 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_FLEXCAN5_CLK_Frequency/193 (read)get_FLEXCAN4_CLK_Frequency/192 (read)get_FLEXCAN3_CLK_Frequency/191 (read)get_FLEXCANB_CLK_Frequency/190 (read)get_FLEXCAN2_CLK_Frequency/189 (read)get_FLEXCAN1_CLK_Frequency/188 (read)get_FLEXCAN0_CLK_Frequency/187 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_EMAC0_TX_CLK_Frequency/185 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_EMAC0_TS_CLK_Frequency/183 (read)get_EMAC_TS_CLK_Frequency/182 (read)get_EMAC0_RX_CLK_Frequency/181 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)get_STM1_CLK_Frequency/201 (read)get_TRACE_CLK_Frequency/202 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntry_hardwareValue/11 (selectorEntry_hardwareValue) @06f59bd0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
clockFeatures/10 (clockFeatures) @06f59b40
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cmuCallbackIndex/9 (cmuCallbackIndex) @06f533a8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
pcfsCallbackIndex/8 (pcfsCallbackIndex) @06f53318
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorCallbackIndex/7 (selectorCallbackIndex) @06f53288
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
pllCallbackIndex/6 (pllCallbackIndex) @06f531f8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
fractional_dividerCallbackIndex/5 (fractional_dividerCallbackIndex) @06f53168
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
gateCallbackIndex/4 (gateCallbackIndex) @06f530d8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
ircoscCallbackIndex/3 (ircoscCallbackIndex) @06f53048
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
xoscCallbackIndex/2 (xoscCallbackIndex) @06f2df78
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
dividertriggerCallbackIndex/1 (dividertriggerCallbackIndex) @06f2dee8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
dividerCallbackIndex/0 (dividerCallbackIndex) @06f2df30
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0 ()
{
  uint32 i;
  const struct Clock_Ip_SelectorConfigType * selectorSCS_CLK;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;

  <bb 4> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
<L0>:
  # DEBUG BEGIN_STMT
  _1 = bufferFreqs[8];
  configuredCoreClock = _1;
  # DEBUG BEGIN_STMT
  _2 = bufferFreqs[9];
  configuredAipsPlatClock = _2;
  # DEBUG BEGIN_STMT
  _3 = bufferFreqs[10];
  configuredAipsSlowClock = _3;
  # DEBUG BEGIN_STMT
  _4 = bufferFreqs[11];
  configuredHseClock = _4;
  # DEBUG BEGIN_STMT

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  return;

}


NOT_UNDER_MCU_CONTROL_A.part.0 ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  <unnamed type> iftmp.61_5;

  <bb 8> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(struct MC_ME_Type *)1076740096B].PRTN1_COFB1_STAT;
  _2 = _1 & 16777216;
  if (_2 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _3 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLSR;
  _4 = _3 & 4;
  if (_4 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 4> [local count: 268435456]:

  <bb 5> [local count: 536870913]:
  # iftmp.61_5 = PHI <0(3), 255(4)>
  clkState[6] = iftmp.61_5;
  goto <bb 7>; [100.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  clkState[6] = 0;

  <bb 7> [local count: 1073741824]:
  return;

}


CONFIG_ELEMENTS_MAPPINGS_01.part.0 ()
{
  uint8 i;
  int _2;
  const struct Clock_Ip_ClockConfigType * config_clock.85_3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  unsigned char _7;
  int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.85_10;
  <unnamed type> _11;
  int _12;
  unsigned char _13;
  unsigned char _14;
  int _16;
  <unnamed type> _17;
  int _18;
  unsigned char _19;
  unsigned char _20;
  int _22;
  <unnamed type> _23;
  int _24;
  unsigned char _25;
  unsigned char _26;

  <bb 14> [local count: 118111598]:
  goto <bb 3>; [100.00%]

  <bb 2> [local count: 955630209]:
  # DEBUG BEGIN_STMT
  _2 = (int) i_1;
  _4 = config_clock.85_3->ircoscs[_2].name;
  _5 = (int) _4;
  _6 = i_1 + 1;
  freqPointers[_5] = _6;
  # DEBUG BEGIN_STMT
  # DEBUG i => _6

  <bb 3> [local count: 1073741809]:
  # i_1 = PHI <_6(2), 0(14)>
  # DEBUG i => i_1
  # DEBUG BEGIN_STMT
  config_clock.85_3 = config_clock;
  _7 = config_clock.85_3->ircoscsCount;
  if (i_1 < _7)
    goto <bb 2>; [89.00%]
  else
    goto <bb 4>; [11.00%]

  <bb 4> [local count: 118111599]:
  # config_clock.85_10 = PHI <config_clock.85_3(3)>
  goto <bb 6>; [100.00%]

  <bb 5> [local count: 955630212]:
  # DEBUG BEGIN_STMT
  _9 = (int) i_8;
  _11 = config_clock.85_10->xoscs[_9].name;
  _12 = (int) _11;
  _13 = i_8 + 1;
  freqPointers[_12] = _13;
  # DEBUG BEGIN_STMT
  # DEBUG i => _13

  <bb 6> [local count: 1073741812]:
  # i_8 = PHI <0(4), _13(5)>
  # DEBUG i => i_8
  # DEBUG BEGIN_STMT
  _14 = config_clock.85_10->xoscsCount;
  if (i_8 < _14)
    goto <bb 5>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 7> [local count: 118111599]:
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 955630219]:
  # DEBUG BEGIN_STMT
  _16 = (int) i_15;
  _17 = config_clock.85_10->plls[_16].name;
  _18 = (int) _17;
  _19 = i_15 + 1;
  freqPointers[_18] = _19;
  # DEBUG BEGIN_STMT
  # DEBUG i => _19

  <bb 9> [local count: 1073741819]:
  # i_15 = PHI <0(7), _19(8)>
  # DEBUG i => i_15
  # DEBUG BEGIN_STMT
  _20 = config_clock.85_10->pllsCount;
  if (i_15 < _20)
    goto <bb 8>; [89.00%]
  else
    goto <bb 10>; [11.00%]

  <bb 10> [local count: 118111600]:
  goto <bb 12>; [100.00%]

  <bb 11> [local count: 955630225]:
  # DEBUG BEGIN_STMT
  _22 = (int) i_21;
  _23 = config_clock.85_10->extClks[_22].name;
  _24 = (int) _23;
  _25 = i_21 + 1;
  freqPointers[_24] = _25;
  # DEBUG BEGIN_STMT
  # DEBUG i => _25

  <bb 12> [local count: 1073741824]:
  # i_21 = PHI <0(10), _25(11)>
  # DEBUG i => i_21
  # DEBUG BEGIN_STMT
  _26 = config_clock.85_10->extClksCount;
  if (i_21 < _26)
    goto <bb 11>; [89.00%]
  else
    goto <bb 13>; [11.00%]

  <bb 13> [local count: 118111601]:
  return;

}


get_TRACE_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725184B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725184B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725184B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_STM1_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_STMB_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_STM0_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_STMA_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_RTC0_CLK_Frequency ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return 0;

}


get_RTC_CLK_Frequency ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return 0;

}


get_QSPI0_SFCK_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_QSPI_SFCK_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCAN5_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCAN4_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCAN3_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCANB_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCAN2_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCAN1_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCAN0_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCANA_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_EMAC0_TX_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_EMAC_TX_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_EMAC0_TS_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_EMAC_TS_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_EMAC0_RX_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_EMAC_RX_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_CLKOUT_STANDBY_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724800B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724800B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724800B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_SWT1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[2];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_SWT0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[2];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_SIUL0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[0];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_QSPI0_TX_MEM_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[19];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_QSPI0_RAM_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[19];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_DCM0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[17];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_SEMA42_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_MSCM_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART8_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPSPI0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_INTM_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_FLEXIO0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_CRC0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_WKPU0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_TSENSE0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_TRGMUX0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_STCU0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_SAI1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_SAI0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_PIT2_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_PIT1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_PIT0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_MUB_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_MUA_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART9_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART7_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART6_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART5_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART4_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART3_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART2_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART15_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART14_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART13_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART12_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART11_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPUART10_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPSPI5_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPSPI4_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPSPI3_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPSPI2_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPSPI1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPI2C1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LPI2C0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_FLASH0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_ERM0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EIM0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_CMP2_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_CMP1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_CMP0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_TEMPSENSE_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_TCM_CM7_1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_TCM_CM7_0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LCU1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_LCU0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EMIOS2_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EMIOS1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EMIOS0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD9_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD8_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD7_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD6_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD5_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD4_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD3_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD31_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD30_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD2_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD29_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD28_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD27_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD26_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD25_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD24_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD23_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD22_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD21_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD20_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD19_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD18_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD17_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD16_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD15_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD14_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD13_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD12_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD11_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD10_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_TCD0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_EDMA0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_DMAMUX1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_DMAMUX0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_BCTU0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_ADC2_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_ADC1_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_ADC0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


CallbackDelay ()
{
  uint32 TimeoutTicks;
  uint32 ElapsedTime;
  uint32 StartTime;
  boolean TimeoutOccurred;
  long unsigned int TimeoutTicks.0_1;

  <bb 2> [local count: 118111600]:
  # DEBUG BEGIN_STMT
  # DEBUG TimeoutOccurred => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  ClockStartTimeout (&StartTime, &ElapsedTime, &TimeoutTicks, 10);

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  TimeoutTicks.0_1 = TimeoutTicks;
  TimeoutOccurred_6 = ClockTimeoutExpired (&StartTime, &ElapsedTime, TimeoutTicks.0_1);
  # DEBUG TimeoutOccurred => TimeoutOccurred_6
  # DEBUG BEGIN_STMT
  if (TimeoutOccurred_6 != 0)
    goto <bb 4>; [11.00%]
  else
    goto <bb 5>; [89.00%]

  <bb 5> [local count: 955630223]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 118111601]:
  StartTime ={v} {CLOBBER};
  ElapsedTime ={v} {CLOBBER};
  TimeoutTicks ={v} {CLOBBER};
  return;

}


CallEmptyCallbacks ()
{
  void (*<T494>) (const struct Clock_Ip_CmuConfigType *) _1;
  void (*<T498>) (Clock_Ip_NameType) _2;
  void (*<T498>) (Clock_Ip_NameType) _3;
  Clock_Ip_CmuStatusType (*<T49c>) (Clock_Ip_NameType) _4;
  void (*<T43f>) (const struct Clock_Ip_DividerConfigType *) _5;
  void (*<T44a>) (const struct Clock_Ip_DividerTriggerConfigType *) _6;
  void (*<T433>) (const struct Clock_Ip_XoscConfigType *) _7;
  void (*<T456>) (const struct Clock_Ip_FracDivConfigType *) _8;
  clock_dfs_status_t (*<T45c>) (Clock_Ip_NameType) _9;
  void (*<T484>) (const struct Clock_Ip_GateConfigType *) _10;
  void (*<T489>) (Clock_Ip_NameType, boolean) _11;
  void (*<T428>) (const struct Clock_Ip_IrcoscConfigType *) _12;
  void (*<T467>) (const struct Clock_Ip_PllConfigType *) _13;
  clock_pll_status_t (*<T46d>) (Clock_Ip_NameType) _14;
  void (*<T478>) (const struct Clock_Ip_SelectorConfigType *) _15;
  void (*<T4a7>) (const struct Clock_Ip_PcfsConfigType *) _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = cmuCallbacks[0].Set;
  _1 (0B);
  # DEBUG BEGIN_STMT
  _2 = cmuCallbacks[0].Disable;
  _2 (145);
  # DEBUG BEGIN_STMT
  _3 = cmuCallbacks[0].Clear;
  _3 (145);
  # DEBUG BEGIN_STMT
  _4 = cmuCallbacks[0].GetStatus;
  _4 (145);
  # DEBUG BEGIN_STMT
  _5 = dividerCallbacks[0].Set;
  _5 (0B);
  # DEBUG BEGIN_STMT
  _6 = dividerTriggerCallbacks[0].Configure;
  _6 (0B);
  # DEBUG BEGIN_STMT
  _7 = extOscCallbacks[0].Reset;
  _7 (0B);
  # DEBUG BEGIN_STMT
  _8 = fracDivCallbacks[0].Set;
  _8 (0B);
  # DEBUG BEGIN_STMT
  _9 = fracDivCallbacks[0].Complete;
  _9 (145);
  # DEBUG BEGIN_STMT
  _10 = gateCallbacks[0].Set;
  _10 (0B);
  # DEBUG BEGIN_STMT
  _11 = gateCallbacks[0].Update;
  _11 (145, 0);
  # DEBUG BEGIN_STMT
  _12 = intOscCallbacks[0].Set;
  _12 (0B);
  # DEBUG BEGIN_STMT
  _13 = pllCallbacks[0].Set;
  _13 (0B);
  # DEBUG BEGIN_STMT
  _14 = pllCallbacks[0].Complete;
  _14 (145);
  # DEBUG BEGIN_STMT
  _15 = selectorCallbacks[0].Set;
  _15 (0B);
  # DEBUG BEGIN_STMT
  _16 = pcfsCallbacks[0].Set;
  _16 (0B);
  return;

}


McMeEnterKey ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  MEM[(struct MC_ME_Type *)1076740096B].CTL_KEY ={v} 23280;
  # DEBUG BEGIN_STMT
  MEM[(struct MC_ME_Type *)1076740096B].CTL_KEY ={v} 42255;
  return;

}


CMU_HSE_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[3].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[3].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[3].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}


CMU_HSE_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.1_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int configuredHseClock.2_6;
  long unsigned int configuredAipsSlowClock.3_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[3].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.1_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#10 => &config_clock.1_2->cmus[_4]
  # DEBUG cmuConfig => D#10
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.1_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[1];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  configuredHseClock.2_6 = configuredHseClock;
  fMonitoredClk_25 = configuredHseClock.2_6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.3_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.3_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (configuredHseClock.2_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[3].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[3].refCount = _19;
  return;

}


CMU_AIPS_PLAT_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[2].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[2].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[2].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}


CMU_AIPS_PLAT_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.4_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int configuredAipsPlatClock.5_6;
  long unsigned int configuredAipsSlowClock.6_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[2].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.4_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#9 => &config_clock.4_2->cmus[_4]
  # DEBUG cmuConfig => D#9
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.4_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[1];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  configuredAipsPlatClock.5_6 = configuredAipsPlatClock;
  fMonitoredClk_25 = configuredAipsPlatClock.5_6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.6_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.6_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (configuredAipsPlatClock.5_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[2].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[2].refCount = _19;
  return;

}


CMU_CORE_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[1].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[1].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[1].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}


CMU_CORE_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.7_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int configuredCoreClock.8_6;
  long unsigned int configuredAipsSlowClock.9_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[1].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.7_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#8 => &config_clock.7_2->cmus[_4]
  # DEBUG cmuConfig => D#8
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.7_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[3];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  configuredCoreClock.8_6 = configuredCoreClock;
  fMonitoredClk_25 = configuredCoreClock.8_6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.9_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.9_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (configuredCoreClock.8_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[1].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[1].refCount = _19;
  return;

}


CMU_FXOSC_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[0].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[0].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[0].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}


CMU_FXOSC_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.10_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int configuredAipsSlowClock.11_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[0].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.10_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#7 => &config_clock.10_2->cmus[_4]
  # DEBUG cmuConfig => D#7
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.10_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[1];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  _6 = bufferFreqs[3];
  fMonitoredClk_25 = _6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.11_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.11_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[0].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[0].refCount = _19;
  return;

}


PCFS_PLL_PHI0_E ()
{
  uint32 K;
  uint32 RATE;
  uint32 fsafe;
  uint32 finput;
  uint32 stepDuration;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  stepDuration_14 = tmpData.input1;
  # DEBUG stepDuration => stepDuration_14
  # DEBUG BEGIN_STMT
  finput_15 = tmpData.input2;
  # DEBUG finput => finput_15
  # DEBUG BEGIN_STMT
  fsafe_16 = tmpData.input3;
  # DEBUG fsafe => fsafe_16
  # DEBUG BEGIN_STMT
  RATE_17 = tmpData.aux1;
  # DEBUG RATE => RATE_17
  # DEBUG BEGIN_STMT
  _1 = tmpData.aux4;
  _2 = _1 << 2;
  _3 = _2 + 191;
  K_18 = _3 >> 7;
  # DEBUG K => K_18
  # DEBUG BEGIN_STMT
  _4 = stepDuration_14 * fsafe_16;
  pcfsEntries[0].sdur = _4;
  # DEBUG BEGIN_STMT
  _5 = RATE_17 * K_18;
  pcfsEntries[0].divc_init = _5;
  # DEBUG BEGIN_STMT
  pcfsEntries[0].divc_rate = RATE_17;
  # DEBUG BEGIN_STMT
  _6 = K_18 + 1;
  _7 = _5 * _6;
  _8 = _7 >> 1;
  _9 = _8 + 999;
  pcfsEntries[0].div_startValue = _9;
  # DEBUG BEGIN_STMT
  _10 = finput_15 * 1000;
  _11 = _10 / fsafe_16;
  _12 = _11 + 4294967295;
  pcfsEntries[0].div_endValue = _12;
  return;

}


PCFS_PLL_PHI0_D ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 118111600]:
  # DEBUG BEGIN_STMT
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _1 = tmpData.aux2;
  _2 = tmpData.aux4;
  _3 = _2 + _10;
  if (_1 >= _3)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 477815111]:
  # DEBUG BEGIN_STMT
  _4 = _1 - _3;
  tmpData.aux2 = _4;
  # DEBUG BEGIN_STMT
  _5 = _10 << 1;
  _6 = _2 + _5;
  tmpData.aux4 = _6;

  <bb 5> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _7 = tmpData.aux4;
  _8 = _7 >> 1;
  tmpData.aux4 = _8;
  # DEBUG BEGIN_STMT
  _9 = _10 >> 2;
  tmpData.aux3 = _9;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = tmpData.aux3;
  if (_10 != 0)
    goto <bb 3>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 7> [local count: 118111601]:
  return;

}


PCFS_PLL_PHI0_C ()
{
  uint32 RATE;
  uint32 fsafe;
  uint32 finput;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;

  <bb 2> [local count: 118111600]:
  # DEBUG BEGIN_STMT
  finput_11 = tmpData.input2;
  # DEBUG finput => finput_11
  # DEBUG BEGIN_STMT
  fsafe_12 = tmpData.input3;
  # DEBUG fsafe => fsafe_12
  # DEBUG BEGIN_STMT
  RATE_13 = tmpData.aux1;
  # DEBUG RATE => RATE_13
  # DEBUG BEGIN_STMT
  _1 = finput_11 * 2048000;
  _2 = fsafe_12 * RATE_13;
  _3 = _1 / _2;
  _4 = 2048000 / RATE_13;
  _5 = _3 - _4;
  _6 = _5 + 256;
  tmpData.aux2 = _6;
  # DEBUG BEGIN_STMT
  tmpData.aux3 = 1073741824;
  # DEBUG BEGIN_STMT
  goto <bb 4>; [100.00%]

  <bb 3> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _7 = _8 >> 2;
  tmpData.aux3 = _7;

  <bb 4> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _8 = tmpData.aux3;
  if (_6 < _8)
    goto <bb 3>; [89.00%]
  else
    goto <bb 5>; [11.00%]

  <bb 5> [local count: 118111601]:
  return;

}


PCFS_PLL_PHI0_B ()
{
  uint8 i;
  uint32 RATE;
  uint32 amaxBrut;
  const uint32 pcfsRate[6];
  const uint32 aMax[6];
  unsigned int _1;
  unsigned int _2;
  long unsigned int _3;

  <bb 2> [local count: 357985524]:
  # DEBUG BEGIN_STMT
  aMax = *.LC0;
  # DEBUG BEGIN_STMT
  pcfsRate = *.LC1;
  # DEBUG BEGIN_STMT
  amaxBrut_11 = tmpData.aux1;
  # DEBUG amaxBrut => amaxBrut_11
  # DEBUG BEGIN_STMT
  # DEBUG RATE => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (amaxBrut_11 > 100)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 178992762]:
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 894749063]:
  # DEBUG BEGIN_STMT
  _1 = (unsigned int) i_7;
  _2 = _1 + 4294967295;
  _3 = aMax[_2];
  if (_3 < amaxBrut_11)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 447374531]:
  # DEBUG BEGIN_STMT
  RATE_12 = pcfsRate[_2];
  # DEBUG RATE => RATE_12

  <bb 5> [local count: 894749063]:
  # RATE_4 = PHI <RATE_5(3), RATE_12(4)>
  # DEBUG RATE => RATE_4
  # DEBUG BEGIN_STMT
  i_13 = i_7 + 1;
  # DEBUG i => i_13

  <bb 6> [local count: 1073741824]:
  # RATE_5 = PHI <RATE_4(5), 0(8)>
  # i_7 = PHI <i_13(5), 1(8)>
  # DEBUG i => i_7
  # DEBUG RATE => RATE_5
  # DEBUG BEGIN_STMT
  if (i_7 != 6)
    goto <bb 3>; [83.33%]
  else
    goto <bb 7>; [16.67%]

  <bb 7> [local count: 357985524]:
  # RATE_6 = PHI <RATE_5(6), 1000(2)>
  # DEBUG RATE => RATE_6
  # DEBUG BEGIN_STMT
  tmpData.aux1 = RATE_6;
  aMax ={v} {CLOBBER};
  pcfsRate ={v} {CLOBBER};
  return;

}


PCFS_PLL_PHI0_A ()
{
  uint32 amaxBrut;
  uint32 fsafe;
  uint32 finput;
  uint32 stepDuration;
  uint32 maxAllowableIDDchange;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.13_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = pcfsEntries[0].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.13_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#6 => &config_clock.13_2->pcfs[_4]
  # DEBUG pcfsConfig => D#6
  # DEBUG BEGIN_STMT
  maxAllowableIDDchange_15 = MEM[(const struct Clock_Ip_PcfsConfigType *)config_clock.13_2].pcfs[_4].maxAllowableIDDchange;
  # DEBUG maxAllowableIDDchange => maxAllowableIDDchange_15
  # DEBUG BEGIN_STMT
  stepDuration_16 = MEM[(const struct Clock_Ip_PcfsConfigType *)config_clock.13_2].pcfs[_4].stepDuration;
  # DEBUG stepDuration => stepDuration_16
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG maxAllowableIDDchange => 50
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmPcfs_Type *)1076723712B].PCFS_SDUR;
  stepDuration_14 = _5 & 65535;
  # DEBUG stepDuration => stepDuration_14

  <bb 5> [local count: 1073741824]:
  # maxAllowableIDDchange_11 = PHI <maxAllowableIDDchange_15(3), 50(4)>
  # stepDuration_12 = PHI <stepDuration_16(3), stepDuration_14(4)>
  # DEBUG stepDuration => stepDuration_12
  # DEBUG maxAllowableIDDchange => maxAllowableIDDchange_11
  # DEBUG BEGIN_STMT
  _6 = bufferFreqs[26];
  finput_17 = _6 / 1000000;
  # DEBUG finput => finput_17
  # DEBUG BEGIN_STMT
  _7 = bufferFreqs[1];
  fsafe_18 = _7 / 1000000;
  # DEBUG fsafe => fsafe_18
  # DEBUG BEGIN_STMT
  tmpData.input1 = stepDuration_12;
  # DEBUG BEGIN_STMT
  tmpData.input2 = finput_17;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fsafe_18;
  # DEBUG BEGIN_STMT
  _8 = maxAllowableIDDchange_11 * stepDuration_12;
  _9 = _8 * 100000;
  _10 = finput_17 * 2360;
  amaxBrut_22 = _9 / _10;
  # DEBUG amaxBrut => amaxBrut_22
  # DEBUG BEGIN_STMT
  tmpData.aux1 = amaxBrut_22;
  return;

}


CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS ()
{
  const struct Clock_Ip_SelectorConfigType * selectorSCS_CLK;
  uint32 i;
  const struct Clock_Ip_ClockConfigType * config_clock.16_1;
  <unnamed type> _2;
  const struct Clock_Ip_ClockConfigType * config_clock.16_4;
  unsigned char _5;
  long unsigned int _6;
  <unnamed type> _7;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;

  <bb 2> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG selectorSCS_CLK => 0B
  # DEBUG BEGIN_STMT
  # DEBUG i => 0
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _2 = config_clock.16_4->selectors[i_13].name;
  if (_2 == 12)
    goto <bb 4>; [5.50%]
  else
    goto <bb 5>; [94.50%]

  <bb 4> [local count: 55807731]:
  # config_clock.16_1 = PHI <config_clock.16_4(3)>
  # i_3 = PHI <i_13(3)>
  # DEBUG BEGIN_STMT
  selectorSCS_CLK_18 = &config_clock.16_1->selectors[i_3];
  # DEBUG selectorSCS_CLK => selectorSCS_CLK_18
  # DEBUG BEGIN_STMT
  goto <bb 7>; [100.00%]

  <bb 5> [local count: 958878293]:
  # DEBUG BEGIN_STMT
  i_17 = i_13 + 1;
  # DEBUG i => i_17

  <bb 6> [local count: 1073741824]:
  # i_13 = PHI <0(2), i_17(5)>
  # DEBUG i => i_13
  # DEBUG BEGIN_STMT
  config_clock.16_4 = config_clock;
  _5 = config_clock.16_4->selectorsCount;
  _6 = (long unsigned int) _5;
  if (_6 > i_13)
    goto <bb 3>; [94.50%]
  else
    goto <bb 7>; [5.50%]

  <bb 7> [local count: 114863532]:
  # selectorSCS_CLK_14 = PHI <selectorSCS_CLK_18(4), 0B(6)>
  # DEBUG selectorSCS_CLK => selectorSCS_CLK_14
  # DEBUG BEGIN_STMT
  if (selectorSCS_CLK_14 != 0B)
    goto <bb 8>; [70.00%]
  else
    goto <bb 12>; [30.00%]

  <bb 8> [local count: 80404472]:
  # DEBUG BEGIN_STMT
  _7 = selectorSCS_CLK_14->value;
  switch (_7) <default: <L8> [33.33%], case 0: <L6> [33.33%], case 8: <L7> [33.33%]>

  <bb 9> [local count: 26801491]:
<L6>:
  CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0 ();
  goto <bb 13>; [100.00%]

  <bb 10> [local count: 26798811]:
<L7>:
  # DEBUG BEGIN_STMT
  _9 = bufferFreqs[28];
  configuredCoreClock = _9;
  # DEBUG BEGIN_STMT
  _10 = bufferFreqs[29];
  configuredAipsPlatClock = _10;
  # DEBUG BEGIN_STMT
  _11 = bufferFreqs[30];
  configuredAipsSlowClock = _11;
  # DEBUG BEGIN_STMT
  _12 = bufferFreqs[31];
  configuredHseClock = _12;
  # DEBUG BEGIN_STMT
  goto <bb 13>; [100.00%]

  <bb 11> [local count: 26798811]:
<L8>:
  # DEBUG BEGIN_STMT
  configuredCoreClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsPlatClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock = 0;
  # DEBUG BEGIN_STMT
  configuredHseClock = 0;
  # DEBUG BEGIN_STMT
  goto <bb 13>; [100.00%]

  <bb 12> [local count: 34459060]:
  # DEBUG BEGIN_STMT
  configuredCoreClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsPlatClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock = 0;
  # DEBUG BEGIN_STMT
  configuredHseClock = 0;

  <bb 13> [local count: 114855491]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  return;

}


IntegerDividers_K ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.17_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.18_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.19_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.17_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.17_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[31];
  _9 = _8 / dividerValue_26;
  bufferFreqs[38] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[38] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.18_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.18_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[29];
  _17 = _16 / dividerValue_27;
  bufferFreqs[39] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[39] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.19_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.19_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[30];
  _25 = _24 / dividerValue_28;
  bufferFreqs[40] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[40] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_J ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.20_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.21_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.22_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.20_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.20_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[26];
  _9 = _8 / dividerValue_26;
  bufferFreqs[35] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[35] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.21_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.21_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[27];
  _17 = _16 / dividerValue_27;
  bufferFreqs[36] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[36] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.22_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.22_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[28];
  _25 = _24 / dividerValue_28;
  bufferFreqs[37] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[37] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_I ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.23_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.24_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.25_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[17];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.23_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.23_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[4];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[26];
  _9 = _8 / dividerValue_28;
  bufferFreqs[32] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[32] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[18];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.24_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.24_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[5];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[26];
  _18 = _17 / dividerValue_29;
  bufferFreqs[33] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[33] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[19];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.25_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.25_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[6];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[26];
  _27 = _26 / dividerValue_30;
  bufferFreqs[34] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[34] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_H ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.26_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.27_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.28_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.26_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.26_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[1];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[26];
  _9 = _8 / dividerValue_28;
  bufferFreqs[29] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[29] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[15];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.27_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.27_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[2];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[26];
  _18 = _17 / dividerValue_29;
  bufferFreqs[30] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[30] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[16];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.28_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.28_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[3];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[26];
  _27 = _26 / dividerValue_30;
  bufferFreqs[31] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[31] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_G ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.29_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.30_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.31_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[8];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.29_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.29_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[0];
  _6 = _5 >> 16;
  _7 = _6 & 15;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[25];
  _9 = _8 / dividerValue_28;
  bufferFreqs[26] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[26] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[9];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.30_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.30_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[1];
  _15 = _14 >> 16;
  _16 = _15 & 15;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[25];
  _18 = _17 / dividerValue_29;
  bufferFreqs[27] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[27] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[13];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.31_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.31_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[0];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[26];
  _27 = _26 / dividerValue_30;
  bufferFreqs[28] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[28] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_F ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.32_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.33_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  unsigned char _18;
  const struct Clock_Ip_ClockConfigType * config_clock.34_19;
  unsigned int _20;
  unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.32_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_35 = config_clock.32_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_35
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_34 = _7 + 1;
  # DEBUG dividerValue => dividerValue_34

  <bb 5> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_35(3), dividerValue_34(4)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[6];
  _9 = _8 / dividerValue_27;
  bufferFreqs[23] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[23] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.33_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_39 = config_clock.33_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_39
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_38 = _15 + 1;
  # DEBUG dividerValue => dividerValue_38

  <bb 11> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_39(9), dividerValue_38(10)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[7];
  _17 = _16 / dividerValue_28;
  bufferFreqs[24] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[24] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _18 = freqPointers[7];
  if (_18 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.34_19 = config_clock;
  _20 = (unsigned int) _18;
  _21 = _20 + 4294967295;
  dividerValue_43 = config_clock.34_19->dividers[_21].value;
  # DEBUG dividerValue => dividerValue_43
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _22 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _23 = _22 >> 25;
  dividerValue_42 = _23 & 63;
  # DEBUG dividerValue => dividerValue_42

  <bb 17> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_43(15), dividerValue_42(16)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[5];
  _25 = _24 / dividerValue_29;
  bufferFreqs[25] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[5];
  bufferFreqs[25] = _26;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_E ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.35_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.36_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.37_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.35_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.35_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[11];
  _9 = _8 / dividerValue_26;
  bufferFreqs[20] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[20] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.36_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.36_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[9];
  _17 = _16 / dividerValue_27;
  bufferFreqs[21] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[21] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.37_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.37_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[10];
  _25 = _24 / dividerValue_28;
  bufferFreqs[22] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[22] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_D ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.38_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.39_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.40_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.38_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.38_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[3];
  _9 = _8 / dividerValue_26;
  bufferFreqs[17] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[17] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.39_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.39_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[4];
  _17 = _16 / dividerValue_27;
  bufferFreqs[18] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[18] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.40_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.40_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[8];
  _25 = _24 / dividerValue_28;
  bufferFreqs[19] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[19] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_C ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.41_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.42_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  const struct Clock_Ip_ClockConfigType * config_clock.43_19;
  unsigned int _20;
  unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[19];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.41_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_35 = config_clock.41_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_35
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[6];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_34 = _7 + 1;
  # DEBUG dividerValue => dividerValue_34

  <bb 5> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_35(3), dividerValue_34(4)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[1];
  _9 = _8 / dividerValue_27;
  bufferFreqs[14] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[14] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[20];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.42_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_39 = config_clock.42_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_39
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_38 = _16 + 1;
  # DEBUG dividerValue => dividerValue_38

  <bb 11> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_39(9), dividerValue_38(10)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[1];
  _18 = _17 / dividerValue_28;
  bufferFreqs[15] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[15] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_10 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.43_19 = config_clock;
  _20 = (unsigned int) _10;
  _21 = _20 + 4294967295;
  dividerValue_43 = config_clock.43_19->dividers[_21].value;
  # DEBUG dividerValue => dividerValue_43
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _22 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _23 = _22 >> 16;
  _24 = _23 & 63;
  dividerValue_42 = _24 + 1;
  # DEBUG dividerValue => dividerValue_42

  <bb 17> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_43(15), dividerValue_42(16)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _25 = bufferFreqs[2];
  _26 = _25 / dividerValue_29;
  bufferFreqs[16] = _26;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[16] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_B ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.44_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.45_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.46_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[16];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.44_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.44_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[3];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[1];
  _9 = _8 / dividerValue_28;
  bufferFreqs[11] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[11] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[17];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.45_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.45_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[4];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[1];
  _18 = _17 / dividerValue_29;
  bufferFreqs[12] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[12] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[18];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.46_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.46_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[5];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[1];
  _27 = _26 / dividerValue_30;
  bufferFreqs[13] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[13] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_A ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.47_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.48_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.49_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.47_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.47_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[1];
  _9 = _8 / dividerValue_28;
  bufferFreqs[8] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[8] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[14];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.48_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.48_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[1];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[1];
  _18 = _17 / dividerValue_29;
  bufferFreqs[9] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[9] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[15];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.49_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.49_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[2];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[1];
  _27 = _26 / dividerValue_30;
  bufferFreqs[10] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[10] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


PLL_C ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = tmpData.output;
  _2 = tmpData.input1;
  _3 = tmpData.input2;
  _4 = _2 / _3;
  _5 = tmpData.aux2;
  _6 = _4 * _5;
  _7 = _1 + _6;
  # DEBUG BEGIN_STMT
  _8 = tmpData.aux4;
  _9 = tmpData.input4;
  _10 = _8 * _9;
  _11 = _7 + _10;
  # DEBUG BEGIN_STMT
  _12 = tmpData.aux5;
  _13 = _9 * _12;
  _14 = tmpData.aux3;
  _15 = _13 / _14;
  _16 = _11 + _15;
  tmpData.output = _16;
  # DEBUG BEGIN_STMT
  bufferFreqs[5] = _16;
  return;

}


PLL_B ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = tmpData.input2;
  _2 = _1 << 14;
  _3 = _1 << 11;
  _4 = _2 + _3;
  tmpData.aux3 = _4;
  # DEBUG BEGIN_STMT
  _5 = tmpData.input1;
  _6 = _5 / _4;
  tmpData.aux4 = _6;
  # DEBUG BEGIN_STMT
  _7 = _4 * _6;
  _8 = _5 - _7;
  tmpData.aux5 = _8;
  # DEBUG BEGIN_STMT
  _9 = tmpData.aux1;
  _10 = _5 * _9;
  tmpData.output = _10;
  return;

}


PLL_A ()
{
  long unsigned int _1;
  unsigned char _2;
  const struct Clock_Ip_ClockConfigType * config_clock.50_3;
  unsigned int _4;
  unsigned int _5;
  unsigned char _6;
  long unsigned int _7;
  unsigned char _8;
  long unsigned int _9;
  short unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  long unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = bufferFreqs[3];
  tmpData.input1 = _1;
  # DEBUG BEGIN_STMT
  _2 = freqPointers[6];
  if (_2 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.50_3 = config_clock;
  _4 = (unsigned int) _2;
  _5 = _4 + 4294967295;
  # DEBUG D#5 => &config_clock.50_3->plls[_5]
  # DEBUG pllConfig => D#5
  # DEBUG BEGIN_STMT
  _6 = MEM[(const struct Clock_Ip_PllConfigType *)config_clock.50_3].plls[_5].predivider;
  _7 = (long unsigned int) _6;
  tmpData.input2 = _7;
  # DEBUG BEGIN_STMT
  _8 = MEM[(const struct Clock_Ip_PllConfigType *)config_clock.50_3].plls[_5].mulFactorDiv;
  _9 = (long unsigned int) _8;
  tmpData.input3 = _9;
  # DEBUG BEGIN_STMT
  _10 = MEM[(const struct Clock_Ip_PllConfigType *)config_clock.50_3].plls[_5].numeratorFracLoopDiv;
  _11 = (long unsigned int) _10;
  tmpData.input4 = _11;
  # DEBUG BEGIN_STMT
  tmpData.input5 = 0;
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _12 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _13 = _12 >> 12;
  _14 = _13 & 7;
  tmpData.input2 = _14;
  # DEBUG BEGIN_STMT
  _15 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _16 = _15 & 255;
  tmpData.input3 = _16;
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLFD;
  _18 = _17 & 32767;
  tmpData.input4 = _18;
  # DEBUG BEGIN_STMT
  _19 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _20 = _19 >> 25;
  _21 = _20 & 63;
  tmpData.input5 = _21;

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _22 = tmpData.input3;
  _23 = tmpData.input2;
  _24 = _22 / _23;
  tmpData.aux1 = _24;
  # DEBUG BEGIN_STMT
  _25 = _23 * _24;
  _26 = _22 - _25;
  tmpData.aux2 = _26;
  return;

}


IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS ()
{
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.51_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  unsigned char _6;
  const struct Clock_Ip_ClockConfigType * config_clock.52_7;
  unsigned int _8;
  unsigned int _9;
  long unsigned int _10;
  unsigned char _11;
  const struct Clock_Ip_ClockConfigType * config_clock.53_12;
  unsigned int _13;
  unsigned int _14;
  long unsigned int _15;
  unsigned char _16;
  const struct Clock_Ip_ClockConfigType * config_clock.54_17;
  unsigned int _18;
  unsigned int _19;
  long unsigned int _20;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[4];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.51_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#1 => &config_clock.51_2->xoscs[_4]
  # DEBUG xoscConfig => D#1
  # DEBUG BEGIN_STMT
  _5 = MEM[(const struct Clock_Ip_XoscConfigType *)config_clock.51_2].xoscs[_4].freq;
  bufferFreqs[3] = _5;
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[3] = 16000000;

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _6 = freqPointers[5];
  if (_6 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.52_7 = config_clock;
  _8 = (unsigned int) _6;
  _9 = _8 + 4294967295;
  # DEBUG D#2 => &config_clock.52_7->xoscs[_9]
  # DEBUG xoscConfig => D#2
  # DEBUG BEGIN_STMT
  _10 = MEM[(const struct Clock_Ip_XoscConfigType *)config_clock.52_7].xoscs[_9].freq;
  bufferFreqs[4] = _10;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[4] = 32768;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  bufferFreqs[2] = 32000;
  # DEBUG BEGIN_STMT
  bufferFreqs[1] = 48000000;
  # DEBUG BEGIN_STMT
  freqPointers[0] = 1;
  # DEBUG BEGIN_STMT
  freqPointers[2] = 2;
  # DEBUG BEGIN_STMT
  _11 = freqPointers[10];
  if (_11 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.53_12 = config_clock;
  _13 = (unsigned int) _11;
  _14 = _13 + 4294967295;
  # DEBUG D#3 => &config_clock.53_12->extClks[_14]
  # DEBUG extClkConfig => D#3
  # DEBUG BEGIN_STMT
  _15 = MEM[(const struct Clock_Ip_ExtClkConfigType *)config_clock.53_12].extClks[_14].value;
  bufferFreqs[6] = _15;
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[6] = 0;

  <bb 11> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _16 = freqPointers[11];
  if (_16 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.54_17 = config_clock;
  _18 = (unsigned int) _16;
  _19 = _18 + 4294967295;
  # DEBUG D#4 => &config_clock.54_17->extClks[_19]
  # DEBUG extClkConfig => D#4
  # DEBUG BEGIN_STMT
  _20 = MEM[(const struct Clock_Ip_ExtClkConfigType *)config_clock.54_17].extClks[_19].value;
  bufferFreqs[7] = _20;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[7] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  freqPointers[10] = 6;
  # DEBUG BEGIN_STMT
  freqPointers[11] = 7;
  return;

}


NOT_UNDER_MCU_CONTROL_B ()
{
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  signed int _5;
  unsigned char _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  signed int _10;
  unsigned char _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  <unnamed type> _15;
  unsigned char _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  <unnamed type> _20;
  clock_element_state_t iftmp.55_21;
  clock_element_state_t iftmp.56_22;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[8];
  if (_1 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _2 ={v} MEM[(struct MC_ME_Type *)1076740096B].PRTN1_COFB1_STAT;
  _3 = _2 & 16777216;
  if (_3 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _4 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[0];
  _5 = (signed int) _4;
  if (_5 >= 0)
    goto <bb 6>; [59.00%]
  else
    goto <bb 5>; [41.00%]

  <bb 5> [local count: 110058537]:

  <bb 6> [local count: 268435456]:
  # iftmp.55_21 = PHI <0(4), 255(5)>
  clkState[8] = iftmp.55_21;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  clkState[8] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _6 = freqPointers[9];
  if (_6 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _7 ={v} MEM[(struct MC_ME_Type *)1076740096B].PRTN1_COFB1_STAT;
  _8 = _7 & 16777216;
  if (_8 != 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 10> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _9 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[1];
  _10 = (signed int) _9;
  if (_10 >= 0)
    goto <bb 12>; [59.00%]
  else
    goto <bb 11>; [41.00%]

  <bb 11> [local count: 110058537]:

  <bb 12> [local count: 268435456]:
  # iftmp.56_22 = PHI <0(10), 255(11)>
  clkState[9] = iftmp.56_22;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  clkState[9] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  clkState[10] = 255;
  # DEBUG BEGIN_STMT
  clkState[11] = 255;
  # DEBUG BEGIN_STMT
  _11 = freqPointers[12];
  if (_11 == 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _12 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].CSS;
  _13 = _12 >> 24;
  _14 = _13 & 63;
  _15 = selectorEntryIndex[_14];
  clkState[12] = _15;

  <bb 16> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _16 = freqPointers[20];
  if (_16 == 0)
    goto <bb 17>; [50.00%]
  else
    goto <bb 18>; [50.00%]

  <bb 17> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].CSS;
  _18 = _17 >> 24;
  _19 = _18 & 63;
  _20 = selectorEntryIndex[_19];
  clkState[20] = _20;

  <bb 18> [local count: 1073741824]:
  return;

}


NOT_UNDER_MCU_CONTROL_A ()
{
  unsigned char _1;
  long unsigned int _3;
  long unsigned int _4;
  unsigned char _5;
  long unsigned int _6;
  signed int _7;
  unsigned char _8;
  long unsigned int _9;
  long unsigned int _10;
  unsigned char _11;
  long unsigned int _12;
  signed int _13;
  unsigned char _14;
  clock_element_state_t iftmp.57_15;
  clock_element_state_t iftmp.58_16;
  clock_element_state_t iftmp.59_17;
  clock_element_state_t iftmp.60_18;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  clkState[0] = 255;
  # DEBUG BEGIN_STMT
  _1 = freqPointers[1];
  if (_1 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _3 ={v} MEM[(struct FIRC_Type *)1076690944B].STDBY_ENABLE;
  _4 = _3 & 1;
  if (_4 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 4> [local count: 268435456]:

  <bb 5> [local count: 536870913]:
  # iftmp.57_15 = PHI <0(3), 255(4)>
  clkState[1] = iftmp.57_15;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _5 = freqPointers[4];
  if (_5 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _6 ={v} MEM[(volatile struct ExtOSC_Type *)1076707328B].STAT;
  _7 = (signed int) _6;
  if (_7 >= 0)
    goto <bb 9>; [59.00%]
  else
    goto <bb 8>; [41.00%]

  <bb 8> [local count: 220117074]:

  <bb 9> [local count: 536870913]:
  # iftmp.58_16 = PHI <0(7), 255(8)>
  clkState[4] = iftmp.58_16;

  <bb 10> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _8 = freqPointers[3];
  if (_8 == 0)
    goto <bb 11>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 11> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _9 ={v} MEM[(struct SIRC_Type *)1076658176B].MISCELLANEOUS_IN;
  _10 = _9 & 256;
  if (_10 == 0)
    goto <bb 13>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 268435456]:

  <bb 13> [local count: 536870913]:
  # iftmp.59_17 = PHI <0(11), 255(12)>
  clkState[3] = iftmp.59_17;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  clkState[2] = 255;
  # DEBUG BEGIN_STMT
  _11 = freqPointers[5];
  if (_11 == 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 18>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _12 ={v} MEM[(struct SXOSC_Type *)1076674560B].SXOSC_STAT;
  _13 = (signed int) _12;
  if (_13 >= 0)
    goto <bb 17>; [59.00%]
  else
    goto <bb 16>; [41.00%]

  <bb 16> [local count: 220117074]:

  <bb 17> [local count: 536870913]:
  # iftmp.60_18 = PHI <0(15), 255(16)>
  clkState[5] = iftmp.60_18;

  <bb 18> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _14 = freqPointers[6];
  if (_14 == 0)
    goto <bb 19>; [50.00%]
  else
    goto <bb 20>; [50.00%]

  <bb 19> [local count: 536870912]:
  NOT_UNDER_MCU_CONTROL_A.part.0 ();

  <bb 20> [local count: 1073741824]:
  return;

}


CONFIG_ELEMENTS_MAPPINGS_02 ()
{
  uint8 j;
  uint8 i;
  int _1;
  <unnamed type> _2;
  int _3;
  unsigned char _4;
  const struct Clock_Ip_ClockConfigType * config_clock.65_5;
  unsigned char _6;
  int _7;
  <unnamed type> _8;
  int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.65_11;
  unsigned char _12;
  int _13;
  <unnamed type> _14;
  int _15;
  unsigned char _16;
  unsigned char _17;
  <unnamed type> _19;
  int _20;
  <unnamed type> _21;
  unsigned char _22;
  unsigned char _23;
  int _24;
  <unnamed type> _25;
  int _26;
  <unnamed type> _27;
  unsigned char _28;
  unsigned char _29;

  <bb 2> [local count: 7299031]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG i => 0
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  _1 = (int) i_30;
  _2 = config_clock.65_5->selectors[_1].name;
  if (_2 <= 20)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 29527898]:
  # DEBUG BEGIN_STMT
  _3 = (int) _2;
  _4 = i_30 + 1;
  freqPointers[_3] = _4;

  <bb 5> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  i_60 = i_30 + 1;
  # DEBUG i => i_60

  <bb 6> [local count: 66354828]:
  # i_30 = PHI <0(2), i_60(5)>
  # DEBUG i => i_30
  # DEBUG BEGIN_STMT
  config_clock.65_5 = config_clock;
  _6 = config_clock.65_5->selectorsCount;
  if (_6 > i_30)
    goto <bb 3>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 7> [local count: 7299031]:
  # config_clock.65_11 = PHI <config_clock.65_5(6)>
  goto <bb 11>; [100.00%]

  <bb 8> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  _7 = (int) i_31;
  _8 = config_clock.65_11->dividers[_7].name;
  if (_8 <= 20)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 29527899]:
  # DEBUG BEGIN_STMT
  _9 = (int) _8;
  _10 = i_31 + 1;
  freqPointers[_9] = _10;

  <bb 10> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  i_58 = i_31 + 1;
  # DEBUG i => i_58

  <bb 11> [local count: 66354828]:
  # i_31 = PHI <i_58(10), 0(7)>
  # DEBUG i => i_31
  # DEBUG BEGIN_STMT
  _12 = config_clock.65_11->dividersCount;
  if (_12 > i_31)
    goto <bb 8>; [89.00%]
  else
    goto <bb 34>; [11.00%]

  <bb 34> [local count: 7299031]:
  goto <bb 15>; [100.00%]

  <bb 12> [local count: 59055798]:
  # DEBUG BEGIN_STMT
  _13 = (int) i_32;
  _14 = config_clock.65_11->fracDivs[_13].name;
  if (_14 <= 20)
    goto <bb 13>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 13> [local count: 29527899]:
  # DEBUG BEGIN_STMT
  _15 = (int) _14;
  _16 = i_32 + 1;
  freqPointers[_15] = _16;

  <bb 14> [local count: 59055798]:
  # DEBUG BEGIN_STMT
  i_56 = i_32 + 1;
  # DEBUG i => i_56

  <bb 15> [local count: 66354829]:
  # i_32 = PHI <i_56(14), 0(34)>
  # DEBUG i => i_32
  # DEBUG BEGIN_STMT
  _17 = config_clock.65_11->fracDivsCount;
  if (_17 > i_32)
    goto <bb 12>; [89.00%]
  else
    goto <bb 32>; [11.00%]

  <bb 32> [local count: 7299031]:
  goto <bb 21>; [100.00%]

  <bb 16> [local count: 1014686024]:
  # DEBUG BEGIN_STMT
  _19 = pcfsEntries[0].name;
  _20 = (int) i_33;
  _21 = config_clock.65_11->pcfs[_20].name;
  if (_19 == _21)
    goto <bb 17>; [67.00%]
  else
    goto <bb 35>; [33.00%]

  <bb 35> [local count: 334846388]:
  goto <bb 29>; [100.00%]

  <bb 17> [local count: 679839636]:
  # DEBUG BEGIN_STMT
  _22 = i_33 + 1;
  pcfsEntries[0].configIndex = _22;

  <bb 19> [local count: 738895437]:
  # j_43 = PHI <1(17), 0(33)>

  <bb 29> [local count: 1073741824]:
  # j_35 = PHI <j_43(19), 1(35)>
  # DEBUG j => j_35
  # DEBUG BEGIN_STMT
  if (j_35 == 0)
    goto <bb 16>; [94.50%]
  else
    goto <bb 20>; [5.50%]

  <bb 20> [local count: 59055800]:
  # DEBUG BEGIN_STMT
  i_53 = i_33 + 1;
  # DEBUG i => i_53

  <bb 21> [local count: 66354831]:
  # i_33 = PHI <i_53(20), 0(32)>
  # DEBUG i => i_33
  # DEBUG BEGIN_STMT
  _23 = config_clock.65_11->pcfsCount;
  if (_23 > i_33)
    goto <bb 33>; [89.00%]
  else
    goto <bb 30>; [11.00%]

  <bb 33> [local count: 59055800]:
  goto <bb 19>; [100.00%]

  <bb 30> [local count: 7299031]:
  goto <bb 27>; [100.00%]

  <bb 22> [local count: 236223206]:
  # DEBUG BEGIN_STMT
  _24 = (int) j_36;
  _25 = cmuEntries[_24].name;
  _26 = (int) i_34;
  _27 = config_clock.65_11->cmus[_26].name;
  if (_25 == _27)
    goto <bb 23>; [34.00%]
  else
    goto <bb 24>; [66.00%]

  <bb 23> [local count: 80315890]:
  # DEBUG BEGIN_STMT
  _28 = i_34 + 1;
  cmuEntries[_24].configIndex = _28;

  <bb 24> [local count: 236223206]:
  # DEBUG BEGIN_STMT
  j_52 = j_36 + 1;
  # DEBUG j => j_52

  <bb 25> [local count: 295279007]:
  # j_36 = PHI <j_52(24), 0(31)>
  # DEBUG j => j_36
  # DEBUG BEGIN_STMT
  if (j_36 != 4)
    goto <bb 22>; [80.00%]
  else
    goto <bb 26>; [20.00%]

  <bb 26> [local count: 59055801]:
  # DEBUG BEGIN_STMT
  i_50 = i_34 + 1;
  # DEBUG i => i_50

  <bb 27> [local count: 66354833]:
  # i_34 = PHI <i_50(26), 0(30)>
  # DEBUG i => i_34
  # DEBUG BEGIN_STMT
  _29 = config_clock.65_11->cmusCount;
  if (_29 > i_34)
    goto <bb 31>; [89.00%]
  else
    goto <bb 28>; [11.00%]

  <bb 31> [local count: 59055801]:
  goto <bb 25>; [100.00%]

  <bb 28> [local count: 7299032]:
  return;

}


CONFIG_ELEMENTS_MAPPINGS_01 ()
{
  uint8 i;
  int _1;

  <bb 2> [local count: 46707770]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG i => 0
  goto <bb 4>; [100.00%]

  <bb 3> [local count: 1027034056]:
  # DEBUG BEGIN_STMT
  _1 = (int) i_3;
  freqPointers[_1] = 0;
  # DEBUG BEGIN_STMT
  i_9 = i_3 + 1;
  # DEBUG i => i_9

  <bb 4> [local count: 1073741824]:
  # i_3 = PHI <0(2), i_9(3)>
  # DEBUG i => i_3
  # DEBUG BEGIN_STMT
  if (i_3 != 22)
    goto <bb 3>; [95.65%]
  else
    goto <bb 5>; [4.35%]

  <bb 5> [local count: 46707769]:
  # i_4 = PHI <0(4)>
  CONFIG_ELEMENTS_MAPPINGS_01.part.0 ();
  return;

}


UpdateFrequencies (power_modes_t powerMode)
{
  uint8 pllEn;
  static const clock_element_state_t convertValueToClockState[256] = {0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 255};
  static const uint8 bufferFreqEntriesCLKOUT_RUN_CLK[3][13] = {"\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00", "\x00\x0f#\x10\x11\x12$\x13\x14\x15\x16\x17\x18", "\x00\x0f#\x10\x11\x12$%&\'(\x17\x18"};
  static const Clock_Ip_NameType selectorEntriesCLKOUT_RUN_CLK[13] = {21, 0, 8, 2, 4, 5, 9, 13, 16, 14, 15, 10, 11};
  static const uint8 bufferFreqEntriesQSPI_MEM_CLK[3] = "\x00\x0e\"";
  static const uint8 bufferFreqEntriesLBIST_CLK[3] = "\x00\r!";
  static const uint8 bufferFreqEntriesDCM_CLK[3] = "\x00\f ";
  static const uint8 bufferFreqEntriesHSE_CLK[3] = "\x00\v\x1f";
  static const uint8 bufferFreqEntriesAIPS_SLOW_CLK[3] = "\x00\n\x1e";
  static const uint8 bufferFreqEntriesAIPS_PLAT_CLK[3] = "\x00\t\x1d";
  static const uint8 bufferFreqEntriesCORE_CLK[3] = "\x00\b\x1c";
  static const uint8 bufferFreqEntriesSCS_CLK[3] = "\x00\x01\x1a";
  static const Clock_Ip_NameType selectorEntriesSCS_CLK[3] = {21, 0, 8};
  <unnamed type> _1;
  unsigned char _2;
  <unnamed type> _3;
  unsigned char _4;
  <unnamed type> _5;
  unsigned char _6;
  <unnamed type> _7;
  unsigned char _8;
  unsigned char _9;
  <unnamed type> _10;
  unsigned char _11;
  int _12;
  <unnamed type> _13;
  <unnamed type> _14;
  unsigned char _15;
  int _16;
  <unnamed type> _17;
  unsigned char _18;
  unsigned char _19;
  <unnamed type> _20;
  int _21;
  <unnamed type> _22;
  int _23;
  <unnamed type> _24;
  unsigned char _25;
  unsigned char _26;
  unsigned char _27;
  unsigned char _28;
  unsigned char _29;
  unsigned char _30;
  unsigned char _31;
  unsigned char _32;
  unsigned char _33;
  unsigned char _34;
  unsigned char _35;
  unsigned char _36;
  unsigned char _37;
  unsigned char _38;
  unsigned char _39;
  unsigned char _40;
  long unsigned int _41;
  long unsigned int _42;
  long unsigned int _43;
  <unnamed type> _44;
  int _45;
  <unnamed type> _46;
  int _47;
  <unnamed type> _48;
  unsigned char _49;
  unsigned char _50;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = clkState[1];
  _2 = _1 & 1;
  freqPointers[1] = _2;
  # DEBUG BEGIN_STMT
  _3 = clkState[3];
  _4 = _3 & 2;
  freqPointers[3] = _4;
  # DEBUG BEGIN_STMT
  pllEn_54 = clkState[6];
  # DEBUG pllEn => pllEn_54
  # DEBUG BEGIN_STMT
  _5 = clkState[4];
  _6 = _5 & 3;
  freqPointers[4] = _6;
  # DEBUG BEGIN_STMT
  _7 = clkState[5];
  _8 = _7 & 4;
  freqPointers[5] = _8;
  # DEBUG BEGIN_STMT
  _9 = pllEn_54 & 5;
  freqPointers[6] = _9;
  # DEBUG BEGIN_STMT
  _10 = clkState[8];
  _11 = _10 & pllEn_54;
  _12 = (int) _11;
  _13 = convertValueToClockState[_12];
  clkState[8] = _13;
  # DEBUG BEGIN_STMT
  _14 = clkState[9];
  _15 = _14 & pllEn_54;
  _16 = (int) _15;
  _17 = convertValueToClockState[_16];
  clkState[9] = _17;
  # DEBUG BEGIN_STMT
  _18 = _13 & 26;
  freqPointers[8] = _18;
  # DEBUG BEGIN_STMT
  _19 = _17 & 27;
  freqPointers[9] = _19;
  # DEBUG BEGIN_STMT
  _20 = clkState[12];
  _21 = (int) _20;
  _22 = selectorEntriesSCS_CLK[_21];
  _23 = (int) _22;
  _24 = clkState[_23];
  _25 = bufferFreqEntriesSCS_CLK[_21];
  _26 = _24 & _25;
  freqPointers[12] = _26;
  # DEBUG BEGIN_STMT
  _27 = bufferFreqEntriesCORE_CLK[_21];
  _28 = _24 & _27;
  freqPointers[13] = _28;
  # DEBUG BEGIN_STMT
  _29 = bufferFreqEntriesAIPS_PLAT_CLK[_21];
  _30 = _24 & _29;
  freqPointers[14] = _30;
  # DEBUG BEGIN_STMT
  _31 = bufferFreqEntriesAIPS_SLOW_CLK[_21];
  _32 = _24 & _31;
  freqPointers[15] = _32;
  # DEBUG BEGIN_STMT
  _33 = bufferFreqEntriesHSE_CLK[_21];
  _34 = _24 & _33;
  freqPointers[16] = _34;
  # DEBUG BEGIN_STMT
  _35 = bufferFreqEntriesDCM_CLK[_21];
  _36 = _24 & _35;
  freqPointers[17] = _36;
  # DEBUG BEGIN_STMT
  _37 = bufferFreqEntriesLBIST_CLK[_21];
  _38 = _24 & _37;
  freqPointers[18] = _38;
  # DEBUG BEGIN_STMT
  _39 = bufferFreqEntriesQSPI_MEM_CLK[_21];
  _40 = _24 & _39;
  freqPointers[19] = _40;
  # DEBUG BEGIN_STMT
  _41 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].CSS;
  _42 = _41 >> 24;
  _43 = _42 & 63;
  _44 = selectorEntryIndex[_43];
  clkState[20] = _44;
  # DEBUG BEGIN_STMT
  _45 = (int) _44;
  _46 = selectorEntriesCLKOUT_RUN_CLK[_45];
  _47 = (int) _46;
  _48 = clkState[_47];
  _49 = bufferFreqEntriesCLKOUT_RUN_CLK[_21][_45];
  _50 = _48 & _49;
  freqPointers[20] = _50;
  return;

}


GetProducerClockFreq (Clock_Ip_NameType clockName)
{
  int _1;
  unsigned char _2;
  int _3;
  uint32 _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = (int) clockName_4(D);
  _2 = freqPointers[_1];
  _3 = (int) _2;
  _6 = bufferFreqs[_3];
  return _6;

}


SpecificPlatformInitClock (const struct Clock_Ip_ClockConfigType * config)
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  config_clock = config_2(D);
  return;

}


SpecificPeripheralClockInitialization (const struct Clock_IP_SpecificPeriphConfigType * config)
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


GetClockState (Clock_Ip_NameType name)
{
  clock_element_state_t retValue;
  int _1;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (name_3(D) <= 20)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (int) name_3(D);
  retValue_6 = clkState[_1];
  # DEBUG retValue => retValue_6
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  retValue_5 = clkState[21];
  # DEBUG retValue => retValue_5

  <bb 5> [local count: 1073741824]:
  # retValue_2 = PHI <retValue_6(3), retValue_5(4)>
  # DEBUG retValue => retValue_2
  # DEBUG BEGIN_STMT
  return retValue_2;

}


UpdateClockState (Clock_Ip_NameType name, clock_element_state_t state)
{
  int _1;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (name_3(D) <= 20)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (int) name_3(D);
  clkState[_1] = state_5(D);

  <bb 4> [local count: 1073741824]:
  return;

}


