Histogram:
ECU3_KATECH_Logic_1000ms ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


ECU3_KATECH_Logic_200ms ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


ECU3_KATECH_Logic_100ms ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


ECU3_KATECH_Logic_20ms ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


ECU3_KATECH_Logic_10ms ()
{
  unsigned char _1;
  short unsigned int _2;
  unsigned char _3;
  short unsigned int _4;
  short unsigned int GV_DIN_CH1.0_5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Digital_Read (0);
  _2 = (short unsigned int) _1;
  GV_DIN_CH1 = _2;
  # DEBUG BEGIN_STMT
  _3 = Digital_Read (1);
  _4 = (short unsigned int) _3;
  GV_DIN_CH2 = _4;
  # DEBUG BEGIN_STMT
  GV_DIN_CH1.0_5 = GV_DIN_CH1;
  Emergency_Switch = GV_DIN_CH1.0_5;
  # DEBUG BEGIN_STMT
  ACU_Arc_check ();
  # DEBUG BEGIN_STMT
  ACU_Arc_check1 ();
  # DEBUG BEGIN_STMT
  ACU_Arc_check2 ();
  # DEBUG BEGIN_STMT
  ACU_Arc_check3 ();
  # DEBUG BEGIN_STMT
  IDB_Arc_check ();
  # DEBUG BEGIN_STMT
  RCU_Arc_check ();
  # DEBUG BEGIN_STMT
  RWA1_Arc_check ();
  # DEBUG BEGIN_STMT
  RWA2_Arc_check ();
  # DEBUG BEGIN_STMT
  ECU_check ();
  return;

}


ECU3_KATECH_Logic_5ms ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


ECU3_KATECH_Logic_2ms ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  System_Check_Func ();
  return;

}


ECU3_KATECH_Logic_init ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


