
Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:
Symbol table:

OsIf_GetCounter/73 (OsIf_GetCounter) @06d85e00
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_AutoBaudCapture/25 (536870913 (estimated locally),0.50 per call) 
  Calls: 
OsIf_MicrosToTicks/72 (OsIf_MicrosToTicks) @06d85d20
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_AutoBaudCapture/25 (536870913 (estimated locally),0.50 per call) 
  Calls: 
currentTick.4732/71 (currentTick) @06d93990
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: Lpuart_Lin_Ip_AutoBaudCapture/25 (addr)Lpuart_Lin_Ip_AutoBaudCapture/25 (write)
  Availability: available
  Varpool flags:
OsIf_GetElapsed/70 (OsIf_GetElapsed) @06d85b60
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_AutoBaudCapture/25 (536870913 (estimated locally),0.50 per call) 
  Calls: 
fallingEgdeCount.4733/69 (fallingEgdeCount) @06d93900
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: Lpuart_Lin_Ip_AutoBaudCapture/25 (read)Lpuart_Lin_Ip_AutoBaudCapture/25 (write)
  Availability: available
  Varpool flags:
Lpuart_Lin_Ip_HwGetIntMode/68 (Lpuart_Lin_Ip_HwGetIntMode) @06d85460
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_IRQHandler/43 (248034361 (estimated locally),0.23 per call) Lpuart_Lin_Ip_IRQHandler/43 (134699661 (estimated locally),0.13 per call) Lpuart_Lin_Ip_IRQHandler/43 (244419636 (estimated locally),0.23 per call) Lpuart_Lin_Ip_IRQHandler/43 (375809638 (estimated locally),0.35 per call) Lpuart_Lin_Ip_IRQHandler/43 (1073741823 (estimated locally),1.00 per call) Lpuart_Lin_Ip_FrameIrqHandler/46 (354334802 (estimated locally),0.33 per call) 
  Calls: 
SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_02/67 (SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_02) @06d850e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_GotoIdleState/42 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_02/66 (SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_02) @06d85000
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_GotoIdleState/42 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Lin_Ip_ProcessParity/65 (Lin_Ip_ProcessParity) @06d6dd20
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_ProcessFrameHeader/47 (88583700 (estimated locally),0.08 per call) Lpuart_Lin_Ip_MasterSendHeader/41 (84632867 (estimated locally),0.08 per call) 
  Calls: 
SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_01/64 (SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_01) @06d6d2a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_AsyncReceiveFrameData/32 (354334802 (estimated locally),0.33 per call) 
  Calls: 
SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01/63 (SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01) @06d6d1c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_AsyncReceiveFrameData/32 (354334802 (estimated locally),0.33 per call) 
  Calls: 
Lin_Ip_MakeChecksumByte/62 (Lin_Ip_MakeChecksumByte) @06d5bb60
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_MakeChecksumByte/24 (248622363 (estimated locally),1.00 per call) 
  Calls: 
SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_00/61 (SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_00) @06d5b8c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_AsyncSendFrameData/29 (354334802 (estimated locally),0.33 per call) 
  Calls: 
SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00/60 (SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00) @06d5b7e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_AsyncSendFrameData/29 (354334802 (estimated locally),0.33 per call) 
  Calls: 
Lpuart_Lin_Ip_HwGetStatusFlag/59 (Lpuart_Lin_Ip_HwGetStatusFlag) @06d5b620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_IRQHandler/43 (751619277 (estimated locally),0.70 per call) Lpuart_Lin_Ip_IRQHandler/43 (408180792 (estimated locally),0.38 per call) Lpuart_Lin_Ip_IRQHandler/43 (488839272 (estimated locally),0.46 per call) Lpuart_Lin_Ip_IRQHandler/43 (627602097 (estimated locally),0.58 per call) Lpuart_Lin_Ip_IRQHandler/43 (751619277 (estimated locally),0.70 per call) Lpuart_Lin_Ip_FrameIrqHandler/46 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_ProcessSendFrameData/49 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_AbortTransferData/34 (1073741824 (estimated locally),9.35 per call) Lpuart_Lin_Ip_SyncReceiveFrameData/33 (1014686025 (estimated locally),27.25 per call) Lpuart_Lin_Ip_SyncSendFrameData/30 (1073741824 (estimated locally),27.64 per call) Lpuart_Lin_Ip_Deinit/28 (1073741824 (estimated locally),9.35 per call) 
  Calls: 
Lpuart_Lin_Ip_TimeoutExpired/58 (Lpuart_Lin_Ip_TimeoutExpired) @06d5b380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_AbortTransferData/34 (1014686025 (estimated locally),8.83 per call) Lpuart_Lin_Ip_SyncReceiveFrameData/33 (1073741824 (estimated locally),28.84 per call) Lpuart_Lin_Ip_SyncSendFrameData/30 (1014686025 (estimated locally),26.12 per call) Lpuart_Lin_Ip_Deinit/28 (1014686025 (estimated locally),8.83 per call) Lpuart_Lin_Ip_HwSetReceiverCmd/1 (118111601 (estimated locally),9.09 per call) Lpuart_Lin_Ip_HwSetTransmitterCmd/0 (118111601 (estimated locally),9.09 per call) 
  Calls: 
Lpuart_Lin_Ip_StartTimeout/57 (Lpuart_Lin_Ip_StartTimeout) @06d5b2a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_AbortTransferData/34 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_SyncReceiveFrameData/33 (114863532 (estimated locally),3.08 per call) Lpuart_Lin_Ip_SyncSendFrameData/30 (114863532 (estimated locally),2.96 per call) Lpuart_Lin_Ip_Deinit/28 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetReceiverCmd/1 (12992276 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetTransmitterCmd/0 (12992276 (estimated locally),1.00 per call) 
  Calls: 
SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_04/56 (SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_04) @06d5b0e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_04/55 (SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_04) @06d5b000
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Lpuart_Lin_Ip_HwClearStatusFlag/54 (Lpuart_Lin_Ip_HwClearStatusFlag) @06cf4a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_IRQHandler/43 (221023419 (estimated locally),0.21 per call) Lpuart_Lin_Ip_IRQHandler/43 (81851339 (estimated locally),0.08 per call) Lpuart_Lin_Ip_IRQHandler/43 (322122547 (estimated locally),0.30 per call) Lpuart_Lin_Ip_ProcessWakeupDetect/26 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_ProcessBreakDetect/44 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_GoToSleepMode/36 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_Init/27 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_FrameErrorIrqHandler/23 (1073741823 (estimated locally),1.00 per call) 
  Calls: 
Lpuart_Lin_Ip_HwSetIntMode/53 (Lpuart_Lin_Ip_HwSetIntMode) @06cf49a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_ProcessSendFrameData/49 (44291850 (estimated locally),0.04 per call) Lpuart_Lin_Ip_AbortTransferData/34 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_AbortTransferData/34 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_AbortTransferData/34 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_SyncReceiveFrameData/33 (12287527 (estimated locally),0.33 per call) Lpuart_Lin_Ip_SyncReceiveFrameData/33 (12287527 (estimated locally),0.33 per call) Lpuart_Lin_Ip_SyncSendFrameData/30 (12818615 (estimated locally),0.33 per call) Lpuart_Lin_Ip_SyncSendFrameData/30 (12818615 (estimated locally),0.33 per call) Lpuart_Lin_Ip_GotoIdleState/42 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_GotoIdleState/42 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_GotoIdleState/42 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_GotoIdleState/42 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_MasterSendHeader/41 (84632867 (estimated locally),0.08 per call) Lpuart_Lin_Ip_ProcessBreakDetect/44 (177167401 (estimated locally),0.17 per call) Lpuart_Lin_Ip_ProcessBreakDetect/44 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_ProcessBreakDetect/44 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_GoToSleepMode/36 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_GoToSleepMode/36 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_GoToSleepMode/36 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_GoToSleepMode/36 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_Init/27 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_Init/27 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_Init/27 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_AutoBaudCapture/25 (131211251 (estimated locally),0.12 per call) 
  Calls: 
Lpuart_Lin_Ip_HwSetParityMode/52 (Lpuart_Lin_Ip_HwSetParityMode) @06cf48c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_Init/27 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Lpuart_Lin_Ip_HwSetBitCountPerChar/51 (Lpuart_Lin_Ip_HwSetBitCountPerChar) @06cf47e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_Init/27 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Lpuart_Lin_Ip_HwInit/50 (Lpuart_Lin_Ip_HwInit) @06cf4700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: Lpuart_Lin_Ip_Init/27 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Lpuart_Lin_Ip_ProcessSendFrameData/49 (Lpuart_Lin_Ip_ProcessSendFrameData) @06cf42a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_FrameIrqHandler/46 (44291850 (estimated locally),0.04 per call) 
  Calls: Lpuart_Lin_Ip_GotoIdleState/42 (21649856 (estimated locally),0.02 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (44291850 (estimated locally),0.04 per call) Lpuart_Lin_Ip_GotoIdleState/42 (402653184 (estimated locally),0.38 per call) Lpuart_Lin_Ip_GotoIdleState/42 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (1073741824 (estimated locally),1.00 per call) 
   Indirect call(31004295 (estimated locally),0.03 per call) 
   Indirect call(281857229 (estimated locally),0.26 per call) 
   Indirect call(375809639 (estimated locally),0.35 per call) 
Lpuart_Lin_Ip_ProcessReceiveFrameData/48 (Lpuart_Lin_Ip_ProcessReceiveFrameData) @06cf4000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_FrameIrqHandler/46 (44291850 (estimated locally),0.04 per call) 
  Calls: Lpuart_Lin_Ip_GotoIdleState/42 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_GetBytetoBuffer/21 (1073741824 (estimated locally),1.00 per call) 
   Indirect call(375809639 (estimated locally),0.35 per call) 
   Indirect call(127775277 (estimated locally),0.12 per call) 
Lpuart_Lin_Ip_ProcessFrameHeader/47 (Lpuart_Lin_Ip_ProcessFrameHeader) @06ce3b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741823 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_FrameIrqHandler/46 (44291850 (estimated locally),0.04 per call) 
  Calls: Lpuart_Lin_Ip_GotoIdleState/42 (30118458 (estimated locally),0.03 per call) Lin_Ip_ProcessParity/65 (88583700 (estimated locally),0.08 per call) Lpuart_Lin_Ip_GotoIdleState/42 (177167401 (estimated locally),0.17 per call) 
   Indirect call(21082921 (estimated locally),0.02 per call) 
   Indirect call(40925670 (estimated locally),0.04 per call) 
   Indirect call(83091511 (estimated locally),0.08 per call) 
   Indirect call(42804718 (estimated locally),0.04 per call) 
   Indirect call(124017180 (estimated locally),0.12 per call) 
   Indirect call(124017180 (estimated locally),0.12 per call) 
Lpuart_Lin_Ip_FrameIrqHandler/46 (Lpuart_Lin_Ip_FrameIrqHandler) @06ce3620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_IRQHandler/43 (408180791 (estimated locally),0.38 per call) 
  Calls: Lpuart_Lin_Ip_ProcessSendFrameData/49 (44291850 (estimated locally),0.04 per call) Lpuart_Lin_Ip_ProcessReceiveFrameData/48 (44291850 (estimated locally),0.04 per call) Lpuart_Lin_Ip_ProcessFrameHeader/47 (44291850 (estimated locally),0.04 per call) Lpuart_Lin_Ip_HwGetIntMode/68 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (1073741824 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_CheckWakeupSignal/45 (Lpuart_Lin_Ip_CheckWakeupSignal) @06ce30e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_ProcessWakeupDetect/26 (357878150 (estimated locally),0.33 per call) 
  Calls: Lpuart_Lin_Ip_GotoIdleState/42 (268435456 (estimated locally),0.25 per call) 
   Indirect call(187904819 (estimated locally),0.17 per call) 
   Indirect call(536870913 (estimated locally),0.50 per call) 
   Indirect call(536870913 (estimated locally),0.50 per call) 
Lpuart_Lin_Ip_ProcessBreakDetect/44 (Lpuart_Lin_Ip_ProcessBreakDetect) @06ce3d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_IRQHandler/43 (124017180 (estimated locally),0.12 per call) 
  Calls: Lpuart_Lin_Ip_HwSetReceiverCmd/1 (177167401 (estimated locally),0.17 per call) Lpuart_Lin_Ip_HwSetTransmitterCmd/0 (177167401 (estimated locally),0.17 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (177167401 (estimated locally),0.17 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwClearStatusFlag/54 (1073741824 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_IRQHandler/43 (Lpuart_Lin_Ip_IRQHandler) @06ce3a80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741823 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_HwClearStatusFlag/54 (221023419 (estimated locally),0.21 per call) Lpuart_Lin_Ip_HwClearStatusFlag/54 (81851339 (estimated locally),0.08 per call) Lpuart_Lin_Ip_HwGetIntMode/68 (248034361 (estimated locally),0.23 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (751619277 (estimated locally),0.70 per call) Lpuart_Lin_Ip_FrameIrqHandler/46 (408180791 (estimated locally),0.38 per call) Lpuart_Lin_Ip_HwGetIntMode/68 (134699661 (estimated locally),0.13 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (408180792 (estimated locally),0.38 per call) Lpuart_Lin_Ip_GotoIdleState/42 (80658480 (estimated locally),0.08 per call) Lpuart_Lin_Ip_FrameErrorIrqHandler/23 (80658480 (estimated locally),0.08 per call) Lpuart_Lin_Ip_HwGetIntMode/68 (244419636 (estimated locally),0.23 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (488839272 (estimated locally),0.46 per call) Lpuart_Lin_Ip_ProcessWakeupDetect/26 (138762824 (estimated locally),0.13 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (627602097 (estimated locally),0.58 per call) Lpuart_Lin_Ip_ProcessBreakDetect/44 (124017180 (estimated locally),0.12 per call) Lpuart_Lin_Ip_HwGetIntMode/68 (375809638 (estimated locally),0.35 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (751619277 (estimated locally),0.70 per call) Lpuart_Lin_Ip_HwClearStatusFlag/54 (322122547 (estimated locally),0.30 per call) Lpuart_Lin_Ip_HwGetIntMode/68 (1073741823 (estimated locally),1.00 per call) 
   Indirect call(57295937 (estimated locally),0.05 per call) 
Lpuart_Lin_Ip_GotoIdleState/42 (Lpuart_Lin_Ip_GotoIdleState) @06ce37e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: Lpuart_Lin_Ip_IRQHandler/43 (80658480 (estimated locally),0.08 per call) Lpuart_Lin_Ip_ProcessSendFrameData/49 (21649856 (estimated locally),0.02 per call) Lpuart_Lin_Ip_ProcessSendFrameData/49 (402653184 (estimated locally),0.38 per call) Lpuart_Lin_Ip_ProcessSendFrameData/49 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_ProcessReceiveFrameData/48 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_ProcessFrameHeader/47 (30118458 (estimated locally),0.03 per call) Lpuart_Lin_Ip_ProcessFrameHeader/47 (177167401 (estimated locally),0.17 per call) Lpuart_Lin_Ip_CheckWakeupSignal/45 (268435456 (estimated locally),0.25 per call) Lpuart_Lin_Ip_AbortTransferData/34 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_SyncReceiveFrameData/33 (12287526 (estimated locally),0.33 per call) Lpuart_Lin_Ip_SyncSendFrameData/30 (12818614 (estimated locally),0.33 per call) 
  Calls: SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_02/67 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_02/66 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_MasterSendHeader/41 (Lpuart_Lin_Ip_MasterSendHeader) @06ce3540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_HwSetIntMode/53 (84632867 (estimated locally),0.08 per call) Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (84632867 (estimated locally),0.08 per call) Lin_Ip_ProcessParity/65 (84632867 (estimated locally),0.08 per call) 
Lpuart_Lin_Ip_SetTimeoutCounter/40 (Lpuart_Lin_Ip_SetTimeoutCounter) @06ce32a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
Lpuart_Lin_Ip_TimeoutService/39 (Lpuart_Lin_Ip_TimeoutService) @06ce3000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
   Indirect call(187904819 (estimated locally),0.17 per call) 
Lpuart_Lin_Ip_GetCurrentNodeState/38 (Lpuart_Lin_Ip_GetCurrentNodeState) @06cb5b60
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
Lpuart_Lin_Ip_SendWakeupSignal/37 (Lpuart_Lin_Ip_SendWakeupSignal) @06cb5620
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_au8WakeupSignal/15 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
Lpuart_Lin_Ip_GoToSleepMode/36 (Lpuart_Lin_Ip_GoToSleepMode) @06cb50e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwClearStatusFlag/54 (1073741824 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_GetReceiveStatus/35 (Lpuart_Lin_Ip_GetReceiveStatus) @06cb5d20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
Lpuart_Lin_Ip_AbortTransferData/34 (Lpuart_Lin_Ip_AbortTransferData) @06cb5a80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)
  Referring: 
  Availability: available
  Function flags: count:114863532 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_GotoIdleState/42 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_TimeoutExpired/58 (1014686025 (estimated locally),8.83 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (1073741824 (estimated locally),9.35 per call) Lpuart_Lin_Ip_StartTimeout/57 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (114863532 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_SyncReceiveFrameData/33 (Lpuart_Lin_Ip_SyncReceiveFrameData) @06cb57e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:37234929 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_GotoIdleState/42 (12287526 (estimated locally),0.33 per call) Lpuart_Lin_Ip_GetBytetoBuffer/21 (18952483 (estimated locally),0.51 per call) Lpuart_Lin_Ip_TimeoutExpired/58 (1073741824 (estimated locally),28.84 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (1014686025 (estimated locally),27.25 per call) Lpuart_Lin_Ip_StartTimeout/57 (114863532 (estimated locally),3.08 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (12287527 (estimated locally),0.33 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (12287527 (estimated locally),0.33 per call) Lpuart_Lin_Ip_StatusBeforeTransfer/22 (37234929 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_AsyncReceiveFrameData/32 (Lpuart_Lin_Ip_AsyncReceiveFrameData) @06cb5540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (354334802 (estimated locally),0.33 per call) SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_01/64 (354334802 (estimated locally),0.33 per call) SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01/63 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_StatusBeforeTransfer/22 (1073741824 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_GetTransmitStatus/31 (Lpuart_Lin_Ip_GetTransmitStatus) @06cb52a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
Lpuart_Lin_Ip_SyncSendFrameData/30 (Lpuart_Lin_Ip_SyncSendFrameData) @06cb5000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:38844287 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_GotoIdleState/42 (12818614 (estimated locally),0.33 per call) Lpuart_Lin_Ip_TimeoutExpired/58 (1014686025 (estimated locally),26.12 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (1073741824 (estimated locally),27.64 per call) Lpuart_Lin_Ip_StartTimeout/57 (114863532 (estimated locally),2.96 per call) Lpuart_Lin_Ip_MakeChecksumByte/24 (12818615 (estimated locally),0.33 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (12818615 (estimated locally),0.33 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (12818615 (estimated locally),0.33 per call) Lpuart_Lin_Ip_StatusBeforeTransfer/22 (38844287 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_AsyncSendFrameData/29 (Lpuart_Lin_Ip_AsyncSendFrameData) @06bb3b60
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (354334802 (estimated locally),0.33 per call) SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_00/61 (354334802 (estimated locally),0.33 per call) SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00/60 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_MakeChecksumByte/24 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_StatusBeforeTransfer/22 (1073741824 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_Deinit/28 (Lpuart_Lin_Ip_Deinit) @06bb3620
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (write)
  Referring: 
  Availability: available
  Function flags: count:114863532 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_HwSetReceiverCmd/1 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetTransmitterCmd/0 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_TimeoutExpired/58 (1014686025 (estimated locally),8.83 per call) Lpuart_Lin_Ip_HwGetStatusFlag/59 (1073741824 (estimated locally),9.35 per call) Lpuart_Lin_Ip_StartTimeout/57 (114863532 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_Init/27 (Lpuart_Lin_Ip_Init) @06bb30e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (write)Lpuart_Lin_Ip_au8WakeupSignal/15 (write)Lpuart_Lin_Ip_apxStateStructureArray/19 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Lpuart_Lin_Ip_HwSetReceiverCmd/1 (714038314 (estimated locally),0.67 per call) Lpuart_Lin_Ip_HwSetTransmitterCmd/0 (714038314 (estimated locally),0.67 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwClearStatusFlag/54 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_HwSetBreakCharTransmitLength/12 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_HwSetParityMode/52 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetBitCountPerChar/51 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetBaudRateDivisor/2 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwSetOversamplingRatio/4 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_HwInit/50 (1073741824 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_ProcessWakeupDetect/26 (Lpuart_Lin_Ip_ProcessWakeupDetect) @06bb3d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_IRQHandler/43 (138762824 (estimated locally),0.13 per call) 
  Calls: Lpuart_Lin_Ip_AutoBaudCapture/25 (118099789 (estimated locally),0.11 per call) Lpuart_Lin_Ip_CheckWakeupSignal/45 (357878150 (estimated locally),0.33 per call) Lpuart_Lin_Ip_HwClearStatusFlag/54 (1073741824 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_AutoBaudCapture/25 (Lpuart_Lin_Ip_AutoBaudCapture) @06bb3a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)fallingEgdeCount.4733/69 (read)fallingEgdeCount.4733/69 (write)currentTick.4732/71 (addr)Lpuart_Lin_Ip_au8WakeupSignal/15 (write)currentTick.4732/71 (write)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_ProcessWakeupDetect/26 (118099789 (estimated locally),0.11 per call) 
  Calls: OsIf_GetCounter/73 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_HwSetIntMode/53 (131211251 (estimated locally),0.12 per call) Lpuart_Lin_Ip_HwSetBaudRateDivisor/2 (131211251 (estimated locally),0.12 per call) OsIf_MicrosToTicks/72 (536870913 (estimated locally),0.50 per call) OsIf_GetElapsed/70 (536870913 (estimated locally),0.50 per call) 
   Indirect call(91847876 (estimated locally),0.09 per call) 
Lpuart_Lin_Ip_MakeChecksumByte/24 (Lpuart_Lin_Ip_MakeChecksumByte) @06bb37e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: local
  Function flags: count:248622364 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_SyncSendFrameData/30 (12818615 (estimated locally),0.33 per call) Lpuart_Lin_Ip_AsyncSendFrameData/29 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_GetBytetoBuffer/21 (354334802 (estimated locally),0.33 per call) 
  Calls: Lin_Ip_MakeChecksumByte/62 (248622363 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_FrameErrorIrqHandler/23 (Lpuart_Lin_Ip_FrameErrorIrqHandler) @06bb3540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)Lpuart_Lin_Ip_apxUserConfigs/18 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741823 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_IRQHandler/43 (80658480 (estimated locally),0.08 per call) 
  Calls: Lpuart_Lin_Ip_HwClearStatusFlag/54 (1073741823 (estimated locally),1.00 per call) 
   Indirect call(168663365 (estimated locally),0.16 per call) 
   Indirect call(255550554 (estimated locally),0.24 per call) 
Lpuart_Lin_Ip_StatusBeforeTransfer/22 (Lpuart_Lin_Ip_StatusBeforeTransfer) @06bb32a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_SyncReceiveFrameData/33 (37234929 (estimated locally),1.00 per call) Lpuart_Lin_Ip_SyncSendFrameData/30 (38844287 (estimated locally),1.00 per call) Lpuart_Lin_Ip_AsyncReceiveFrameData/32 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_AsyncSendFrameData/29 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Lpuart_Lin_Ip_GetBytetoBuffer/21 (Lpuart_Lin_Ip_GetBytetoBuffer) @06bb3000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: Lpuart_Lin_Ip_apxBases/16 (read)Lpuart_Lin_Ip_apxStateStructureArray/19 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_ProcessReceiveFrameData/48 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_SyncReceiveFrameData/33 (18952483 (estimated locally),0.51 per call) 
  Calls: Lpuart_Lin_Ip_MakeChecksumByte/24 (354334802 (estimated locally),0.33 per call) 
Lpuart_Lin_Ip_apxStateStructureArray/19 (Lpuart_Lin_Ip_apxStateStructureArray) @06baa318
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: Lpuart_Lin_Ip_GetBytetoBuffer/21 (read)Lpuart_Lin_Ip_ProcessWakeupDetect/26 (read)Lpuart_Lin_Ip_AutoBaudCapture/25 (read)Lpuart_Lin_Ip_TimeoutService/39 (read)Lpuart_Lin_Ip_FrameIrqHandler/46 (read)Lpuart_Lin_Ip_MasterSendHeader/41 (read)Lpuart_Lin_Ip_Init/27 (write)Lpuart_Lin_Ip_SetTimeoutCounter/40 (read)Lpuart_Lin_Ip_GotoIdleState/42 (read)Lpuart_Lin_Ip_FrameErrorIrqHandler/23 (read)Lpuart_Lin_Ip_SyncSendFrameData/30 (read)Lpuart_Lin_Ip_Deinit/28 (write)Lpuart_Lin_Ip_GetTransmitStatus/31 (read)Lpuart_Lin_Ip_GetReceiveStatus/35 (read)Lpuart_Lin_Ip_GoToSleepMode/36 (read)Lpuart_Lin_Ip_SendWakeupSignal/37 (read)Lpuart_Lin_Ip_GetCurrentNodeState/38 (read)Lpuart_Lin_Ip_AsyncReceiveFrameData/32 (read)Lpuart_Lin_Ip_ProcessBreakDetect/44 (read)Lpuart_Lin_Ip_ProcessSendFrameData/49 (read)Lpuart_Lin_Ip_AsyncSendFrameData/29 (read)Lpuart_Lin_Ip_AbortTransferData/34 (read)Lpuart_Lin_Ip_SyncReceiveFrameData/33 (read)Lpuart_Lin_Ip_MakeChecksumByte/24 (read)Lpuart_Lin_Ip_ProcessFrameHeader/47 (read)Lpuart_Lin_Ip_ProcessReceiveFrameData/48 (read)Lpuart_Lin_Ip_CheckWakeupSignal/45 (read)Lpuart_Lin_Ip_Deinit/28 (read)Lpuart_Lin_Ip_AsyncSendFrameData/29 (read)Lpuart_Lin_Ip_AsyncReceiveFrameData/32 (read)Lpuart_Lin_Ip_ProcessBreakDetect/44 (read)Lpuart_Lin_Ip_ProcessBreakDetect/44 (read)Lpuart_Lin_Ip_SyncSendFrameData/30 (read)Lpuart_Lin_Ip_SyncReceiveFrameData/33 (read)Lpuart_Lin_Ip_IRQHandler/43 (read)
  Availability: available
  Varpool flags:
Lpuart_Lin_Ip_apxUserConfigs/18 (Lpuart_Lin_Ip_apxUserConfigs) @06baa288
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: Lpuart_Lin_Ip_FrameErrorIrqHandler/23 (read)Lpuart_Lin_Ip_Init/27 (write)Lpuart_Lin_Ip_MasterSendHeader/41 (read)Lpuart_Lin_Ip_TimeoutService/39 (read)Lpuart_Lin_Ip_GotoIdleState/42 (read)Lpuart_Lin_Ip_AutoBaudCapture/25 (read)Lpuart_Lin_Ip_AsyncReceiveFrameData/32 (read)Lpuart_Lin_Ip_ProcessBreakDetect/44 (read)Lpuart_Lin_Ip_ProcessReceiveFrameData/48 (read)Lpuart_Lin_Ip_AsyncSendFrameData/29 (read)Lpuart_Lin_Ip_SyncSendFrameData/30 (read)Lpuart_Lin_Ip_ProcessSendFrameData/49 (read)Lpuart_Lin_Ip_ProcessFrameHeader/47 (read)Lpuart_Lin_Ip_SyncReceiveFrameData/33 (read)Lpuart_Lin_Ip_CheckWakeupSignal/45 (read)Lpuart_Lin_Ip_IRQHandler/43 (read)
  Availability: available
  Varpool flags:
Lpuart_Lin_Ip_axStateStructure/17 (Lpuart_Lin_Ip_axStateStructure) @06baa1f8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags:
Lpuart_Lin_Ip_apxBases/16 (Lpuart_Lin_Ip_apxBases) @06baa168
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: Lpuart_Lin_Ip_GetBytetoBuffer/21 (read)Lpuart_Lin_Ip_AutoBaudCapture/25 (read)Lpuart_Lin_Ip_GoToSleepMode/36 (read)Lpuart_Lin_Ip_MasterSendHeader/41 (read)Lpuart_Lin_Ip_SendWakeupSignal/37 (read)Lpuart_Lin_Ip_GotoIdleState/42 (read)Lpuart_Lin_Ip_FrameIrqHandler/46 (read)Lpuart_Lin_Ip_SyncSendFrameData/30 (read)Lpuart_Lin_Ip_Init/27 (read)Lpuart_Lin_Ip_Deinit/28 (read)Lpuart_Lin_Ip_AsyncReceiveFrameData/32 (read)Lpuart_Lin_Ip_ProcessBreakDetect/44 (read)Lpuart_Lin_Ip_ProcessSendFrameData/49 (read)Lpuart_Lin_Ip_AsyncSendFrameData/29 (read)Lpuart_Lin_Ip_AbortTransferData/34 (read)Lpuart_Lin_Ip_SyncReceiveFrameData/33 (read)Lpuart_Lin_Ip_FrameErrorIrqHandler/23 (read)Lpuart_Lin_Ip_ProcessWakeupDetect/26 (read)Lpuart_Lin_Ip_ProcessFrameHeader/47 (read)Lpuart_Lin_Ip_CheckWakeupSignal/45 (read)Lpuart_Lin_Ip_IRQHandler/43 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
Lpuart_Lin_Ip_au8WakeupSignal/15 (Lpuart_Lin_Ip_au8WakeupSignal) @06baa090
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: Lpuart_Lin_Ip_Init/27 (write)Lpuart_Lin_Ip_AutoBaudCapture/25 (write)Lpuart_Lin_Ip_SendWakeupSignal/37 (read)
  Availability: available
  Varpool flags:
Lpuart_Lin_Ip_HwSetBreakCharDetectLength/13 (Lpuart_Lin_Ip_HwSetBreakCharDetectLength) @06b9b0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_GotoIdleState/42 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_MasterSendHeader/41 (84632867 (estimated locally),0.08 per call) Lpuart_Lin_Ip_ProcessBreakDetect/44 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_AsyncReceiveFrameData/32 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_AsyncSendFrameData/29 (354334802 (estimated locally),0.33 per call) Lpuart_Lin_Ip_Init/27 (536870913 (estimated locally),0.50 per call) Lpuart_Lin_Ip_Init/27 (536870913 (estimated locally),0.50 per call) 
  Calls: SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_04/56 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_04/55 (1073741824 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_HwSetBreakCharTransmitLength/12 (Lpuart_Lin_Ip_HwSetBreakCharTransmitLength) @06b97e00
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_Init/27 (536870913 (estimated locally),0.50 per call) 
  Calls: 
Lpuart_Lin_Ip_HwSetOversamplingRatio/4 (Lpuart_Lin_Ip_HwSetOversamplingRatio) @06b38380
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_Init/27 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
Lpuart_Lin_Ip_HwSetBaudRateDivisor/2 (Lpuart_Lin_Ip_HwSetBaudRateDivisor) @06b31d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_Init/27 (1073741824 (estimated locally),1.00 per call) Lpuart_Lin_Ip_AutoBaudCapture/25 (131211251 (estimated locally),0.12 per call) 
  Calls: 
Lpuart_Lin_Ip_HwSetReceiverCmd/1 (Lpuart_Lin_Ip_HwSetReceiverCmd) @06b31a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:12992276 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_ProcessBreakDetect/44 (177167401 (estimated locally),0.17 per call) Lpuart_Lin_Ip_Deinit/28 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_Init/27 (714038314 (estimated locally),0.67 per call) 
  Calls: Lpuart_Lin_Ip_TimeoutExpired/58 (118111601 (estimated locally),9.09 per call) Lpuart_Lin_Ip_StartTimeout/57 (12992276 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_HwSetTransmitterCmd/0 (Lpuart_Lin_Ip_HwSetTransmitterCmd) @06b317e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:12992276 (estimated locally) body local optimize_size
  Called by: Lpuart_Lin_Ip_ProcessBreakDetect/44 (177167401 (estimated locally),0.17 per call) Lpuart_Lin_Ip_Deinit/28 (114863532 (estimated locally),1.00 per call) Lpuart_Lin_Ip_Init/27 (714038314 (estimated locally),0.67 per call) 
  Calls: Lpuart_Lin_Ip_TimeoutExpired/58 (118111601 (estimated locally),9.09 per call) Lpuart_Lin_Ip_StartTimeout/57 (12992276 (estimated locally),1.00 per call) 
Lpuart_Lin_Ip_ProcessSendFrameData (const uint32 u32Instance, const uint8 tmpByte)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  struct LPUART_Type * base;
  boolean tmpBuffAndSize;
  boolean tmpCheckSumAndSize;
  uint8 tmpSize;
  _Bool _1;
  void (*<T2e6>) (uint32, void *) _2;
  unsigned char _3;
  unsigned char _4;
  unsigned char _5;
  const uint8 * _6;
  unsigned char _7;
  void (*<T2e6>) (uint32, void *) _8;
  const uint8 * _9;
  unsigned char _10;
  unsigned char _11;
  unsigned char _12;
  int _13;
  int _14;
  int _15;
  unsigned char _16;
  unsigned char _17;
  void (*<T2e6>) (uint32, void *) _18;
  <unnamed type> _19;
  int iftmp.29_20;
  int iftmp.30_21;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG sendFlag => 1
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  base_28 = Lpuart_Lin_Ip_apxBases[u32Instance_27(D)];
  # DEBUG base => base_28
  # DEBUG BEGIN_STMT
  pUserConfig_29 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_27(D)];
  # DEBUG pUserConfig => pUserConfig_29
  # DEBUG BEGIN_STMT
  linCurrentState_30 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_27(D)];
  # DEBUG linCurrentState => linCurrentState_30
  # DEBUG BEGIN_STMT
  _1 = Lpuart_Lin_Ip_HwGetStatusFlag (base_28, 131095);
  if (_1 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  linCurrentState_30->currentEventId ={v} 9;
  # DEBUG BEGIN_STMT
  _2 = pUserConfig_29->Callback;
  if (_2 != 0B)
    goto <bb 4>; [70.00%]
  else
    goto <bb 5>; [30.00%]

  <bb 4> [local count: 375809639]:
  # DEBUG BEGIN_STMT
  _2 (u32Instance_27(D), linCurrentState_30);

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  linCurrentState_30->isTxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_27(D));
  # DEBUG BEGIN_STMT
  # DEBUG sendFlag => 0
  # DEBUG BEGIN_STMT
  goto <bb 25>; [100.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _3 ={v} linCurrentState_30->txSize;
  _4 = linCurrentState_30->cntByte;
  tmpSize_32 = _3 - _4;
  # DEBUG tmpSize => tmpSize_32
  # DEBUG BEGIN_STMT
  if (tmpSize_32 == 1)
    goto <bb 7>; [34.00%]
  else
    goto <bb 8>; [66.00%]

  <bb 7> [local count: 182536110]:
  _5 = linCurrentState_30->checkSum;
  if (_5 != tmpByte_33(D))
    goto <bb 9>; [66.00%]
  else
    goto <bb 8>; [34.00%]

  <bb 8> [local count: 416397080]:

  <bb 9> [local count: 536870912]:
  # iftmp.29_20 = PHI <1(7), 0(8)>
  tmpCheckSumAndSize_34 = (boolean) iftmp.29_20;
  # DEBUG tmpCheckSumAndSize => tmpCheckSumAndSize_34
  # DEBUG BEGIN_STMT
  _6 = linCurrentState_30->txBuff;
  _7 = *_6;
  if (_7 != tmpByte_33(D))
    goto <bb 10>; [66.00%]
  else
    goto <bb 11>; [34.00%]

  <bb 10> [local count: 354334802]:
  if (tmpSize_32 != 1)
    goto <bb 12>; [66.00%]
  else
    goto <bb 11>; [34.00%]

  <bb 11> [local count: 303009943]:

  <bb 12> [local count: 536870911]:
  # iftmp.30_21 = PHI <1(10), 0(11)>
  tmpBuffAndSize_35 = (boolean) iftmp.30_21;
  # DEBUG tmpBuffAndSize => tmpBuffAndSize_35
  # DEBUG BEGIN_STMT
  if (tmpBuffAndSize_35 != 0)
    goto <bb 14>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 13> [local count: 268435456]:
  if (tmpCheckSumAndSize_34 != 0)
    goto <bb 14>; [50.00%]
  else
    goto <bb 17>; [50.00%]

  <bb 14> [local count: 402653184]:
  # DEBUG BEGIN_STMT
  linCurrentState_30->currentEventId ={v} 9;
  # DEBUG BEGIN_STMT
  _8 = pUserConfig_29->Callback;
  if (_8 != 0B)
    goto <bb 15>; [70.00%]
  else
    goto <bb 16>; [30.00%]

  <bb 15> [local count: 281857229]:
  # DEBUG BEGIN_STMT
  _8 (u32Instance_27(D), linCurrentState_30);

  <bb 16> [local count: 402653184]:
  # DEBUG BEGIN_STMT
  linCurrentState_30->isTxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_27(D));
  # DEBUG BEGIN_STMT
  # DEBUG sendFlag => 0
  # DEBUG BEGIN_STMT
  goto <bb 25>; [100.00%]

  <bb 17> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  _9 = _6 + 1;
  linCurrentState_30->txBuff = _9;
  # DEBUG BEGIN_STMT
  _10 = _4 + 1;
  linCurrentState_30->cntByte = _10;
  # DEBUG sendFlag => 1
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _11 ={v} linCurrentState_30->txSize;
  if (_10 < _11)
    goto <bb 18>; [67.00%]
  else
    goto <bb 21>; [33.00%]

  <bb 18> [local count: 89925878]:
  # DEBUG BEGIN_STMT
  _12 ={v} linCurrentState_30->txSize;
  _13 = (int) _12;
  _14 = (int) _10;
  _15 = _13 - _14;
  if (_15 == 1)
    goto <bb 19>; [34.00%]
  else
    goto <bb 20>; [66.00%]

  <bb 19> [local count: 30574798]:
  # DEBUG BEGIN_STMT
  _16 = linCurrentState_30->checkSum;
  # DEBUG base => base_28
  # DEBUG data => _16
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwPutchar
  # DEBUG BEGIN_STMT
  # DEBUG D#1 => &base_28->DATA
  # DEBUG dataRegBytes => D#1
  # DEBUG BEGIN_STMT
  MEM[(volatile uint8 *)base_28 + 28B] ={v} _16;
  goto <bb 25>; [100.00%]

  <bb 20> [local count: 59351079]:
  # DEBUG BEGIN_STMT
  _17 = *_9;
  # DEBUG base => base_28
  # DEBUG data => _17
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwPutchar
  # DEBUG BEGIN_STMT
  # DEBUG D#1 => &base_28->DATA
  # DEBUG dataRegBytes => D#1
  # DEBUG BEGIN_STMT
  MEM[(volatile uint8 *)base_28 + 28B] ={v} _17;
  goto <bb 25>; [100.00%]

  <bb 21> [local count: 44291850]:
  # DEBUG BEGIN_STMT
  linCurrentState_30->currentEventId ={v} 11;
  # DEBUG BEGIN_STMT
  linCurrentState_30->currentNodeState ={v} 10;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_28, 196629, 0);
  # DEBUG BEGIN_STMT
  _18 = pUserConfig_29->Callback;
  if (_18 != 0B)
    goto <bb 22>; [70.00%]
  else
    goto <bb 23>; [30.00%]

  <bb 22> [local count: 31004295]:
  # DEBUG BEGIN_STMT
  _18 (u32Instance_27(D), linCurrentState_30);

  <bb 23> [local count: 44291850]:
  # DEBUG BEGIN_STMT
  linCurrentState_30->isTxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  _19 ={v} linCurrentState_30->currentNodeState;
  if (_19 != 1)
    goto <bb 24>; [48.88%]
  else
    goto <bb 25>; [51.12%]

  <bb 24> [local count: 21649856]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_27(D));

  <bb 25> [local count: 1073741824]:
  # DEBUG base => NULL
  # DEBUG data => NULL
  # DEBUG base => NULL
  # DEBUG data => NULL
  return;

}


Lpuart_Lin_Ip_ProcessReceiveFrameData (const uint32 u32Instance)
{
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  Lpuart_Lin_Ip_StatusType retVal;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  unsigned char _1;
  unsigned char _2;
  unsigned char _3;
  uint8 * _4;
  unsigned char _5;
  unsigned char _6;
  unsigned char _7;
  unsigned char _8;
  unsigned char _9;
  void (*<T2e6>) (uint32, void *) _10;
  void (*<T2e6>) (uint32, void *) _11;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  linCurrentState_17 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_16(D)];
  # DEBUG linCurrentState => linCurrentState_17
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  pUserConfig_18 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_16(D)];
  # DEBUG pUserConfig => pUserConfig_18
  # DEBUG BEGIN_STMT
  _1 = linCurrentState_17->cntByte;
  _2 ={v} linCurrentState_17->rxSize;
  _3 = _2 + 255;
  _4 = linCurrentState_17->rxBuff;
  retVal_20 = Lpuart_Lin_Ip_GetBytetoBuffer (_1, _3, _4, u32Instance_16(D));
  # DEBUG retVal => retVal_20
  # DEBUG BEGIN_STMT
  _5 = linCurrentState_17->cntByte;
  _6 ={v} linCurrentState_17->rxSize;
  if (_5 < _6)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _7 = _5 + 1;
  linCurrentState_17->cntByte = _7;

  <bb 4> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (retVal_20 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 ={v} linCurrentState_17->rxSize;
  _9 = linCurrentState_17->cntByte;
  if (_8 == _9)
    goto <bb 6>; [34.00%]
  else
    goto <bb 11>; [66.00%]

  <bb 6> [local count: 182536110]:
  # DEBUG BEGIN_STMT
  _10 = pUserConfig_18->Callback;
  if (_10 != 0B)
    goto <bb 7>; [70.00%]
  else
    goto <bb 11>; [30.00%]

  <bb 7> [local count: 127775277]:
  # DEBUG BEGIN_STMT
  _10 (u32Instance_16(D), linCurrentState_17);
  goto <bb 11>; [100.00%]

  <bb 8> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _11 = pUserConfig_18->Callback;
  if (_11 != 0B)
    goto <bb 9>; [70.00%]
  else
    goto <bb 10>; [30.00%]

  <bb 9> [local count: 375809639]:
  # DEBUG BEGIN_STMT
  _11 (u32Instance_16(D), linCurrentState_17);

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  linCurrentState_17->isRxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_16(D));

  <bb 11> [local count: 1073741824]:
  return;

}


Lpuart_Lin_Ip_ProcessFrameHeader (const uint32 u32Instance, const uint8 tmpByte)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  struct LPUART_Type * base;
  <unnamed type> _1;
  void (*<T2e6>) (uint32, void *) _2;
  unsigned char _3;
  void (*<T2e6>) (uint32, void *) _4;
  _Bool _5;
  unsigned char _6;
  void (*<T2e6>) (uint32, void *) _7;
  void (*<T2e6>) (uint32, void *) _8;
  unsigned char _9;
  void (*<T2e6>) (uint32, void *) _10;
  void (*<T2e6>) (uint32, void *) _11;

  <bb 2> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  base_17 = Lpuart_Lin_Ip_apxBases[u32Instance_16(D)];
  # DEBUG base => base_17
  # DEBUG BEGIN_STMT
  pUserConfig_18 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_16(D)];
  # DEBUG pUserConfig => pUserConfig_18
  # DEBUG BEGIN_STMT
  linCurrentState_19 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_16(D)];
  # DEBUG linCurrentState => linCurrentState_19
  # DEBUG BEGIN_STMT
  _1 ={v} linCurrentState_19->currentNodeState;
  switch (_1) <default: <L32> [25.00%], case 4: <L0> [25.00%], case 5: <L6> [25.00%], case 6: <L12> [25.00%]>

  <bb 3> [local count: 268435456]:
<L0>:
  # DEBUG BEGIN_STMT
  if (tmpByte_20(D) == 85)
    goto <bb 4>; [34.00%]
  else
    goto <bb 5>; [66.00%]

  <bb 4> [local count: 91268055]:
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentEventId ={v} 4;
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentNodeState ={v} 6;
  goto <bb 24>; [100.00%]

  <bb 5> [local count: 177167401]:
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentEventId ={v} 5;
  # DEBUG BEGIN_STMT
  _2 = pUserConfig_18->Callback;
  if (_2 != 0B)
    goto <bb 6>; [70.00%]
  else
    goto <bb 7>; [30.00%]

  <bb 6> [local count: 124017180]:
  # DEBUG BEGIN_STMT
  _2 (u32Instance_16(D), linCurrentState_19);

  <bb 7> [local count: 177167401]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_16(D));
  goto <bb 24>; [100.00%]

  <bb 8> [local count: 268435456]:
<L6>:
  # DEBUG BEGIN_STMT
  if (tmpByte_20(D) == 85)
    goto <bb 9>; [34.00%]
  else
    goto <bb 10>; [66.00%]

  <bb 9> [local count: 91268055]:
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentNodeState ={v} 6;
  # DEBUG BEGIN_STMT
  _3 = linCurrentState_19->currentPid;
  # DEBUG base => base_17
  # DEBUG data => _3
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwPutchar
  # DEBUG BEGIN_STMT
  # DEBUG D#1 => &base_17->DATA
  # DEBUG dataRegBytes => D#1
  # DEBUG BEGIN_STMT
  MEM[(volatile uint8 *)base_17 + 28B] ={v} _3;
  goto <bb 24>; [100.00%]

  <bb 10> [local count: 177167401]:
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentEventId ={v} 9;
  # DEBUG BEGIN_STMT
  linCurrentState_19->isBusBusy ={v} 0;
  # DEBUG BEGIN_STMT
  _4 = pUserConfig_18->Callback;
  if (_4 != 0B)
    goto <bb 11>; [70.00%]
  else
    goto <bb 24>; [30.00%]

  <bb 11> [local count: 124017180]:
  # DEBUG BEGIN_STMT
  _4 (u32Instance_16(D), linCurrentState_19);
  goto <bb 24>; [100.00%]

  <bb 12> [local count: 268435456]:
<L12>:
  # DEBUG BEGIN_STMT
  _5 = pUserConfig_18->nodeFunction;
  if (_5 != 0)
    goto <bb 13>; [67.00%]
  else
    goto <bb 18>; [33.00%]

  <bb 13> [local count: 179851755]:
  # DEBUG BEGIN_STMT
  _6 = linCurrentState_19->currentPid;
  if (_6 == tmpByte_20(D))
    goto <bb 14>; [34.00%]
  else
    goto <bb 16>; [66.00%]

  <bb 14> [local count: 61149597]:
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentEventId ={v} 6;
  # DEBUG BEGIN_STMT
  linCurrentState_19->isBusBusy ={v} 0;
  # DEBUG BEGIN_STMT
  _7 = pUserConfig_18->Callback;
  if (_7 != 0B)
    goto <bb 15>; [70.00%]
  else
    goto <bb 24>; [30.00%]

  <bb 15> [local count: 42804718]:
  # DEBUG BEGIN_STMT
  _7 (u32Instance_16(D), linCurrentState_19);
  goto <bb 24>; [100.00%]

  <bb 16> [local count: 118702158]:
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentEventId ={v} 9;
  # DEBUG BEGIN_STMT
  linCurrentState_19->isBusBusy ={v} 0;
  # DEBUG BEGIN_STMT
  _8 = pUserConfig_18->Callback;
  if (_8 != 0B)
    goto <bb 17>; [70.00%]
  else
    goto <bb 24>; [30.00%]

  <bb 17> [local count: 83091511]:
  # DEBUG BEGIN_STMT
  _8 (u32Instance_16(D), linCurrentState_19);
  goto <bb 24>; [100.00%]

  <bb 18> [local count: 88583700]:
  # DEBUG BEGIN_STMT
  _9 = Lin_Ip_ProcessParity (tmpByte_20(D), 0);
  linCurrentState_19->currentId = _9;
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentPid = tmpByte_20(D);
  # DEBUG BEGIN_STMT
  if (_9 != 255)
    goto <bb 19>; [66.00%]
  else
    goto <bb 21>; [34.00%]

  <bb 19> [local count: 58465242]:
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentEventId ={v} 6;
  # DEBUG BEGIN_STMT
  linCurrentState_19->isBusBusy ={v} 0;
  # DEBUG BEGIN_STMT
  _10 = pUserConfig_18->Callback;
  if (_10 != 0B)
    goto <bb 20>; [70.00%]
  else
    goto <bb 24>; [30.00%]

  <bb 20> [local count: 40925670]:
  # DEBUG BEGIN_STMT
  _10 (u32Instance_16(D), linCurrentState_19);
  goto <bb 24>; [100.00%]

  <bb 21> [local count: 30118458]:
  # DEBUG BEGIN_STMT
  linCurrentState_19->currentEventId ={v} 7;
  # DEBUG BEGIN_STMT
  _11 = pUserConfig_18->Callback;
  if (_11 != 0B)
    goto <bb 22>; [70.00%]
  else
    goto <bb 23>; [30.00%]

  <bb 22> [local count: 21082921]:
  # DEBUG BEGIN_STMT
  _11 (u32Instance_16(D), linCurrentState_19);

  <bb 23> [local count: 30118458]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_16(D));

  <bb 24> [local count: 1073741824]:
<L32>:
  # DEBUG base => NULL
  # DEBUG data => NULL
  return;

}


Lpuart_Lin_Ip_FrameIrqHandler (const uint32 u32Instance)
{
  const struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct LPUART_Type * base;
  _Bool _1;
  _Bool _2;
  <unnamed type> _3;
  long unsigned int _14;
  unsigned char _15;
  long unsigned int _16;
  unsigned char _17;
  long unsigned int _18;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  base_7 = Lpuart_Lin_Ip_apxBases[u32Instance_6(D)];
  # DEBUG base => base_7
  # DEBUG BEGIN_STMT
  linCurrentState_8 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_6(D)];
  # DEBUG linCurrentState => linCurrentState_8
  # DEBUG BEGIN_STMT
  _1 = Lpuart_Lin_Ip_HwGetStatusFlag (base_7, 131093);
  if (_1 != 0)
    goto <bb 3>; [33.00%]
  else
    goto <bb 9>; [67.00%]

  <bb 3> [local count: 354334802]:
  _2 = Lpuart_Lin_Ip_HwGetIntMode (base_7, 196629);
  if (_2 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 4> [local count: 177167401]:
  # DEBUG BEGIN_STMT
  _3 ={v} linCurrentState_8->currentNodeState;
  switch (_3) <default: <L13> [25.00%], case 4 ... 6: <L11> [25.00%], case 7: <L5> [25.00%], case 9: <L12> [25.00%]>

  <bb 5> [local count: 44291850]:
<L11>:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_7
  # DEBUG readData => &tmpByte
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwGetchar
  # DEBUG BEGIN_STMT
  _14 ={v} base_7->DATA;
  _15 = (unsigned char) _14;
  # DEBUG tmpByte => _15
  # DEBUG base => NULL
  # DEBUG readData => NULL
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_ProcessFrameHeader (u32Instance_6(D), _15);
  # DEBUG BEGIN_STMT
  goto <bb 9>; [100.00%]

  <bb 6> [local count: 44291850]:
<L5>:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_ProcessReceiveFrameData (u32Instance_6(D));
  # DEBUG BEGIN_STMT
  goto <bb 9>; [100.00%]

  <bb 7> [local count: 44291850]:
<L12>:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_7
  # DEBUG readData => &tmpByte
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwGetchar
  # DEBUG BEGIN_STMT
  _16 ={v} base_7->DATA;
  _17 = (unsigned char) _16;
  # DEBUG tmpByte => _17
  # DEBUG base => NULL
  # DEBUG readData => NULL
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_ProcessSendFrameData (u32Instance_6(D), _17);
  # DEBUG BEGIN_STMT
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 44291850]:
<L13>:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_7
  # DEBUG readData => &tmpByte
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwGetchar
  # DEBUG BEGIN_STMT
  _18 ={v} base_7->DATA;
  # DEBUG tmpByte => (unsigned char) _18

  <bb 9> [local count: 1073741824]:
  # DEBUG base => NULL
  # DEBUG readData => NULL
  # DEBUG D#6 => {CLOBBER}
  # DEBUG tmpByte => D#6
  return;

}


Lpuart_Lin_Ip_CheckWakeupSignal (const uint32 u32Instance)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  uint32 wakeupSignalLength;
  uint32 (*<T2e1>) (uint32, uint32 *) _1;
  uint32 (*<T2e1>) (uint32, uint32 *) _2;
  long unsigned int wakeupSignalLength.24_3;
  void (*<T2e6>) (uint32, void *) _4;
  long unsigned int _19;
  long unsigned int _20;
  _Bool _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  wakeupSignalLength = 0;
  # DEBUG BEGIN_STMT
  pUserConfig_10 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_9(D)];
  # DEBUG pUserConfig => pUserConfig_10
  # DEBUG BEGIN_STMT
  base_11 = Lpuart_Lin_Ip_apxBases[u32Instance_9(D)];
  # DEBUG base => base_11
  # DEBUG BEGIN_STMT
  linCurrentState_12 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_9(D)];
  # DEBUG linCurrentState => linCurrentState_12
  # DEBUG BEGIN_STMT
  # DEBUG base => base_11
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwGetRxDataPolarity
  # DEBUG BEGIN_STMT
  _19 ={v} MEM[(const struct LPUART_Type *)base_11].STAT;
  _20 = _19 >> 28;
  _21 = (_Bool) _20;
  # DEBUG base => NULL
  if (_21 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = pUserConfig_10->timerGetTimeIntervalCallback;
  _1 (u32Instance_9(D), &wakeupSignalLength);
  # DEBUG BEGIN_STMT
  # DEBUG base => base_11
  # DEBUG polarity => 1
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwSetRxDataPolarity
  # DEBUG BEGIN_STMT
  _22 ={v} base_11->STAT;
  _23 = _22 & 803225599;
  _24 = _23 | 268435456;
  base_11->STAT ={v} _24;
  goto <bb 8>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_11
  # DEBUG polarity => 0
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwSetRxDataPolarity
  # DEBUG BEGIN_STMT
  _25 ={v} base_11->STAT;
  _26 = _25 & 803225599;
  base_11->STAT ={v} _26;
  # DEBUG base => NULL
  # DEBUG polarity => NULL
  # DEBUG BEGIN_STMT
  _2 = pUserConfig_10->timerGetTimeIntervalCallback;
  _2 (u32Instance_9(D), &wakeupSignalLength);
  # DEBUG BEGIN_STMT
  wakeupSignalLength.24_3 = wakeupSignalLength;
  if (wakeupSignalLength.24_3 > 149999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 5> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  linCurrentState_12->currentEventId ={v} 1;
  # DEBUG BEGIN_STMT
  _4 = pUserConfig_10->Callback;
  if (_4 != 0B)
    goto <bb 6>; [70.00%]
  else
    goto <bb 7>; [30.00%]

  <bb 6> [local count: 187904819]:
  # DEBUG BEGIN_STMT
  _4 (u32Instance_9(D), linCurrentState_12);

  <bb 7> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_9(D));

  <bb 8> [local count: 1073741824]:
  # DEBUG base => NULL
  # DEBUG polarity => NULL
  wakeupSignalLength ={v} {CLOBBER};
  return;

}


Lpuart_Lin_Ip_ProcessBreakDetect (const uint32 u32Instance)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  _Bool _1;
  <unnamed type> _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  _Bool _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _29;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  pUserConfig_14 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_13(D)];
  # DEBUG pUserConfig => pUserConfig_14
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  base_15 = Lpuart_Lin_Ip_apxBases[u32Instance_13(D)];
  # DEBUG base => base_15
  # DEBUG BEGIN_STMT
  linCurrentState_16 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_13(D)];
  # DEBUG linCurrentState => linCurrentState_16
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwClearStatusFlag (base_15, 131103);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetBreakCharDetectLength (base_15, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_15, 65551, 0);
  # DEBUG BEGIN_STMT
  # DEBUG base => base_15
  # DEBUG readData => &discardData
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwGetchar
  # DEBUG BEGIN_STMT
  _29 ={v} MEM[(const struct LPUART_Type *)base_15].DATA;
  # DEBUG discardData => (unsigned char) _29
  # DEBUG base => NULL
  # DEBUG readData => NULL
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_15, 196629, 1);
  # DEBUG BEGIN_STMT
  _1 = pUserConfig_14->nodeFunction;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _2 ={v} linCurrentState_16->currentNodeState;
  if (_2 == 3)
    goto <bb 4>; [34.00%]
  else
    goto <bb 8>; [66.00%]

  <bb 4> [local count: 182536110]:
  # DEBUG BEGIN_STMT
  _3 = pUserConfig_14->u32HeaderTimeoutValue;
  _4 = _3 / 500;
  _5 = _4 + 1;
  # DEBUG u32Instance => u32Instance_13(D)
  # DEBUG u32TimeoutValue => _5
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_SetTimeoutCounter
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_30 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_13(D)];
  # DEBUG linCurrentState => linCurrentState_30
  # DEBUG BEGIN_STMT
  linCurrentState_30->timeoutCounterFlag ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_30->timeoutCounter ={v} _5;
  # DEBUG u32Instance => NULL
  # DEBUG u32TimeoutValue => NULL
  # DEBUG linCurrentState => NULL
  # DEBUG BEGIN_STMT
  linCurrentState_16->currentNodeState ={v} 5;
  # DEBUG BEGIN_STMT
  # DEBUG base => base_15
  # DEBUG data => 85
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwPutchar
  # DEBUG BEGIN_STMT
  # DEBUG D#1 => &base_15->DATA
  # DEBUG dataRegBytes => D#1
  # DEBUG BEGIN_STMT
  MEM[(volatile uint8 *)base_15 + 28B] ={v} 85;
  goto <bb 8>; [100.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  linCurrentState_16->isBusBusy ={v} 1;
  # DEBUG BEGIN_STMT
  linCurrentState_16->currentEventId ={v} 3;
  # DEBUG BEGIN_STMT
  linCurrentState_16->currentNodeState ={v} 4;
  # DEBUG BEGIN_STMT
  _6 ={v} linCurrentState_16->baudrateEvalEnable;
  if (_6 != 0)
    goto <bb 6>; [33.00%]
  else
    goto <bb 7>; [67.00%]

  <bb 6> [local count: 177167401]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_15, 65550, 1);
  # DEBUG BEGIN_STMT
  linCurrentState_16->fallingEdgeInterruptCount ={v} 0;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetTransmitterCmd (base_15, 1);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetReceiverCmd (base_15, 1);

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _7 = pUserConfig_14->u32HeaderTimeoutValue;
  _8 = _7 / 500;
  _9 = _8 + 1;
  # DEBUG u32Instance => u32Instance_13(D)
  # DEBUG u32TimeoutValue => _9
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_SetTimeoutCounter
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_31 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_13(D)];
  # DEBUG linCurrentState => linCurrentState_31
  # DEBUG BEGIN_STMT
  linCurrentState_31->timeoutCounterFlag ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_31->timeoutCounter ={v} _9;

  <bb 8> [local count: 1073741824]:
  # DEBUG u32Instance => NULL
  # DEBUG u32TimeoutValue => NULL
  # DEBUG linCurrentState => NULL
  # DEBUG base => NULL
  # DEBUG data => NULL
  # DEBUG D#4 => {CLOBBER}
  # DEBUG discardData => D#4
  return;

}


Lpuart_Lin_Ip_IRQHandler (const uint32 u32Instance)
{
  boolean bSpuriousIntAvailable;
  boolean activeEdgeIntState;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  _Bool _1;
  _Bool _2;
  _Bool _3;
  _Bool _4;
  _Bool _5;
  _Bool _6;
  _Bool _7;
  _Bool _8;
  _Bool _9;
  void (*<T2e6>) (uint32, void *) _10;
  int iftmp.23_12;

  <bb 2> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG bSpuriousIntAvailable => 0
  # DEBUG BEGIN_STMT
  pUserConfig_21 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_20(D)];
  # DEBUG pUserConfig => pUserConfig_21
  # DEBUG BEGIN_STMT
  base_22 = Lpuart_Lin_Ip_apxBases[u32Instance_20(D)];
  # DEBUG base => base_22
  # DEBUG BEGIN_STMT
  linCurrentState_23 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_20(D)];
  # DEBUG linCurrentState => linCurrentState_23
  # DEBUG BEGIN_STMT
  activeEdgeIntState_25 = Lpuart_Lin_Ip_HwGetIntMode (base_22, 65550);
  # DEBUG activeEdgeIntState => activeEdgeIntState_25
  # DEBUG BEGIN_STMT
  if (linCurrentState_23 == 0B)
    goto <bb 3>; [30.00%]
  else
    goto <bb 4>; [70.00%]

  <bb 3> [local count: 322122547]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwClearStatusFlag (base_22, 0);
  goto <bb 23>; [100.00%]

  <bb 4> [local count: 751619277]:
  # DEBUG BEGIN_STMT
  _1 = Lpuart_Lin_Ip_HwGetStatusFlag (base_22, 131103);
  if (_1 != 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 5> [local count: 375809638]:
  _2 = Lpuart_Lin_Ip_HwGetIntMode (base_22, 65551);
  if (_2 != 0)
    goto <bb 6>; [33.00%]
  else
    goto <bb 7>; [67.00%]

  <bb 6> [local count: 124017180]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_ProcessBreakDetect (u32Instance_20(D));
  goto <bb 17>; [100.00%]

  <bb 7> [local count: 627602097]:
  # DEBUG BEGIN_STMT
  _3 = Lpuart_Lin_Ip_HwGetStatusFlag (base_22, 131102);
  if (_3 != 0)
    goto <bb 8>; [67.00%]
  else
    goto <bb 10>; [33.00%]

  <bb 8> [local count: 420493404]:
  if (activeEdgeIntState_25 != 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 10>; [67.00%]

  <bb 9> [local count: 138762824]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_ProcessWakeupDetect (u32Instance_20(D));
  goto <bb 17>; [100.00%]

  <bb 10> [local count: 488839272]:
  # DEBUG BEGIN_STMT
  _4 = Lpuart_Lin_Ip_HwGetStatusFlag (base_22, 131089);
  if (_4 != 0)
    goto <bb 11>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 11> [local count: 244419636]:
  _5 = Lpuart_Lin_Ip_HwGetIntMode (base_22, 196633);
  if (_5 != 0)
    goto <bb 12>; [33.00%]
  else
    goto <bb 13>; [67.00%]

  <bb 12> [local count: 80658480]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_FrameErrorIrqHandler (u32Instance_20(D));
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_20(D));
  goto <bb 17>; [100.00%]

  <bb 13> [local count: 408180792]:
  # DEBUG BEGIN_STMT
  _6 = Lpuart_Lin_Ip_HwGetStatusFlag (base_22, 131093);
  if (_6 != 0)
    goto <bb 14>; [33.00%]
  else
    goto <bb 16>; [67.00%]

  <bb 14> [local count: 134699661]:
  _7 = Lpuart_Lin_Ip_HwGetIntMode (base_22, 196629);
  if (_7 != 0)
    goto <bb 16>; [50.00%]
  else
    goto <bb 24>; [50.00%]

  <bb 24> [local count: 67349831]:

  <bb 16> [local count: 408180791]:
  # iftmp.23_12 = PHI <1(14), 0(24), 0(13)>
  bSpuriousIntAvailable_37 = (boolean) iftmp.23_12;
  # DEBUG bSpuriousIntAvailable => bSpuriousIntAvailable_37
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_FrameIrqHandler (u32Instance_20(D));

  <bb 17> [local count: 751619277]:
  # bSpuriousIntAvailable_11 = PHI <0(6), 0(9), 0(12), bSpuriousIntAvailable_37(16)>
  # DEBUG bSpuriousIntAvailable => bSpuriousIntAvailable_11
  # DEBUG BEGIN_STMT
  _8 = Lpuart_Lin_Ip_HwGetStatusFlag (base_22, 131091);
  if (_8 != 0)
    goto <bb 18>; [33.00%]
  else
    goto <bb 21>; [67.00%]

  <bb 18> [local count: 248034361]:
  _9 = Lpuart_Lin_Ip_HwGetIntMode (base_22, 196635);
  if (_9 != 0)
    goto <bb 19>; [33.00%]
  else
    goto <bb 21>; [67.00%]

  <bb 19> [local count: 81851339]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwClearStatusFlag (base_22, 131091);
  # DEBUG BEGIN_STMT
  linCurrentState_23->currentEventId ={v} 13;
  # DEBUG BEGIN_STMT
  _10 = pUserConfig_21->Callback;
  if (_10 != 0B)
    goto <bb 20>; [70.00%]
  else
    goto <bb 23>; [30.00%]

  <bb 20> [local count: 57295937]:
  # DEBUG BEGIN_STMT
  _10 (u32Instance_20(D), linCurrentState_23);
  goto <bb 23>; [100.00%]

  <bb 21> [local count: 669767938]:
  # DEBUG BEGIN_STMT
  if (bSpuriousIntAvailable_11 != 0)
    goto <bb 22>; [33.00%]
  else
    goto <bb 23>; [67.00%]

  <bb 22> [local count: 221023419]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwClearStatusFlag (base_22, 0);

  <bb 23> [local count: 1073741824]:
  return;

}


Lpuart_Lin_Ip_GotoIdleState (const uint32 u32Instance)
{
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  _Bool _1;
  unsigned char _2;
  long unsigned int _22;
  long unsigned int _23;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_6 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_5(D)];
  # DEBUG linCurrentState => linCurrentState_6
  # DEBUG BEGIN_STMT
  base_7 = Lpuart_Lin_Ip_apxBases[u32Instance_5(D)];
  # DEBUG base => base_7
  # DEBUG BEGIN_STMT
  pUserConfig_8 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_5(D)];
  # DEBUG pUserConfig => pUserConfig_8
  # DEBUG BEGIN_STMT
  linCurrentState_6->currentEventId ={v} 0;
  # DEBUG BEGIN_STMT
  # DEBUG base => base_7
  # DEBUG polarity => 0
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwSetRxDataPolarity
  # DEBUG BEGIN_STMT
  _22 ={v} base_7->STAT;
  _23 = _22 & 803225599;
  base_7->STAT ={v} _23;
  # DEBUG base => NULL
  # DEBUG polarity => NULL
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_7, 65550, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_7, 196633, 1);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_7, 196629, 0);
  # DEBUG BEGIN_STMT
  _1 = pUserConfig_8->nodeFunction;
  if (_1 != 0)
    goto <bb 4>; [67.00%]
  else
    goto <bb 3>; [33.00%]

  <bb 3> [local count: 354334802]:
  # DEBUG BEGIN_STMT
  _2 = pUserConfig_8->u8BreakLengthDetect;
  Lpuart_Lin_Ip_HwSetBreakCharDetectLength (base_7, _2);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_7, 65551, 1);

  <bb 4> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_02 ();
  # DEBUG BEGIN_STMT
  linCurrentState_6->currentNodeState ={v} 2;
  # DEBUG BEGIN_STMT
  linCurrentState_6->isBusBusy ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_6->isTxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_6->isRxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_6->timeoutCounterFlag ={v} 0;
  # DEBUG BEGIN_STMT
  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_02 ();
  return;

}


Lpuart_Lin_Ip_MasterSendHeader (const uint32 u32Instance, const uint8 u8Id)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  Lpuart_Lin_Ip_StatusType retVal;
  <unnamed type> _1;
  _Bool _2;
  _Bool _3;
  unsigned char _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  pUserConfig_9 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_8(D)];
  # DEBUG pUserConfig => pUserConfig_9
  # DEBUG BEGIN_STMT
  base_10 = Lpuart_Lin_Ip_apxBases[u32Instance_8(D)];
  # DEBUG base => base_10
  # DEBUG BEGIN_STMT
  linCurrentState_11 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_8(D)];
  # DEBUG linCurrentState => linCurrentState_11
  # DEBUG BEGIN_STMT
  _1 ={v} linCurrentState_11->currentNodeState;
  # DEBUG checkSleepMode => _1 == 1
  # DEBUG BEGIN_STMT
  _2 = pUserConfig_9->nodeFunction;
  if (_2 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 3> [local count: 536870913]:
  if (u8Id_12(D) > 63)
    goto <bb 7>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 4> [local count: 268435456]:
  if (_1 == 1)
    goto <bb 7>; [34.00%]
  else
    goto <bb 5>; [66.00%]

  <bb 5> [local count: 177167401]:
  # DEBUG BEGIN_STMT
  _3 ={v} linCurrentState_11->isBusBusy;
  if (_3 != 0)
    goto <bb 7>; [52.23%]
  else
    goto <bb 6>; [47.77%]

  <bb 6> [local count: 84632867]:
  # DEBUG BEGIN_STMT
  linCurrentState_11->currentId = u8Id_12(D);
  # DEBUG BEGIN_STMT
  _4 = Lin_Ip_ProcessParity (u8Id_12(D), 1);
  linCurrentState_11->currentPid = _4;
  # DEBUG BEGIN_STMT
  linCurrentState_11->currentNodeState ={v} 3;
  # DEBUG BEGIN_STMT
  linCurrentState_11->currentEventId ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_11->isBusBusy ={v} 1;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetBreakCharDetectLength (base_10, 1);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_10, 65551, 1);
  # DEBUG BEGIN_STMT
  # DEBUG base => base_10
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwQueueBreakField
  # DEBUG BEGIN_STMT
  base_10->DATA ={v} 8192;

  <bb 7> [local count: 1073741824]:
  # retVal_5 = PHI <1(3), 2(5), 0(6), 1(2), 1(4)>
  # DEBUG base => NULL
  # DEBUG retVal => retVal_5
  # DEBUG BEGIN_STMT
  return retVal_5;

}


Lpuart_Lin_Ip_SetTimeoutCounter (const uint32 u32Instance, const uint32 u32TimeoutValue)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_3 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_2(D)];
  # DEBUG linCurrentState => linCurrentState_3
  # DEBUG BEGIN_STMT
  linCurrentState_3->timeoutCounterFlag ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_3->timeoutCounter ={v} u32TimeoutValue_5(D);
  return;

}


Lpuart_Lin_Ip_TimeoutService (const uint32 u32Instance)
{
  Lpuart_Lin_Ip_NodeStateType state;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  long unsigned int _1;
  void (*<T2e6>) (uint32, void *) _2;
  long unsigned int _3;
  long unsigned int _4;
  _Bool _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_9 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_8(D)];
  # DEBUG linCurrentState => linCurrentState_9
  # DEBUG BEGIN_STMT
  pUserConfig_10 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_8(D)];
  # DEBUG pUserConfig => pUserConfig_10
  # DEBUG BEGIN_STMT
  state_11 ={v} linCurrentState_9->currentNodeState;
  # DEBUG state => state_11
  # DEBUG BEGIN_STMT
  switch (state_11) <default: <L14> [50.00%], case 4 ... 7: <L0> [50.00%], case 9: <L0> [50.00%]>

  <bb 3> [local count: 536870913]:
<L0>:
  # DEBUG BEGIN_STMT
  _1 ={v} linCurrentState_9->timeoutCounter;
  if (_1 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  linCurrentState_9->timeoutCounterFlag ={v} 1;
  # DEBUG BEGIN_STMT
  linCurrentState_9->isTxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_9->currentEventId ={v} 14;
  # DEBUG BEGIN_STMT
  _2 = pUserConfig_10->Callback;
  if (_2 != 0B)
    goto <bb 5>; [70.00%]
  else
    goto <bb 7>; [30.00%]

  <bb 5> [local count: 187904819]:
  # DEBUG BEGIN_STMT
  _2 (u32Instance_8(D), linCurrentState_9);
  goto <bb 7>; [100.00%]

  <bb 6> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _3 ={v} linCurrentState_9->timeoutCounter;
  _4 = _3 + 4294967295;
  linCurrentState_9->timeoutCounter ={v} _4;

  <bb 7> [local count: 1073741824]:
<L14>:
  # DEBUG BEGIN_STMT
  _5 ={v} linCurrentState_9->timeoutCounterFlag;
  # DEBUG BEGIN_STMT
  return;

}


Lpuart_Lin_Ip_GetCurrentNodeState (const uint32 u32Instance)
{
  const struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  Lpuart_Lin_Ip_NodeStateType retVal;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_4 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_3(D)];
  # DEBUG linCurrentState => linCurrentState_4
  # DEBUG BEGIN_STMT
  if (linCurrentState_4 != 0B)
    goto <bb 3>; [70.00%]
  else
    goto <bb 4>; [30.00%]

  <bb 3> [local count: 751619278]:
  # DEBUG BEGIN_STMT
  retVal_5 ={v} linCurrentState_4->currentNodeState;
  # DEBUG retVal => retVal_5

  <bb 4> [local count: 1073741824]:
  # retVal_1 = PHI <0(2), retVal_5(3)>
  # DEBUG retVal => retVal_1
  # DEBUG BEGIN_STMT
  return retVal_1;

}


Lpuart_Lin_Ip_SendWakeupSignal (const uint32 u32Instance)
{
  Lpuart_Lin_Ip_StatusType retVal;
  const struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  _Bool _1;
  unsigned char _2;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  linCurrentState_7 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_6(D)];
  # DEBUG linCurrentState => linCurrentState_7
  # DEBUG BEGIN_STMT
  base_8 = Lpuart_Lin_Ip_apxBases[u32Instance_6(D)];
  # DEBUG base => base_8
  # DEBUG BEGIN_STMT
  _1 ={v} linCurrentState_7->isBusBusy;
  if (_1 != 0)
    goto <bb 4>; [35.00%]
  else
    goto <bb 3>; [65.00%]

  <bb 3> [local count: 697932186]:
  # DEBUG BEGIN_STMT
  _2 = Lpuart_Lin_Ip_au8WakeupSignal[u32Instance_6(D)];
  # DEBUG base => base_8
  # DEBUG data => _2
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwPutchar
  # DEBUG BEGIN_STMT
  # DEBUG D#1 => &base_8->DATA
  # DEBUG dataRegBytes => D#1
  # DEBUG BEGIN_STMT
  MEM[(volatile uint8 *)base_8 + 28B] ={v} _2;

  <bb 4> [local count: 1073741824]:
  # retVal_3 = PHI <0(3), 2(2)>
  # DEBUG base => NULL
  # DEBUG data => NULL
  # DEBUG retVal => retVal_3
  # DEBUG BEGIN_STMT
  return retVal_3;

}


Lpuart_Lin_Ip_GoToSleepMode (const uint32 u32Instance)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  long unsigned int _14;
  long unsigned int _15;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_3 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_2(D)];
  # DEBUG linCurrentState => linCurrentState_3
  # DEBUG BEGIN_STMT
  base_4 = Lpuart_Lin_Ip_apxBases[u32Instance_2(D)];
  # DEBUG base => base_4
  # DEBUG BEGIN_STMT
  linCurrentState_3->currentNodeState ={v} 1;
  # DEBUG BEGIN_STMT
  linCurrentState_3->isTxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_3->isRxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_3->isBusBusy ={v} 0;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwClearStatusFlag (base_4, 131102);
  # DEBUG BEGIN_STMT
  # DEBUG base => base_4
  # DEBUG polarity => 0
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwSetRxDataPolarity
  # DEBUG BEGIN_STMT
  _14 ={v} base_4->STAT;
  _15 = _14 & 803225599;
  base_4->STAT ={v} _15;
  # DEBUG base => NULL
  # DEBUG polarity => NULL
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_4, 196629, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_4, 65550, 1);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_4, 196633, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_4, 65551, 0);
  return;

}


Lpuart_Lin_Ip_GetReceiveStatus (const uint32 u32Instance, uint8 * const pBytesRemaining)
{
  Lpuart_Lin_Ip_StatusType retVal;
  const struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  unsigned char _1;
  unsigned char _2;
  unsigned char _3;
  <unnamed type> _4;
  _Bool _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  linCurrentState_9 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_8(D)];
  # DEBUG linCurrentState => linCurrentState_9
  # DEBUG BEGIN_STMT
  _1 ={v} linCurrentState_9->rxSize;
  _2 = linCurrentState_9->cntByte;
  _3 = _1 - _2;
  *pBytesRemaining_10(D) = _3;
  # DEBUG BEGIN_STMT
  _4 ={v} linCurrentState_9->currentEventId;
  if (_4 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  if (_3 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _5 ={v} linCurrentState_9->timeoutCounterFlag;
  if (_5 != 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 3

  <bb 6> [local count: 1073741824]:
  # retVal_6 = PHI <0(2), 0(3), 2(4), 3(5)>
  # DEBUG retVal => retVal_6
  # DEBUG BEGIN_STMT
  return retVal_6;

}


Lpuart_Lin_Ip_AbortTransferData (const uint32 u32Instance)
{
  uint32 timeoutTicks;
  uint32 startTime;
  struct LPUART_Type * base;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  _Bool _1;
  long unsigned int startTime.20_2;
  long unsigned int timeoutTicks.21_3;
  _Bool _4;

  <bb 2> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_9 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_8(D)];
  # DEBUG linCurrentState => linCurrentState_9
  # DEBUG BEGIN_STMT
  base_10 = Lpuart_Lin_Ip_apxBases[u32Instance_8(D)];
  # DEBUG base => base_10
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_10, 196629, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_10, 196633, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_10, 65551, 0);
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_StartTimeout (&startTime, &timeoutTicks, 65535, 0);

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Lpuart_Lin_Ip_HwGetStatusFlag (base_10, 131094);
  if (_1 != 0)
    goto <bb 5>; [5.50%]
  else
    goto <bb 4>; [94.50%]

  <bb 4> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  startTime.20_2 = startTime;
  timeoutTicks.21_3 = timeoutTicks;
  _4 = Lpuart_Lin_Ip_TimeoutExpired (startTime.20_2, timeoutTicks.21_3, 0);
  if (_4 != 0)
    goto <bb 5>; [5.50%]
  else
    goto <bb 6>; [94.50%]

  <bb 6> [local count: 958878293]:
  goto <bb 3>; [100.00%]

  <bb 5> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_8(D));
  # DEBUG BEGIN_STMT
  linCurrentState_9->isTxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_9->isRxBusy ={v} 0;
  startTime ={v} {CLOBBER};
  timeoutTicks ={v} {CLOBBER};
  return;

}


Lpuart_Lin_Ip_SyncReceiveFrameData (const uint32 u32Instance, uint8 * pRxBuff, const uint8 u8RxSize)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  uint32 startTime;
  uint32 timeoutTicks;
  uint8 byteCnt;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  volatile Lpuart_Lin_Ip_StatusType retVal;
  <unnamed type> _1;
  <unnamed type> retVal.13_2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  _Bool _9;
  long unsigned int startTime.14_10;
  long unsigned int timeoutTicks.15_11;
  _Bool _12;
  <unnamed type> _13;
  <unnamed type> retVal.16_14;
  <unnamed type> _15;
  <unnamed type> retVal.17_16;
  Lpuart_Lin_Ip_StatusType _47;

  <bb 2> [local count: 37234929]:
  # DEBUG BEGIN_STMT
  retVal ={v} 0;
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG byteCnt => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_26 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_25(D)];
  # DEBUG linCurrentState => linCurrentState_26
  # DEBUG BEGIN_STMT
  base_27 = Lpuart_Lin_Ip_apxBases[u32Instance_25(D)];
  # DEBUG base => base_27
  # DEBUG BEGIN_STMT
  _1 = Lpuart_Lin_Ip_StatusBeforeTransfer (u8RxSize_28(D), linCurrentState_26);
  retVal ={v} _1;
  # DEBUG BEGIN_STMT
  retVal.13_2 ={v} retVal;
  if (retVal.13_2 != 0)
    goto <bb 16>; [67.00%]
  else
    goto <bb 3>; [33.00%]

  <bb 3> [local count: 12287527]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_27, 196629, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_27, 65551, 0);
  # DEBUG BEGIN_STMT
  linCurrentState_26->currentEventId ={v} 0;

  <bb 4> [local count: 114863532]:
  # byteCnt_17 = PHI <0(3), byteCnt_45(17)>
  # DEBUG byteCnt => byteCnt_17
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  pUserConfig_34 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_25(D)];
  # DEBUG pUserConfig => pUserConfig_34
  # DEBUG BEGIN_STMT
  _3 = pUserConfig_34->u32ResponseTimeoutValue;
  _4 = (long unsigned int) u8RxSize_28(D);
  _5 = _4 + 1;
  _6 = _3 * _5;
  _7 = _6 / 500;
  _8 = _7 + 1;
  # DEBUG u32Instance => u32Instance_25(D)
  # DEBUG u32TimeoutValue => _8
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_SetTimeoutCounter
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_50 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_25(D)];
  # DEBUG linCurrentState => linCurrentState_50
  # DEBUG BEGIN_STMT
  linCurrentState_50->timeoutCounterFlag ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_50->timeoutCounter ={v} _8;
  # DEBUG u32Instance => NULL
  # DEBUG u32TimeoutValue => NULL
  # DEBUG linCurrentState => NULL
  # DEBUG BEGIN_STMT
  retVal ={v} 3;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_StartTimeout (&startTime, &timeoutTicks, 65535, 0);
  # DEBUG BEGIN_STMT
  goto <bb 7>; [100.00%]

  <bb 5> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _9 = Lpuart_Lin_Ip_HwGetStatusFlag (base_27, 131093);
  if (_9 != 0)
    goto <bb 6>; [5.50%]
  else
    goto <bb 18>; [94.50%]

  <bb 6> [local count: 55807731]:
  # DEBUG BEGIN_STMT
  retVal ={v} 0;
  # DEBUG BEGIN_STMT
  goto <bb 8>; [100.00%]

  <bb 18> [local count: 958878294]:

  <bb 7> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  startTime.14_10 = startTime;
  timeoutTicks.15_11 = timeoutTicks;
  _12 = Lpuart_Lin_Ip_TimeoutExpired (startTime.14_10, timeoutTicks.15_11, 0);
  if (_12 != 0)
    goto <bb 8>; [5.50%]
  else
    goto <bb 5>; [94.50%]

  <bb 8> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  _13 ={v} linCurrentState_26->currentEventId;
  if (_13 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 57431766]:
  # DEBUG BEGIN_STMT
  retVal ={v} 1;
  goto <bb 13>; [100.00%]

  <bb 10> [local count: 57431766]:
  # DEBUG BEGIN_STMT
  retVal.16_14 ={v} retVal;
  if (retVal.16_14 == 0)
    goto <bb 11>; [33.00%]
  else
    goto <bb 12>; [67.00%]

  <bb 11> [local count: 18952483]:
  # DEBUG BEGIN_STMT
  _15 = Lpuart_Lin_Ip_GetBytetoBuffer (byteCnt_17, u8RxSize_28(D), pRxBuff_41(D), u32Instance_25(D));
  retVal ={v} _15;
  goto <bb 13>; [100.00%]

  <bb 12> [local count: 38479283]:
  # DEBUG BEGIN_STMT
  retVal ={v} 3;

  <bb 13> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  retVal.17_16 ={v} retVal;
  if (retVal.17_16 != 0)
    goto <bb 15>; [5.50%]
  else
    goto <bb 14>; [94.50%]

  <bb 14> [local count: 108546037]:
  # DEBUG BEGIN_STMT
  byteCnt_45 = byteCnt_17 + 1;
  # DEBUG byteCnt => byteCnt_45
  if (byteCnt_17 < u8RxSize_28(D))
    goto <bb 17>; [94.50%]
  else
    goto <bb 15>; [5.50%]

  <bb 17> [local count: 102576005]:
  goto <bb 4>; [100.00%]

  <bb 15> [local count: 12287526]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_25(D));

  <bb 16> [local count: 37234929]:
  # DEBUG BEGIN_STMT
  _47 ={v} retVal;
  timeoutTicks ={v} {CLOBBER};
  startTime ={v} {CLOBBER};
  return _47;

}


Lpuart_Lin_Ip_AsyncReceiveFrameData (const uint32 u32Instance, uint8 * pRxBuff, const uint8 u8RxSize)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  Lpuart_Lin_Ip_StatusType retVal;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_11 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_10(D)];
  # DEBUG linCurrentState => linCurrentState_11
  # DEBUG BEGIN_STMT
  base_12 = Lpuart_Lin_Ip_apxBases[u32Instance_10(D)];
  # DEBUG base => base_12
  # DEBUG BEGIN_STMT
  retVal_15 = Lpuart_Lin_Ip_StatusBeforeTransfer (u8RxSize_13(D), linCurrentState_11);
  # DEBUG retVal => retVal_15
  # DEBUG BEGIN_STMT
  if (retVal_15 != 0)
    goto <bb 4>; [67.00%]
  else
    goto <bb 3>; [33.00%]

  <bb 3> [local count: 354334802]:
  # DEBUG BEGIN_STMT
  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01 ();
  # DEBUG BEGIN_STMT
  linCurrentState_11->rxBuff = pRxBuff_17(D);
  # DEBUG BEGIN_STMT
  _1 = u8RxSize_13(D) + 1;
  linCurrentState_11->rxSize ={v} _1;
  # DEBUG BEGIN_STMT
  linCurrentState_11->cntByte = 0;
  # DEBUG BEGIN_STMT
  linCurrentState_11->currentNodeState ={v} 7;
  # DEBUG BEGIN_STMT
  linCurrentState_11->currentEventId ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_11->isBusBusy ={v} 1;
  # DEBUG BEGIN_STMT
  linCurrentState_11->isRxBusy ={v} 1;
  # DEBUG BEGIN_STMT
  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_01 ();
  # DEBUG BEGIN_STMT
  pUserConfig_26 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_10(D)];
  # DEBUG pUserConfig => pUserConfig_26
  # DEBUG BEGIN_STMT
  _2 = pUserConfig_26->u32ResponseTimeoutValue;
  _3 = (long unsigned int) u8RxSize_13(D);
  _4 = _3 + 1;
  _5 = _2 * _4;
  _6 = _5 / 500;
  _7 = _6 + 1;
  # DEBUG u32Instance => u32Instance_10(D)
  # DEBUG u32TimeoutValue => _7
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_SetTimeoutCounter
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_28 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_10(D)];
  # DEBUG linCurrentState => linCurrentState_28
  # DEBUG BEGIN_STMT
  linCurrentState_28->timeoutCounterFlag ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_28->timeoutCounter ={v} _7;
  # DEBUG u32Instance => NULL
  # DEBUG u32TimeoutValue => NULL
  # DEBUG linCurrentState => NULL
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetBreakCharDetectLength (base_12, 0);

  <bb 4> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return retVal_15;

}


Lpuart_Lin_Ip_GetTransmitStatus (const uint32 u32Instance, uint8 * const pBytesRemaining)
{
  uint8 u8LocalBytesRemaining;
  const struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  Lpuart_Lin_Ip_StatusType retVal;
  unsigned char _1;
  unsigned char _2;
  <unnamed type> _3;
  _Bool _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG bBytesCountReturn => pBytesRemaining_7(D) != 0B
  # DEBUG BEGIN_STMT
  # DEBUG u8LocalBytesRemaining => 0
  # DEBUG BEGIN_STMT
  linCurrentState_10 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_9(D)];
  # DEBUG linCurrentState => linCurrentState_10
  # DEBUG BEGIN_STMT
  _1 ={v} linCurrentState_10->txSize;
  _2 = linCurrentState_10->cntByte;
  u8LocalBytesRemaining_11 = _1 - _2;
  # DEBUG u8LocalBytesRemaining => u8LocalBytesRemaining_11
  # DEBUG BEGIN_STMT
  _3 ={v} linCurrentState_10->currentEventId;
  if (_3 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  if (u8LocalBytesRemaining_11 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _4 ={v} linCurrentState_10->timeoutCounterFlag;
  if (_4 != 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 3

  <bb 6> [local count: 1073741824]:
  # retVal_5 = PHI <0(2), 0(3), 2(4), 3(5)>
  # DEBUG retVal => retVal_5
  # DEBUG BEGIN_STMT
  if (pBytesRemaining_7(D) != 0B)
    goto <bb 7>; [70.00%]
  else
    goto <bb 8>; [30.00%]

  <bb 7> [local count: 751619278]:
  # DEBUG BEGIN_STMT
  *pBytesRemaining_7(D) = u8LocalBytesRemaining_11;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return retVal_5;

}


Lpuart_Lin_Ip_SyncSendFrameData (const uint32 u32Instance, const uint8 * pTxBuff, const uint8 u8TxSize)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  uint32 timeoutTicks;
  uint32 startTime;
  uint8 sendByte;
  uint8 byteCnt;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  Lpuart_Lin_Ip_StatusType retVal;
  unsigned char _1;
  unsigned char _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  <unnamed type> _9;
  sizetype _10;
  const uint8 * _11;
  _Bool _12;
  long unsigned int startTime.10_13;
  long unsigned int timeoutTicks.11_14;
  _Bool _15;
  long unsigned int _50;
  unsigned char _51;

  <bb 2> [local count: 38844287]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 1
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG byteCnt => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_28 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_27(D)];
  # DEBUG linCurrentState => linCurrentState_28
  # DEBUG BEGIN_STMT
  base_29 = Lpuart_Lin_Ip_apxBases[u32Instance_27(D)];
  # DEBUG base => base_29
  # DEBUG BEGIN_STMT
  retVal_32 = Lpuart_Lin_Ip_StatusBeforeTransfer (u8TxSize_30(D), linCurrentState_28);
  # DEBUG retVal => retVal_32
  # DEBUG BEGIN_STMT
  if (retVal_32 != 0)
    goto <bb 17>; [67.00%]
  else
    goto <bb 3>; [33.00%]

  <bb 3> [local count: 12818615]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_29, 196629, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_29, 65551, 0);
  # DEBUG BEGIN_STMT
  linCurrentState_28->currentEventId ={v} 0;
  # DEBUG BEGIN_STMT
  _1 = linCurrentState_28->currentPid;
  _2 = Lpuart_Lin_Ip_MakeChecksumByte (u32Instance_27(D), pTxBuff_36(D), u8TxSize_30(D), _1);
  linCurrentState_28->checkSum = _2;
  # DEBUG BEGIN_STMT
  pUserConfig_39 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_27(D)];
  # DEBUG pUserConfig => pUserConfig_39
  # DEBUG BEGIN_STMT
  _3 = pUserConfig_39->u32ResponseTimeoutValue;
  _4 = (long unsigned int) u8TxSize_30(D);
  _5 = _4 + 1;
  _6 = _3 * _5;
  _7 = _6 / 500;
  _8 = _7 + 1;
  # DEBUG u32Instance => u32Instance_27(D)
  # DEBUG u32TimeoutValue => _8
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_SetTimeoutCounter
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_45 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_27(D)];
  # DEBUG linCurrentState => linCurrentState_45
  # DEBUG BEGIN_STMT
  linCurrentState_45->timeoutCounterFlag ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_45->timeoutCounter ={v} _8;

  <bb 4> [local count: 121451518]:
  # byteCnt_19 = PHI <0(3), byteCnt_46(18)>
  # DEBUG u32Instance => NULL
  # DEBUG u32TimeoutValue => NULL
  # DEBUG linCurrentState => NULL
  # DEBUG byteCnt => byteCnt_19
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _9 ={v} linCurrentState_28->currentEventId;
  if (_9 != 0)
    goto <bb 16>; [2.75%]
  else
    goto <bb 5>; [97.25%]

  <bb 5> [local count: 118111601]:
  if (byteCnt_19 > u8TxSize_30(D))
    goto <bb 16>; [2.75%]
  else
    goto <bb 6>; [97.25%]

  <bb 6> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  if (byteCnt_19 < u8TxSize_30(D))
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 57431766]:
  # DEBUG BEGIN_STMT
  _10 = (sizetype) byteCnt_19;
  _11 = pTxBuff_36(D) + _10;
  sendByte_41 = *_11;
  # DEBUG sendByte => sendByte_41
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 57431766]:
  # DEBUG BEGIN_STMT
  sendByte_40 = linCurrentState_28->checkSum;
  # DEBUG sendByte => sendByte_40

  <bb 9> [local count: 114863532]:
  # sendByte_20 = PHI <sendByte_41(7), sendByte_40(8)>
  # DEBUG sendByte => sendByte_20
  # DEBUG BEGIN_STMT
  # DEBUG base => base_29
  # DEBUG data => sendByte_20
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwPutchar
  # DEBUG BEGIN_STMT
  # DEBUG D#1 => &base_29->DATA
  # DEBUG dataRegBytes => D#1
  # DEBUG BEGIN_STMT
  MEM[(volatile uint8 *)base_29 + 28B] ={v} sendByte_20;
  # DEBUG base => NULL
  # DEBUG data => NULL
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 3
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_StartTimeout (&startTime, &timeoutTicks, 65535, 0);

  <bb 10> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _12 = Lpuart_Lin_Ip_HwGetStatusFlag (base_29, 131093);
  if (_12 != 0)
    goto <bb 11>; [5.50%]
  else
    goto <bb 13>; [94.50%]

  <bb 11> [local count: 59055800]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_29
  # DEBUG readData => &readbackByte
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwGetchar
  # DEBUG BEGIN_STMT
  _50 ={v} MEM[(const struct LPUART_Type *)base_29].DATA;
  _51 = (unsigned char) _50;
  # DEBUG readbackByte => _51
  # DEBUG base => NULL
  # DEBUG readData => NULL
  # DEBUG BEGIN_STMT
  # DEBUG readbackByte => _51
  # DEBUG sendByte => sendByte_20
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_CheckReadbackByte
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  if (sendByte_20 != _51)
    goto <bb 12>; [66.00%]
  else
    goto <bb 14>; [34.00%]

  <bb 12> [local count: 38976828]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 1
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  startTime.10_13 = startTime;
  timeoutTicks.11_14 = timeoutTicks;
  _15 = Lpuart_Lin_Ip_TimeoutExpired (startTime.10_13, timeoutTicks.11_14, 0);
  if (_15 != 0)
    goto <bb 14>; [5.50%]
  else
    goto <bb 19>; [94.50%]

  <bb 19> [local count: 958878293]:
  goto <bb 10>; [100.00%]

  <bb 14> [local count: 114863532]:
  # retVal_16 = PHI <1(12), 3(13), 0(11)>
  # DEBUG readbackByte => NULL
  # DEBUG sendByte => NULL
  # DEBUG retVal => NULL
  # DEBUG retVal => retVal_16
  # DEBUG BEGIN_STMT
  byteCnt_46 = byteCnt_19 + 1;
  # DEBUG byteCnt => byteCnt_46
  if (byteCnt_19 < u8TxSize_30(D))
    goto <bb 15>; [97.25%]
  else
    goto <bb 16>; [2.75%]

  <bb 15> [local count: 111704785]:
  if (retVal_16 == 0)
    goto <bb 18>; [97.25%]
  else
    goto <bb 16>; [2.75%]

  <bb 18> [local count: 108632903]:
  goto <bb 4>; [100.00%]

  <bb 16> [local count: 12818614]:
  # retVal_17 = PHI <1(5), retVal_16(14), retVal_16(15), 1(4)>
  # DEBUG retVal => retVal_17
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_GotoIdleState (u32Instance_27(D));

  <bb 17> [local count: 38844287]:
  # retVal_18 = PHI <retVal_32(2), retVal_17(16)>
  # DEBUG retVal => retVal_18
  # DEBUG BEGIN_STMT
  # DEBUG D#5 => {CLOBBER}
  # DEBUG readbackByte => D#5
  startTime ={v} {CLOBBER};
  timeoutTicks ={v} {CLOBBER};
  return retVal_18;

}


Lpuart_Lin_Ip_AsyncSendFrameData (const uint32 u32Instance, const uint8 * pTxBuff, const uint8 u8TxSize)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  Lpuart_Lin_Ip_StatusType retVal;
  unsigned char _1;
  unsigned char _2;
  unsigned char _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const uint8 * _10;
  unsigned char _11;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_15 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_14(D)];
  # DEBUG linCurrentState => linCurrentState_15
  # DEBUG BEGIN_STMT
  base_16 = Lpuart_Lin_Ip_apxBases[u32Instance_14(D)];
  # DEBUG base => base_16
  # DEBUG BEGIN_STMT
  retVal_19 = Lpuart_Lin_Ip_StatusBeforeTransfer (u8TxSize_17(D), linCurrentState_15);
  # DEBUG retVal => retVal_19
  # DEBUG BEGIN_STMT
  if (retVal_19 != 0)
    goto <bb 4>; [67.00%]
  else
    goto <bb 3>; [33.00%]

  <bb 3> [local count: 354334802]:
  # DEBUG BEGIN_STMT
  _1 = linCurrentState_15->currentPid;
  _2 = Lpuart_Lin_Ip_MakeChecksumByte (u32Instance_14(D), pTxBuff_20(D), u8TxSize_17(D), _1);
  linCurrentState_15->checkSum = _2;
  # DEBUG BEGIN_STMT
  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00 ();
  # DEBUG BEGIN_STMT
  linCurrentState_15->txBuff = pTxBuff_20(D);
  # DEBUG BEGIN_STMT
  _3 = u8TxSize_17(D) + 1;
  linCurrentState_15->txSize ={v} _3;
  # DEBUG BEGIN_STMT
  linCurrentState_15->cntByte = 0;
  # DEBUG BEGIN_STMT
  linCurrentState_15->currentNodeState ={v} 9;
  # DEBUG BEGIN_STMT
  linCurrentState_15->currentEventId ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_15->isBusBusy ={v} 1;
  # DEBUG BEGIN_STMT
  linCurrentState_15->isTxBusy ={v} 1;
  # DEBUG BEGIN_STMT
  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_00 ();
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetBreakCharDetectLength (base_16, 0);
  # DEBUG BEGIN_STMT
  pUserConfig_33 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_14(D)];
  # DEBUG pUserConfig => pUserConfig_33
  # DEBUG BEGIN_STMT
  _4 = pUserConfig_33->u32ResponseTimeoutValue;
  _5 = (long unsigned int) u8TxSize_17(D);
  _6 = _5 + 1;
  _7 = _4 * _6;
  _8 = _7 / 500;
  _9 = _8 + 1;
  # DEBUG u32Instance => u32Instance_14(D)
  # DEBUG u32TimeoutValue => _9
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_SetTimeoutCounter
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_34 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_14(D)];
  # DEBUG linCurrentState => linCurrentState_34
  # DEBUG BEGIN_STMT
  linCurrentState_34->timeoutCounterFlag ={v} 0;
  # DEBUG BEGIN_STMT
  linCurrentState_34->timeoutCounter ={v} _9;
  # DEBUG u32Instance => NULL
  # DEBUG u32TimeoutValue => NULL
  # DEBUG linCurrentState => NULL
  # DEBUG BEGIN_STMT
  _10 = linCurrentState_15->txBuff;
  _11 = *_10;
  # DEBUG base => base_16
  # DEBUG data => _11
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwPutchar
  # DEBUG BEGIN_STMT
  # DEBUG D#1 => &base_16->DATA
  # DEBUG dataRegBytes => D#1
  # DEBUG BEGIN_STMT
  MEM[(volatile uint8 *)base_16 + 28B] ={v} _11;

  <bb 4> [local count: 1073741824]:
  # DEBUG base => NULL
  # DEBUG data => NULL
  # DEBUG BEGIN_STMT
  return retVal_19;

}


Lpuart_Lin_Ip_Deinit (const uint32 u32Instance)
{
  uint32 timeoutTicks;
  uint32 startTime;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  _Bool _1;
  long unsigned int startTime.6_2;
  long unsigned int timeoutTicks.7_3;
  _Bool _4;

  <bb 2> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  base_9 = Lpuart_Lin_Ip_apxBases[u32Instance_8(D)];
  # DEBUG base => base_9
  # DEBUG BEGIN_STMT
  linCurrentState_10 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_8(D)];
  # DEBUG linCurrentState => linCurrentState_10
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_StartTimeout (&startTime, &timeoutTicks, 65535, 0);

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Lpuart_Lin_Ip_HwGetStatusFlag (base_9, 131094);
  if (_1 != 0)
    goto <bb 5>; [5.50%]
  else
    goto <bb 4>; [94.50%]

  <bb 4> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  startTime.6_2 = startTime;
  timeoutTicks.7_3 = timeoutTicks;
  _4 = Lpuart_Lin_Ip_TimeoutExpired (startTime.6_2, timeoutTicks.7_3, 0);
  if (_4 != 0)
    goto <bb 5>; [5.50%]
  else
    goto <bb 6>; [94.50%]

  <bb 6> [local count: 958878293]:
  goto <bb 3>; [100.00%]

  <bb 5> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetTransmitterCmd (base_9, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetReceiverCmd (base_9, 0);
  # DEBUG BEGIN_STMT
  linCurrentState_10->currentNodeState ={v} 0;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_8(D)] = 0B;
  startTime ={v} {CLOBBER};
  timeoutTicks ={v} {CLOBBER};
  return;

}


Lpuart_Lin_Ip_Init (const uint32 u32Instance, const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig)
{
  struct Lpuart_Lin_Ip_StateStructType * pCrtStateStruct;
  struct LPUART_Type * base;
  _Bool _1;
  _Bool _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  _Bool _6;
  unsigned char _7;
  unsigned char _8;
  unsigned char _9;
  uint8 * _10;
  unsigned char _11;
  unsigned char _12;
  _Bool _13;
  _Bool _14;
  struct Lpuart_Lin_Ip_StateStructType * _15;
  long unsigned int _52;
  long unsigned int _53;
  long unsigned int _54;
  long unsigned int _55;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  base_22 = Lpuart_Lin_Ip_apxBases[u32Instance_21(D)];
  # DEBUG base => base_22
  # DEBUG BEGIN_STMT
  pCrtStateStruct_24 = pUserConfig_23(D)->pStateStruct;
  # DEBUG pCrtStateStruct => pCrtStateStruct_24
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_apxUserConfigs[u32Instance_21(D)] = pUserConfig_23(D);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwInit (base_22);
  # DEBUG BEGIN_STMT
  _1 = pUserConfig_23(D)->autobaudEnable;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _2 = pUserConfig_23(D)->nodeFunction;
  if (_2 != 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  pCrtStateStruct_24->fallingEdgeInterruptCount ={v} 0;
  # DEBUG BEGIN_STMT
  pCrtStateStruct_24->baudrateEvalEnable ={v} 1;

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = pUserConfig_23(D)->u32OverSamplingRatio;
  if (_3 <= 7)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_22
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwEnableBothEdgeSamplingCmd
  # DEBUG BEGIN_STMT
  _52 ={v} base_22->BAUD;
  _53 = _52 | 131072;
  base_22->BAUD ={v} _53;

  <bb 7> [local count: 1073741824]:
  # DEBUG base => NULL
  # DEBUG BEGIN_STMT
  _4 = _3 + 4294967295;
  Lpuart_Lin_Ip_HwSetOversamplingRatio (base_22, _4);
  # DEBUG BEGIN_STMT
  _5 = pUserConfig_23(D)->u32BaudRateDivisor;
  Lpuart_Lin_Ip_HwSetBaudRateDivisor (base_22, _5);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetBitCountPerChar (base_22, 0, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetParityMode (base_22, 0);
  # DEBUG BEGIN_STMT
  # DEBUG base => base_22
  # DEBUG stopBitCount => 0
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwSetStopBitCount
  # DEBUG BEGIN_STMT
  _54 ={v} base_22->BAUD;
  _55 = _54 & 4294959103;
  base_22->BAUD ={v} _55;
  # DEBUG base => NULL
  # DEBUG stopBitCount => NULL
  # DEBUG BEGIN_STMT
  _6 = pUserConfig_23(D)->nodeFunction;
  if (_6 != 0)
    goto <bb 8>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 8> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _7 = pUserConfig_23(D)->u8BreakLength;
  Lpuart_Lin_Ip_HwSetBreakCharTransmitLength (base_22, _7);
  # DEBUG BEGIN_STMT
  _8 = pUserConfig_23(D)->u8BreakLengthDetect;
  Lpuart_Lin_Ip_HwSetBreakCharDetectLength (base_22, _8);
  goto <bb 10>; [100.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _9 = pUserConfig_23(D)->u8BreakLengthDetect;
  Lpuart_Lin_Ip_HwSetBreakCharDetectLength (base_22, _9);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_22, 65551, 1);

  <bb 10> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwClearStatusFlag (base_22, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_22, 196629, 0);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_22, 196633, 1);
  # DEBUG BEGIN_STMT
  pCrtStateStruct_24->currentNodeState ={v} 2;
  # DEBUG BEGIN_STMT
  pCrtStateStruct_24->isTxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  pCrtStateStruct_24->isRxBusy ={v} 0;
  # DEBUG BEGIN_STMT
  pCrtStateStruct_24->isBusBusy ={v} 0;
  # DEBUG BEGIN_STMT
  pCrtStateStruct_24->timeoutCounterFlag ={v} 0;
  # DEBUG BEGIN_STMT
  pCrtStateStruct_24->timeoutCounter ={v} 0;
  # DEBUG BEGIN_STMT
  _10 = pUserConfig_23(D)->classicPID;
  pCrtStateStruct_24->classicPID = _10;
  # DEBUG BEGIN_STMT
  _11 = pUserConfig_23(D)->numOfClassicPID;
  pCrtStateStruct_24->numOfClassicPID = _11;
  # DEBUG BEGIN_STMT
  _12 = pUserConfig_23(D)->u8WakeupByte;
  Lpuart_Lin_Ip_au8WakeupSignal[u32Instance_21(D)] = _12;
  # DEBUG BEGIN_STMT
  _13 = pUserConfig_23(D)->autobaudEnable;
  if (_13 != 0)
    goto <bb 11>; [67.00%]
  else
    goto <bb 12>; [33.00%]

  <bb 11> [local count: 719407023]:
  _14 = pUserConfig_23(D)->nodeFunction;
  if (_14 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 714038314]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetTransmitterCmd (base_22, 1);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetReceiverCmd (base_22, 1);

  <bb 13> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _15 = pUserConfig_23(D)->pStateStruct;
  Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_21(D)] = _15;
  return;

}


Lpuart_Lin_Ip_ProcessWakeupDetect (const uint32 u32Instance)
{
  struct LPUART_Type * base;
  const struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  <unnamed type> _1;
  _Bool _2;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  linCurrentState_6 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_5(D)];
  # DEBUG linCurrentState => linCurrentState_6
  # DEBUG BEGIN_STMT
  base_7 = Lpuart_Lin_Ip_apxBases[u32Instance_5(D)];
  # DEBUG base => base_7
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwClearStatusFlag (base_7, 131102);
  # DEBUG BEGIN_STMT
  _1 ={v} linCurrentState_6->currentNodeState;
  switch (_1) <default: <L6> [33.33%], case 1: <L0> [33.33%], case 4: <L1> [33.33%]>

  <bb 3> [local count: 357878150]:
<L0>:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_CheckWakeupSignal (u32Instance_5(D));
  # DEBUG BEGIN_STMT
  goto <bb 6>; [100.00%]

  <bb 4> [local count: 357878150]:
<L1>:
  # DEBUG BEGIN_STMT
  _2 ={v} linCurrentState_6->baudrateEvalEnable;
  if (_2 != 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 118099789]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_AutoBaudCapture (u32Instance_5(D));

  <bb 6> [local count: 1073634452]:
<L6>:
  return;

}


Lpuart_Lin_Ip_AutoBaudCapture (const uint32 u32Instance)
{
  struct LPUART_Type * base;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  uint8 wakeupByte;
  uint32 masterBaudrateDivisor;
  uint32 tickPerMicros;
  uint32 u32ElapsedTicks;
  static uint8 fallingEgdeCount;
  static uint32 currentTick;
  unsigned char fallingEgdeCount.25_1;
  unsigned char _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  void (*<T2e6>) (uint32, void *) _17;
  long unsigned int _18;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG masterBaudrateDivisor => 0
  # DEBUG BEGIN_STMT
  # DEBUG wakeupByte => 248
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  linCurrentState_31 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_30(D)];
  # DEBUG linCurrentState => linCurrentState_31
  # DEBUG BEGIN_STMT
  base_32 = Lpuart_Lin_Ip_apxBases[u32Instance_30(D)];
  # DEBUG base => base_32
  # DEBUG BEGIN_STMT
  pUserConfig_33 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_30(D)];
  # DEBUG pUserConfig => pUserConfig_33
  # DEBUG BEGIN_STMT
  fallingEgdeCount.25_1 = fallingEgdeCount;
  _2 = fallingEgdeCount.25_1 + 1;
  fallingEgdeCount = _2;
  if (fallingEgdeCount.25_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 24>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  u32ElapsedTicks_38 = OsIf_GetElapsed (&currentTick, 0);
  # DEBUG u32ElapsedTicks => u32ElapsedTicks_38
  # DEBUG BEGIN_STMT
  tickPerMicros_40 = OsIf_MicrosToTicks (1000000, 0);
  # DEBUG tickPerMicros => tickPerMicros_40
  # DEBUG BEGIN_STMT
  _3 = tickPerMicros_40 * 51041;
  if (_3 <= u32ElapsedTicks_38)
    goto <bb 4>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 4> [local count: 268435456]:
  _4 = tickPerMicros_40 * 53125;
  if (_4 >= u32ElapsedTicks_38)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  # DEBUG masterBaudrateDivisor => 19200
  # DEBUG BEGIN_STMT
  # DEBUG wakeupByte => 128

  <bb 6> [local count: 536870913]:
  # masterBaudrateDivisor_19 = PHI <0(3), 0(4), 19200(5)>
  # wakeupByte_24 = PHI <248(3), 248(4), 128(5)>
  # DEBUG wakeupByte => wakeupByte_24
  # DEBUG masterBaudrateDivisor => masterBaudrateDivisor_19
  # DEBUG BEGIN_STMT
  _5 = tickPerMicros_40 * 68055;
  if (_5 <= u32ElapsedTicks_38)
    goto <bb 7>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 7> [local count: 268435456]:
  _6 = tickPerMicros_40 * 70833;
  if (_6 >= u32ElapsedTicks_38)
    goto <bb 8>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 8> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  # DEBUG masterBaudrateDivisor => 14400
  # DEBUG BEGIN_STMT
  # DEBUG wakeupByte => 128

  <bb 9> [local count: 536870913]:
  # masterBaudrateDivisor_20 = PHI <masterBaudrateDivisor_19(6), masterBaudrateDivisor_19(7), 14400(8)>
  # wakeupByte_25 = PHI <wakeupByte_24(6), wakeupByte_24(7), 128(8)>
  # DEBUG wakeupByte => wakeupByte_25
  # DEBUG masterBaudrateDivisor => masterBaudrateDivisor_20
  # DEBUG BEGIN_STMT
  _7 = tickPerMicros_40 * 102083;
  if (_7 <= u32ElapsedTicks_38)
    goto <bb 10>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 10> [local count: 268435456]:
  _8 = tickPerMicros_40 * 106250;
  if (_8 >= u32ElapsedTicks_38)
    goto <bb 11>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 11> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  # DEBUG masterBaudrateDivisor => 9600

  <bb 12> [local count: 536870913]:
  # masterBaudrateDivisor_21 = PHI <masterBaudrateDivisor_20(9), masterBaudrateDivisor_20(10), 9600(11)>
  # DEBUG masterBaudrateDivisor => masterBaudrateDivisor_21
  # DEBUG BEGIN_STMT
  _9 = tickPerMicros_40 * 204166;
  if (_9 <= u32ElapsedTicks_38)
    goto <bb 13>; [50.00%]
  else
    goto <bb 15>; [50.00%]

  <bb 13> [local count: 268435456]:
  _10 = tickPerMicros_40 * 212500;
  if (_10 >= u32ElapsedTicks_38)
    goto <bb 14>; [50.00%]
  else
    goto <bb 15>; [50.00%]

  <bb 14> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  # DEBUG masterBaudrateDivisor => 4800

  <bb 15> [local count: 536870913]:
  # masterBaudrateDivisor_22 = PHI <masterBaudrateDivisor_21(12), masterBaudrateDivisor_21(13), 4800(14)>
  # DEBUG masterBaudrateDivisor => masterBaudrateDivisor_22
  # DEBUG BEGIN_STMT
  _11 = tickPerMicros_40 * 408333;
  if (_11 <= u32ElapsedTicks_38)
    goto <bb 16>; [50.00%]
  else
    goto <bb 17>; [50.00%]

  <bb 16> [local count: 268435456]:
  _12 = tickPerMicros_40 * 425000;
  if (_12 >= u32ElapsedTicks_38)
    goto <bb 18>; [50.00%]
  else
    goto <bb 17>; [50.00%]

  <bb 17> [local count: 402653184]:
  # DEBUG masterBaudrateDivisor => masterBaudrateDivisor_22
  # DEBUG BEGIN_STMT
  if (masterBaudrateDivisor_22 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 335544320]:
  # masterBaudrateDivisor_28 = PHI <masterBaudrateDivisor_22(17), 2400(16)>
  # DEBUG masterBaudrateDivisor => NULL
  # DEBUG BEGIN_STMT
  _13 = pUserConfig_33->u32ChannelClock;
  _14 = pUserConfig_33->u32OverSamplingRatio;
  _15 = _14 * masterBaudrateDivisor_28;
  masterBaudrateDivisor_41 = _13 / _15;
  # DEBUG masterBaudrateDivisor => masterBaudrateDivisor_41

  <bb 19> [local count: 536870913]:
  # masterBaudrateDivisor_23 = PHI <masterBaudrateDivisor_22(17), masterBaudrateDivisor_41(18)>
  # DEBUG masterBaudrateDivisor => masterBaudrateDivisor_23
  # DEBUG BEGIN_STMT
  if (masterBaudrateDivisor_23 != 0)
    goto <bb 20>; [50.00%]
  else
    goto <bb 25>; [50.00%]

  <bb 20> [local count: 268435456]:
  _16 = pUserConfig_33->u32BaudRateDivisor;
  if (_16 != masterBaudrateDivisor_23)
    goto <bb 21>; [48.88%]
  else
    goto <bb 25>; [51.12%]

  <bb 21> [local count: 131211251]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetBaudRateDivisor (base_32, masterBaudrateDivisor_23);
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_au8WakeupSignal[u32Instance_30(D)] = wakeupByte_25;
  # DEBUG BEGIN_STMT
  linCurrentState_31->currentEventId ={v} 2;
  # DEBUG BEGIN_STMT
  linCurrentState_31->baudrateEvalEnable ={v} 0;
  # DEBUG BEGIN_STMT
  _17 = pUserConfig_33->Callback;
  if (_17 != 0B)
    goto <bb 22>; [70.00%]
  else
    goto <bb 23>; [30.00%]

  <bb 22> [local count: 91847876]:
  # DEBUG BEGIN_STMT
  _17 (u32Instance_30(D), linCurrentState_31);

  <bb 23> [local count: 131211251]:
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwSetIntMode (base_32, 65550, 0);
  # DEBUG BEGIN_STMT
  linCurrentState_31->currentNodeState ={v} 6;
  # DEBUG BEGIN_STMT
  linCurrentState_31->currentEventId ={v} 4;
  goto <bb 25>; [100.00%]

  <bb 24> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _18 = OsIf_GetCounter (0);
  currentTick = _18;

  <bb 25> [local count: 1073741824]:
  return;

}


Lpuart_Lin_Ip_MakeChecksumByte (const uint32 u32Instance, const uint8 * buffer, const uint8 sizeBuffer, const uint8 PID)
{
  const uint8 numOfClassicPID;
  const struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  uint8 retVal;
  const uint8 * classicPID;
  uint8 checkSum;
  sizetype _1;
  const uint8 * _2;
  unsigned char _3;

  <bb 2> [local count: 248622364]:
  # DEBUG BEGIN_STMT
  # DEBUG checkSum => PID_6(D)
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  linCurrentState_9 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_8(D)];
  # DEBUG linCurrentState => linCurrentState_9
  # DEBUG BEGIN_STMT
  numOfClassicPID_10 = linCurrentState_9->numOfClassicPID;
  # DEBUG numOfClassicPID => numOfClassicPID_10
  # DEBUG BEGIN_STMT
  classicPID_11 = linCurrentState_9->classicPID;
  # DEBUG classicPID => classicPID_11
  # DEBUG BEGIN_STMT
  if (numOfClassicPID_10 == 255)
    goto <bb 7>; [34.00%]
  else
    goto <bb 3>; [66.00%]

  <bb 3> [local count: 164090760]:
  # DEBUG BEGIN_STMT
  if (classicPID_11 != 0B)
    goto <bb 8>; [70.00%]
  else
    goto <bb 7>; [30.00%]

  <bb 8> [local count: 114863532]:
  goto <bb 6>; [100.00%]

  <bb 4> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _1 = (sizetype) retVal_5;
  _2 = classicPID_11 + _1;
  _3 = *_2;
  if (_3 == PID_6(D))
    goto <bb 7>; [5.50%]
  else
    goto <bb 5>; [94.50%]

  <bb 5> [local count: 958878293]:
  # DEBUG BEGIN_STMT
  retVal_12 = retVal_5 + 1;
  # DEBUG retVal => retVal_12

  <bb 6> [local count: 1073741824]:
  # retVal_5 = PHI <retVal_12(5), 0(8)>
  # DEBUG retVal => retVal_5
  # DEBUG BEGIN_STMT
  if (retVal_5 < numOfClassicPID_10)
    goto <bb 4>; [94.50%]
  else
    goto <bb 7>; [5.50%]

  <bb 7> [local count: 248622363]:
  # checkSum_4 = PHI <0(2), PID_6(D)(3), 0(4), PID_6(D)(6)>
  # DEBUG checkSum => checkSum_4
  # DEBUG BEGIN_STMT
  retVal_16 = Lin_Ip_MakeChecksumByte (buffer_13(D), sizeBuffer_14(D), checkSum_4);
  # DEBUG retVal => retVal_16
  # DEBUG BEGIN_STMT
  return retVal_16;

}


Lpuart_Lin_Ip_FrameErrorIrqHandler (const uint32 u32Instance)
{
  const struct Lpuart_Lin_Ip_UserConfigType * pUserConfig;
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  struct LPUART_Type * base;
  <unnamed type> _1;
  void (*<T2e6>) (uint32, void *) _2;
  <unnamed type> _3;
  void (*<T2e6>) (uint32, void *) _4;
  long unsigned int _15;

  <bb 2> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  base_8 = Lpuart_Lin_Ip_apxBases[u32Instance_7(D)];
  # DEBUG base => base_8
  # DEBUG BEGIN_STMT
  linCurrentState_9 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_7(D)];
  # DEBUG linCurrentState => linCurrentState_9
  # DEBUG BEGIN_STMT
  pUserConfig_10 = Lpuart_Lin_Ip_apxUserConfigs[u32Instance_7(D)];
  # DEBUG pUserConfig => pUserConfig_10
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_HwClearStatusFlag (base_8, 131089);
  # DEBUG BEGIN_STMT
  # DEBUG base => base_8
  # DEBUG readData => &tmpByte
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwGetchar
  # DEBUG BEGIN_STMT
  _15 ={v} MEM[(const struct LPUART_Type *)base_8].DATA;
  # DEBUG tmpByte => (unsigned char) _15
  # DEBUG base => NULL
  # DEBUG readData => NULL
  # DEBUG BEGIN_STMT
  linCurrentState_9->currentEventId ={v} 8;
  # DEBUG BEGIN_STMT
  _1 ={v} linCurrentState_9->currentNodeState;
  if (_1 == 9)
    goto <bb 3>; [34.00%]
  else
    goto <bb 5>; [66.00%]

  <bb 3> [local count: 365072220]:
  # DEBUG BEGIN_STMT
  _2 = pUserConfig_10->Callback;
  if (_2 != 0B)
    goto <bb 4>; [70.00%]
  else
    goto <bb 8>; [30.00%]

  <bb 4> [local count: 255550554]:
  # DEBUG BEGIN_STMT
  _2 (u32Instance_7(D), linCurrentState_9);
  goto <bb 8>; [100.00%]

  <bb 5> [local count: 708669604]:
  # DEBUG BEGIN_STMT
  _3 ={v} linCurrentState_9->currentNodeState;
  if (_3 == 7)
    goto <bb 6>; [34.00%]
  else
    goto <bb 8>; [66.00%]

  <bb 6> [local count: 240947665]:
  # DEBUG BEGIN_STMT
  _4 = pUserConfig_10->Callback;
  if (_4 != 0B)
    goto <bb 7>; [70.00%]
  else
    goto <bb 8>; [30.00%]

  <bb 7> [local count: 168663365]:
  # DEBUG BEGIN_STMT
  _4 (u32Instance_7(D), linCurrentState_9);

  <bb 8> [local count: 1073741824]:
  # DEBUG D#2 => {CLOBBER}
  # DEBUG tmpByte => D#2
  return;

}


Lpuart_Lin_Ip_StatusBeforeTransfer (const uint8 u8Size, const struct Lpuart_Lin_Ip_StateStructType * linCurrentState)
{
  Lpuart_Lin_Ip_StatusType retVal;
  <unnamed type> _1;
  unsigned char _2;
  _Bool _3;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  _1 ={v} linCurrentState_6(D)->currentNodeState;
  # DEBUG checkSleepMode => _1 == 1
  # DEBUG BEGIN_STMT
  _2 = u8Size_7(D) + 255;
  if (_2 > 7)
    goto <bb 6>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 536870913]:
  if (_1 == 1)
    goto <bb 6>; [34.00%]
  else
    goto <bb 4>; [66.00%]

  <bb 4> [local count: 354334802]:
  # DEBUG BEGIN_STMT
  _3 ={v} linCurrentState_6(D)->isBusBusy;
  if (_3 != 0)
    goto <bb 5>; [35.00%]
  else
    goto <bb 6>; [65.00%]

  <bb 5> [local count: 124017181]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 2

  <bb 6> [local count: 1073741824]:
  # retVal_4 = PHI <1(3), 0(4), 2(5), 1(2)>
  # DEBUG retVal => retVal_4
  # DEBUG BEGIN_STMT
  return retVal_4;

}


Lpuart_Lin_Ip_GetBytetoBuffer (const uint8 byteCnt, const uint8 u8BuffSize, uint8 * pBuff, const uint32 u32Instance)
{
  struct Lpuart_Lin_Ip_StateStructType * linCurrentState;
  const struct LPUART_Type * base;
  Lpuart_Lin_Ip_StatusType retVal;
  sizetype _1;
  uint8 * _2;
  unsigned char _3;
  unsigned char _4;
  long unsigned int _18;
  unsigned char _19;
  long unsigned int _20;
  unsigned char _21;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0
  # DEBUG BEGIN_STMT
  base_9 = Lpuart_Lin_Ip_apxBases[u32Instance_8(D)];
  # DEBUG base => base_9
  # DEBUG BEGIN_STMT
  linCurrentState_10 = Lpuart_Lin_Ip_apxStateStructureArray[u32Instance_8(D)];
  # DEBUG linCurrentState => linCurrentState_10
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (byteCnt_11(D) < u8BuffSize_12(D))
    goto <bb 3>; [67.00%]
  else
    goto <bb 4>; [33.00%]

  <bb 3> [local count: 719407023]:
  # DEBUG BEGIN_STMT
  _1 = (sizetype) byteCnt_11(D);
  _2 = pBuff_13(D) + _1;
  # DEBUG base => base_9
  # DEBUG readData => _2
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwGetchar
  # DEBUG BEGIN_STMT
  _18 ={v} base_9->DATA;
  _19 = (unsigned char) _18;
  *_2 = _19;
  goto <bb 7>; [100.00%]

  <bb 4> [local count: 354334802]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_9
  # DEBUG readData => &checkSum
  # DEBUG INLINE_ENTRY Lpuart_Lin_Ip_HwGetchar
  # DEBUG BEGIN_STMT
  _20 ={v} base_9->DATA;
  _21 = (unsigned char) _20;
  # DEBUG checkSum => _21
  # DEBUG base => NULL
  # DEBUG readData => NULL
  # DEBUG BEGIN_STMT
  _3 = linCurrentState_10->currentPid;
  _4 = Lpuart_Lin_Ip_MakeChecksumByte (u32Instance_8(D), pBuff_13(D), u8BuffSize_12(D), _3);
  if (_4 != _21)
    goto <bb 5>; [66.00%]
  else
    goto <bb 6>; [34.00%]

  <bb 5> [local count: 233860969]:
  # DEBUG BEGIN_STMT
  linCurrentState_10->currentEventId ={v} 10;
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 1
  goto <bb 7>; [100.00%]

  <bb 6> [local count: 120473833]:
  # DEBUG BEGIN_STMT
  linCurrentState_10->currentEventId ={v} 12;
  # DEBUG BEGIN_STMT
  linCurrentState_10->currentNodeState ={v} 8;
  # DEBUG BEGIN_STMT
  # DEBUG retVal => 0

  <bb 7> [local count: 1073741824]:
  # retVal_5 = PHI <0(3), 1(5), 0(6)>
  # DEBUG base => NULL
  # DEBUG readData => NULL
  # DEBUG retVal => retVal_5
  # DEBUG BEGIN_STMT
  # DEBUG D#3 => {CLOBBER}
  # DEBUG checkSum => D#3
  return retVal_5;

}


Lpuart_Lin_Ip_HwSetBreakCharDetectLength (struct LPUART_Type * base, uint8 length)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_04 ();
  # DEBUG BEGIN_STMT
  _1 ={v} base_8(D)->STAT;
  _2 = _1 & 1038106623;
  _3 = (long unsigned int) length_9(D);
  _4 = _3 << 25;
  _5 = _2 | _4;
  base_8(D)->STAT ={v} _5;
  # DEBUG BEGIN_STMT
  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_04 ();
  return;

}


Lpuart_Lin_Ip_HwSetBreakCharTransmitLength (struct LPUART_Type * base, uint8 length)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_7(D)->STAT;
  _2 = _1 & 1004552191;
  _3 = (long unsigned int) length_8(D);
  _4 = _3 << 26;
  _5 = _2 | _4;
  base_7(D)->STAT ={v} _5;
  return;

}


Lpuart_Lin_Ip_HwSetOversamplingRatio (struct LPUART_Type * base, uint32 overSamplingRatio)
{
  uint32 baudRegValTemp;
  long unsigned int _1;
  long unsigned int _2;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  baudRegValTemp_5 ={v} base_4(D)->BAUD;
  # DEBUG baudRegValTemp => baudRegValTemp_5
  # DEBUG BEGIN_STMT
  baudRegValTemp_6 = baudRegValTemp_5 & 3774873599;
  # DEBUG baudRegValTemp => baudRegValTemp_6
  # DEBUG BEGIN_STMT
  _1 = overSamplingRatio_7(D) << 24;
  _2 = _1 & 520093696;
  baudRegValTemp_8 = _2 | baudRegValTemp_6;
  # DEBUG baudRegValTemp => baudRegValTemp_8
  # DEBUG BEGIN_STMT
  base_4(D)->BAUD ={v} baudRegValTemp_8;
  return;

}


Lpuart_Lin_Ip_HwSetBaudRateDivisor (struct LPUART_Type * base, uint32 baudRateDivisor)
{
  uint32 baudRegValTemp;
  long unsigned int _1;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  baudRegValTemp_4 ={v} base_3(D)->BAUD;
  # DEBUG baudRegValTemp => baudRegValTemp_4
  # DEBUG BEGIN_STMT
  baudRegValTemp_5 = baudRegValTemp_4 & 4294959104;
  # DEBUG baudRegValTemp => baudRegValTemp_5
  # DEBUG BEGIN_STMT
  _1 = baudRateDivisor_6(D) & 8191;
  baudRegValTemp_7 = _1 | baudRegValTemp_5;
  # DEBUG baudRegValTemp => baudRegValTemp_7
  # DEBUG BEGIN_STMT
  base_3(D)->BAUD ={v} baudRegValTemp_7;
  return;

}


Lpuart_Lin_Ip_HwSetReceiverCmd (struct LPUART_Type * base, boolean enable)
{
  uint32 timeoutTicks;
  uint32 startTime;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  _Bool _6;
  long unsigned int startTime.4_7;
  long unsigned int timeoutTicks.5_8;
  _Bool _9;
  long unsigned int iftmp.3_10;

  <bb 2> [local count: 12992276]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} base_13(D)->CTRL;
  _2 = _1 & 4294705151;
  if (enable_14(D) != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 6496138]:

  <bb 4> [local count: 12992276]:
  # iftmp.3_10 = PHI <262144(2), 0(3)>
  _3 = _2 | iftmp.3_10;
  base_13(D)->CTRL ={v} _3;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_StartTimeout (&startTime, &timeoutTicks, 65535, 0);

  <bb 5> [local count: 118111600]:

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _4 ={v} base_13(D)->CTRL;
  _5 = _4 & 262144;
  _6 = _5 != 0;
  if (_6 != enable_14(D))
    goto <bb 10>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 10> [local count: 955630224]:
  goto <bb 6>; [100.00%]

  <bb 7> [local count: 118111601]:
  # DEBUG BEGIN_STMT
  startTime.4_7 = startTime;
  timeoutTicks.5_8 = timeoutTicks;
  _9 = Lpuart_Lin_Ip_TimeoutExpired (startTime.4_7, timeoutTicks.5_8, 0);
  if (_9 != 0)
    goto <bb 8>; [11.00%]
  else
    goto <bb 9>; [89.00%]

  <bb 9> [local count: 105119325]:
  goto <bb 5>; [100.00%]

  <bb 8> [local count: 12992276]:
  startTime ={v} {CLOBBER};
  timeoutTicks ={v} {CLOBBER};
  return;

}


Lpuart_Lin_Ip_HwSetTransmitterCmd (struct LPUART_Type * base, boolean enable)
{
  uint32 timeoutTicks;
  uint32 startTime;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  _Bool _6;
  long unsigned int startTime.1_7;
  long unsigned int timeoutTicks.2_8;
  _Bool _9;
  long unsigned int iftmp.0_10;

  <bb 2> [local count: 12992276]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} base_13(D)->CTRL;
  _2 = _1 & 4294443007;
  if (enable_14(D) != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 6496138]:

  <bb 4> [local count: 12992276]:
  # iftmp.0_10 = PHI <524288(2), 0(3)>
  _3 = _2 | iftmp.0_10;
  base_13(D)->CTRL ={v} _3;
  # DEBUG BEGIN_STMT
  Lpuart_Lin_Ip_StartTimeout (&startTime, &timeoutTicks, 65535, 0);

  <bb 5> [local count: 118111600]:

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _4 ={v} base_13(D)->CTRL;
  _5 = _4 & 524288;
  _6 = _5 != 0;
  if (_6 != enable_14(D))
    goto <bb 10>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 10> [local count: 955630224]:
  goto <bb 6>; [100.00%]

  <bb 7> [local count: 118111601]:
  # DEBUG BEGIN_STMT
  startTime.1_7 = startTime;
  timeoutTicks.2_8 = timeoutTicks;
  _9 = Lpuart_Lin_Ip_TimeoutExpired (startTime.1_7, timeoutTicks.2_8, 0);
  if (_9 != 0)
    goto <bb 8>; [11.00%]
  else
    goto <bb 9>; [89.00%]

  <bb 9> [local count: 105119325]:
  goto <bb 5>; [100.00%]

  <bb 8> [local count: 12992276]:
  startTime ={v} {CLOBBER};
  timeoutTicks ={v} {CLOBBER};
  return;

}


