board.c:303:0:pwm_init	8	static
board.c:328:0:Set_PWM_Duty	24	static
board.c:355:0:SPI_init	8	static
board.c:361:0:SPI_test	32	static
board.c:388:0:Lin1callback	0	static
board.c:408:0:Lin2callback	0	static
board.c:429:0:Lin_tx_test	24	static
board.c:458:0:i2c0_init	8	static
board.c:480:0:i2c1_init	8	static
board.c:508:0:i2c_test	8	static
board.c:584:0:i2c_delay	8	static
board.c:556:0:sda_in	0	static
board.c:570:0:sda_out	0	static
board.c:596:0:CAN0_Callback	24	static
board.c:653:0:CAN1_Callback	24	static
board.c:710:0:CAN2_Callback	24	static
board.c:764:0:CAN3_Callback	24	static
board.c:818:0:CAN4_Callback	24	static
board.c:872:0:CAN5_Callback	24	static
board.c:926:0:get_can_data	0	static
board.c:936:0:can_main_ECU3	48	static
board.c:1447:0:ECU3_Data_Init	32	static
board.c:2269:0:clear_tx_buf	0	static
board.c:2278:0:clear_tx_ring	8	static
board.c:2300:0:can_send_txring	32	static
board.c:2328:0:can_transmit_txring	32	static
board.c:2287:0:can_tx_check	24	static
board.c:2385:0:DIN_TEST	8	static
board.c:2390:0:Digital_Write	0	static
board.c:2426:0:Digital_Read	0	static
board.c:2469:0:led_onoff	8	static
board.c:2551:0:ADC_Read	0	static
board.c:2592:0:Adc0EndOfChainNoti	8	static
board.c:2600:0:Adc1EndOfChainNoti	8	static
board.c:2607:0:Adc2EndOfChainNoti	8	static
board.c:2620:0:Adc_Read_ch	0	static
board.c:2628:0:tmr_delay	8	static
board.c:2643:0:Pit_Callback	16	static
board.c:2665:0:board_init	0	static
board.c:2675:0:Uart_Init	8	static
board.c:2710:0:UART0_RX_Callback	4	static
board.c:2727:0:UART2_RX_Callback	4	static
board.c:2744:0:UART10_RX_Callback	4	static
board.c:2760:0:UART13_RX_Callback	4	static
board.c:2776:0:UART1_RX_Callback	4	static
board.c:2792:0:UART9_RX_Callback	4	static
board.c:2810:0:Gvar_init	0	static
board.c:2830:0:register_bus_off_callback	8	static
board.c:2840:0:get_char	0	static
board.c:2853:0:put_char	16	static
board.c:2975:0:debug_printf	280	static
board.c:375:0:Lin_init	8	static
board.c:626:0:CAN0_ErrCallback	16	static
board.c:683:0:CAN1_ErrCallback	16	static
board.c:738:0:CAN2_ErrCallback	16	static
board.c:791:0:CAN3_ErrCallback	16	static
board.c:845:0:CAN4_ErrCallback	16	static
board.c:899:0:CAN5_ErrCallback	16	static
board.c:2479:0:Adc_Init	16	static
board.c:2861:0:get_line	16	static
board.c:2904:0:UART0_get_cmd	8	static
board.c:2995:0:setupCanTJA1153	72	static
board.c:1174:0:Can_Init_ECU3	24	static
