CgmXPcfsSdurDivcDiveDivs (const struct Clock_Ip_PcfsConfigType * config)
{
  uint32 swIndex;
  uint32 hwIndex;
  uint32 instance;
  <unnamed type> _1;
  int _2;
  unsigned char _3;
  unsigned char _4;
  unsigned char _5;
  long unsigned int _6;
  volatile struct cgmPcfs_Type * _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = config_19(D)->name;
  _2 = (int) _1;
  _3 = clockFeatures[_2][2];
  instance_20 = (uint32) _3;
  # DEBUG instance => instance_20
  # DEBUG BEGIN_STMT
  _4 = clockFeatures[_2][4];
  hwIndex_21 = (uint32) _4;
  # DEBUG hwIndex => hwIndex_21
  # DEBUG BEGIN_STMT
  _5 = clockFeatures[_2][5];
  swIndex_22 = (uint32) _5;
  # DEBUG swIndex => swIndex_22
  # DEBUG BEGIN_STMT
  _6 = pcfsEntries[swIndex_22].sdur;
  _7 = cgmPcfs[instance_20];
  _8 = _6 & 65535;
  _7->PCFS_SDUR ={v} _8;
  # DEBUG BEGIN_STMT
  _9 = pcfsEntries[swIndex_22].divc_rate;
  _10 = _9 & 255;
  _11 = pcfsEntries[swIndex_22].divc_init;
  _12 = _11 << 16;
  _13 = _10 | _12;
  _7->PCFS[hwIndex_21].DIVC ={v} _13;
  # DEBUG BEGIN_STMT
  _14 = pcfsEntries[swIndex_22].div_endValue;
  _15 = _14 & 1048575;
  _7->PCFS[hwIndex_21].DIVE ={v} _15;
  # DEBUG BEGIN_STMT
  _16 = pcfsEntries[swIndex_22].div_startValue;
  _17 = _16 & 1048575;
  _7->PCFS[hwIndex_21].DIVS ={v} _17;
  return;

}


ProgressiveFrequencyClockSwitchEmpty (const struct Clock_Ip_PcfsConfigType * config)
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


