SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 = msr_UART_EXCLUSIVE_AREA_08[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_9 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_9
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_9];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_13);
  # DEBUG reg_tmp => reg_tmp_13
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_UART_EXCLUSIVE_AREA_08[u32CoreId_9] = reg_tmp_13;
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_13 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_9];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_9] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 = msr_UART_EXCLUSIVE_AREA_07[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_9 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_9
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_9];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_13);
  # DEBUG reg_tmp => reg_tmp_13
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_UART_EXCLUSIVE_AREA_07[u32CoreId_9] = reg_tmp_13;
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_13 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_9];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_9] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 = msr_UART_EXCLUSIVE_AREA_06[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_9 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_9
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_9];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_13);
  # DEBUG reg_tmp => reg_tmp_13
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_UART_EXCLUSIVE_AREA_06[u32CoreId_9] = reg_tmp_13;
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_13 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_9];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_9] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 = msr_UART_EXCLUSIVE_AREA_05[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_9 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_9
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_9];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_13);
  # DEBUG reg_tmp => reg_tmp_13
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_UART_EXCLUSIVE_AREA_05[u32CoreId_9] = reg_tmp_13;
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_13 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_9];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_9] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 = msr_UART_EXCLUSIVE_AREA_04[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_9 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_9
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_9];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_13);
  # DEBUG reg_tmp => reg_tmp_13
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_UART_EXCLUSIVE_AREA_04[u32CoreId_9] = reg_tmp_13;
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_13 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_9];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_9] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 = msr_UART_EXCLUSIVE_AREA_03[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_9 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_9
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_9];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_13);
  # DEBUG reg_tmp => reg_tmp_13
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_UART_EXCLUSIVE_AREA_03[u32CoreId_9] = reg_tmp_13;
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_13 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_9];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_9] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 = msr_UART_EXCLUSIVE_AREA_02[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_9 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_9
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_9];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_13);
  # DEBUG reg_tmp => reg_tmp_13
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_UART_EXCLUSIVE_AREA_02[u32CoreId_9] = reg_tmp_13;
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_13 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_9];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_9] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 = msr_UART_EXCLUSIVE_AREA_01[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_9 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_9
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_9];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_13);
  # DEBUG reg_tmp => reg_tmp_13
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_UART_EXCLUSIVE_AREA_01[u32CoreId_9] = reg_tmp_13;
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_13 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_9];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_9] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 = msr_UART_EXCLUSIVE_AREA_00[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_9 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_9
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_9];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_13);
  # DEBUG reg_tmp => reg_tmp_13
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_UART_EXCLUSIVE_AREA_00[u32CoreId_9] = reg_tmp_13;
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_13 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_9];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_9] ={v} _5;
  return;

}


Uart_schm_read_msr ()
{
  register uint32 reg_tmp;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_1);
  # DEBUG reg_tmp => reg_tmp_1
  # DEBUG BEGIN_STMT
  return reg_tmp_1;

}


