Callgraph clone;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;LPUART_Uart_ClearStatusFlag.part.0;67;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;part
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_StartSendDataUsingInt;50;../RTD/src/Lpuart_Uart_Ip.c;1416;34;inlining to
Callgraph clone;LPUART_Uart_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;215;20;Lpuart_Uart_Ip_StartSendDataUsingInt;50;../RTD/src/Lpuart_Uart_Ip.c;1416;34;inlining to
Callgraph clone;LPUART_Uart_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;215;20;Lpuart_Uart_Ip_CompleteSendDataUsingInt;51;../RTD/src/Lpuart_Uart_Ip.c;1515;13;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_CompleteSendDataUsingInt;51;../RTD/src/Lpuart_Uart_Ip.c;1515;13;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_CompleteSendDataUsingInt;51;../RTD/src/Lpuart_Uart_Ip.c;1515;13;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34;inlining to
Callgraph clone;LPUART_Uart_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34;inlining to
Callgraph clone;LPUART_Uart_FlushRxBuffer;24;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;705;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34;inlining to
Callgraph clone;LPUART_Uart_Getchar;16;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;543;21;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;53;../RTD/src/Lpuart_Uart_Ip.c;1786;13;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;53;../RTD/src/Lpuart_Uart_Ip.c;1786;13;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;53;../RTD/src/Lpuart_Uart_Ip.c;1786;13;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;53;../RTD/src/Lpuart_Uart_Ip.c;1786;13;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;53;../RTD/src/Lpuart_Uart_Ip.c;1786;13;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;53;../RTD/src/Lpuart_Uart_Ip.c;1786;13;inlining to
Callgraph clone;LPUART_Uart_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20;Lpuart_Uart_Ip_CompleteReceiveDataUsingInt;53;../RTD/src/Lpuart_Uart_Ip.c;1786;13;inlining to
Callgraph clone;LPUART_Uart_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_Putchar;13;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;475;20;Lpuart_Uart_Ip_PutData;54;../RTD/src/Lpuart_Uart_Ip.c;1932;13;inlining to
Callgraph removal;LPUART_Uart_Putchar;13;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;475;20
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_TxEmptyIrqHandler;47;../RTD/src/Lpuart_Uart_Ip.c;1235;13;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_TxEmptyIrqHandler;47;../RTD/src/Lpuart_Uart_Ip.c;1235;13;inlining to
Callgraph removal;LPUART_Uart_SetIntMode;100;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20
Callgraph clone;LPUART_Uart_Getchar;16;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;543;21;Lpuart_Uart_Ip_GetData;55;../RTD/src/Lpuart_Uart_Ip.c;1991;13;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph removal;LPUART_Uart_ClearStatusFlag;20;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20
Callgraph removal;LPUART_Uart_SetReceiverCmd;104;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20
Callgraph clone;LPUART_Uart_EnableBothEdgeSamplingCmd;7;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;311;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;LPUART_Uart_Init;0;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;194;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph removal;LPUART_Uart_Init;0;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;194;20
Callgraph removal;LPUART_Uart_EnableBothEdgeSamplingCmd;115;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;311;20
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_Deinit;31;../RTD/src/Lpuart_Uart_Ip.c;308;6;inlining to
Callgraph removal;LPUART_Uart_SetIntMode;122;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20
Callgraph removal;LPUART_Uart_SetIntMode;123;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20
Callgraph clone;LPUART_Uart_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;215;20;Lpuart_Uart_Ip_SyncSend;32;../RTD/src/Lpuart_Uart_Ip.c;349;27;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_SyncSend;32;../RTD/src/Lpuart_Uart_Ip.c;349;27;inlining to
Callgraph clone;LPUART_Uart_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;215;20;Lpuart_Uart_Ip_SyncSend;32;../RTD/src/Lpuart_Uart_Ip.c;349;27;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_SyncSend;32;../RTD/src/Lpuart_Uart_Ip.c;349;27;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_SyncSend;32;../RTD/src/Lpuart_Uart_Ip.c;349;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SyncSend;32;../RTD/src/Lpuart_Uart_Ip.c;349;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SyncSend;32;../RTD/src/Lpuart_Uart_Ip.c;349;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SyncSend;32;../RTD/src/Lpuart_Uart_Ip.c;349;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SyncSend;32;../RTD/src/Lpuart_Uart_Ip.c;349;27;inlining to
Callgraph removal;DevAssert;137;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;138;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;LPUART_Uart_SetTransmitterCmd;1;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;215;20
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;33;../RTD/src/Lpuart_Uart_Ip.c;429;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;33;../RTD/src/Lpuart_Uart_Ip.c;429;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;33;../RTD/src/Lpuart_Uart_Ip.c;429;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;33;../RTD/src/Lpuart_Uart_Ip.c;429;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;33;../RTD/src/Lpuart_Uart_Ip.c;429;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncSend;33;../RTD/src/Lpuart_Uart_Ip.c;429;27;inlining to
Callgraph removal;DevAssert;144;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_GetTransmitStatus;34;../RTD/src/Lpuart_Uart_Ip.c;491;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_GetTransmitStatus;34;../RTD/src/Lpuart_Uart_Ip.c;491;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_GetTransmitStatus;34;../RTD/src/Lpuart_Uart_Ip.c;491;27;inlining to
Callgraph clone;LPUART_Uart_FlushTxBuffer;23;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;693;20;Lpuart_Uart_Ip_AbortSendingData;35;../RTD/src/Lpuart_Uart_Ip.c;546;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AbortSendingData;35;../RTD/src/Lpuart_Uart_Ip.c;546;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AbortSendingData;35;../RTD/src/Lpuart_Uart_Ip.c;546;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AbortSendingData;35;../RTD/src/Lpuart_Uart_Ip.c;546;27;inlining to
Callgraph removal;LPUART_Uart_FlushTxBuffer;23;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;693;20
Callgraph clone;LPUART_Uart_Getchar;16;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;543;21;Lpuart_Uart_Ip_SyncReceive;36;../RTD/src/Lpuart_Uart_Ip.c;602;27;inlining to
Callgraph clone;LPUART_Uart_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20;Lpuart_Uart_Ip_SyncReceive;36;../RTD/src/Lpuart_Uart_Ip.c;602;27;inlining to
Callgraph clone;LPUART_Uart_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20;Lpuart_Uart_Ip_SyncReceive;36;../RTD/src/Lpuart_Uart_Ip.c;602;27;inlining to
Callgraph clone;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20;Lpuart_Uart_Ip_SyncReceive;36;../RTD/src/Lpuart_Uart_Ip.c;602;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SyncReceive;36;../RTD/src/Lpuart_Uart_Ip.c;602;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SyncReceive;36;../RTD/src/Lpuart_Uart_Ip.c;602;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SyncReceive;36;../RTD/src/Lpuart_Uart_Ip.c;602;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SyncReceive;36;../RTD/src/Lpuart_Uart_Ip.c;602;27;inlining to
Callgraph removal;DevAssert;156;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;LPUART_Uart_SetReceiverCmd;2;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;230;20
Callgraph removal;LPUART_Uart_SetIntMode;11;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;414;20
Callgraph removal;LPUART_Uart_Getchar;152;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;543;21
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;38;../RTD/src/Lpuart_Uart_Ip.c;757;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;38;../RTD/src/Lpuart_Uart_Ip.c;757;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;38;../RTD/src/Lpuart_Uart_Ip.c;757;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;38;../RTD/src/Lpuart_Uart_Ip.c;757;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;38;../RTD/src/Lpuart_Uart_Ip.c;757;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AsyncReceive;38;../RTD/src/Lpuart_Uart_Ip.c;757;27;inlining to
Callgraph removal;DevAssert;160;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;161;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;163;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;159;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_GetReceiveStatus;39;../RTD/src/Lpuart_Uart_Ip.c;819;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_GetReceiveStatus;39;../RTD/src/Lpuart_Uart_Ip.c;819;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_GetReceiveStatus;39;../RTD/src/Lpuart_Uart_Ip.c;819;27;inlining to
Callgraph removal;DevAssert;164;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;166;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph clone;LPUART_Uart_FlushRxBuffer;24;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;705;20;Lpuart_Uart_Ip_AbortReceivingData;40;../RTD/src/Lpuart_Uart_Ip.c;872;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AbortReceivingData;40;../RTD/src/Lpuart_Uart_Ip.c;872;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AbortReceivingData;40;../RTD/src/Lpuart_Uart_Ip.c;872;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_AbortReceivingData;40;../RTD/src/Lpuart_Uart_Ip.c;872;27;inlining to
Callgraph removal;DevAssert;167;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;169;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;LPUART_Uart_FlushRxBuffer;24;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;705;20
Callgraph clone;LPUART_Uart_EnableBothEdgeSamplingCmd;7;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;311;20;Lpuart_Uart_Ip_SetBaudRate;41;../RTD/src/Lpuart_Uart_Ip.c;933;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SetBaudRate;41;../RTD/src/Lpuart_Uart_Ip.c;933;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SetBaudRate;41;../RTD/src/Lpuart_Uart_Ip.c;933;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SetBaudRate;41;../RTD/src/Lpuart_Uart_Ip.c;933;27;inlining to
Callgraph removal;DevAssert;170;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;171;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;LPUART_Uart_EnableBothEdgeSamplingCmd;7;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;311;20
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_GetBaudRate;42;../RTD/src/Lpuart_Uart_Ip.c;1045;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_GetBaudRate;42;../RTD/src/Lpuart_Uart_Ip.c;1045;6;inlining to
Callgraph removal;DevAssert;173;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;174;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SetTxBuffer;43;../RTD/src/Lpuart_Uart_Ip.c;1067;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SetTxBuffer;43;../RTD/src/Lpuart_Uart_Ip.c;1067;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SetTxBuffer;43;../RTD/src/Lpuart_Uart_Ip.c;1067;27;inlining to
Callgraph removal;DevAssert;175;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;176;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;177;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SetRxBuffer;44;../RTD/src/Lpuart_Uart_Ip.c;1094;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SetRxBuffer;44;../RTD/src/Lpuart_Uart_Ip.c;1094;27;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_SetRxBuffer;44;../RTD/src/Lpuart_Uart_Ip.c;1094;27;inlining to
Callgraph removal;DevAssert;178;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;179;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;DevAssert;180;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph clone;LPUART_Uart_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;LPUART_Uart_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;LPUART_Uart_Getchar;16;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;543;21;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;LPUART_Uart_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;LPUART_Uart_Getchar;16;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;543;21;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph removal;DevAssert;25;C:/NXP/S32DS.3.4/S32DS/software/PlatformSDK_S32K3_2021_03/SW32K3_RTD_4_4_0_9_0_D2103/Base_TS_T40D34M9I0R0/include/Devassert.h;65;20
Callgraph removal;LPUART_Uart_Getchar;16;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;543;21
Callgraph removal;LPUART_Uart_GetStatusFlag;19;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23
Callgraph removal;LPUART_Uart_GetIntMode;12;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23
Callgraph removal;LPUART_Uart_Getchar;185;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;543;21
Callgraph removal;LPUART_Uart_GetIntMode;183;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23
Callgraph removal;LPUART_Uart_GetStatusFlag;182;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;602;23
Callgraph removal;LPUART_Uart_GetIntMode;181;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;429;23
Callgraph clone;LPUART_Uart_CheckTimeout;22;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;666;23;LPUART_Uart_CheckTimeout.constprop.0;186;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;666;23;constprop
Callgraph clone;LPUART_Uart_ClearErrorFlags;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;650;20;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34;inlining to
Callgraph clone;LPUART_Uart_Getchar9;17;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;557;22;Lpuart_Uart_Ip_GetData;55;../RTD/src/Lpuart_Uart_Ip.c;1991;13;inlining to
Callgraph clone;LPUART_Uart_ClearErrorFlags;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;650;20;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag.part.0;67;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;inlining to
Callgraph clone;LPUART_Uart_ClearStatusFlag.part.0;67;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;inlining to
Callgraph clone;LPUART_Uart_ClearErrorFlags;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;650;20;Lpuart_Uart_Ip_AbortReceivingData;40;../RTD/src/Lpuart_Uart_Ip.c;872;27;inlining to
Callgraph clone;LPUART_Uart_Getchar10;18;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;578;22;Lpuart_Uart_Ip_GetData;55;../RTD/src/Lpuart_Uart_Ip.c;1991;13;inlining to
Callgraph clone;LPUART_Uart_Putchar9;14;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;490;20;Lpuart_Uart_Ip_PutData;54;../RTD/src/Lpuart_Uart_Ip.c;1932;13;inlining to
Callgraph clone;LPUART_Uart_SetBaudRateDivisor;3;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;244;20;Lpuart_Uart_Ip_SetBaudRate;41;../RTD/src/Lpuart_Uart_Ip.c;933;27;inlining to
Callgraph clone;LPUART_Uart_Putchar10;15;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;514;20;Lpuart_Uart_Ip_PutData;54;../RTD/src/Lpuart_Uart_Ip.c;1932;13;inlining to
Callgraph clone;LPUART_Uart_SetOversamplingRatio;5;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;277;20;Lpuart_Uart_Ip_SetBaudRate;41;../RTD/src/Lpuart_Uart_Ip.c;933;27;inlining to
Callgraph clone;LPUART_Uart_SetBaudRateDivisor;3;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;244;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;LPUART_Uart_SetStopBitCount;10;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;398;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;LPUART_Uart_SetOversamplingRatio;5;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;277;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;LPUART_Uart_SetParityMode;9;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;381;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;LPUART_Uart_SetBitCountPerChar;8;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;328;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;LPUART_Uart_SetBitCountPerChar;8;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;328;20;Lpuart_Uart_Ip_Init;30;../RTD/src/Lpuart_Uart_Ip.c;224;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_RxIrqHandler;46;../RTD/src/Lpuart_Uart_Ip.c;1193;13;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_TxCompleteIrqHandler;48;../RTD/src/Lpuart_Uart_Ip.c;1273;13;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13;Lpuart_Uart_Ip_SyncReceive;36;../RTD/src/Lpuart_Uart_Ip.c;602;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_TxEmptyIrqHandler;47;../RTD/src/Lpuart_Uart_Ip.c;1235;13;Lpuart_Uart_Ip_IRQHandler;45;../RTD/src/Lpuart_Uart_Ip.c;1120;6;inlining to
Callgraph clone;Lpuart_Uart_Ip_StartSendDataUsingInt;50;../RTD/src/Lpuart_Uart_Ip.c;1416;34;Lpuart_Uart_Ip_AsyncSend;33;../RTD/src/Lpuart_Uart_Ip.c;429;27;inlining to
Callgraph clone;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34;Lpuart_Uart_Ip_AsyncReceive;38;../RTD/src/Lpuart_Uart_Ip.c;757;27;inlining to
Callgraph removal;LPUART_Uart_CheckTimeout;22;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;666;23
Callgraph removal;LPUART_Uart_Putchar9;14;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;490;20
Callgraph removal;LPUART_Uart_Putchar10;15;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;514;20
Callgraph removal;LPUART_Uart_Getchar9;17;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;557;22
Callgraph removal;LPUART_Uart_Getchar10;18;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;578;22
Callgraph removal;LPUART_Uart_SetBaudRateDivisor;3;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;244;20
Callgraph removal;LPUART_Uart_SetOversamplingRatio;5;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;277;20
Callgraph removal;LPUART_Uart_SetBitCountPerChar;8;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;328;20
Callgraph removal;LPUART_Uart_SetBitCountPerChar;192;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;328;20
Callgraph removal;LPUART_Uart_SetStopBitCount;10;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;398;20
Callgraph removal;LPUART_Uart_SetParityMode;9;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;381;20
Callgraph removal;Lpuart_Uart_Ip_StartSendDataUsingInt;50;../RTD/src/Lpuart_Uart_Ip.c;1416;34
Callgraph removal;Lpuart_Uart_Ip_StartGetData;37;../RTD/src/Lpuart_Uart_Ip.c;687;13
Callgraph removal;LPUART_Uart_ClearStatusFlag.part.0;189;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20
Callgraph removal;Lpuart_Uart_Ip_StartReceiveDataUsingInt;52;../RTD/src/Lpuart_Uart_Ip.c;1661;34
Callgraph removal;LPUART_Uart_ClearErrorFlags;187;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;650;20
Callgraph removal;LPUART_Uart_ClearErrorFlags;21;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;650;20
Callgraph removal;LPUART_Uart_SetOversamplingRatio;191;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;277;20
Callgraph removal;LPUART_Uart_ClearErrorFlags;188;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;650;20
Callgraph removal;Lpuart_Uart_Ip_ErrIrqHandler;49;../RTD/src/Lpuart_Uart_Ip.c;1303;13
Callgraph removal;LPUART_Uart_ClearStatusFlag.part.0;67;../RTD/include/Lpuart_Uart_Ip_HwAccess.h;618;20
Callgraph removal;Lpuart_Uart_Ip_RxIrqHandler;46;../RTD/src/Lpuart_Uart_Ip.c;1193;13
Callgraph removal;Lpuart_Uart_Ip_TxEmptyIrqHandler;47;../RTD/src/Lpuart_Uart_Ip.c;1235;13
Callgraph removal;Lpuart_Uart_Ip_TxCompleteIrqHandler;48;../RTD/src/Lpuart_Uart_Ip.c;1273;13
