Symbol table:

CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0) @0733a700
  Type: function definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: bufferFreqs/25 (read)configuredCoreClock/29 (write)bufferFreqs/25 (read)configuredAipsPlatClock/30 (write)bufferFreqs/25 (read)configuredAipsSlowClock/31 (write)bufferFreqs/25 (read)configuredHseClock/32 (write)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (26801491 (estimated locally),0.23 per call) 
  Calls: 
NOT_UNDER_MCU_CONTROL_A.part.0/230 (NOT_UNDER_MCU_CONTROL_A.part.0) @0733a9a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: clkState/27 (write)clkState/27 (write)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: NOT_UNDER_MCU_CONTROL_A/44 (536870912 (estimated locally),0.50 per call) 
  Calls: 
CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (CONFIG_ELEMENTS_MAPPINGS_01.part.0) @0733a000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: freqPointers/26 (write)config_clock/33 (read)freqPointers/26 (write)freqPointers/26 (write)freqPointers/26 (write)
  Referring: 
  Availability: local
  Function flags: count:118111598 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: CONFIG_ELEMENTS_MAPPINGS_01/42 (46707769 (estimated locally),1.00 per call) 
  Calls: 
*.LC1/228 (*.LC1) @067e9c18
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: 
  Referring: PCFS_PLL_PHI0_B/63 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
*.LC0/227 (*.LC0) @067e9b88
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: 
  Referring: PCFS_PLL_PHI0_B/63 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
pcfsCallbacks/226 (pcfsCallbacks) @07090288
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
selectorCallbacks/225 (selectorCallbacks) @070901b0
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
pllCallbacks/224 (pllCallbacks) @07090048
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
intOscCallbacks/223 (intOscCallbacks) @0708ef30
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
gateCallbacks/222 (gateCallbacks) @0708edc8
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
fracDivCallbacks/221 (fracDivCallbacks) @0708ec60
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
extOscCallbacks/220 (extOscCallbacks) @0708eb88
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
dividerTriggerCallbacks/219 (dividerTriggerCallbacks) @0708eab0
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
dividerCallbacks/218 (dividerCallbacks) @0708e9d8
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
cmuCallbacks/217 (cmuCallbacks) @0708e750
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
ClockTimeoutExpired/216 (ClockTimeoutExpired) @07084b60
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: CallbackDelay/77 (1073741824 (estimated locally),9.09 per call) 
  Calls: 
ClockStartTimeout/215 (ClockStartTimeout) @07084a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: CallbackDelay/77 (118111600 (estimated locally),1.00 per call) 
  Calls: 
bufferFreqEntriesCLKOUT_RUN_CLK.5132/214 (bufferFreqEntriesCLKOUT_RUN_CLK) @0708e318
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntriesCLKOUT_RUN_CLK.5131/213 (selectorEntriesCLKOUT_RUN_CLK) @0708e2d0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesQSPI_MEM_CLK.5130/212 (bufferFreqEntriesQSPI_MEM_CLK) @0708e288
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesLBIST_CLK.5129/211 (bufferFreqEntriesLBIST_CLK) @0708e240
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesDCM_CLK.5128/210 (bufferFreqEntriesDCM_CLK) @0708e1f8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesHSE_CLK.5127/209 (bufferFreqEntriesHSE_CLK) @0708e1b0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesAIPS_SLOW_CLK.5126/208 (bufferFreqEntriesAIPS_SLOW_CLK) @0708e168
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesAIPS_PLAT_CLK.5125/207 (bufferFreqEntriesAIPS_PLAT_CLK) @0708e120
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesCORE_CLK.5124/206 (bufferFreqEntriesCORE_CLK) @0708e0d8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesSCS_CLK.5123/205 (bufferFreqEntriesSCS_CLK) @0708e090
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntriesSCS_CLK.5122/204 (selectorEntriesSCS_CLK) @0708e048
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
convertValueToClockState.5133/203 (convertValueToClockState) @0708e000
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
get_TRACE_CLK_Frequency/202 (get_TRACE_CLK_Frequency) @0707ab60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_STM1_CLK_Frequency/201 (get_STM1_CLK_Frequency) @0707a620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_STMB_CLK_Frequency/200 (1073741824 (estimated locally),1.00 per call) 
get_STMB_CLK_Frequency/200 (get_STMB_CLK_Frequency) @0707a0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_STM1_CLK_Frequency/201 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_STM0_CLK_Frequency/199 (get_STM0_CLK_Frequency) @0707ad20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_STMA_CLK_Frequency/198 (1073741824 (estimated locally),1.00 per call) 
get_STMA_CLK_Frequency/198 (get_STMA_CLK_Frequency) @0707aa80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_STM0_CLK_Frequency/199 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_RTC0_CLK_Frequency/197 (get_RTC0_CLK_Frequency) @0707a7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_RTC_CLK_Frequency/196 (1073741824 (estimated locally),1.00 per call) 
get_RTC_CLK_Frequency/196 (get_RTC_CLK_Frequency) @0707a540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_RTC0_CLK_Frequency/197 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_QSPI0_SFCK_CLK_Frequency/195 (get_QSPI0_SFCK_CLK_Frequency) @0707a2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_QSPI_SFCK_CLK_Frequency/194 (1073741824 (estimated locally),1.00 per call) 
get_QSPI_SFCK_CLK_Frequency/194 (get_QSPI_SFCK_CLK_Frequency) @0707a000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_QSPI0_SFCK_CLK_Frequency/195 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_FLEXCAN5_CLK_Frequency/193 (get_FLEXCAN5_CLK_Frequency) @0706db60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANB_CLK_Frequency/190 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCAN4_CLK_Frequency/192 (get_FLEXCAN4_CLK_Frequency) @0706d620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANB_CLK_Frequency/190 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCAN3_CLK_Frequency/191 (get_FLEXCAN3_CLK_Frequency) @0706d0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANB_CLK_Frequency/190 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCANB_CLK_Frequency/190 (get_FLEXCANB_CLK_Frequency) @0706dd20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_FLEXCAN5_CLK_Frequency/193 (1073741824 (estimated locally),1.00 per call) get_FLEXCAN4_CLK_Frequency/192 (1073741824 (estimated locally),1.00 per call) get_FLEXCAN3_CLK_Frequency/191 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_FLEXCAN2_CLK_Frequency/189 (get_FLEXCAN2_CLK_Frequency) @0706da80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANA_CLK_Frequency/186 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCAN1_CLK_Frequency/188 (get_FLEXCAN1_CLK_Frequency) @0706d7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANA_CLK_Frequency/186 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCAN0_CLK_Frequency/187 (get_FLEXCAN0_CLK_Frequency) @0706d540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANA_CLK_Frequency/186 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCANA_CLK_Frequency/186 (get_FLEXCANA_CLK_Frequency) @0706d2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_FLEXCAN2_CLK_Frequency/189 (1073741824 (estimated locally),1.00 per call) get_FLEXCAN1_CLK_Frequency/188 (1073741824 (estimated locally),1.00 per call) get_FLEXCAN0_CLK_Frequency/187 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_EMAC0_TX_CLK_Frequency/185 (get_EMAC0_TX_CLK_Frequency) @0706d000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_EMAC_TX_CLK_Frequency/184 (1073741824 (estimated locally),1.00 per call) 
get_EMAC_TX_CLK_Frequency/184 (get_EMAC_TX_CLK_Frequency) @07064b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_EMAC0_TX_CLK_Frequency/185 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_EMAC0_TS_CLK_Frequency/183 (get_EMAC0_TS_CLK_Frequency) @07064620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_EMAC_TS_CLK_Frequency/182 (1073741824 (estimated locally),1.00 per call) 
get_EMAC_TS_CLK_Frequency/182 (get_EMAC_TS_CLK_Frequency) @070640e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_EMAC0_TS_CLK_Frequency/183 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_EMAC0_RX_CLK_Frequency/181 (get_EMAC0_RX_CLK_Frequency) @07064d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_EMAC_RX_CLK_Frequency/180 (1073741824 (estimated locally),1.00 per call) 
get_EMAC_RX_CLK_Frequency/180 (get_EMAC_RX_CLK_Frequency) @07064a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_EMAC0_RX_CLK_Frequency/181 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CLKOUT_STANDBY_CLK_Frequency/179 (get_CLKOUT_STANDBY_CLK_Frequency) @070647e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SWT1_CLK_Frequency/178 (get_SWT1_CLK_Frequency) @07064540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_SWT0_CLK_Frequency/177 (1073741824 (estimated locally),1.00 per call) 
get_SWT0_CLK_Frequency/177 (get_SWT0_CLK_Frequency) @070642a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_SWT1_CLK_Frequency/178 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_SIUL0_CLK_Frequency/176 (get_SIUL0_CLK_Frequency) @07064000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_QSPI0_TX_MEM_CLK_Frequency/175 (get_QSPI0_TX_MEM_CLK_Frequency) @07061b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_QSPI0_RAM_CLK_Frequency/174 (1073741824 (estimated locally),1.00 per call) 
get_QSPI0_RAM_CLK_Frequency/174 (get_QSPI0_RAM_CLK_Frequency) @07061620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_QSPI0_TX_MEM_CLK_Frequency/175 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_DCM0_CLK_Frequency/173 (get_DCM0_CLK_Frequency) @070610e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SEMA42_CLK_Frequency/172 (get_SEMA42_CLK_Frequency) @07061d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/165 (1073741824 (estimated locally),1.00 per call) 
get_MSCM_CLK_Frequency/171 (get_MSCM_CLK_Frequency) @07061a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/165 (1073741824 (estimated locally),1.00 per call) 
get_LPUART8_CLK_Frequency/170 (get_LPUART8_CLK_Frequency) @070617e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/165 (1073741824 (estimated locally),1.00 per call) 
get_LPUART0_CLK_Frequency/169 (get_LPUART0_CLK_Frequency) @07061540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/165 (1073741824 (estimated locally),1.00 per call) 
get_LPSPI0_CLK_Frequency/168 (get_LPSPI0_CLK_Frequency) @070612a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/165 (1073741824 (estimated locally),1.00 per call) 
get_INTM_CLK_Frequency/167 (get_INTM_CLK_Frequency) @07061000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/165 (1073741824 (estimated locally),1.00 per call) 
get_FLEXIO0_CLK_Frequency/166 (get_FLEXIO0_CLK_Frequency) @0705eb60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/165 (1073741824 (estimated locally),1.00 per call) 
get_CRC0_CLK_Frequency/165 (get_CRC0_CLK_Frequency) @0705e620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_SEMA42_CLK_Frequency/172 (1073741824 (estimated locally),1.00 per call) get_MSCM_CLK_Frequency/171 (1073741824 (estimated locally),1.00 per call) get_LPUART8_CLK_Frequency/170 (1073741824 (estimated locally),1.00 per call) get_LPUART0_CLK_Frequency/169 (1073741824 (estimated locally),1.00 per call) get_LPSPI0_CLK_Frequency/168 (1073741824 (estimated locally),1.00 per call) get_INTM_CLK_Frequency/167 (1073741824 (estimated locally),1.00 per call) get_FLEXIO0_CLK_Frequency/166 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_WKPU0_CLK_Frequency/164 (get_WKPU0_CLK_Frequency) @0705e0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_TSENSE0_CLK_Frequency/163 (get_TSENSE0_CLK_Frequency) @0705ed20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_TRGMUX0_CLK_Frequency/162 (get_TRGMUX0_CLK_Frequency) @0705ea80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_STCU0_CLK_Frequency/161 (get_STCU0_CLK_Frequency) @0705e7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_SAI1_CLK_Frequency/160 (get_SAI1_CLK_Frequency) @0705e540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_SAI0_CLK_Frequency/159 (get_SAI0_CLK_Frequency) @0705e2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_PIT2_CLK_Frequency/158 (get_PIT2_CLK_Frequency) @0705e000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_PIT1_CLK_Frequency/157 (get_PIT1_CLK_Frequency) @07057b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_PIT0_CLK_Frequency/156 (get_PIT0_CLK_Frequency) @07057620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_MUB_CLK_Frequency/155 (get_MUB_CLK_Frequency) @070570e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_MUA_CLK_Frequency/154 (get_MUA_CLK_Frequency) @07057d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART9_CLK_Frequency/153 (get_LPUART9_CLK_Frequency) @07057a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART7_CLK_Frequency/152 (get_LPUART7_CLK_Frequency) @070577e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART6_CLK_Frequency/151 (get_LPUART6_CLK_Frequency) @07057540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART5_CLK_Frequency/150 (get_LPUART5_CLK_Frequency) @070572a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART4_CLK_Frequency/149 (get_LPUART4_CLK_Frequency) @07057000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART3_CLK_Frequency/148 (get_LPUART3_CLK_Frequency) @07054b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART2_CLK_Frequency/147 (get_LPUART2_CLK_Frequency) @07054620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART1_CLK_Frequency/146 (get_LPUART1_CLK_Frequency) @070540e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART15_CLK_Frequency/145 (get_LPUART15_CLK_Frequency) @07054d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART14_CLK_Frequency/144 (get_LPUART14_CLK_Frequency) @07054a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART13_CLK_Frequency/143 (get_LPUART13_CLK_Frequency) @070547e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART12_CLK_Frequency/142 (get_LPUART12_CLK_Frequency) @07054540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART11_CLK_Frequency/141 (get_LPUART11_CLK_Frequency) @070542a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPUART10_CLK_Frequency/140 (get_LPUART10_CLK_Frequency) @07054000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPSPI5_CLK_Frequency/139 (get_LPSPI5_CLK_Frequency) @07051b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPSPI4_CLK_Frequency/138 (get_LPSPI4_CLK_Frequency) @07051620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPSPI3_CLK_Frequency/137 (get_LPSPI3_CLK_Frequency) @070510e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPSPI2_CLK_Frequency/136 (get_LPSPI2_CLK_Frequency) @07051d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPSPI1_CLK_Frequency/135 (get_LPSPI1_CLK_Frequency) @07051a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPI2C1_CLK_Frequency/134 (get_LPI2C1_CLK_Frequency) @070517e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_LPI2C0_CLK_Frequency/133 (get_LPI2C0_CLK_Frequency) @07051540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_FLASH0_CLK_Frequency/132 (get_FLASH0_CLK_Frequency) @070512a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_ERM0_CLK_Frequency/131 (get_ERM0_CLK_Frequency) @07051000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_EIM0_CLK_Frequency/130 (get_EIM0_CLK_Frequency) @0704eb60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_CMP2_CLK_Frequency/129 (get_CMP2_CLK_Frequency) @0704e620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_CMP1_CLK_Frequency/128 (get_CMP1_CLK_Frequency) @0704e0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/127 (1073741824 (estimated locally),1.00 per call) 
get_CMP0_CLK_Frequency/127 (get_CMP0_CLK_Frequency) @0704ed20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_WKPU0_CLK_Frequency/164 (1073741824 (estimated locally),1.00 per call) get_TSENSE0_CLK_Frequency/163 (1073741824 (estimated locally),1.00 per call) get_TRGMUX0_CLK_Frequency/162 (1073741824 (estimated locally),1.00 per call) get_STCU0_CLK_Frequency/161 (1073741824 (estimated locally),1.00 per call) get_SAI1_CLK_Frequency/160 (1073741824 (estimated locally),1.00 per call) get_SAI0_CLK_Frequency/159 (1073741824 (estimated locally),1.00 per call) get_PIT2_CLK_Frequency/158 (1073741824 (estimated locally),1.00 per call) get_PIT1_CLK_Frequency/157 (1073741824 (estimated locally),1.00 per call) get_PIT0_CLK_Frequency/156 (1073741824 (estimated locally),1.00 per call) get_MUB_CLK_Frequency/155 (1073741824 (estimated locally),1.00 per call) get_MUA_CLK_Frequency/154 (1073741824 (estimated locally),1.00 per call) get_LPUART9_CLK_Frequency/153 (1073741824 (estimated locally),1.00 per call) get_LPUART7_CLK_Frequency/152 (1073741824 (estimated locally),1.00 per call) get_LPUART6_CLK_Frequency/151 (1073741824 (estimated locally),1.00 per call) get_LPUART5_CLK_Frequency/150 (1073741824 (estimated locally),1.00 per call) get_LPUART4_CLK_Frequency/149 (1073741824 (estimated locally),1.00 per call) get_LPUART3_CLK_Frequency/148 (1073741824 (estimated locally),1.00 per call) get_LPUART2_CLK_Frequency/147 (1073741824 (estimated locally),1.00 per call) get_LPUART1_CLK_Frequency/146 (1073741824 (estimated locally),1.00 per call) get_LPUART15_CLK_Frequency/145 (1073741824 (estimated locally),1.00 per call) get_LPUART14_CLK_Frequency/144 (1073741824 (estimated locally),1.00 per call) get_LPUART13_CLK_Frequency/143 (1073741824 (estimated locally),1.00 per call) get_LPUART12_CLK_Frequency/142 (1073741824 (estimated locally),1.00 per call) get_LPUART11_CLK_Frequency/141 (1073741824 (estimated locally),1.00 per call) get_LPUART10_CLK_Frequency/140 (1073741824 (estimated locally),1.00 per call) get_LPSPI5_CLK_Frequency/139 (1073741824 (estimated locally),1.00 per call) get_LPSPI4_CLK_Frequency/138 (1073741824 (estimated locally),1.00 per call) get_LPSPI3_CLK_Frequency/137 (1073741824 (estimated locally),1.00 per call) get_LPSPI2_CLK_Frequency/136 (1073741824 (estimated locally),1.00 per call) get_LPSPI1_CLK_Frequency/135 (1073741824 (estimated locally),1.00 per call) get_LPI2C1_CLK_Frequency/134 (1073741824 (estimated locally),1.00 per call) get_LPI2C0_CLK_Frequency/133 (1073741824 (estimated locally),1.00 per call) get_FLASH0_CLK_Frequency/132 (1073741824 (estimated locally),1.00 per call) get_ERM0_CLK_Frequency/131 (1073741824 (estimated locally),1.00 per call) get_EIM0_CLK_Frequency/130 (1073741824 (estimated locally),1.00 per call) get_CMP2_CLK_Frequency/129 (1073741824 (estimated locally),1.00 per call) get_CMP1_CLK_Frequency/128 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_TEMPSENSE_CLK_Frequency/126 (get_TEMPSENSE_CLK_Frequency) @0704ea80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_TCM_CM7_1_CLK_Frequency/125 (get_TCM_CM7_1_CLK_Frequency) @0704e7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_TCM_CM7_0_CLK_Frequency/124 (get_TCM_CM7_0_CLK_Frequency) @0704e540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_LCU1_CLK_Frequency/123 (get_LCU1_CLK_Frequency) @0704e2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_LCU0_CLK_Frequency/122 (get_LCU0_CLK_Frequency) @0704e000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EMIOS2_CLK_Frequency/121 (get_EMIOS2_CLK_Frequency) @07048b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EMIOS1_CLK_Frequency/120 (get_EMIOS1_CLK_Frequency) @07048620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EMIOS0_CLK_Frequency/119 (get_EMIOS0_CLK_Frequency) @070480e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD9_CLK_Frequency/118 (get_EDMA0_TCD9_CLK_Frequency) @07048d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD8_CLK_Frequency/117 (get_EDMA0_TCD8_CLK_Frequency) @07048a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD7_CLK_Frequency/116 (get_EDMA0_TCD7_CLK_Frequency) @070487e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD6_CLK_Frequency/115 (get_EDMA0_TCD6_CLK_Frequency) @07048540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD5_CLK_Frequency/114 (get_EDMA0_TCD5_CLK_Frequency) @070482a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD4_CLK_Frequency/113 (get_EDMA0_TCD4_CLK_Frequency) @07048000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD3_CLK_Frequency/112 (get_EDMA0_TCD3_CLK_Frequency) @07046b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD31_CLK_Frequency/111 (get_EDMA0_TCD31_CLK_Frequency) @07046620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD30_CLK_Frequency/110 (get_EDMA0_TCD30_CLK_Frequency) @070460e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD2_CLK_Frequency/109 (get_EDMA0_TCD2_CLK_Frequency) @07046d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD29_CLK_Frequency/108 (get_EDMA0_TCD29_CLK_Frequency) @07046a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD28_CLK_Frequency/107 (get_EDMA0_TCD28_CLK_Frequency) @070467e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD27_CLK_Frequency/106 (get_EDMA0_TCD27_CLK_Frequency) @07046540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD26_CLK_Frequency/105 (get_EDMA0_TCD26_CLK_Frequency) @070462a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD25_CLK_Frequency/104 (get_EDMA0_TCD25_CLK_Frequency) @07046000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD24_CLK_Frequency/103 (get_EDMA0_TCD24_CLK_Frequency) @07043b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD23_CLK_Frequency/102 (get_EDMA0_TCD23_CLK_Frequency) @07043620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD22_CLK_Frequency/101 (get_EDMA0_TCD22_CLK_Frequency) @070430e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD21_CLK_Frequency/100 (get_EDMA0_TCD21_CLK_Frequency) @07043d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD20_CLK_Frequency/99 (get_EDMA0_TCD20_CLK_Frequency) @07043a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD1_CLK_Frequency/98 (get_EDMA0_TCD1_CLK_Frequency) @070437e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD19_CLK_Frequency/97 (get_EDMA0_TCD19_CLK_Frequency) @07043540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD18_CLK_Frequency/96 (get_EDMA0_TCD18_CLK_Frequency) @070432a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD17_CLK_Frequency/95 (get_EDMA0_TCD17_CLK_Frequency) @07043000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD16_CLK_Frequency/94 (get_EDMA0_TCD16_CLK_Frequency) @0703eb60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD15_CLK_Frequency/93 (get_EDMA0_TCD15_CLK_Frequency) @0703e620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD14_CLK_Frequency/92 (get_EDMA0_TCD14_CLK_Frequency) @0703e0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD13_CLK_Frequency/91 (get_EDMA0_TCD13_CLK_Frequency) @0703ed20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD12_CLK_Frequency/90 (get_EDMA0_TCD12_CLK_Frequency) @0703ea80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD11_CLK_Frequency/89 (get_EDMA0_TCD11_CLK_Frequency) @0703e7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD10_CLK_Frequency/88 (get_EDMA0_TCD10_CLK_Frequency) @0703e540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD0_CLK_Frequency/87 (get_EDMA0_TCD0_CLK_Frequency) @0703e2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_CLK_Frequency/86 (get_EDMA0_CLK_Frequency) @0703e000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_DMAMUX1_CLK_Frequency/85 (get_DMAMUX1_CLK_Frequency) @07038a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_DMAMUX0_CLK_Frequency/84 (get_DMAMUX0_CLK_Frequency) @07038540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_BCTU0_CLK_Frequency/83 (get_BCTU0_CLK_Frequency) @07038ee0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_ADC2_CLK_Frequency/82 (get_ADC2_CLK_Frequency) @07038c40
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_ADC1_CLK_Frequency/81 (get_ADC1_CLK_Frequency) @070389a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/80 (1073741824 (estimated locally),1.00 per call) 
get_ADC0_CLK_Frequency/80 (get_ADC0_CLK_Frequency) @07038700
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_TEMPSENSE_CLK_Frequency/126 (1073741824 (estimated locally),1.00 per call) get_TCM_CM7_1_CLK_Frequency/125 (1073741824 (estimated locally),1.00 per call) get_TCM_CM7_0_CLK_Frequency/124 (1073741824 (estimated locally),1.00 per call) get_LCU1_CLK_Frequency/123 (1073741824 (estimated locally),1.00 per call) get_LCU0_CLK_Frequency/122 (1073741824 (estimated locally),1.00 per call) get_EMIOS2_CLK_Frequency/121 (1073741824 (estimated locally),1.00 per call) get_EMIOS1_CLK_Frequency/120 (1073741824 (estimated locally),1.00 per call) get_EMIOS0_CLK_Frequency/119 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD9_CLK_Frequency/118 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD8_CLK_Frequency/117 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD7_CLK_Frequency/116 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD6_CLK_Frequency/115 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD5_CLK_Frequency/114 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD4_CLK_Frequency/113 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD3_CLK_Frequency/112 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD31_CLK_Frequency/111 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD30_CLK_Frequency/110 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD2_CLK_Frequency/109 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD29_CLK_Frequency/108 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD28_CLK_Frequency/107 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD27_CLK_Frequency/106 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD26_CLK_Frequency/105 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD25_CLK_Frequency/104 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD24_CLK_Frequency/103 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD23_CLK_Frequency/102 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD22_CLK_Frequency/101 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD21_CLK_Frequency/100 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD20_CLK_Frequency/99 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD1_CLK_Frequency/98 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD19_CLK_Frequency/97 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD18_CLK_Frequency/96 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD17_CLK_Frequency/95 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD16_CLK_Frequency/94 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD15_CLK_Frequency/93 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD14_CLK_Frequency/92 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD13_CLK_Frequency/91 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD12_CLK_Frequency/90 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD11_CLK_Frequency/89 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD10_CLK_Frequency/88 (1073741824 (estimated locally),1.00 per call) get_EDMA0_TCD0_CLK_Frequency/87 (1073741824 (estimated locally),1.00 per call) get_EDMA0_CLK_Frequency/86 (1073741824 (estimated locally),1.00 per call) get_DMAMUX1_CLK_Frequency/85 (1073741824 (estimated locally),1.00 per call) get_DMAMUX0_CLK_Frequency/84 (1073741824 (estimated locally),1.00 per call) get_BCTU0_CLK_Frequency/83 (1073741824 (estimated locally),1.00 per call) get_ADC2_CLK_Frequency/82 (1073741824 (estimated locally),1.00 per call) get_ADC1_CLK_Frequency/81 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
consumerClockCallbacks/79 (consumerClockCallbacks) @07037240
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: get_ADC0_CLK_Frequency/80 (addr)get_ADC1_CLK_Frequency/81 (addr)get_ADC2_CLK_Frequency/82 (addr)get_BCTU0_CLK_Frequency/83 (addr)get_CLKOUT_STANDBY_CLK_Frequency/179 (addr)get_CMP0_CLK_Frequency/127 (addr)get_CMP1_CLK_Frequency/128 (addr)get_CMP2_CLK_Frequency/129 (addr)get_CRC0_CLK_Frequency/165 (addr)get_DCM0_CLK_Frequency/173 (addr)get_DMAMUX0_CLK_Frequency/84 (addr)get_DMAMUX1_CLK_Frequency/85 (addr)get_EDMA0_CLK_Frequency/86 (addr)get_EDMA0_TCD0_CLK_Frequency/87 (addr)get_EDMA0_TCD10_CLK_Frequency/88 (addr)get_EDMA0_TCD11_CLK_Frequency/89 (addr)get_EDMA0_TCD12_CLK_Frequency/90 (addr)get_EDMA0_TCD13_CLK_Frequency/91 (addr)get_EDMA0_TCD14_CLK_Frequency/92 (addr)get_EDMA0_TCD15_CLK_Frequency/93 (addr)get_EDMA0_TCD16_CLK_Frequency/94 (addr)get_EDMA0_TCD17_CLK_Frequency/95 (addr)get_EDMA0_TCD18_CLK_Frequency/96 (addr)get_EDMA0_TCD19_CLK_Frequency/97 (addr)get_EDMA0_TCD1_CLK_Frequency/98 (addr)get_EDMA0_TCD20_CLK_Frequency/99 (addr)get_EDMA0_TCD21_CLK_Frequency/100 (addr)get_EDMA0_TCD22_CLK_Frequency/101 (addr)get_EDMA0_TCD23_CLK_Frequency/102 (addr)get_EDMA0_TCD24_CLK_Frequency/103 (addr)get_EDMA0_TCD25_CLK_Frequency/104 (addr)get_EDMA0_TCD26_CLK_Frequency/105 (addr)get_EDMA0_TCD27_CLK_Frequency/106 (addr)get_EDMA0_TCD28_CLK_Frequency/107 (addr)get_EDMA0_TCD29_CLK_Frequency/108 (addr)get_EDMA0_TCD2_CLK_Frequency/109 (addr)get_EDMA0_TCD30_CLK_Frequency/110 (addr)get_EDMA0_TCD31_CLK_Frequency/111 (addr)get_EDMA0_TCD3_CLK_Frequency/112 (addr)get_EDMA0_TCD4_CLK_Frequency/113 (addr)get_EDMA0_TCD5_CLK_Frequency/114 (addr)get_EDMA0_TCD6_CLK_Frequency/115 (addr)get_EDMA0_TCD7_CLK_Frequency/116 (addr)get_EDMA0_TCD8_CLK_Frequency/117 (addr)get_EDMA0_TCD9_CLK_Frequency/118 (addr)get_EIM0_CLK_Frequency/130 (addr)get_EMAC_RX_CLK_Frequency/180 (addr)get_EMAC0_RX_CLK_Frequency/181 (addr)get_EMAC_TS_CLK_Frequency/182 (addr)get_EMAC0_TS_CLK_Frequency/183 (addr)get_EMAC_TX_CLK_Frequency/184 (addr)get_EMAC0_TX_CLK_Frequency/185 (addr)get_EMIOS0_CLK_Frequency/119 (addr)get_EMIOS1_CLK_Frequency/120 (addr)get_EMIOS2_CLK_Frequency/121 (addr)get_ERM0_CLK_Frequency/131 (addr)get_FLASH0_CLK_Frequency/132 (addr)get_FLEXCANA_CLK_Frequency/186 (addr)get_FLEXCAN0_CLK_Frequency/187 (addr)get_FLEXCAN1_CLK_Frequency/188 (addr)get_FLEXCAN2_CLK_Frequency/189 (addr)get_FLEXCANB_CLK_Frequency/190 (addr)get_FLEXCAN3_CLK_Frequency/191 (addr)get_FLEXCAN4_CLK_Frequency/192 (addr)get_FLEXCAN5_CLK_Frequency/193 (addr)get_FLEXIO0_CLK_Frequency/166 (addr)get_INTM_CLK_Frequency/167 (addr)get_LCU0_CLK_Frequency/122 (addr)get_LCU1_CLK_Frequency/123 (addr)get_LPI2C0_CLK_Frequency/133 (addr)get_LPI2C1_CLK_Frequency/134 (addr)get_LPSPI0_CLK_Frequency/168 (addr)get_LPSPI1_CLK_Frequency/135 (addr)get_LPSPI2_CLK_Frequency/136 (addr)get_LPSPI3_CLK_Frequency/137 (addr)get_LPSPI4_CLK_Frequency/138 (addr)get_LPSPI5_CLK_Frequency/139 (addr)get_LPUART0_CLK_Frequency/169 (addr)get_LPUART10_CLK_Frequency/140 (addr)get_LPUART11_CLK_Frequency/141 (addr)get_LPUART12_CLK_Frequency/142 (addr)get_LPUART13_CLK_Frequency/143 (addr)get_LPUART14_CLK_Frequency/144 (addr)get_LPUART15_CLK_Frequency/145 (addr)get_LPUART1_CLK_Frequency/146 (addr)get_LPUART2_CLK_Frequency/147 (addr)get_LPUART3_CLK_Frequency/148 (addr)get_LPUART4_CLK_Frequency/149 (addr)get_LPUART5_CLK_Frequency/150 (addr)get_LPUART6_CLK_Frequency/151 (addr)get_LPUART7_CLK_Frequency/152 (addr)get_LPUART8_CLK_Frequency/170 (addr)get_LPUART9_CLK_Frequency/153 (addr)get_MSCM_CLK_Frequency/171 (addr)get_MUA_CLK_Frequency/154 (addr)get_MUB_CLK_Frequency/155 (addr)get_PIT0_CLK_Frequency/156 (addr)get_PIT1_CLK_Frequency/157 (addr)get_PIT2_CLK_Frequency/158 (addr)get_QSPI0_RAM_CLK_Frequency/174 (addr)get_QSPI_SFCK_CLK_Frequency/194 (addr)get_QSPI0_SFCK_CLK_Frequency/195 (addr)get_QSPI0_TX_MEM_CLK_Frequency/175 (addr)get_RTC_CLK_Frequency/196 (addr)get_RTC0_CLK_Frequency/197 (addr)get_SAI0_CLK_Frequency/159 (addr)get_SAI1_CLK_Frequency/160 (addr)get_SEMA42_CLK_Frequency/172 (addr)get_SIUL0_CLK_Frequency/176 (addr)get_STCU0_CLK_Frequency/161 (addr)get_STMA_CLK_Frequency/198 (addr)get_STM0_CLK_Frequency/199 (addr)get_STMB_CLK_Frequency/200 (addr)get_STM1_CLK_Frequency/201 (addr)get_SWT0_CLK_Frequency/177 (addr)get_SWT1_CLK_Frequency/178 (addr)get_TCM_CM7_0_CLK_Frequency/124 (addr)get_TCM_CM7_1_CLK_Frequency/125 (addr)get_TEMPSENSE_CLK_Frequency/126 (addr)get_TRACE_CLK_Frequency/202 (addr)get_TRGMUX0_CLK_Frequency/162 (addr)get_TSENSE0_CLK_Frequency/163 (addr)get_WKPU0_CLK_Frequency/164 (addr)
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
calcFreqCallbacks/78 (calcFreqCallbacks) @06f84ea0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: CONFIG_ELEMENTS_MAPPINGS_01/42 (addr)CONFIG_ELEMENTS_MAPPINGS_02/43 (addr)NOT_UNDER_MCU_CONTROL_A/44 (addr)NOT_UNDER_MCU_CONTROL_B/45 (addr)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (addr)PLL_A/47 (addr)PLL_B/48 (addr)PLL_C/49 (addr)IntegerDividers_A/50 (addr)IntegerDividers_B/51 (addr)IntegerDividers_C/52 (addr)IntegerDividers_D/53 (addr)IntegerDividers_E/54 (addr)IntegerDividers_F/55 (addr)IntegerDividers_G/56 (addr)IntegerDividers_H/57 (addr)IntegerDividers_I/58 (addr)IntegerDividers_J/59 (addr)IntegerDividers_K/60 (addr)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (addr)PCFS_PLL_PHI0_A/62 (addr)PCFS_PLL_PHI0_B/63 (addr)PCFS_PLL_PHI0_C/64 (addr)PCFS_PLL_PHI0_D/65 (addr)PCFS_PLL_PHI0_E/66 (addr)CMU_FXOSC_CLK_A/67 (addr)CMU_FXOSC_CLK_B/68 (addr)CMU_CORE_CLK_A/69 (addr)CMU_CORE_CLK_B/70 (addr)CMU_AIPS_PLAT_CLK_A/71 (addr)CMU_AIPS_PLAT_CLK_B/72 (addr)CMU_HSE_CLK_A/73 (addr)CMU_HSE_CLK_B/74 (addr)CallEmptyCallbacks/76 (addr)CallbackDelay/77 (addr)
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
CallbackDelay/77 (CallbackDelay) @06fda460
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:118111600 (estimated locally) body optimize_size
  Called by: 
  Calls: ClockTimeoutExpired/216 (1073741824 (estimated locally),9.09 per call) ClockStartTimeout/215 (118111600 (estimated locally),1.00 per call) 
CallEmptyCallbacks/76 (CallEmptyCallbacks) @06fda1c0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuCallbacks/217 (read)cmuCallbacks/217 (read)cmuCallbacks/217 (read)cmuCallbacks/217 (read)dividerCallbacks/218 (read)dividerTriggerCallbacks/219 (read)extOscCallbacks/220 (read)fracDivCallbacks/221 (read)fracDivCallbacks/221 (read)gateCallbacks/222 (read)gateCallbacks/222 (read)intOscCallbacks/223 (read)pllCallbacks/224 (read)pllCallbacks/224 (read)selectorCallbacks/225 (read)pcfsCallbacks/226 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
McMeEnterKey/75 (McMeEnterKey) @06fd2e00
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_HSE_CLK_B/74 (CMU_HSE_CLK_B) @06fd2d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_HSE_CLK_A/73 (CMU_HSE_CLK_A) @06fd2a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)configuredHseClock/32 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_AIPS_PLAT_CLK_B/72 (CMU_AIPS_PLAT_CLK_B) @06fd27e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_AIPS_PLAT_CLK_A/71 (CMU_AIPS_PLAT_CLK_A) @06fd2540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)configuredAipsPlatClock/30 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_CORE_CLK_B/70 (CMU_CORE_CLK_B) @06fd22a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_CORE_CLK_A/69 (CMU_CORE_CLK_A) @06fd2000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)configuredCoreClock/29 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_FXOSC_CLK_B/68 (CMU_FXOSC_CLK_B) @06f86d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_FXOSC_CLK_A/67 (CMU_FXOSC_CLK_A) @06f86a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_E/66 (PCFS_PLL_PHI0_E) @06f867e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)pcfsEntries/34 (write)pcfsEntries/34 (write)pcfsEntries/34 (write)pcfsEntries/34 (write)pcfsEntries/34 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_D/65 (PCFS_PLL_PHI0_D) @06f86540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:118111600 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_C/64 (PCFS_PLL_PHI0_C) @06f862a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:118111600 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_B/63 (PCFS_PLL_PHI0_B) @06f86000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: *.LC0/227 (read)*.LC1/228 (read)tmpData/28 (read)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:357985524 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_A/62 (PCFS_PLL_PHI0_A) @06f78d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: pcfsEntries/34 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS) @06f78a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: config_clock/33 (read)bufferFreqs/25 (read)configuredCoreClock/29 (write)bufferFreqs/25 (read)configuredAipsPlatClock/30 (write)bufferFreqs/25 (read)configuredAipsSlowClock/31 (write)bufferFreqs/25 (read)configuredHseClock/32 (write)configuredCoreClock/29 (write)configuredAipsPlatClock/30 (write)configuredAipsSlowClock/31 (write)configuredHseClock/32 (write)configuredCoreClock/29 (write)configuredAipsPlatClock/30 (write)configuredAipsSlowClock/31 (write)configuredHseClock/32 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:114863532 (estimated locally) body optimize_size
  Called by: 
  Calls: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (26801491 (estimated locally),0.23 per call) 
IntegerDividers_K/60 (IntegerDividers_K) @06f787e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_J/59 (IntegerDividers_J) @06f78540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_I/58 (IntegerDividers_I) @06f782a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_H/57 (IntegerDividers_H) @06f78000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_G/56 (IntegerDividers_G) @06f20d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_F/55 (IntegerDividers_F) @06f20a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (read)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_E/54 (IntegerDividers_E) @06f207e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_D/53 (IntegerDividers_D) @06f20540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_C/52 (IntegerDividers_C) @06f202a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_B/51 (IntegerDividers_B) @06f20000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_A/50 (IntegerDividers_A) @06f15d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PLL_C/49 (PLL_C) @06f15a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PLL_B/48 (PLL_B) @06f157e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (write)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PLL_A/47 (PLL_A) @06f15540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: bufferFreqs/25 (read)tmpData/28 (write)freqPointers/26 (read)config_clock/33 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS) @06f152a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (write)freqPointers/26 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (write)freqPointers/26 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
NOT_UNDER_MCU_CONTROL_B/45 (NOT_UNDER_MCU_CONTROL_B) @06f15000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)clkState/27 (write)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)clkState/27 (write)clkState/27 (write)clkState/27 (write)freqPointers/26 (read)selectorEntryIndex/23 (read)clkState/27 (write)freqPointers/26 (read)selectorEntryIndex/23 (read)clkState/27 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
NOT_UNDER_MCU_CONTROL_A/44 (NOT_UNDER_MCU_CONTROL_A) @06ebcee0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: clkState/27 (write)freqPointers/26 (read)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)freqPointers/26 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: NOT_UNDER_MCU_CONTROL_A.part.0/230 (536870912 (estimated locally),0.50 per call) 
CONFIG_ELEMENTS_MAPPINGS_02/43 (CONFIG_ELEMENTS_MAPPINGS_02) @06ebcc40
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (write)config_clock/33 (read)freqPointers/26 (write)freqPointers/26 (write)pcfsEntries/34 (read)pcfsEntries/34 (write)cmuEntries/35 (read)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:7299031 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CONFIG_ELEMENTS_MAPPINGS_01/42 (CONFIG_ELEMENTS_MAPPINGS_01) @06ebc9a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:46707770 (estimated locally) body optimize_size
  Called by: 
  Calls: CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (46707769 (estimated locally),1.00 per call) 
UpdateFrequencies/41 (UpdateFrequencies) @06ebc700
  Type: function definition analyzed
  Visibility: externally_visible public
  References: clkState/27 (read)freqPointers/26 (write)clkState/27 (read)freqPointers/26 (write)clkState/27 (read)clkState/27 (read)freqPointers/26 (write)clkState/27 (read)freqPointers/26 (write)freqPointers/26 (write)clkState/27 (read)convertValueToClockState.5133/203 (read)clkState/27 (write)clkState/27 (read)convertValueToClockState.5133/203 (read)clkState/27 (write)freqPointers/26 (write)freqPointers/26 (write)clkState/27 (read)selectorEntriesSCS_CLK.5122/204 (read)clkState/27 (read)bufferFreqEntriesSCS_CLK.5123/205 (read)freqPointers/26 (write)bufferFreqEntriesCORE_CLK.5124/206 (read)freqPointers/26 (write)bufferFreqEntriesAIPS_PLAT_CLK.5125/207 (read)freqPointers/26 (write)bufferFreqEntriesAIPS_SLOW_CLK.5126/208 (read)freqPointers/26 (write)bufferFreqEntriesHSE_CLK.5127/209 (read)freqPointers/26 (write)bufferFreqEntriesDCM_CLK.5128/210 (read)freqPointers/26 (write)bufferFreqEntriesLBIST_CLK.5129/211 (read)freqPointers/26 (write)bufferFreqEntriesQSPI_MEM_CLK.5130/212 (read)freqPointers/26 (write)selectorEntryIndex/23 (read)clkState/27 (write)selectorEntriesCLKOUT_RUN_CLK.5131/213 (read)clkState/27 (read)bufferFreqEntriesCLKOUT_RUN_CLK.5132/214 (read)freqPointers/26 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
GetProducerClockFreq/40 (GetProducerClockFreq) @06ebc000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
SpecificPlatformInitClock/39 (SpecificPlatformInitClock) @06eb7a80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: config_clock/33 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
SpecificPeripheralClockInitialization/38 (SpecificPeripheralClockInitialization) @06eb7ee0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
GetClockState/37 (GetClockState) @06eb7c40
  Type: function definition analyzed
  Visibility: externally_visible public
  References: clkState/27 (read)clkState/27 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
UpdateClockState/36 (UpdateClockState) @06eb79a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: clkState/27 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
cmuEntries/35 (cmuEntries) @06eb4870
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: CMU_FXOSC_CLK_A/67 (write)CMU_AIPS_PLAT_CLK_B/72 (read)CMU_AIPS_PLAT_CLK_B/72 (write)CMU_AIPS_PLAT_CLK_B/72 (write)CMU_HSE_CLK_A/73 (read)CMU_AIPS_PLAT_CLK_A/71 (read)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (read)CMU_CORE_CLK_B/70 (read)CMU_CORE_CLK_B/70 (write)CMU_CORE_CLK_B/70 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CMU_CORE_CLK_A/69 (read)CMU_CORE_CLK_A/69 (write)CMU_CORE_CLK_A/69 (write)CMU_HSE_CLK_A/73 (write)CMU_FXOSC_CLK_B/68 (read)CMU_FXOSC_CLK_B/68 (write)CMU_FXOSC_CLK_B/68 (write)CMU_HSE_CLK_A/73 (write)CMU_FXOSC_CLK_A/67 (read)CMU_FXOSC_CLK_A/67 (write)CMU_HSE_CLK_B/74 (read)CMU_HSE_CLK_B/74 (write)CMU_HSE_CLK_B/74 (write)
  Availability: available
  Varpool flags: initialized
pcfsEntries/34 (pcfsEntries) @06eb4708
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (read)PCFS_PLL_PHI0_A/62 (read)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)
  Availability: available
  Varpool flags: initialized
config_clock/33 (config_clock) @06eb4678
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CMU_AIPS_PLAT_CLK_A/71 (read)CMU_CORE_CLK_A/69 (read)CMU_FXOSC_CLK_A/67 (read)PCFS_PLL_PHI0_A/62 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)IntegerDividers_K/60 (read)IntegerDividers_J/59 (read)IntegerDividers_J/59 (read)IntegerDividers_J/59 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)IntegerDividers_F/55 (read)IntegerDividers_F/55 (read)IntegerDividers_F/55 (read)IntegerDividers_E/54 (read)IntegerDividers_E/54 (read)IntegerDividers_E/54 (read)IntegerDividers_D/53 (read)IntegerDividers_D/53 (read)IntegerDividers_D/53 (read)IntegerDividers_C/52 (read)IntegerDividers_C/52 (read)IntegerDividers_C/52 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)PLL_A/47 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (read)IntegerDividers_K/60 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)CONFIG_ELEMENTS_MAPPINGS_02/43 (read)IntegerDividers_K/60 (read)CMU_HSE_CLK_A/73 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)SpecificPlatformInitClock/39 (write)
  Availability: available
  Varpool flags: initialized
configuredHseClock/32 (configuredHseClock) @06eb4480
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_HSE_CLK_A/73 (read)
  Availability: available
  Varpool flags: initialized
configuredAipsSlowClock/31 (configuredAipsSlowClock) @06eb43f0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CMU_CORE_CLK_A/69 (read)CMU_FXOSC_CLK_A/67 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_AIPS_PLAT_CLK_A/71 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_HSE_CLK_A/73 (read)
  Availability: available
  Varpool flags: initialized
configuredAipsPlatClock/30 (configuredAipsPlatClock) @06eb4360
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_AIPS_PLAT_CLK_A/71 (read)
  Availability: available
  Varpool flags: initialized
configuredCoreClock/29 (configuredCoreClock) @06eb42d0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_CORE_CLK_A/69 (read)
  Availability: available
  Varpool flags: initialized
tmpData/28 (tmpData) @06eb4240
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CMU_AIPS_PLAT_CLK_B/72 (read)CMU_AIPS_PLAT_CLK_B/72 (read)CMU_CORE_CLK_A/69 (write)CMU_CORE_CLK_A/69 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_CORE_CLK_B/70 (read)CMU_CORE_CLK_B/70 (read)CMU_FXOSC_CLK_A/67 (write)CMU_FXOSC_CLK_A/67 (write)CMU_CORE_CLK_A/69 (write)CMU_CORE_CLK_A/69 (write)CMU_FXOSC_CLK_B/68 (read)CMU_FXOSC_CLK_B/68 (read)PCFS_PLL_PHI0_E/66 (read)PCFS_PLL_PHI0_E/66 (read)CMU_FXOSC_CLK_A/67 (write)CMU_FXOSC_CLK_A/67 (write)PCFS_PLL_PHI0_E/66 (read)PCFS_PLL_PHI0_E/66 (read)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_D/65 (write)PCFS_PLL_PHI0_D/65 (write)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_C/64 (read)PCFS_PLL_PHI0_C/64 (write)PCFS_PLL_PHI0_C/64 (write)PCFS_PLL_PHI0_C/64 (write)PCFS_PLL_PHI0_C/64 (read)PLL_A/47 (write)PCFS_PLL_PHI0_C/64 (read)PCFS_PLL_PHI0_C/64 (read)PCFS_PLL_PHI0_D/65 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_AIPS_PLAT_CLK_A/71 (write)PLL_C/49 (read)PLL_C/49 (read)PLL_C/49 (read)PLL_C/49 (read)PLL_C/49 (read)PCFS_PLL_PHI0_A/62 (write)PCFS_PLL_PHI0_A/62 (write)PCFS_PLL_PHI0_B/63 (read)PCFS_PLL_PHI0_B/63 (write)CMU_HSE_CLK_A/73 (write)CMU_HSE_CLK_A/73 (write)PLL_B/48 (read)PLL_B/48 (write)PLL_B/48 (read)PLL_C/49 (read)PLL_C/49 (read)PCFS_PLL_PHI0_A/62 (write)PCFS_PLL_PHI0_A/62 (write)PLL_C/49 (read)PLL_C/49 (write)PLL_B/48 (write)PLL_B/48 (write)PLL_B/48 (read)PLL_B/48 (write)PLL_A/47 (read)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (read)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_D/65 (write)PCFS_PLL_PHI0_E/66 (read)CMU_HSE_CLK_A/73 (write)CMU_HSE_CLK_A/73 (write)CMU_HSE_CLK_B/74 (read)CMU_HSE_CLK_B/74 (read)
  Availability: available
  Varpool flags:
clkState/27 (clkState) @06eb41b0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_A.part.0/230 (write)NOT_UNDER_MCU_CONTROL_A.part.0/230 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)UpdateClockState/36 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)GetClockState/37 (read)GetClockState/37 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags:
freqPointers/26 (freqPointers) @06eb4120
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: NOT_UNDER_MCU_CONTROL_B/45 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)get_FLEXCANA_CLK_Frequency/186 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)get_EMAC_TX_CLK_Frequency/184 (read)get_EMAC_TS_CLK_Frequency/182 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)GetProducerClockFreq/40 (read)UpdateFrequencies/41 (write)get_TRACE_CLK_Frequency/202 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_SWT0_CLK_Frequency/177 (read)get_QSPI0_RAM_CLK_Frequency/174 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)UpdateFrequencies/41 (write)NOT_UNDER_MCU_CONTROL_A/44 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)get_ADC0_CLK_Frequency/80 (read)get_DCM0_CLK_Frequency/173 (read)UpdateFrequencies/41 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)IntegerDividers_K/60 (read)IntegerDividers_F/55 (read)IntegerDividers_F/55 (read)IntegerDividers_J/59 (read)get_STMA_CLK_Frequency/198 (read)get_SIUL0_CLK_Frequency/176 (read)get_CRC0_CLK_Frequency/165 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)IntegerDividers_E/54 (read)CONFIG_ELEMENTS_MAPPINGS_01/42 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)IntegerDividers_D/53 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (read)UpdateFrequencies/41 (write)get_FLEXCANB_CLK_Frequency/190 (read)get_CMP0_CLK_Frequency/127 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)get_STMB_CLK_Frequency/200 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)PLL_A/47 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)
  Availability: available
  Varpool flags:
bufferFreqs/25 (bufferFreqs) @06eb4090
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)CMU_CORE_CLK_A/69 (read)CMU_FXOSC_CLK_A/67 (read)PCFS_PLL_PHI0_A/62 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)IntegerDividers_K/60 (write)IntegerDividers_K/60 (write)IntegerDividers_J/59 (write)IntegerDividers_J/59 (write)IntegerDividers_J/59 (read)IntegerDividers_J/59 (write)IntegerDividers_J/59 (write)IntegerDividers_J/59 (read)IntegerDividers_J/59 (write)IntegerDividers_J/59 (write)IntegerDividers_I/58 (read)IntegerDividers_I/58 (write)IntegerDividers_I/58 (write)IntegerDividers_I/58 (read)IntegerDividers_I/58 (write)IntegerDividers_I/58 (write)IntegerDividers_I/58 (read)IntegerDividers_I/58 (write)IntegerDividers_I/58 (write)IntegerDividers_H/57 (read)IntegerDividers_H/57 (write)IntegerDividers_H/57 (write)IntegerDividers_H/57 (read)IntegerDividers_H/57 (write)IntegerDividers_H/57 (write)IntegerDividers_H/57 (read)IntegerDividers_H/57 (write)IntegerDividers_H/57 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (write)IntegerDividers_G/56 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (write)IntegerDividers_G/56 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (write)IntegerDividers_G/56 (write)IntegerDividers_F/55 (write)IntegerDividers_F/55 (write)IntegerDividers_F/55 (read)IntegerDividers_F/55 (write)IntegerDividers_F/55 (write)IntegerDividers_F/55 (read)IntegerDividers_F/55 (write)IntegerDividers_F/55 (read)IntegerDividers_F/55 (write)IntegerDividers_E/54 (read)IntegerDividers_E/54 (write)IntegerDividers_E/54 (write)IntegerDividers_E/54 (read)IntegerDividers_E/54 (write)IntegerDividers_E/54 (write)IntegerDividers_E/54 (read)IntegerDividers_E/54 (write)IntegerDividers_E/54 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IntegerDividers_D/53 (read)IntegerDividers_D/53 (write)IntegerDividers_D/53 (write)IntegerDividers_D/53 (read)IntegerDividers_D/53 (write)IntegerDividers_D/53 (write)IntegerDividers_D/53 (read)IntegerDividers_D/53 (write)IntegerDividers_D/53 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (write)IntegerDividers_C/52 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (write)IntegerDividers_C/52 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (write)IntegerDividers_C/52 (write)IntegerDividers_B/51 (read)IntegerDividers_B/51 (write)IntegerDividers_B/51 (write)IntegerDividers_B/51 (read)IntegerDividers_B/51 (write)IntegerDividers_B/51 (write)IntegerDividers_B/51 (read)IntegerDividers_B/51 (write)IntegerDividers_B/51 (write)IntegerDividers_A/50 (read)IntegerDividers_A/50 (write)IntegerDividers_A/50 (write)IntegerDividers_A/50 (read)IntegerDividers_A/50 (write)IntegerDividers_A/50 (write)IntegerDividers_A/50 (read)IntegerDividers_A/50 (write)IntegerDividers_A/50 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)PLL_C/49 (write)IntegerDividers_J/59 (read)IntegerDividers_K/60 (write)IntegerDividers_K/60 (write)IntegerDividers_K/60 (read)IntegerDividers_K/60 (write)IntegerDividers_K/60 (write)IntegerDividers_K/60 (read)PCFS_PLL_PHI0_A/62 (read)PLL_A/47 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)get_TRACE_CLK_Frequency/202 (read)get_CRC0_CLK_Frequency/165 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_CMP0_CLK_Frequency/127 (read)get_FLEXCANB_CLK_Frequency/190 (read)IntegerDividers_K/60 (read)get_SWT0_CLK_Frequency/177 (read)GetProducerClockFreq/40 (read)get_ADC0_CLK_Frequency/80 (read)CMU_HSE_CLK_A/73 (read)CMU_AIPS_PLAT_CLK_A/71 (read)get_EMAC_TS_CLK_Frequency/182 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_STMB_CLK_Frequency/200 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)get_SIUL0_CLK_Frequency/176 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)get_DCM0_CLK_Frequency/173 (read)get_STMA_CLK_Frequency/198 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)IntegerDividers_F/55 (read)get_QSPI0_RAM_CLK_Frequency/174 (read)CMU_FXOSC_CLK_A/67 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)
  Availability: available
  Varpool flags:
HwPllName/24 (HwPllName) @06eb4000
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntryIndex/23 (selectorEntryIndex) @06e79f30
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: NOT_UNDER_MCU_CONTROL_B/45 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
hardwareValue_selectorEntry/22 (hardwareValue_selectorEntry) @06e79ca8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: get_STMB_CLK_Frequency/200 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_STMA_CLK_Frequency/198 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_TRACE_CLK_Frequency/202 (read)get_FLEXCANB_CLK_Frequency/190 (read)get_EMAC_TS_CLK_Frequency/182 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
clockName_sourceType/21 (clockName_sourceType) @06e79f78
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
mcmeTriggerPartitions/20 (mcmeTriggerPartitions) @06e79ee8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
mcmeGetPartitions/19 (mcmeGetPartitions) @06e79ea0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
mcmeSetPartitions/18 (mcmeSetPartitions) @06e79e58
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cmu/17 (cmu) @06e79e10
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
pll/16 (pll) @06e79dc8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
xosc/15 (xosc) @06e79d80
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cgmPcfs/14 (cgmPcfs) @06e79d38
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cgm/13 (cgm) @06e79cf0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
enableDisableMask/12 (enableDisableMask) @06e79c60
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: get_STMB_CLK_Frequency/200 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_STMA_CLK_Frequency/198 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_TRACE_CLK_Frequency/202 (read)get_FLEXCANB_CLK_Frequency/190 (read)get_EMAC_TS_CLK_Frequency/182 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntry_hardwareValue/11 (selectorEntry_hardwareValue) @06e79bd0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
clockFeatures/10 (clockFeatures) @06e79b40
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cmuCallbackIndex/9 (cmuCallbackIndex) @06e733a8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
pcfsCallbackIndex/8 (pcfsCallbackIndex) @06e73318
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorCallbackIndex/7 (selectorCallbackIndex) @06e73288
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
pllCallbackIndex/6 (pllCallbackIndex) @06e731f8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
fractional_dividerCallbackIndex/5 (fractional_dividerCallbackIndex) @06e73168
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
gateCallbackIndex/4 (gateCallbackIndex) @06e730d8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
ircoscCallbackIndex/3 (ircoscCallbackIndex) @06e73048
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
xoscCallbackIndex/2 (xoscCallbackIndex) @06e5bf78
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
dividertriggerCallbackIndex/1 (dividertriggerCallbackIndex) @06e5bee8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
dividerCallbackIndex/0 (dividerCallbackIndex) @06e5bf30
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0 ()
{
  uint32 i;
  const struct Clock_Ip_SelectorConfigType * selectorSCS_CLK;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;

  <bb 4> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
<L0>:
  # DEBUG BEGIN_STMT
  _1 = bufferFreqs[8];
  configuredCoreClock = _1;
  # DEBUG BEGIN_STMT
  _2 = bufferFreqs[9];
  configuredAipsPlatClock = _2;
  # DEBUG BEGIN_STMT
  _3 = bufferFreqs[10];
  configuredAipsSlowClock = _3;
  # DEBUG BEGIN_STMT
  _4 = bufferFreqs[11];
  configuredHseClock = _4;
  # DEBUG BEGIN_STMT

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  return;

}


NOT_UNDER_MCU_CONTROL_A.part.0 ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  <unnamed type> iftmp.61_5;

  <bb 8> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(struct MC_ME_Type *)1076740096B].PRTN1_COFB1_STAT;
  _2 = _1 & 16777216;
  if (_2 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _3 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLSR;
  _4 = _3 & 4;
  if (_4 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 4> [local count: 268435456]:

  <bb 5> [local count: 536870913]:
  # iftmp.61_5 = PHI <0(3), 255(4)>
  clkState[6] = iftmp.61_5;
  goto <bb 7>; [100.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  clkState[6] = 0;

  <bb 7> [local count: 1073741824]:
  return;

}


CONFIG_ELEMENTS_MAPPINGS_01.part.0 ()
{
  uint8 i;
  int _2;
  const struct Clock_Ip_ClockConfigType * config_clock.85_3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  unsigned char _7;
  int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.85_10;
  <unnamed type> _11;
  int _12;
  unsigned char _13;
  unsigned char _14;
  int _16;
  <unnamed type> _17;
  int _18;
  unsigned char _19;
  unsigned char _20;
  int _22;
  <unnamed type> _23;
  int _24;
  unsigned char _25;
  unsigned char _26;

  <bb 14> [local count: 118111598]:
  goto <bb 3>; [100.00%]

  <bb 2> [local count: 955630209]:
  # DEBUG BEGIN_STMT
  _2 = (int) i_1;
  _4 = config_clock.85_3->ircoscs[_2].name;
  _5 = (int) _4;
  _6 = i_1 + 1;
  freqPointers[_5] = _6;
  # DEBUG BEGIN_STMT
  # DEBUG i => _6

  <bb 3> [local count: 1073741809]:
  # i_1 = PHI <_6(2), 0(14)>
  # DEBUG i => i_1
  # DEBUG BEGIN_STMT
  config_clock.85_3 = config_clock;
  _7 = config_clock.85_3->ircoscsCount;
  if (i_1 < _7)
    goto <bb 2>; [89.00%]
  else
    goto <bb 4>; [11.00%]

  <bb 4> [local count: 118111599]:
  # config_clock.85_10 = PHI <config_clock.85_3(3)>
  goto <bb 6>; [100.00%]

  <bb 5> [local count: 955630212]:
  # DEBUG BEGIN_STMT
  _9 = (int) i_8;
  _11 = config_clock.85_10->xoscs[_9].name;
  _12 = (int) _11;
  _13 = i_8 + 1;
  freqPointers[_12] = _13;
  # DEBUG BEGIN_STMT
  # DEBUG i => _13

  <bb 6> [local count: 1073741812]:
  # i_8 = PHI <0(4), _13(5)>
  # DEBUG i => i_8
  # DEBUG BEGIN_STMT
  _14 = config_clock.85_10->xoscsCount;
  if (i_8 < _14)
    goto <bb 5>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 7> [local count: 118111599]:
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 955630219]:
  # DEBUG BEGIN_STMT
  _16 = (int) i_15;
  _17 = config_clock.85_10->plls[_16].name;
  _18 = (int) _17;
  _19 = i_15 + 1;
  freqPointers[_18] = _19;
  # DEBUG BEGIN_STMT
  # DEBUG i => _19

  <bb 9> [local count: 1073741819]:
  # i_15 = PHI <0(7), _19(8)>
  # DEBUG i => i_15
  # DEBUG BEGIN_STMT
  _20 = config_clock.85_10->pllsCount;
  if (i_15 < _20)
    goto <bb 8>; [89.00%]
  else
    goto <bb 10>; [11.00%]

  <bb 10> [local count: 118111600]:
  goto <bb 12>; [100.00%]

  <bb 11> [local count: 955630225]:
  # DEBUG BEGIN_STMT
  _22 = (int) i_21;
  _23 = config_clock.85_10->extClks[_22].name;
  _24 = (int) _23;
  _25 = i_21 + 1;
  freqPointers[_24] = _25;
  # DEBUG BEGIN_STMT
  # DEBUG i => _25

  <bb 12> [local count: 1073741824]:
  # i_21 = PHI <0(10), _25(11)>
  # DEBUG i => i_21
  # DEBUG BEGIN_STMT
  _26 = config_clock.85_10->extClksCount;
  if (i_21 < _26)
    goto <bb 11>; [89.00%]
  else
    goto <bb 13>; [11.00%]

  <bb 13> [local count: 118111601]:
  return;

}


get_TRACE_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725184B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725184B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725184B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_STM1_CLK_Frequency ()
{
  uint32 retval.364;

  <bb 2> [local count: 1073741824]:
  retval.364_3 = get_STMB_CLK_Frequency (); [tail call]
  return retval.364_3;

}


get_STMB_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_STM0_CLK_Frequency ()
{
  uint32 retval.363;

  <bb 2> [local count: 1073741824]:
  retval.363_3 = get_STMA_CLK_Frequency (); [tail call]
  return retval.363_3;

}


get_STMA_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_RTC0_CLK_Frequency ()
{
  uint32 retval.362;

  <bb 2> [local count: 1073741824]:
  retval.362_1 = get_RTC_CLK_Frequency (); [tail call]
  return retval.362_1;

}


get_RTC_CLK_Frequency ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return 0;

}


get_QSPI0_SFCK_CLK_Frequency ()
{
  uint32 retval.361;

  <bb 2> [local count: 1073741824]:
  retval.361_3 = get_QSPI_SFCK_CLK_Frequency (); [tail call]
  return retval.361_3;

}


get_QSPI_SFCK_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCAN5_CLK_Frequency ()
{
  uint32 retval.360;

  <bb 2> [local count: 1073741824]:
  retval.360_3 = get_FLEXCANB_CLK_Frequency (); [tail call]
  return retval.360_3;

}


get_FLEXCAN4_CLK_Frequency ()
{
  uint32 retval.359;

  <bb 2> [local count: 1073741824]:
  retval.359_3 = get_FLEXCANB_CLK_Frequency (); [tail call]
  return retval.359_3;

}


get_FLEXCAN3_CLK_Frequency ()
{
  uint32 retval.358;

  <bb 2> [local count: 1073741824]:
  retval.358_3 = get_FLEXCANB_CLK_Frequency (); [tail call]
  return retval.358_3;

}


get_FLEXCANB_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_FLEXCAN2_CLK_Frequency ()
{
  uint32 retval.357;

  <bb 2> [local count: 1073741824]:
  retval.357_3 = get_FLEXCANA_CLK_Frequency (); [tail call]
  return retval.357_3;

}


get_FLEXCAN1_CLK_Frequency ()
{
  uint32 retval.356;

  <bb 2> [local count: 1073741824]:
  retval.356_3 = get_FLEXCANA_CLK_Frequency (); [tail call]
  return retval.356_3;

}


get_FLEXCAN0_CLK_Frequency ()
{
  uint32 retval.355;

  <bb 2> [local count: 1073741824]:
  retval.355_3 = get_FLEXCANA_CLK_Frequency (); [tail call]
  return retval.355_3;

}


get_FLEXCANA_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_EMAC0_TX_CLK_Frequency ()
{
  uint32 retval.354;

  <bb 2> [local count: 1073741824]:
  retval.354_3 = get_EMAC_TX_CLK_Frequency (); [tail call]
  return retval.354_3;

}


get_EMAC_TX_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_EMAC0_TS_CLK_Frequency ()
{
  uint32 retval.353;

  <bb 2> [local count: 1073741824]:
  retval.353_3 = get_EMAC_TS_CLK_Frequency (); [tail call]
  return retval.353_3;

}


get_EMAC_TS_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_EMAC0_RX_CLK_Frequency ()
{
  uint32 retval.352;

  <bb 2> [local count: 1073741824]:
  retval.352_3 = get_EMAC_RX_CLK_Frequency (); [tail call]
  return retval.352_3;

}


get_EMAC_RX_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_CLKOUT_STANDBY_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724800B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724800B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724800B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}


get_SWT1_CLK_Frequency ()
{
  uint32 retval.351;

  <bb 2> [local count: 1073741824]:
  retval.351_2 = get_SWT0_CLK_Frequency (); [tail call]
  return retval.351_2;

}


get_SWT0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[2];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_SIUL0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[0];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_QSPI0_TX_MEM_CLK_Frequency ()
{
  uint32 retval.350;

  <bb 2> [local count: 1073741824]:
  retval.350_2 = get_QSPI0_RAM_CLK_Frequency (); [tail call]
  return retval.350_2;

}


get_QSPI0_RAM_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[19];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_DCM0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[17];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_SEMA42_CLK_Frequency ()
{
  uint32 retval.349;

  <bb 2> [local count: 1073741824]:
  retval.349_2 = get_CRC0_CLK_Frequency (); [tail call]
  return retval.349_2;

}


get_MSCM_CLK_Frequency ()
{
  uint32 retval.348;

  <bb 2> [local count: 1073741824]:
  retval.348_2 = get_CRC0_CLK_Frequency (); [tail call]
  return retval.348_2;

}


get_LPUART8_CLK_Frequency ()
{
  uint32 retval.347;

  <bb 2> [local count: 1073741824]:
  retval.347_2 = get_CRC0_CLK_Frequency (); [tail call]
  return retval.347_2;

}


get_LPUART0_CLK_Frequency ()
{
  uint32 retval.346;

  <bb 2> [local count: 1073741824]:
  retval.346_2 = get_CRC0_CLK_Frequency (); [tail call]
  return retval.346_2;

}


get_LPSPI0_CLK_Frequency ()
{
  uint32 retval.345;

  <bb 2> [local count: 1073741824]:
  retval.345_2 = get_CRC0_CLK_Frequency (); [tail call]
  return retval.345_2;

}


get_INTM_CLK_Frequency ()
{
  uint32 retval.344;

  <bb 2> [local count: 1073741824]:
  retval.344_2 = get_CRC0_CLK_Frequency (); [tail call]
  return retval.344_2;

}


get_FLEXIO0_CLK_Frequency ()
{
  uint32 retval.343;

  <bb 2> [local count: 1073741824]:
  retval.343_2 = get_CRC0_CLK_Frequency (); [tail call]
  return retval.343_2;

}


get_CRC0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_WKPU0_CLK_Frequency ()
{
  uint32 retval.342;

  <bb 2> [local count: 1073741824]:
  retval.342_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.342_2;

}


get_TSENSE0_CLK_Frequency ()
{
  uint32 retval.341;

  <bb 2> [local count: 1073741824]:
  retval.341_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.341_2;

}


get_TRGMUX0_CLK_Frequency ()
{
  uint32 retval.340;

  <bb 2> [local count: 1073741824]:
  retval.340_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.340_2;

}


get_STCU0_CLK_Frequency ()
{
  uint32 retval.339;

  <bb 2> [local count: 1073741824]:
  retval.339_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.339_2;

}


get_SAI1_CLK_Frequency ()
{
  uint32 retval.338;

  <bb 2> [local count: 1073741824]:
  retval.338_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.338_2;

}


get_SAI0_CLK_Frequency ()
{
  uint32 retval.337;

  <bb 2> [local count: 1073741824]:
  retval.337_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.337_2;

}


get_PIT2_CLK_Frequency ()
{
  uint32 retval.336;

  <bb 2> [local count: 1073741824]:
  retval.336_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.336_2;

}


get_PIT1_CLK_Frequency ()
{
  uint32 retval.335;

  <bb 2> [local count: 1073741824]:
  retval.335_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.335_2;

}


get_PIT0_CLK_Frequency ()
{
  uint32 retval.334;

  <bb 2> [local count: 1073741824]:
  retval.334_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.334_2;

}


get_MUB_CLK_Frequency ()
{
  uint32 retval.333;

  <bb 2> [local count: 1073741824]:
  retval.333_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.333_2;

}


get_MUA_CLK_Frequency ()
{
  uint32 retval.332;

  <bb 2> [local count: 1073741824]:
  retval.332_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.332_2;

}


get_LPUART9_CLK_Frequency ()
{
  uint32 retval.331;

  <bb 2> [local count: 1073741824]:
  retval.331_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.331_2;

}


get_LPUART7_CLK_Frequency ()
{
  uint32 retval.330;

  <bb 2> [local count: 1073741824]:
  retval.330_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.330_2;

}


get_LPUART6_CLK_Frequency ()
{
  uint32 retval.329;

  <bb 2> [local count: 1073741824]:
  retval.329_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.329_2;

}


get_LPUART5_CLK_Frequency ()
{
  uint32 retval.328;

  <bb 2> [local count: 1073741824]:
  retval.328_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.328_2;

}


get_LPUART4_CLK_Frequency ()
{
  uint32 retval.327;

  <bb 2> [local count: 1073741824]:
  retval.327_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.327_2;

}


get_LPUART3_CLK_Frequency ()
{
  uint32 retval.326;

  <bb 2> [local count: 1073741824]:
  retval.326_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.326_2;

}


get_LPUART2_CLK_Frequency ()
{
  uint32 retval.325;

  <bb 2> [local count: 1073741824]:
  retval.325_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.325_2;

}


get_LPUART1_CLK_Frequency ()
{
  uint32 retval.324;

  <bb 2> [local count: 1073741824]:
  retval.324_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.324_2;

}


get_LPUART15_CLK_Frequency ()
{
  uint32 retval.323;

  <bb 2> [local count: 1073741824]:
  retval.323_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.323_2;

}


get_LPUART14_CLK_Frequency ()
{
  uint32 retval.322;

  <bb 2> [local count: 1073741824]:
  retval.322_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.322_2;

}


get_LPUART13_CLK_Frequency ()
{
  uint32 retval.321;

  <bb 2> [local count: 1073741824]:
  retval.321_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.321_2;

}


get_LPUART12_CLK_Frequency ()
{
  uint32 retval.320;

  <bb 2> [local count: 1073741824]:
  retval.320_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.320_2;

}


get_LPUART11_CLK_Frequency ()
{
  uint32 retval.319;

  <bb 2> [local count: 1073741824]:
  retval.319_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.319_2;

}


get_LPUART10_CLK_Frequency ()
{
  uint32 retval.318;

  <bb 2> [local count: 1073741824]:
  retval.318_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.318_2;

}


get_LPSPI5_CLK_Frequency ()
{
  uint32 retval.317;

  <bb 2> [local count: 1073741824]:
  retval.317_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.317_2;

}


get_LPSPI4_CLK_Frequency ()
{
  uint32 retval.316;

  <bb 2> [local count: 1073741824]:
  retval.316_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.316_2;

}


get_LPSPI3_CLK_Frequency ()
{
  uint32 retval.315;

  <bb 2> [local count: 1073741824]:
  retval.315_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.315_2;

}


get_LPSPI2_CLK_Frequency ()
{
  uint32 retval.314;

  <bb 2> [local count: 1073741824]:
  retval.314_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.314_2;

}


get_LPSPI1_CLK_Frequency ()
{
  uint32 retval.313;

  <bb 2> [local count: 1073741824]:
  retval.313_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.313_2;

}


get_LPI2C1_CLK_Frequency ()
{
  uint32 retval.312;

  <bb 2> [local count: 1073741824]:
  retval.312_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.312_2;

}


get_LPI2C0_CLK_Frequency ()
{
  uint32 retval.311;

  <bb 2> [local count: 1073741824]:
  retval.311_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.311_2;

}


get_FLASH0_CLK_Frequency ()
{
  uint32 retval.310;

  <bb 2> [local count: 1073741824]:
  retval.310_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.310_2;

}


get_ERM0_CLK_Frequency ()
{
  uint32 retval.309;

  <bb 2> [local count: 1073741824]:
  retval.309_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.309_2;

}


get_EIM0_CLK_Frequency ()
{
  uint32 retval.308;

  <bb 2> [local count: 1073741824]:
  retval.308_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.308_2;

}


get_CMP2_CLK_Frequency ()
{
  uint32 retval.307;

  <bb 2> [local count: 1073741824]:
  retval.307_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.307_2;

}


get_CMP1_CLK_Frequency ()
{
  uint32 retval.306;

  <bb 2> [local count: 1073741824]:
  retval.306_2 = get_CMP0_CLK_Frequency (); [tail call]
  return retval.306_2;

}


get_CMP0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


get_TEMPSENSE_CLK_Frequency ()
{
  uint32 retval.305;

  <bb 2> [local count: 1073741824]:
  retval.305_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.305_2;

}


get_TCM_CM7_1_CLK_Frequency ()
{
  uint32 retval.304;

  <bb 2> [local count: 1073741824]:
  retval.304_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.304_2;

}


get_TCM_CM7_0_CLK_Frequency ()
{
  uint32 retval.303;

  <bb 2> [local count: 1073741824]:
  retval.303_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.303_2;

}


get_LCU1_CLK_Frequency ()
{
  uint32 retval.302;

  <bb 2> [local count: 1073741824]:
  retval.302_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.302_2;

}


get_LCU0_CLK_Frequency ()
{
  uint32 retval.301;

  <bb 2> [local count: 1073741824]:
  retval.301_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.301_2;

}


get_EMIOS2_CLK_Frequency ()
{
  uint32 retval.300;

  <bb 2> [local count: 1073741824]:
  retval.300_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.300_2;

}


get_EMIOS1_CLK_Frequency ()
{
  uint32 retval.299;

  <bb 2> [local count: 1073741824]:
  retval.299_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.299_2;

}


get_EMIOS0_CLK_Frequency ()
{
  uint32 retval.298;

  <bb 2> [local count: 1073741824]:
  retval.298_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.298_2;

}


get_EDMA0_TCD9_CLK_Frequency ()
{
  uint32 retval.297;

  <bb 2> [local count: 1073741824]:
  retval.297_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.297_2;

}


get_EDMA0_TCD8_CLK_Frequency ()
{
  uint32 retval.296;

  <bb 2> [local count: 1073741824]:
  retval.296_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.296_2;

}


get_EDMA0_TCD7_CLK_Frequency ()
{
  uint32 retval.295;

  <bb 2> [local count: 1073741824]:
  retval.295_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.295_2;

}


get_EDMA0_TCD6_CLK_Frequency ()
{
  uint32 retval.294;

  <bb 2> [local count: 1073741824]:
  retval.294_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.294_2;

}


get_EDMA0_TCD5_CLK_Frequency ()
{
  uint32 retval.293;

  <bb 2> [local count: 1073741824]:
  retval.293_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.293_2;

}


get_EDMA0_TCD4_CLK_Frequency ()
{
  uint32 retval.292;

  <bb 2> [local count: 1073741824]:
  retval.292_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.292_2;

}


get_EDMA0_TCD3_CLK_Frequency ()
{
  uint32 retval.291;

  <bb 2> [local count: 1073741824]:
  retval.291_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.291_2;

}


get_EDMA0_TCD31_CLK_Frequency ()
{
  uint32 retval.290;

  <bb 2> [local count: 1073741824]:
  retval.290_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.290_2;

}


get_EDMA0_TCD30_CLK_Frequency ()
{
  uint32 retval.289;

  <bb 2> [local count: 1073741824]:
  retval.289_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.289_2;

}


get_EDMA0_TCD2_CLK_Frequency ()
{
  uint32 retval.288;

  <bb 2> [local count: 1073741824]:
  retval.288_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.288_2;

}


get_EDMA0_TCD29_CLK_Frequency ()
{
  uint32 retval.287;

  <bb 2> [local count: 1073741824]:
  retval.287_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.287_2;

}


get_EDMA0_TCD28_CLK_Frequency ()
{
  uint32 retval.286;

  <bb 2> [local count: 1073741824]:
  retval.286_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.286_2;

}


get_EDMA0_TCD27_CLK_Frequency ()
{
  uint32 retval.285;

  <bb 2> [local count: 1073741824]:
  retval.285_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.285_2;

}


get_EDMA0_TCD26_CLK_Frequency ()
{
  uint32 retval.284;

  <bb 2> [local count: 1073741824]:
  retval.284_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.284_2;

}


get_EDMA0_TCD25_CLK_Frequency ()
{
  uint32 retval.283;

  <bb 2> [local count: 1073741824]:
  retval.283_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.283_2;

}


get_EDMA0_TCD24_CLK_Frequency ()
{
  uint32 retval.282;

  <bb 2> [local count: 1073741824]:
  retval.282_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.282_2;

}


get_EDMA0_TCD23_CLK_Frequency ()
{
  uint32 retval.281;

  <bb 2> [local count: 1073741824]:
  retval.281_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.281_2;

}


get_EDMA0_TCD22_CLK_Frequency ()
{
  uint32 retval.280;

  <bb 2> [local count: 1073741824]:
  retval.280_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.280_2;

}


get_EDMA0_TCD21_CLK_Frequency ()
{
  uint32 retval.279;

  <bb 2> [local count: 1073741824]:
  retval.279_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.279_2;

}


get_EDMA0_TCD20_CLK_Frequency ()
{
  uint32 retval.278;

  <bb 2> [local count: 1073741824]:
  retval.278_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.278_2;

}


get_EDMA0_TCD1_CLK_Frequency ()
{
  uint32 retval.277;

  <bb 2> [local count: 1073741824]:
  retval.277_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.277_2;

}


get_EDMA0_TCD19_CLK_Frequency ()
{
  uint32 retval.276;

  <bb 2> [local count: 1073741824]:
  retval.276_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.276_2;

}


get_EDMA0_TCD18_CLK_Frequency ()
{
  uint32 retval.275;

  <bb 2> [local count: 1073741824]:
  retval.275_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.275_2;

}


get_EDMA0_TCD17_CLK_Frequency ()
{
  uint32 retval.274;

  <bb 2> [local count: 1073741824]:
  retval.274_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.274_2;

}


get_EDMA0_TCD16_CLK_Frequency ()
{
  uint32 retval.273;

  <bb 2> [local count: 1073741824]:
  retval.273_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.273_2;

}


get_EDMA0_TCD15_CLK_Frequency ()
{
  uint32 retval.272;

  <bb 2> [local count: 1073741824]:
  retval.272_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.272_2;

}


get_EDMA0_TCD14_CLK_Frequency ()
{
  uint32 retval.271;

  <bb 2> [local count: 1073741824]:
  retval.271_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.271_2;

}


get_EDMA0_TCD13_CLK_Frequency ()
{
  uint32 retval.270;

  <bb 2> [local count: 1073741824]:
  retval.270_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.270_2;

}


get_EDMA0_TCD12_CLK_Frequency ()
{
  uint32 retval.269;

  <bb 2> [local count: 1073741824]:
  retval.269_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.269_2;

}


get_EDMA0_TCD11_CLK_Frequency ()
{
  uint32 retval.268;

  <bb 2> [local count: 1073741824]:
  retval.268_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.268_2;

}


get_EDMA0_TCD10_CLK_Frequency ()
{
  uint32 retval.267;

  <bb 2> [local count: 1073741824]:
  retval.267_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.267_2;

}


get_EDMA0_TCD0_CLK_Frequency ()
{
  uint32 retval.266;

  <bb 2> [local count: 1073741824]:
  retval.266_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.266_2;

}


get_EDMA0_CLK_Frequency ()
{
  uint32 retval.265;

  <bb 2> [local count: 1073741824]:
  retval.265_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.265_2;

}


get_DMAMUX1_CLK_Frequency ()
{
  uint32 retval.264;

  <bb 2> [local count: 1073741824]:
  retval.264_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.264_2;

}


get_DMAMUX0_CLK_Frequency ()
{
  uint32 retval.263;

  <bb 2> [local count: 1073741824]:
  retval.263_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.263_2;

}


get_BCTU0_CLK_Frequency ()
{
  uint32 retval.262;

  <bb 2> [local count: 1073741824]:
  retval.262_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.262_2;

}


get_ADC2_CLK_Frequency ()
{
  uint32 retval.261;

  <bb 2> [local count: 1073741824]:
  retval.261_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.261_2;

}


get_ADC1_CLK_Frequency ()
{
  uint32 retval.260;

  <bb 2> [local count: 1073741824]:
  retval.260_2 = get_ADC0_CLK_Frequency (); [tail call]
  return retval.260_2;

}


get_ADC0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}


CallbackDelay ()
{
  uint32 TimeoutTicks;
  uint32 ElapsedTime;
  uint32 StartTime;
  boolean TimeoutOccurred;
  long unsigned int TimeoutTicks.0_1;

  <bb 2> [local count: 118111600]:
  # DEBUG BEGIN_STMT
  # DEBUG TimeoutOccurred => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  ClockStartTimeout (&StartTime, &ElapsedTime, &TimeoutTicks, 10);

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  TimeoutTicks.0_1 = TimeoutTicks;
  TimeoutOccurred_6 = ClockTimeoutExpired (&StartTime, &ElapsedTime, TimeoutTicks.0_1);
  # DEBUG TimeoutOccurred => TimeoutOccurred_6
  # DEBUG BEGIN_STMT
  if (TimeoutOccurred_6 != 0)
    goto <bb 4>; [11.00%]
  else
    goto <bb 5>; [89.00%]

  <bb 5> [local count: 955630223]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 118111601]:
  StartTime ={v} {CLOBBER};
  ElapsedTime ={v} {CLOBBER};
  TimeoutTicks ={v} {CLOBBER};
  return;

}


CallEmptyCallbacks ()
{
  void (*<T494>) (const struct Clock_Ip_CmuConfigType *) _1;
  void (*<T498>) (Clock_Ip_NameType) _2;
  void (*<T498>) (Clock_Ip_NameType) _3;
  Clock_Ip_CmuStatusType (*<T49c>) (Clock_Ip_NameType) _4;
  void (*<T43f>) (const struct Clock_Ip_DividerConfigType *) _5;
  void (*<T44a>) (const struct Clock_Ip_DividerTriggerConfigType *) _6;
  void (*<T433>) (const struct Clock_Ip_XoscConfigType *) _7;
  void (*<T456>) (const struct Clock_Ip_FracDivConfigType *) _8;
  clock_dfs_status_t (*<T45c>) (Clock_Ip_NameType) _9;
  void (*<T484>) (const struct Clock_Ip_GateConfigType *) _10;
  void (*<T489>) (Clock_Ip_NameType, boolean) _11;
  void (*<T428>) (const struct Clock_Ip_IrcoscConfigType *) _12;
  void (*<T467>) (const struct Clock_Ip_PllConfigType *) _13;
  clock_pll_status_t (*<T46d>) (Clock_Ip_NameType) _14;
  void (*<T478>) (const struct Clock_Ip_SelectorConfigType *) _15;
  void (*<T4a7>) (const struct Clock_Ip_PcfsConfigType *) _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = cmuCallbacks[0].Set;
  _1 (0B);
  # DEBUG BEGIN_STMT
  _2 = cmuCallbacks[0].Disable;
  _2 (145);
  # DEBUG BEGIN_STMT
  _3 = cmuCallbacks[0].Clear;
  _3 (145);
  # DEBUG BEGIN_STMT
  _4 = cmuCallbacks[0].GetStatus;
  _4 (145);
  # DEBUG BEGIN_STMT
  _5 = dividerCallbacks[0].Set;
  _5 (0B);
  # DEBUG BEGIN_STMT
  _6 = dividerTriggerCallbacks[0].Configure;
  _6 (0B);
  # DEBUG BEGIN_STMT
  _7 = extOscCallbacks[0].Reset;
  _7 (0B);
  # DEBUG BEGIN_STMT
  _8 = fracDivCallbacks[0].Set;
  _8 (0B);
  # DEBUG BEGIN_STMT
  _9 = fracDivCallbacks[0].Complete;
  _9 (145);
  # DEBUG BEGIN_STMT
  _10 = gateCallbacks[0].Set;
  _10 (0B);
  # DEBUG BEGIN_STMT
  _11 = gateCallbacks[0].Update;
  _11 (145, 0);
  # DEBUG BEGIN_STMT
  _12 = intOscCallbacks[0].Set;
  _12 (0B);
  # DEBUG BEGIN_STMT
  _13 = pllCallbacks[0].Set;
  _13 (0B);
  # DEBUG BEGIN_STMT
  _14 = pllCallbacks[0].Complete;
  _14 (145);
  # DEBUG BEGIN_STMT
  _15 = selectorCallbacks[0].Set;
  _15 (0B);
  # DEBUG BEGIN_STMT
  _16 = pcfsCallbacks[0].Set;
  _16 (0B);
  return;

}


McMeEnterKey ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  MEM[(struct MC_ME_Type *)1076740096B].CTL_KEY ={v} 23280;
  # DEBUG BEGIN_STMT
  MEM[(struct MC_ME_Type *)1076740096B].CTL_KEY ={v} 42255;
  return;

}


CMU_HSE_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[3].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[3].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[3].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}


CMU_HSE_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.1_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int configuredHseClock.2_6;
  long unsigned int configuredAipsSlowClock.3_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[3].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.1_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#10 => &config_clock.1_2->cmus[_4]
  # DEBUG cmuConfig => D#10
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.1_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[1];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  configuredHseClock.2_6 = configuredHseClock;
  fMonitoredClk_25 = configuredHseClock.2_6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.3_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.3_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (configuredHseClock.2_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[3].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[3].refCount = _19;
  return;

}


CMU_AIPS_PLAT_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[2].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[2].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[2].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}


CMU_AIPS_PLAT_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.4_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int configuredAipsPlatClock.5_6;
  long unsigned int configuredAipsSlowClock.6_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[2].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.4_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#9 => &config_clock.4_2->cmus[_4]
  # DEBUG cmuConfig => D#9
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.4_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[1];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  configuredAipsPlatClock.5_6 = configuredAipsPlatClock;
  fMonitoredClk_25 = configuredAipsPlatClock.5_6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.6_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.6_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (configuredAipsPlatClock.5_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[2].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[2].refCount = _19;
  return;

}


CMU_CORE_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[1].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[1].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[1].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}


CMU_CORE_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.7_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int configuredCoreClock.8_6;
  long unsigned int configuredAipsSlowClock.9_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[1].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.7_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#8 => &config_clock.7_2->cmus[_4]
  # DEBUG cmuConfig => D#8
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.7_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[3];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  configuredCoreClock.8_6 = configuredCoreClock;
  fMonitoredClk_25 = configuredCoreClock.8_6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.9_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.9_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (configuredCoreClock.8_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[1].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[1].refCount = _19;
  return;

}


CMU_FXOSC_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[0].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[0].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[0].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}


CMU_FXOSC_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.10_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int configuredAipsSlowClock.11_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[0].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.10_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#7 => &config_clock.10_2->cmus[_4]
  # DEBUG cmuConfig => D#7
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.10_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[1];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  _6 = bufferFreqs[3];
  fMonitoredClk_25 = _6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.11_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.11_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[0].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[0].refCount = _19;
  return;

}


PCFS_PLL_PHI0_E ()
{
  uint32 K;
  uint32 RATE;
  uint32 fsafe;
  uint32 finput;
  uint32 stepDuration;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  stepDuration_14 = tmpData.input1;
  # DEBUG stepDuration => stepDuration_14
  # DEBUG BEGIN_STMT
  finput_15 = tmpData.input2;
  # DEBUG finput => finput_15
  # DEBUG BEGIN_STMT
  fsafe_16 = tmpData.input3;
  # DEBUG fsafe => fsafe_16
  # DEBUG BEGIN_STMT
  RATE_17 = tmpData.aux1;
  # DEBUG RATE => RATE_17
  # DEBUG BEGIN_STMT
  _1 = tmpData.aux4;
  _2 = _1 << 2;
  _3 = _2 + 191;
  K_18 = _3 >> 7;
  # DEBUG K => K_18
  # DEBUG BEGIN_STMT
  _4 = stepDuration_14 * fsafe_16;
  pcfsEntries[0].sdur = _4;
  # DEBUG BEGIN_STMT
  _5 = RATE_17 * K_18;
  pcfsEntries[0].divc_init = _5;
  # DEBUG BEGIN_STMT
  pcfsEntries[0].divc_rate = RATE_17;
  # DEBUG BEGIN_STMT
  _6 = K_18 + 1;
  _7 = _5 * _6;
  _8 = _7 >> 1;
  _9 = _8 + 999;
  pcfsEntries[0].div_startValue = _9;
  # DEBUG BEGIN_STMT
  _10 = finput_15 * 1000;
  _11 = _10 / fsafe_16;
  _12 = _11 + 4294967295;
  pcfsEntries[0].div_endValue = _12;
  return;

}


PCFS_PLL_PHI0_D ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 118111600]:
  # DEBUG BEGIN_STMT
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _1 = tmpData.aux2;
  _2 = tmpData.aux4;
  _3 = _2 + _10;
  if (_1 >= _3)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 477815111]:
  # DEBUG BEGIN_STMT
  _4 = _1 - _3;
  tmpData.aux2 = _4;
  # DEBUG BEGIN_STMT
  _5 = _10 << 1;
  _6 = _2 + _5;
  tmpData.aux4 = _6;

  <bb 5> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _7 = tmpData.aux4;
  _8 = _7 >> 1;
  tmpData.aux4 = _8;
  # DEBUG BEGIN_STMT
  _9 = _10 >> 2;
  tmpData.aux3 = _9;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = tmpData.aux3;
  if (_10 != 0)
    goto <bb 3>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 7> [local count: 118111601]:
  return;

}


PCFS_PLL_PHI0_C ()
{
  uint32 RATE;
  uint32 fsafe;
  uint32 finput;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;

  <bb 2> [local count: 118111600]:
  # DEBUG BEGIN_STMT
  finput_11 = tmpData.input2;
  # DEBUG finput => finput_11
  # DEBUG BEGIN_STMT
  fsafe_12 = tmpData.input3;
  # DEBUG fsafe => fsafe_12
  # DEBUG BEGIN_STMT
  RATE_13 = tmpData.aux1;
  # DEBUG RATE => RATE_13
  # DEBUG BEGIN_STMT
  _1 = finput_11 * 2048000;
  _2 = fsafe_12 * RATE_13;
  _3 = _1 / _2;
  _4 = 2048000 / RATE_13;
  _5 = _3 - _4;
  _6 = _5 + 256;
  tmpData.aux2 = _6;
  # DEBUG BEGIN_STMT
  tmpData.aux3 = 1073741824;
  # DEBUG BEGIN_STMT
  goto <bb 4>; [100.00%]

  <bb 3> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _7 = _8 >> 2;
  tmpData.aux3 = _7;

  <bb 4> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _8 = tmpData.aux3;
  if (_6 < _8)
    goto <bb 3>; [89.00%]
  else
    goto <bb 5>; [11.00%]

  <bb 5> [local count: 118111601]:
  return;

}


PCFS_PLL_PHI0_B ()
{
  uint8 i;
  uint32 RATE;
  uint32 amaxBrut;
  const uint32 pcfsRate[6];
  const uint32 aMax[6];
  unsigned int _1;
  unsigned int _2;
  long unsigned int _3;

  <bb 2> [local count: 357985524]:
  # DEBUG BEGIN_STMT
  aMax = *.LC0;
  # DEBUG BEGIN_STMT
  pcfsRate = *.LC1;
  # DEBUG BEGIN_STMT
  amaxBrut_11 = tmpData.aux1;
  # DEBUG amaxBrut => amaxBrut_11
  # DEBUG BEGIN_STMT
  # DEBUG RATE => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (amaxBrut_11 > 100)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 178992762]:
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 894749063]:
  # DEBUG BEGIN_STMT
  _1 = (unsigned int) i_7;
  _2 = _1 + 4294967295;
  _3 = aMax[_2];
  if (_3 < amaxBrut_11)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 447374531]:
  # DEBUG BEGIN_STMT
  RATE_12 = pcfsRate[_2];
  # DEBUG RATE => RATE_12

  <bb 5> [local count: 894749063]:
  # RATE_4 = PHI <RATE_5(3), RATE_12(4)>
  # DEBUG RATE => RATE_4
  # DEBUG BEGIN_STMT
  i_13 = i_7 + 1;
  # DEBUG i => i_13

  <bb 6> [local count: 1073741824]:
  # RATE_5 = PHI <RATE_4(5), 0(8)>
  # i_7 = PHI <i_13(5), 1(8)>
  # DEBUG i => i_7
  # DEBUG RATE => RATE_5
  # DEBUG BEGIN_STMT
  if (i_7 != 6)
    goto <bb 3>; [83.33%]
  else
    goto <bb 7>; [16.67%]

  <bb 7> [local count: 357985524]:
  # RATE_6 = PHI <RATE_5(6), 1000(2)>
  # DEBUG RATE => RATE_6
  # DEBUG BEGIN_STMT
  tmpData.aux1 = RATE_6;
  aMax ={v} {CLOBBER};
  pcfsRate ={v} {CLOBBER};
  return;

}


PCFS_PLL_PHI0_A ()
{
  uint32 amaxBrut;
  uint32 fsafe;
  uint32 finput;
  uint32 stepDuration;
  uint32 maxAllowableIDDchange;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.13_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = pcfsEntries[0].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.13_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#6 => &config_clock.13_2->pcfs[_4]
  # DEBUG pcfsConfig => D#6
  # DEBUG BEGIN_STMT
  maxAllowableIDDchange_15 = MEM[(const struct Clock_Ip_PcfsConfigType *)config_clock.13_2].pcfs[_4].maxAllowableIDDchange;
  # DEBUG maxAllowableIDDchange => maxAllowableIDDchange_15
  # DEBUG BEGIN_STMT
  stepDuration_16 = MEM[(const struct Clock_Ip_PcfsConfigType *)config_clock.13_2].pcfs[_4].stepDuration;
  # DEBUG stepDuration => stepDuration_16
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG maxAllowableIDDchange => 50
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmPcfs_Type *)1076723712B].PCFS_SDUR;
  stepDuration_14 = _5 & 65535;
  # DEBUG stepDuration => stepDuration_14

  <bb 5> [local count: 1073741824]:
  # maxAllowableIDDchange_11 = PHI <maxAllowableIDDchange_15(3), 50(4)>
  # stepDuration_12 = PHI <stepDuration_16(3), stepDuration_14(4)>
  # DEBUG stepDuration => stepDuration_12
  # DEBUG maxAllowableIDDchange => maxAllowableIDDchange_11
  # DEBUG BEGIN_STMT
  _6 = bufferFreqs[26];
  finput_17 = _6 / 1000000;
  # DEBUG finput => finput_17
  # DEBUG BEGIN_STMT
  _7 = bufferFreqs[1];
  fsafe_18 = _7 / 1000000;
  # DEBUG fsafe => fsafe_18
  # DEBUG BEGIN_STMT
  tmpData.input1 = stepDuration_12;
  # DEBUG BEGIN_STMT
  tmpData.input2 = finput_17;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fsafe_18;
  # DEBUG BEGIN_STMT
  _8 = maxAllowableIDDchange_11 * stepDuration_12;
  _9 = _8 * 100000;
  _10 = finput_17 * 2360;
  amaxBrut_22 = _9 / _10;
  # DEBUG amaxBrut => amaxBrut_22
  # DEBUG BEGIN_STMT
  tmpData.aux1 = amaxBrut_22;
  return;

}


CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS ()
{
  const struct Clock_Ip_SelectorConfigType * selectorSCS_CLK;
  uint32 i;
  const struct Clock_Ip_ClockConfigType * config_clock.16_1;
  <unnamed type> _2;
  const struct Clock_Ip_ClockConfigType * config_clock.16_4;
  unsigned char _5;
  long unsigned int _6;
  <unnamed type> _7;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;

  <bb 2> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG selectorSCS_CLK => 0B
  # DEBUG BEGIN_STMT
  # DEBUG i => 0
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _2 = config_clock.16_4->selectors[i_13].name;
  if (_2 == 12)
    goto <bb 4>; [5.50%]
  else
    goto <bb 5>; [94.50%]

  <bb 4> [local count: 55807731]:
  # config_clock.16_1 = PHI <config_clock.16_4(3)>
  # i_3 = PHI <i_13(3)>
  # DEBUG BEGIN_STMT
  selectorSCS_CLK_18 = &config_clock.16_1->selectors[i_3];
  # DEBUG selectorSCS_CLK => selectorSCS_CLK_18
  # DEBUG BEGIN_STMT
  goto <bb 7>; [100.00%]

  <bb 5> [local count: 958878293]:
  # DEBUG BEGIN_STMT
  i_17 = i_13 + 1;
  # DEBUG i => i_17

  <bb 6> [local count: 1073741824]:
  # i_13 = PHI <0(2), i_17(5)>
  # DEBUG i => i_13
  # DEBUG BEGIN_STMT
  config_clock.16_4 = config_clock;
  _5 = config_clock.16_4->selectorsCount;
  _6 = (long unsigned int) _5;
  if (_6 > i_13)
    goto <bb 3>; [94.50%]
  else
    goto <bb 7>; [5.50%]

  <bb 7> [local count: 114863532]:
  # selectorSCS_CLK_14 = PHI <selectorSCS_CLK_18(4), 0B(6)>
  # DEBUG selectorSCS_CLK => selectorSCS_CLK_14
  # DEBUG BEGIN_STMT
  if (selectorSCS_CLK_14 != 0B)
    goto <bb 8>; [70.00%]
  else
    goto <bb 12>; [30.00%]

  <bb 8> [local count: 80404472]:
  # DEBUG BEGIN_STMT
  _7 = selectorSCS_CLK_14->value;
  switch (_7) <default: <L8> [33.33%], case 0: <L6> [33.33%], case 8: <L7> [33.33%]>

  <bb 9> [local count: 26801491]:
<L6>:
  CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0 ();
  goto <bb 13>; [100.00%]

  <bb 10> [local count: 26798811]:
<L7>:
  # DEBUG BEGIN_STMT
  _9 = bufferFreqs[28];
  configuredCoreClock = _9;
  # DEBUG BEGIN_STMT
  _10 = bufferFreqs[29];
  configuredAipsPlatClock = _10;
  # DEBUG BEGIN_STMT
  _11 = bufferFreqs[30];
  configuredAipsSlowClock = _11;
  # DEBUG BEGIN_STMT
  _12 = bufferFreqs[31];
  configuredHseClock = _12;
  # DEBUG BEGIN_STMT
  goto <bb 13>; [100.00%]

  <bb 11> [local count: 26798811]:
<L8>:
  # DEBUG BEGIN_STMT
  configuredCoreClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsPlatClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock = 0;
  # DEBUG BEGIN_STMT
  configuredHseClock = 0;
  # DEBUG BEGIN_STMT
  goto <bb 13>; [100.00%]

  <bb 12> [local count: 34459060]:
  # DEBUG BEGIN_STMT
  configuredCoreClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsPlatClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock = 0;
  # DEBUG BEGIN_STMT
  configuredHseClock = 0;

  <bb 13> [local count: 114855491]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  return;

}


IntegerDividers_K ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.17_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.18_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.19_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.17_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.17_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[31];
  _9 = _8 / dividerValue_26;
  bufferFreqs[38] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[38] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.18_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.18_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[29];
  _17 = _16 / dividerValue_27;
  bufferFreqs[39] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[39] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.19_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.19_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[30];
  _25 = _24 / dividerValue_28;
  bufferFreqs[40] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[40] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_J ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.20_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.21_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.22_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.20_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.20_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[26];
  _9 = _8 / dividerValue_26;
  bufferFreqs[35] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[35] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.21_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.21_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[27];
  _17 = _16 / dividerValue_27;
  bufferFreqs[36] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[36] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.22_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.22_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[28];
  _25 = _24 / dividerValue_28;
  bufferFreqs[37] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[37] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_I ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.23_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.24_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.25_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[17];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.23_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.23_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[4];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[26];
  _9 = _8 / dividerValue_28;
  bufferFreqs[32] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[32] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[18];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.24_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.24_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[5];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[26];
  _18 = _17 / dividerValue_29;
  bufferFreqs[33] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[33] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[19];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.25_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.25_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[6];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[26];
  _27 = _26 / dividerValue_30;
  bufferFreqs[34] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[34] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_H ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.26_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.27_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.28_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.26_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.26_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[1];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[26];
  _9 = _8 / dividerValue_28;
  bufferFreqs[29] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[29] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[15];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.27_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.27_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[2];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[26];
  _18 = _17 / dividerValue_29;
  bufferFreqs[30] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[30] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[16];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.28_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.28_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[3];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[26];
  _27 = _26 / dividerValue_30;
  bufferFreqs[31] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[31] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_G ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.29_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.30_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.31_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[8];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.29_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.29_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[0];
  _6 = _5 >> 16;
  _7 = _6 & 15;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[25];
  _9 = _8 / dividerValue_28;
  bufferFreqs[26] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[26] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[9];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.30_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.30_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[1];
  _15 = _14 >> 16;
  _16 = _15 & 15;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[25];
  _18 = _17 / dividerValue_29;
  bufferFreqs[27] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[27] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[13];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.31_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.31_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[0];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[26];
  _27 = _26 / dividerValue_30;
  bufferFreqs[28] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[28] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_F ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.32_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.33_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  unsigned char _18;
  const struct Clock_Ip_ClockConfigType * config_clock.34_19;
  unsigned int _20;
  unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.32_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_35 = config_clock.32_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_35
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_34 = _7 + 1;
  # DEBUG dividerValue => dividerValue_34

  <bb 5> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_35(3), dividerValue_34(4)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[6];
  _9 = _8 / dividerValue_27;
  bufferFreqs[23] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[23] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.33_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_39 = config_clock.33_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_39
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_38 = _15 + 1;
  # DEBUG dividerValue => dividerValue_38

  <bb 11> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_39(9), dividerValue_38(10)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[7];
  _17 = _16 / dividerValue_28;
  bufferFreqs[24] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[24] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _18 = freqPointers[7];
  if (_18 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.34_19 = config_clock;
  _20 = (unsigned int) _18;
  _21 = _20 + 4294967295;
  dividerValue_43 = config_clock.34_19->dividers[_21].value;
  # DEBUG dividerValue => dividerValue_43
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _22 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _23 = _22 >> 25;
  dividerValue_42 = _23 & 63;
  # DEBUG dividerValue => dividerValue_42

  <bb 17> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_43(15), dividerValue_42(16)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[5];
  _25 = _24 / dividerValue_29;
  bufferFreqs[25] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[5];
  bufferFreqs[25] = _26;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_E ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.35_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.36_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.37_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.35_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.35_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[11];
  _9 = _8 / dividerValue_26;
  bufferFreqs[20] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[20] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.36_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.36_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[9];
  _17 = _16 / dividerValue_27;
  bufferFreqs[21] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[21] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.37_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.37_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[10];
  _25 = _24 / dividerValue_28;
  bufferFreqs[22] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[22] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_D ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.38_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.39_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.40_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.38_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.38_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[3];
  _9 = _8 / dividerValue_26;
  bufferFreqs[17] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[17] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.39_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.39_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[4];
  _17 = _16 / dividerValue_27;
  bufferFreqs[18] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[18] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.40_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.40_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[8];
  _25 = _24 / dividerValue_28;
  bufferFreqs[19] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[19] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_C ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.41_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.42_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  const struct Clock_Ip_ClockConfigType * config_clock.43_19;
  unsigned int _20;
  unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[19];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.41_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_35 = config_clock.41_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_35
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[6];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_34 = _7 + 1;
  # DEBUG dividerValue => dividerValue_34

  <bb 5> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_35(3), dividerValue_34(4)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[1];
  _9 = _8 / dividerValue_27;
  bufferFreqs[14] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[14] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[20];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.42_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_39 = config_clock.42_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_39
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_38 = _16 + 1;
  # DEBUG dividerValue => dividerValue_38

  <bb 11> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_39(9), dividerValue_38(10)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[1];
  _18 = _17 / dividerValue_28;
  bufferFreqs[15] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[15] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_10 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.43_19 = config_clock;
  _20 = (unsigned int) _10;
  _21 = _20 + 4294967295;
  dividerValue_43 = config_clock.43_19->dividers[_21].value;
  # DEBUG dividerValue => dividerValue_43
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _22 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _23 = _22 >> 16;
  _24 = _23 & 63;
  dividerValue_42 = _24 + 1;
  # DEBUG dividerValue => dividerValue_42

  <bb 17> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_43(15), dividerValue_42(16)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _25 = bufferFreqs[2];
  _26 = _25 / dividerValue_29;
  bufferFreqs[16] = _26;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[16] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_B ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.44_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.45_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.46_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[16];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.44_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.44_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[3];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[1];
  _9 = _8 / dividerValue_28;
  bufferFreqs[11] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[11] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[17];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.45_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.45_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[4];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[1];
  _18 = _17 / dividerValue_29;
  bufferFreqs[12] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[12] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[18];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.46_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.46_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[5];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[1];
  _27 = _26 / dividerValue_30;
  bufferFreqs[13] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[13] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


IntegerDividers_A ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.47_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.48_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.49_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.47_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.47_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[1];
  _9 = _8 / dividerValue_28;
  bufferFreqs[8] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[8] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[14];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.48_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.48_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[1];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[1];
  _18 = _17 / dividerValue_29;
  bufferFreqs[9] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[9] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[15];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.49_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.49_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[2];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[1];
  _27 = _26 / dividerValue_30;
  bufferFreqs[10] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[10] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}


PLL_C ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = tmpData.output;
  _2 = tmpData.input1;
  _3 = tmpData.input2;
  _4 = _2 / _3;
  _5 = tmpData.aux2;
  _6 = _4 * _5;
  _7 = _1 + _6;
  # DEBUG BEGIN_STMT
  _8 = tmpData.aux4;
  _9 = tmpData.input4;
  _10 = _8 * _9;
  _11 = _7 + _10;
  # DEBUG BEGIN_STMT
  _12 = tmpData.aux5;
  _13 = _9 * _12;
  _14 = tmpData.aux3;
  _15 = _13 / _14;
  _16 = _11 + _15;
  tmpData.output = _16;
  # DEBUG BEGIN_STMT
  bufferFreqs[5] = _16;
  return;

}


PLL_B ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = tmpData.input2;
  _2 = _1 << 14;
  _3 = _1 << 11;
  _4 = _2 + _3;
  tmpData.aux3 = _4;
  # DEBUG BEGIN_STMT
  _5 = tmpData.input1;
  _6 = _5 / _4;
  tmpData.aux4 = _6;
  # DEBUG BEGIN_STMT
  _7 = _4 * _6;
  _8 = _5 - _7;
  tmpData.aux5 = _8;
  # DEBUG BEGIN_STMT
  _9 = tmpData.aux1;
  _10 = _5 * _9;
  tmpData.output = _10;
  return;

}


PLL_A ()
{
  long unsigned int _1;
  unsigned char _2;
  const struct Clock_Ip_ClockConfigType * config_clock.50_3;
  unsigned int _4;
  unsigned int _5;
  unsigned char _6;
  long unsigned int _7;
  unsigned char _8;
  long unsigned int _9;
  short unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  long unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = bufferFreqs[3];
  tmpData.input1 = _1;
  # DEBUG BEGIN_STMT
  _2 = freqPointers[6];
  if (_2 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.50_3 = config_clock;
  _4 = (unsigned int) _2;
  _5 = _4 + 4294967295;
  # DEBUG D#5 => &config_clock.50_3->plls[_5]
  # DEBUG pllConfig => D#5
  # DEBUG BEGIN_STMT
  _6 = MEM[(const struct Clock_Ip_PllConfigType *)config_clock.50_3].plls[_5].predivider;
  _7 = (long unsigned int) _6;
  tmpData.input2 = _7;
  # DEBUG BEGIN_STMT
  _8 = MEM[(const struct Clock_Ip_PllConfigType *)config_clock.50_3].plls[_5].mulFactorDiv;
  _9 = (long unsigned int) _8;
  tmpData.input3 = _9;
  # DEBUG BEGIN_STMT
  _10 = MEM[(const struct Clock_Ip_PllConfigType *)config_clock.50_3].plls[_5].numeratorFracLoopDiv;
  _11 = (long unsigned int) _10;
  tmpData.input4 = _11;
  # DEBUG BEGIN_STMT
  tmpData.input5 = 0;
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _12 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _13 = _12 >> 12;
  _14 = _13 & 7;
  tmpData.input2 = _14;
  # DEBUG BEGIN_STMT
  _15 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _16 = _15 & 255;
  tmpData.input3 = _16;
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLFD;
  _18 = _17 & 32767;
  tmpData.input4 = _18;
  # DEBUG BEGIN_STMT
  _19 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _20 = _19 >> 25;
  _21 = _20 & 63;
  tmpData.input5 = _21;

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _22 = tmpData.input3;
  _23 = tmpData.input2;
  _24 = _22 / _23;
  tmpData.aux1 = _24;
  # DEBUG BEGIN_STMT
  _25 = _23 * _24;
  _26 = _22 - _25;
  tmpData.aux2 = _26;
  return;

}


IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS ()
{
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.51_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  unsigned char _6;
  const struct Clock_Ip_ClockConfigType * config_clock.52_7;
  unsigned int _8;
  unsigned int _9;
  long unsigned int _10;
  unsigned char _11;
  const struct Clock_Ip_ClockConfigType * config_clock.53_12;
  unsigned int _13;
  unsigned int _14;
  long unsigned int _15;
  unsigned char _16;
  const struct Clock_Ip_ClockConfigType * config_clock.54_17;
  unsigned int _18;
  unsigned int _19;
  long unsigned int _20;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[4];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.51_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#1 => &config_clock.51_2->xoscs[_4]
  # DEBUG xoscConfig => D#1
  # DEBUG BEGIN_STMT
  _5 = MEM[(const struct Clock_Ip_XoscConfigType *)config_clock.51_2].xoscs[_4].freq;
  bufferFreqs[3] = _5;
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[3] = 16000000;

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _6 = freqPointers[5];
  if (_6 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.52_7 = config_clock;
  _8 = (unsigned int) _6;
  _9 = _8 + 4294967295;
  # DEBUG D#2 => &config_clock.52_7->xoscs[_9]
  # DEBUG xoscConfig => D#2
  # DEBUG BEGIN_STMT
  _10 = MEM[(const struct Clock_Ip_XoscConfigType *)config_clock.52_7].xoscs[_9].freq;
  bufferFreqs[4] = _10;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[4] = 32768;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  bufferFreqs[2] = 32000;
  # DEBUG BEGIN_STMT
  bufferFreqs[1] = 48000000;
  # DEBUG BEGIN_STMT
  freqPointers[0] = 1;
  # DEBUG BEGIN_STMT
  freqPointers[2] = 2;
  # DEBUG BEGIN_STMT
  _11 = freqPointers[10];
  if (_11 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.53_12 = config_clock;
  _13 = (unsigned int) _11;
  _14 = _13 + 4294967295;
  # DEBUG D#3 => &config_clock.53_12->extClks[_14]
  # DEBUG extClkConfig => D#3
  # DEBUG BEGIN_STMT
  _15 = MEM[(const struct Clock_Ip_ExtClkConfigType *)config_clock.53_12].extClks[_14].value;
  bufferFreqs[6] = _15;
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[6] = 0;

  <bb 11> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _16 = freqPointers[11];
  if (_16 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.54_17 = config_clock;
  _18 = (unsigned int) _16;
  _19 = _18 + 4294967295;
  # DEBUG D#4 => &config_clock.54_17->extClks[_19]
  # DEBUG extClkConfig => D#4
  # DEBUG BEGIN_STMT
  _20 = MEM[(const struct Clock_Ip_ExtClkConfigType *)config_clock.54_17].extClks[_19].value;
  bufferFreqs[7] = _20;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[7] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  freqPointers[10] = 6;
  # DEBUG BEGIN_STMT
  freqPointers[11] = 7;
  return;

}


NOT_UNDER_MCU_CONTROL_B ()
{
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  signed int _5;
  unsigned char _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  signed int _10;
  unsigned char _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  <unnamed type> _15;
  unsigned char _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  <unnamed type> _20;
  clock_element_state_t iftmp.55_21;
  clock_element_state_t iftmp.56_22;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[8];
  if (_1 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _2 ={v} MEM[(struct MC_ME_Type *)1076740096B].PRTN1_COFB1_STAT;
  _3 = _2 & 16777216;
  if (_3 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _4 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[0];
  _5 = (signed int) _4;
  if (_5 >= 0)
    goto <bb 6>; [59.00%]
  else
    goto <bb 5>; [41.00%]

  <bb 5> [local count: 110058537]:

  <bb 6> [local count: 268435456]:
  # iftmp.55_21 = PHI <0(4), 255(5)>
  clkState[8] = iftmp.55_21;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  clkState[8] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _6 = freqPointers[9];
  if (_6 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _7 ={v} MEM[(struct MC_ME_Type *)1076740096B].PRTN1_COFB1_STAT;
  _8 = _7 & 16777216;
  if (_8 != 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 10> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _9 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[1];
  _10 = (signed int) _9;
  if (_10 >= 0)
    goto <bb 12>; [59.00%]
  else
    goto <bb 11>; [41.00%]

  <bb 11> [local count: 110058537]:

  <bb 12> [local count: 268435456]:
  # iftmp.56_22 = PHI <0(10), 255(11)>
  clkState[9] = iftmp.56_22;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  clkState[9] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  clkState[10] = 255;
  # DEBUG BEGIN_STMT
  clkState[11] = 255;
  # DEBUG BEGIN_STMT
  _11 = freqPointers[12];
  if (_11 == 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _12 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].CSS;
  _13 = _12 >> 24;
  _14 = _13 & 63;
  _15 = selectorEntryIndex[_14];
  clkState[12] = _15;

  <bb 16> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _16 = freqPointers[20];
  if (_16 == 0)
    goto <bb 17>; [50.00%]
  else
    goto <bb 18>; [50.00%]

  <bb 17> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].CSS;
  _18 = _17 >> 24;
  _19 = _18 & 63;
  _20 = selectorEntryIndex[_19];
  clkState[20] = _20;

  <bb 18> [local count: 1073741824]:
  return;

}


NOT_UNDER_MCU_CONTROL_A ()
{
  unsigned char _1;
  long unsigned int _3;
  long unsigned int _4;
  unsigned char _5;
  long unsigned int _6;
  signed int _7;
  unsigned char _8;
  long unsigned int _9;
  long unsigned int _10;
  unsigned char _11;
  long unsigned int _12;
  signed int _13;
  unsigned char _14;
  clock_element_state_t iftmp.57_15;
  clock_element_state_t iftmp.58_16;
  clock_element_state_t iftmp.59_17;
  clock_element_state_t iftmp.60_18;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  clkState[0] = 255;
  # DEBUG BEGIN_STMT
  _1 = freqPointers[1];
  if (_1 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _3 ={v} MEM[(struct FIRC_Type *)1076690944B].STDBY_ENABLE;
  _4 = _3 & 1;
  if (_4 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 4> [local count: 268435456]:

  <bb 5> [local count: 536870913]:
  # iftmp.57_15 = PHI <0(3), 255(4)>
  clkState[1] = iftmp.57_15;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _5 = freqPointers[4];
  if (_5 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _6 ={v} MEM[(volatile struct ExtOSC_Type *)1076707328B].STAT;
  _7 = (signed int) _6;
  if (_7 >= 0)
    goto <bb 9>; [59.00%]
  else
    goto <bb 8>; [41.00%]

  <bb 8> [local count: 220117074]:

  <bb 9> [local count: 536870913]:
  # iftmp.58_16 = PHI <0(7), 255(8)>
  clkState[4] = iftmp.58_16;

  <bb 10> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _8 = freqPointers[3];
  if (_8 == 0)
    goto <bb 11>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 11> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _9 ={v} MEM[(struct SIRC_Type *)1076658176B].MISCELLANEOUS_IN;
  _10 = _9 & 256;
  if (_10 == 0)
    goto <bb 13>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 268435456]:

  <bb 13> [local count: 536870913]:
  # iftmp.59_17 = PHI <0(11), 255(12)>
  clkState[3] = iftmp.59_17;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  clkState[2] = 255;
  # DEBUG BEGIN_STMT
  _11 = freqPointers[5];
  if (_11 == 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 18>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _12 ={v} MEM[(struct SXOSC_Type *)1076674560B].SXOSC_STAT;
  _13 = (signed int) _12;
  if (_13 >= 0)
    goto <bb 17>; [59.00%]
  else
    goto <bb 16>; [41.00%]

  <bb 16> [local count: 220117074]:

  <bb 17> [local count: 536870913]:
  # iftmp.60_18 = PHI <0(15), 255(16)>
  clkState[5] = iftmp.60_18;

  <bb 18> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _14 = freqPointers[6];
  if (_14 == 0)
    goto <bb 19>; [50.00%]
  else
    goto <bb 20>; [50.00%]

  <bb 19> [local count: 536870912]:
  NOT_UNDER_MCU_CONTROL_A.part.0 ();

  <bb 20> [local count: 1073741824]:
  return;

}


CONFIG_ELEMENTS_MAPPINGS_02 ()
{
  uint8 j;
  uint8 i;
  int _1;
  <unnamed type> _2;
  int _3;
  unsigned char _4;
  const struct Clock_Ip_ClockConfigType * config_clock.65_5;
  unsigned char _6;
  int _7;
  <unnamed type> _8;
  int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.65_11;
  unsigned char _12;
  int _13;
  <unnamed type> _14;
  int _15;
  unsigned char _16;
  unsigned char _17;
  <unnamed type> _19;
  int _20;
  <unnamed type> _21;
  unsigned char _22;
  unsigned char _23;
  int _24;
  <unnamed type> _25;
  int _26;
  <unnamed type> _27;
  unsigned char _28;
  unsigned char _29;

  <bb 2> [local count: 7299031]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG i => 0
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  _1 = (int) i_30;
  _2 = config_clock.65_5->selectors[_1].name;
  if (_2 <= 20)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 29527898]:
  # DEBUG BEGIN_STMT
  _3 = (int) _2;
  _4 = i_30 + 1;
  freqPointers[_3] = _4;

  <bb 5> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  i_60 = i_30 + 1;
  # DEBUG i => i_60

  <bb 6> [local count: 66354828]:
  # i_30 = PHI <0(2), i_60(5)>
  # DEBUG i => i_30
  # DEBUG BEGIN_STMT
  config_clock.65_5 = config_clock;
  _6 = config_clock.65_5->selectorsCount;
  if (_6 > i_30)
    goto <bb 3>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 7> [local count: 7299031]:
  # config_clock.65_11 = PHI <config_clock.65_5(6)>
  goto <bb 11>; [100.00%]

  <bb 8> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  _7 = (int) i_31;
  _8 = config_clock.65_11->dividers[_7].name;
  if (_8 <= 20)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 29527899]:
  # DEBUG BEGIN_STMT
  _9 = (int) _8;
  _10 = i_31 + 1;
  freqPointers[_9] = _10;

  <bb 10> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  i_58 = i_31 + 1;
  # DEBUG i => i_58

  <bb 11> [local count: 66354828]:
  # i_31 = PHI <i_58(10), 0(7)>
  # DEBUG i => i_31
  # DEBUG BEGIN_STMT
  _12 = config_clock.65_11->dividersCount;
  if (_12 > i_31)
    goto <bb 8>; [89.00%]
  else
    goto <bb 34>; [11.00%]

  <bb 34> [local count: 7299031]:
  goto <bb 15>; [100.00%]

  <bb 12> [local count: 59055798]:
  # DEBUG BEGIN_STMT
  _13 = (int) i_32;
  _14 = config_clock.65_11->fracDivs[_13].name;
  if (_14 <= 20)
    goto <bb 13>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 13> [local count: 29527899]:
  # DEBUG BEGIN_STMT
  _15 = (int) _14;
  _16 = i_32 + 1;
  freqPointers[_15] = _16;

  <bb 14> [local count: 59055798]:
  # DEBUG BEGIN_STMT
  i_56 = i_32 + 1;
  # DEBUG i => i_56

  <bb 15> [local count: 66354829]:
  # i_32 = PHI <i_56(14), 0(34)>
  # DEBUG i => i_32
  # DEBUG BEGIN_STMT
  _17 = config_clock.65_11->fracDivsCount;
  if (_17 > i_32)
    goto <bb 12>; [89.00%]
  else
    goto <bb 32>; [11.00%]

  <bb 32> [local count: 7299031]:
  goto <bb 21>; [100.00%]

  <bb 16> [local count: 1014686024]:
  # DEBUG BEGIN_STMT
  _19 = pcfsEntries[0].name;
  _20 = (int) i_33;
  _21 = config_clock.65_11->pcfs[_20].name;
  if (_19 == _21)
    goto <bb 17>; [67.00%]
  else
    goto <bb 35>; [33.00%]

  <bb 35> [local count: 334846388]:
  goto <bb 29>; [100.00%]

  <bb 17> [local count: 679839636]:
  # DEBUG BEGIN_STMT
  _22 = i_33 + 1;
  pcfsEntries[0].configIndex = _22;

  <bb 19> [local count: 738895437]:
  # j_43 = PHI <1(17), 0(33)>

  <bb 29> [local count: 1073741824]:
  # j_35 = PHI <j_43(19), 1(35)>
  # DEBUG j => j_35
  # DEBUG BEGIN_STMT
  if (j_35 == 0)
    goto <bb 16>; [94.50%]
  else
    goto <bb 20>; [5.50%]

  <bb 20> [local count: 59055800]:
  # DEBUG BEGIN_STMT
  i_53 = i_33 + 1;
  # DEBUG i => i_53

  <bb 21> [local count: 66354831]:
  # i_33 = PHI <i_53(20), 0(32)>
  # DEBUG i => i_33
  # DEBUG BEGIN_STMT
  _23 = config_clock.65_11->pcfsCount;
  if (_23 > i_33)
    goto <bb 33>; [89.00%]
  else
    goto <bb 30>; [11.00%]

  <bb 33> [local count: 59055800]:
  goto <bb 19>; [100.00%]

  <bb 30> [local count: 7299031]:
  goto <bb 27>; [100.00%]

  <bb 22> [local count: 236223206]:
  # DEBUG BEGIN_STMT
  _24 = (int) j_36;
  _25 = cmuEntries[_24].name;
  _26 = (int) i_34;
  _27 = config_clock.65_11->cmus[_26].name;
  if (_25 == _27)
    goto <bb 23>; [34.00%]
  else
    goto <bb 24>; [66.00%]

  <bb 23> [local count: 80315890]:
  # DEBUG BEGIN_STMT
  _28 = i_34 + 1;
  cmuEntries[_24].configIndex = _28;

  <bb 24> [local count: 236223206]:
  # DEBUG BEGIN_STMT
  j_52 = j_36 + 1;
  # DEBUG j => j_52

  <bb 25> [local count: 295279007]:
  # j_36 = PHI <j_52(24), 0(31)>
  # DEBUG j => j_36
  # DEBUG BEGIN_STMT
  if (j_36 != 4)
    goto <bb 22>; [80.00%]
  else
    goto <bb 26>; [20.00%]

  <bb 26> [local count: 59055801]:
  # DEBUG BEGIN_STMT
  i_50 = i_34 + 1;
  # DEBUG i => i_50

  <bb 27> [local count: 66354833]:
  # i_34 = PHI <i_50(26), 0(30)>
  # DEBUG i => i_34
  # DEBUG BEGIN_STMT
  _29 = config_clock.65_11->cmusCount;
  if (_29 > i_34)
    goto <bb 31>; [89.00%]
  else
    goto <bb 28>; [11.00%]

  <bb 31> [local count: 59055801]:
  goto <bb 25>; [100.00%]

  <bb 28> [local count: 7299032]:
  return;

}


CONFIG_ELEMENTS_MAPPINGS_01 ()
{
  uint8 i;
  int _1;

  <bb 2> [local count: 46707770]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG i => 0
  goto <bb 4>; [100.00%]

  <bb 3> [local count: 1027034056]:
  # DEBUG BEGIN_STMT
  _1 = (int) i_3;
  freqPointers[_1] = 0;
  # DEBUG BEGIN_STMT
  i_9 = i_3 + 1;
  # DEBUG i => i_9

  <bb 4> [local count: 1073741824]:
  # i_3 = PHI <0(2), i_9(3)>
  # DEBUG i => i_3
  # DEBUG BEGIN_STMT
  if (i_3 != 22)
    goto <bb 3>; [95.65%]
  else
    goto <bb 5>; [4.35%]

  <bb 5> [local count: 46707769]:
  # i_4 = PHI <0(4)>
  CONFIG_ELEMENTS_MAPPINGS_01.part.0 ();
  return;

}


UpdateFrequencies (power_modes_t powerMode)
{
  uint8 pllEn;
  static const clock_element_state_t convertValueToClockState[256] = {0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 255};
  static const uint8 bufferFreqEntriesCLKOUT_RUN_CLK[3][13] = {"\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00", "\x00\x0f#\x10\x11\x12$\x13\x14\x15\x16\x17\x18", "\x00\x0f#\x10\x11\x12$%&\'(\x17\x18"};
  static const Clock_Ip_NameType selectorEntriesCLKOUT_RUN_CLK[13] = {21, 0, 8, 2, 4, 5, 9, 13, 16, 14, 15, 10, 11};
  static const uint8 bufferFreqEntriesQSPI_MEM_CLK[3] = "\x00\x0e\"";
  static const uint8 bufferFreqEntriesLBIST_CLK[3] = "\x00\r!";
  static const uint8 bufferFreqEntriesDCM_CLK[3] = "\x00\f ";
  static const uint8 bufferFreqEntriesHSE_CLK[3] = "\x00\v\x1f";
  static const uint8 bufferFreqEntriesAIPS_SLOW_CLK[3] = "\x00\n\x1e";
  static const uint8 bufferFreqEntriesAIPS_PLAT_CLK[3] = "\x00\t\x1d";
  static const uint8 bufferFreqEntriesCORE_CLK[3] = "\x00\b\x1c";
  static const uint8 bufferFreqEntriesSCS_CLK[3] = "\x00\x01\x1a";
  static const Clock_Ip_NameType selectorEntriesSCS_CLK[3] = {21, 0, 8};
  <unnamed type> _1;
  unsigned char _2;
  <unnamed type> _3;
  unsigned char _4;
  <unnamed type> _5;
  unsigned char _6;
  <unnamed type> _7;
  unsigned char _8;
  unsigned char _9;
  <unnamed type> _10;
  unsigned char _11;
  int _12;
  <unnamed type> _13;
  <unnamed type> _14;
  unsigned char _15;
  int _16;
  <unnamed type> _17;
  unsigned char _18;
  unsigned char _19;
  <unnamed type> _20;
  int _21;
  <unnamed type> _22;
  int _23;
  <unnamed type> _24;
  unsigned char _25;
  unsigned char _26;
  unsigned char _27;
  unsigned char _28;
  unsigned char _29;
  unsigned char _30;
  unsigned char _31;
  unsigned char _32;
  unsigned char _33;
  unsigned char _34;
  unsigned char _35;
  unsigned char _36;
  unsigned char _37;
  unsigned char _38;
  unsigned char _39;
  unsigned char _40;
  long unsigned int _41;
  long unsigned int _42;
  long unsigned int _43;
  <unnamed type> _44;
  int _45;
  <unnamed type> _46;
  int _47;
  <unnamed type> _48;
  unsigned char _49;
  unsigned char _50;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = clkState[1];
  _2 = _1 & 1;
  freqPointers[1] = _2;
  # DEBUG BEGIN_STMT
  _3 = clkState[3];
  _4 = _3 & 2;
  freqPointers[3] = _4;
  # DEBUG BEGIN_STMT
  pllEn_54 = clkState[6];
  # DEBUG pllEn => pllEn_54
  # DEBUG BEGIN_STMT
  _5 = clkState[4];
  _6 = _5 & 3;
  freqPointers[4] = _6;
  # DEBUG BEGIN_STMT
  _7 = clkState[5];
  _8 = _7 & 4;
  freqPointers[5] = _8;
  # DEBUG BEGIN_STMT
  _9 = pllEn_54 & 5;
  freqPointers[6] = _9;
  # DEBUG BEGIN_STMT
  _10 = clkState[8];
  _11 = _10 & pllEn_54;
  _12 = (int) _11;
  _13 = convertValueToClockState[_12];
  clkState[8] = _13;
  # DEBUG BEGIN_STMT
  _14 = clkState[9];
  _15 = _14 & pllEn_54;
  _16 = (int) _15;
  _17 = convertValueToClockState[_16];
  clkState[9] = _17;
  # DEBUG BEGIN_STMT
  _18 = _13 & 26;
  freqPointers[8] = _18;
  # DEBUG BEGIN_STMT
  _19 = _17 & 27;
  freqPointers[9] = _19;
  # DEBUG BEGIN_STMT
  _20 = clkState[12];
  _21 = (int) _20;
  _22 = selectorEntriesSCS_CLK[_21];
  _23 = (int) _22;
  _24 = clkState[_23];
  _25 = bufferFreqEntriesSCS_CLK[_21];
  _26 = _24 & _25;
  freqPointers[12] = _26;
  # DEBUG BEGIN_STMT
  _27 = bufferFreqEntriesCORE_CLK[_21];
  _28 = _24 & _27;
  freqPointers[13] = _28;
  # DEBUG BEGIN_STMT
  _29 = bufferFreqEntriesAIPS_PLAT_CLK[_21];
  _30 = _24 & _29;
  freqPointers[14] = _30;
  # DEBUG BEGIN_STMT
  _31 = bufferFreqEntriesAIPS_SLOW_CLK[_21];
  _32 = _24 & _31;
  freqPointers[15] = _32;
  # DEBUG BEGIN_STMT
  _33 = bufferFreqEntriesHSE_CLK[_21];
  _34 = _24 & _33;
  freqPointers[16] = _34;
  # DEBUG BEGIN_STMT
  _35 = bufferFreqEntriesDCM_CLK[_21];
  _36 = _24 & _35;
  freqPointers[17] = _36;
  # DEBUG BEGIN_STMT
  _37 = bufferFreqEntriesLBIST_CLK[_21];
  _38 = _24 & _37;
  freqPointers[18] = _38;
  # DEBUG BEGIN_STMT
  _39 = bufferFreqEntriesQSPI_MEM_CLK[_21];
  _40 = _24 & _39;
  freqPointers[19] = _40;
  # DEBUG BEGIN_STMT
  _41 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].CSS;
  _42 = _41 >> 24;
  _43 = _42 & 63;
  _44 = selectorEntryIndex[_43];
  clkState[20] = _44;
  # DEBUG BEGIN_STMT
  _45 = (int) _44;
  _46 = selectorEntriesCLKOUT_RUN_CLK[_45];
  _47 = (int) _46;
  _48 = clkState[_47];
  _49 = bufferFreqEntriesCLKOUT_RUN_CLK[_21][_45];
  _50 = _48 & _49;
  freqPointers[20] = _50;
  return;

}


GetProducerClockFreq (Clock_Ip_NameType clockName)
{
  int _1;
  unsigned char _2;
  int _3;
  uint32 _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = (int) clockName_4(D);
  _2 = freqPointers[_1];
  _3 = (int) _2;
  _6 = bufferFreqs[_3];
  return _6;

}


SpecificPlatformInitClock (const struct Clock_Ip_ClockConfigType * config)
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  config_clock = config_2(D);
  return;

}


SpecificPeripheralClockInitialization (const struct Clock_IP_SpecificPeriphConfigType * config)
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


GetClockState (Clock_Ip_NameType name)
{
  clock_element_state_t retValue;
  int _1;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (name_3(D) <= 20)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (int) name_3(D);
  retValue_6 = clkState[_1];
  # DEBUG retValue => retValue_6
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  retValue_5 = clkState[21];
  # DEBUG retValue => retValue_5

  <bb 5> [local count: 1073741824]:
  # retValue_2 = PHI <retValue_6(3), retValue_5(4)>
  # DEBUG retValue => retValue_2
  # DEBUG BEGIN_STMT
  return retValue_2;

}


UpdateClockState (Clock_Ip_NameType name, clock_element_state_t state)
{
  int _1;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (name_3(D) <= 20)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (int) name_3(D);
  clkState[_1] = state_5(D);

  <bb 4> [local count: 1073741824]:
  return;

}


