VERSION ""


NS_ : 
	NS_DESC_
	CM_
	BA_DEF_
	BA_
	VAL_
	CAT_DEF_
	CAT_
	FILTER
	BA_DEF_DEF_
	EV_DATA_
	ENVVAR_DATA_
	SGTYPE_
	SGTYPE_VAL_
	BA_DEF_SGTYPE_
	BA_SGTYPE_
	SIG_TYPE_REF_
	VAL_TABLE_
	SIG_GROUP_
	SIG_VALTYPE_
	SIGTYPE_VALTYPE_
	BO_TX_BU_
	BA_DEF_REL_
	BA_REL_
	BA_DEF_DEF_REL_
	BU_SG_REL_
	BU_EV_REL_
	BU_BO_REL_
	SG_MUL_VAL_

BS_:

BU_: CGW VESS VCU
VAL_TABLE_ SysMode 3 "SysOFF" 2 "RUN" 1 "Ready" 0 "Initialize" ;
VAL_TABLE_ BitSTA 1 "True" 0 "False" ;
VAL_TABLE_ IntLck 1 "Connected" 0 "Disconnected" ;
VAL_TABLE_ CE_STA 2 "INVALID" 1 "ON" 0 "OFF" ;
VAL_TABLE_ CommSta 2 "Invalid Communication" 1 "Normal Communication" 0 "N/A" ;
VAL_TABLE_ LampCmd_t 3 "BLINKING" 2 "OFF" 1 "ON" 0 "N/A" ;


BO_ 940 VCU_3ACh: 8 VCU
 SG_ Charging_Sts_IND : 12|3@0+ (1,0) [0|7] "" Vector__XXX

BO_ 581 VCU_245h: 8 VCU
 SG_ DrivingPosition : 28|3@0+ (1,0) [0|7] "" Vector__XXX
 SG_ VCU_Ready : 25|2@0+ (1,0) [0|3] "" Vector__XXX

BO_ 529 VCU_211h: 8 VCU
 SG_ PW : 7|8@0+ (0.4,0) [0|102] "" Vector__XXX

BO_ 1857 VESS_DGN_REQ: 8 VESS
 SG_ DGN_REQ_VESS : 7|64@0+ (1,0) [0|1.84467440737096E+019] "" Vector__XXX

BO_ 1792 DIAG_FUNC_REQ: 8 CGW
 SG_ DIAG_REQ_FUNC : 7|64@0+ (1,0) [0|1.84467440737096E+019] "" Vector__XXX

BO_ 1416 CGW_588h_VC: 8 CGW
 SG_ VC_DOM : 11|4@0+ (1,0) [0|15] "" Vector__XXX

BO_ 882 CGW_372h: 8 CGW
 SG_ GoodbyeSoundCmd : 7|2@0+ (1,0) [0|3] "" Vector__XXX
 SG_ WelcomeSoundCmd : 5|2@0+ (1,0) [0|3] "" Vector__XXX

BO_ 771 ICM_303h: 8 CGW
 SG_ Speed_Combi : 17|10@0+ (1,0) [0|1023] "km/h" Vector__XXX

BO_ 336 ICM_150h: 8 CGW
 SG_ VessSoundSetCmd : 51|2@0+ (1,0) [0|3] "" Vector__XXX
 SG_ VessWelcomeOnOffSetCmd : 53|2@0+ (1,0) [0|3] "" Vector__XXX
 SG_ FactoryModeSetCmd : 0|1@0+ (1,0) [0|1] "" Vector__XXX

BO_ 1865 VESS_DGN_RESP: 8 VESS
 SG_ DGN_RESP_VESS : 7|64@0+ (1,0) [0|1.84467440737096E+019] "" Vector__XXX

BO_ 1394 VESS_PCAN_STS: 8 VESS
 SG_ MsgAliveCnt_VESS_PCAN : 63|8@0+ (1,0) [0|255] "" Vector__XXX
 SG_ BusOffCnt_VESS_PCAN : 55|8@0+ (1,0) [0|255] "" Vector__XXX
 SG_ TxErrCnt_VESS_PCAN : 47|8@0+ (1,0) [0|255] "" Vector__XXX
 SG_ RxErrCnt_VESS_PCAN : 39|8@0+ (1,0) [0|255] "" Vector__XXX
 SG_ SupplyVolt_VESS_PCAN : 31|8@0+ (0.1,0) [0|25.5] "" Vector__XXX
 SG_ DTCInfo_VESS_PCAN : 17|2@0+ (1,0) [0|3] "" Vector__XXX
 SG_ CMXVersion_VESS_PCAN : 7|16@0+ (1,0) [0|65535] "" Vector__XXX

BO_ 836 VESS_344h: 8 VESS
 SG_ VessSoundSetSts : 5|2@0+ (1,0) [0|3] "" Vector__XXX
 SG_ VessWelcomeOnOffSetSts : 3|2@0+ (1,0) [0|3] "" Vector__XXX
 SG_ VesstWarnCmd : 1|2@0+ (1,0) [0|3] "" Vector__XXX



CM_ SG_ 940 Charging_Sts_IND "0x3=DuringCharging(GreenFlash)
0x0=NoConnection_NoCharging(Off)
0x1=Connection_NoCharging(Green)
0x2=Connection_NoCharging_ScheduledChargSet(Blue)
0x4=ChargingComplete(Green)
0x5=ChargingFailure(RedFlash)
0x7=Invalid
0x6=ChargingDoorOpen(White)";
CM_ SG_ 581 DrivingPosition "Driving Position
0x0=P
0x1=R
0x2=N
0x3=D
0x4=L
0x7=Invalid";
CM_ SG_ 581 VCU_Ready "Electric Powertrain System Ready for driving.
0x0=Not Ready
0x1=Ready
0x2=Emergency(Blinking)";
CM_ SG_ 529 PW "pedal value
0xFF=Invalid value";
CM_ SG_ 1416 VC_DOM "vehicle code, Domestic/Export
0x0=domestic vehicle
0x1=general export vehicle
0x2=EU export vehicle";
CM_ SG_ 882 GoodbyeSoundCmd "Goodbye Sound Request to VESS
0x0=No_Activation
0x1=Activation
0x3=Invalid";
CM_ SG_ 882 WelcomeSoundCmd "Welcome Sound Request to VESS
0x0=No_Activation
0x1=Activation
0x3=Invalid";
CM_ SG_ 771 Speed_Combi "vehicle speed by combi
0x3FF=Invalid value";
CM_ SG_ 336 VessSoundSetCmd "Vess Sound Mode Set Command
0x0=NoActivation
0x1=Sound1
0x2=Sound2";
CM_ SG_ 336 VessWelcomeOnOffSetCmd "Vess Welcome Sound On/Off Set Command
0x0=NoActivation
0x1=Off
0x2=On";
CM_ SG_ 336 FactoryModeSetCmd "Factory Mode Command
0x0=No_Activation
0x1=Activation";
CM_ SG_ 1394 MsgAliveCnt_VESS_PCAN "0xFE=Init
0xFF=Invalid";
CM_ SG_ 1394 BusOffCnt_VESS_PCAN "0xFE=Init
0xFF=Invalid";
CM_ SG_ 1394 TxErrCnt_VESS_PCAN "0xFF=Invalid value";
CM_ SG_ 1394 RxErrCnt_VESS_PCAN "0xFF=Invalid value";
CM_ SG_ 1394 SupplyVolt_VESS_PCAN "0xFE=Init
0xFF=Invalid";
CM_ SG_ 1394 DTCInfo_VESS_PCAN "0x0=No_DTC_recorded
0x1=DTC_Available
0x2=DTCRecordingUnitDefect
0x3=Invalid_Value";
CM_ SG_ 836 VessSoundSetSts "Vess Sound Mode Set Status
0x0=NotUsed
0x1=Sound1
0x2=Sound2
0x3=Invalid";
CM_ SG_ 836 VessWelcomeOnOffSetSts "Vess Welcome Sound On/Off Set Status
0x0=NotUsed
0x1=Off
0x2=On
0x3=Invalid";
CM_ SG_ 836 VesstWarnCmd "Vess Warning Command
0x0=OFF

0x1=ON
";
BA_DEF_ SG_  "GenSigTimeoutTime_ABS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_AF1" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_AF2_Audio" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_AF_GPRS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_AirCon" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BCM" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_AirCon" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_BCM" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_BSW" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_DCDC" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_ETG" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_GPRS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_Meter" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_OBC" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_PEPS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_SRS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_Test" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_Test_PPS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_WP_FR" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BD_WP_RR" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_BSW" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_ECM" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_EPS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_ETG" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_GW_VMS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_Meter" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_PEPS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_SRS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_SlopeSensor" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_Slope_Filter" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_TCU" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_TPMS" INT 0 0;
BA_DEF_ SG_  "GenSigTimeoutTime_Test_BMC" INT 0 0;
BA_DEF_ SG_  "GenSigCycleTime" INT 0 0;
BA_DEF_ SG_  "GenSigCycleTimeActive" INT 0 0;
BA_DEF_ SG_  "GenSigInactiveValue" INT 0 0;
BA_DEF_ SG_  "GenSigStartValue" INT 0 0;
BA_DEF_ SG_  "GenSigSendType" ENUM  "cyclic","OnChange","OnWrite","IfActive","OnChangeWithRepetition","OnWriteWithRepetition","IfActiveWithRepetition","NoSigSendType","OnChangeAndIfActive","OnChangeAndIfActiveWithRepetition","CA","CE","Event";
BA_DEF_ BO_  "GenMsgILSupport" ENUM  "No","Yes";
BA_DEF_ BO_  "StartDelay" INT 0 100;
BA_DEF_ BO_  "GenMsgStartDelayTime" INT 0 0;
BA_DEF_ BO_  "GenMsgDelayTime" INT 0 0;
BA_DEF_ BO_  "GenMsgNrOfRepetition" INT 0 0;
BA_DEF_ BO_  "GenMsgCycleTimeFast" INT 0 0;
BA_DEF_ BO_  "GenMsgCycleTime" INT 0 0;
BA_DEF_ BO_  "GenMsgSendType" ENUM  "cyclic","Event","IfActive","CE","CA","NoMsgSendType";
BA_DEF_ BO_  "DiagResponse" ENUM  "No","Yes";
BA_DEF_ BO_  "DiagRequest" ENUM  "No","Yes";
BA_DEF_ BO_  "DiagState" ENUM  "No","Yes";
BA_DEF_ BO_  "NmMessage" ENUM  "No","Yes";
BA_DEF_ BU_  "CANoeDrift" INT 0 0;
BA_DEF_ BU_  "CANoeJitterMax" INT 0 0;
BA_DEF_ BU_  "CANoeJitterMin" INT 0 0;
BA_DEF_ BU_  "CANoeStartDelay" INT 0 10;
BA_DEF_ BU_  "ECU" STRING ;
BA_DEF_ BU_  "ILUsed" ENUM  "No","Yes";
BA_DEF_ BU_  "NmCAN" INT 1 2;
BA_DEF_ BU_  "NmNode" ENUM  "Yes","No";
BA_DEF_ BU_  "NmStationAddress" HEX 0 241;
BA_DEF_ BU_  "NodeLayerModules" STRING ;
BA_DEF_  "ILTxTimeout" INT 0 100;
BA_DEF_  "NmBaseAddress" HEX 0 2047;
BA_DEF_  "NmMessageCount" INT 0 255;
BA_DEF_  "VersionDay" INT 0 49;
BA_DEF_  "VersionMonth" INT 0 18;
BA_DEF_  "VersionNumber" INT 0 65535;
BA_DEF_  "VersionWeek" INT 0 82;
BA_DEF_  "VersionYear" INT 2009 2030;
BA_DEF_  "Manufacturer" STRING ;
BA_DEF_  "NmType" STRING ;
BA_DEF_  "BusType" STRING ;
BA_DEF_  "Baudrate" INT 0 1000000;
BA_DEF_  "DBName" STRING ;
BA_DEF_DEF_  "GenSigTimeoutTime_ABS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_AF1" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_AF2_Audio" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_AF_GPRS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_AirCon" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BCM" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_AirCon" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_BCM" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_BSW" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_DCDC" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_ETG" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_GPRS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_Meter" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_OBC" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_PEPS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_SRS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_Test" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_Test_PPS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_WP_FR" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BD_WP_RR" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_BSW" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_ECM" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_EPS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_ETG" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_GW_VMS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_Meter" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_PEPS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_SRS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_SlopeSensor" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_Slope_Filter" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_TCU" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_TPMS" 0;
BA_DEF_DEF_  "GenSigTimeoutTime_Test_BMC" 0;
BA_DEF_DEF_  "GenSigCycleTime" 0;
BA_DEF_DEF_  "GenSigCycleTimeActive" 0;
BA_DEF_DEF_  "GenSigInactiveValue" 0;
BA_DEF_DEF_  "GenSigStartValue" 0;
BA_DEF_DEF_  "GenSigSendType" "cyclic";
BA_DEF_DEF_  "GenMsgILSupport" "Yes";
BA_DEF_DEF_  "StartDelay" 0;
BA_DEF_DEF_  "GenMsgStartDelayTime" 0;
BA_DEF_DEF_  "GenMsgDelayTime" 0;
BA_DEF_DEF_  "GenMsgNrOfRepetition" 0;
BA_DEF_DEF_  "GenMsgCycleTimeFast" 0;
BA_DEF_DEF_  "GenMsgCycleTime" 0;
BA_DEF_DEF_  "GenMsgSendType" "cyclic";
BA_DEF_DEF_  "DiagResponse" "No";
BA_DEF_DEF_  "DiagRequest" "No";
BA_DEF_DEF_  "DiagState" "No";
BA_DEF_DEF_  "NmMessage" "No";
BA_DEF_DEF_  "CANoeDrift" 0;
BA_DEF_DEF_  "CANoeJitterMax" 0;
BA_DEF_DEF_  "CANoeJitterMin" 0;
BA_DEF_DEF_  "CANoeStartDelay" 0;
BA_DEF_DEF_  "ECU" "";
BA_DEF_DEF_  "ILUsed" "Yes";
BA_DEF_DEF_  "NmCAN" 2;
BA_DEF_DEF_  "NmNode" "No";
BA_DEF_DEF_  "NmStationAddress" 0;
BA_DEF_DEF_  "NodeLayerModules" "OSEKNM01.dll,CANoeILNLVector.dll";
BA_DEF_DEF_  "ILTxTimeout" 0;
BA_DEF_DEF_  "NmBaseAddress" 1024;
BA_DEF_DEF_  "NmMessageCount" 128;
BA_DEF_DEF_  "VersionDay" 0;
BA_DEF_DEF_  "VersionMonth" 0;
BA_DEF_DEF_  "VersionNumber" 0;
BA_DEF_DEF_  "VersionWeek" 0;
BA_DEF_DEF_  "VersionYear" 2013;
BA_DEF_DEF_  "Manufacturer" "";
BA_DEF_DEF_  "NmType" "";
BA_DEF_DEF_  "BusType" "";
BA_DEF_DEF_  "Baudrate" 500000;
BA_DEF_DEF_  "DBName" "";
BA_ "DBName" "CAN_CH1";

