IPA function summary for CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 inlinable
  global time:     10.000000
  self size:       11
  global size:     11
  min size:       0
  self stack:      0
  global stack:    0
    size:8.000000, time:8.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for NOT_UNDER_MCU_CONTROL_A.part.0/230 inlinable
  global time:     9.000000
  self size:       13
  global size:     13
  min size:       0
  self stack:      0
  global stack:    0
    size:10.000000, time:7.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 inlinable
  global time:     217.272731
  self size:       28
  global size:     28
  min size:       0
  self stack:      0
  global stack:    0
    size:25.000000, time:215.272731
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_TRACE_CLK_Frequency/202 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_STM1_CLK_Frequency/201 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_STMB_CLK_Frequency/200 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_STMB_CLK_Frequency/200 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_STM0_CLK_Frequency/199 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_STMA_CLK_Frequency/198 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_STMA_CLK_Frequency/198 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_RTC0_CLK_Frequency/197 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_RTC_CLK_Frequency/196 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 1 stack: 0

IPA function summary for get_RTC_CLK_Frequency/196 inlinable
  global time:     2.000000
  self size:       3
  global size:     3
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_QSPI0_SFCK_CLK_Frequency/195 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_QSPI_SFCK_CLK_Frequency/194 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_QSPI_SFCK_CLK_Frequency/194 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_FLEXCAN5_CLK_Frequency/193 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANB_CLK_Frequency/190 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCAN4_CLK_Frequency/192 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANB_CLK_Frequency/190 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCAN3_CLK_Frequency/191 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANB_CLK_Frequency/190 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCANB_CLK_Frequency/190 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_FLEXCAN2_CLK_Frequency/189 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANA_CLK_Frequency/186 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCAN1_CLK_Frequency/188 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANA_CLK_Frequency/186 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCAN0_CLK_Frequency/187 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANA_CLK_Frequency/186 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCANA_CLK_Frequency/186 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_EMAC0_TX_CLK_Frequency/185 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_EMAC_TX_CLK_Frequency/184 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_EMAC_TX_CLK_Frequency/184 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_EMAC0_TS_CLK_Frequency/183 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_EMAC_TS_CLK_Frequency/182 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_EMAC_TS_CLK_Frequency/182 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_EMAC0_RX_CLK_Frequency/181 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_EMAC_RX_CLK_Frequency/180 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_EMAC_RX_CLK_Frequency/180 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_CLKOUT_STANDBY_CLK_Frequency/179 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_SWT1_CLK_Frequency/178 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_SWT0_CLK_Frequency/177 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_SWT0_CLK_Frequency/177 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_SIUL0_CLK_Frequency/176 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_QSPI0_TX_MEM_CLK_Frequency/175 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_QSPI0_RAM_CLK_Frequency/174 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_QSPI0_RAM_CLK_Frequency/174 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_DCM0_CLK_Frequency/173 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_SEMA42_CLK_Frequency/172 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/165 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_MSCM_CLK_Frequency/171 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/165 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART8_CLK_Frequency/170 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/165 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART0_CLK_Frequency/169 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/165 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPSPI0_CLK_Frequency/168 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/165 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_INTM_CLK_Frequency/167 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/165 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_FLEXIO0_CLK_Frequency/166 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/165 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_CRC0_CLK_Frequency/165 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_WKPU0_CLK_Frequency/164 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_TSENSE0_CLK_Frequency/163 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_TRGMUX0_CLK_Frequency/162 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_STCU0_CLK_Frequency/161 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_SAI1_CLK_Frequency/160 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_SAI0_CLK_Frequency/159 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_PIT2_CLK_Frequency/158 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_PIT1_CLK_Frequency/157 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_PIT0_CLK_Frequency/156 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_MUB_CLK_Frequency/155 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_MUA_CLK_Frequency/154 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART9_CLK_Frequency/153 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART7_CLK_Frequency/152 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART6_CLK_Frequency/151 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART5_CLK_Frequency/150 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART4_CLK_Frequency/149 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART3_CLK_Frequency/148 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART2_CLK_Frequency/147 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART1_CLK_Frequency/146 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART15_CLK_Frequency/145 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART14_CLK_Frequency/144 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART13_CLK_Frequency/143 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART12_CLK_Frequency/142 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART11_CLK_Frequency/141 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPUART10_CLK_Frequency/140 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPSPI5_CLK_Frequency/139 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPSPI4_CLK_Frequency/138 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPSPI3_CLK_Frequency/137 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPSPI2_CLK_Frequency/136 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPSPI1_CLK_Frequency/135 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPI2C1_CLK_Frequency/134 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LPI2C0_CLK_Frequency/133 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_FLASH0_CLK_Frequency/132 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_ERM0_CLK_Frequency/131 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EIM0_CLK_Frequency/130 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_CMP2_CLK_Frequency/129 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_CMP1_CLK_Frequency/128 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/127 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_CMP0_CLK_Frequency/127 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_TEMPSENSE_CLK_Frequency/126 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_TCM_CM7_1_CLK_Frequency/125 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_TCM_CM7_0_CLK_Frequency/124 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LCU1_CLK_Frequency/123 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_LCU0_CLK_Frequency/122 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EMIOS2_CLK_Frequency/121 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EMIOS1_CLK_Frequency/120 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EMIOS0_CLK_Frequency/119 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD9_CLK_Frequency/118 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD8_CLK_Frequency/117 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD7_CLK_Frequency/116 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD6_CLK_Frequency/115 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD5_CLK_Frequency/114 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD4_CLK_Frequency/113 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD3_CLK_Frequency/112 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD31_CLK_Frequency/111 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD30_CLK_Frequency/110 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD2_CLK_Frequency/109 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD29_CLK_Frequency/108 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD28_CLK_Frequency/107 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD27_CLK_Frequency/106 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD26_CLK_Frequency/105 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD25_CLK_Frequency/104 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD24_CLK_Frequency/103 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD23_CLK_Frequency/102 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD22_CLK_Frequency/101 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD21_CLK_Frequency/100 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD20_CLK_Frequency/99 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD1_CLK_Frequency/98 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD19_CLK_Frequency/97 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD18_CLK_Frequency/96 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD17_CLK_Frequency/95 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD16_CLK_Frequency/94 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD15_CLK_Frequency/93 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD14_CLK_Frequency/92 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD13_CLK_Frequency/91 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD12_CLK_Frequency/90 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD11_CLK_Frequency/89 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD10_CLK_Frequency/88 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_TCD0_CLK_Frequency/87 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_EDMA0_CLK_Frequency/86 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_DMAMUX1_CLK_Frequency/85 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_DMAMUX0_CLK_Frequency/84 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_BCTU0_CLK_Frequency/83 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_ADC2_CLK_Frequency/82 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_ADC1_CLK_Frequency/81 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/80 function not considered for inlining
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0

IPA function summary for get_ADC0_CLK_Frequency/80 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CallbackDelay/77 inlinable
  global time:     170.545455
  self size:       16
  global size:     16
  min size:       20
  self stack:      12
  global stack:    12
    size:3.000000, time:27.272727
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    ClockTimeoutExpired/216 function body not available
      loop depth: 1 freq:9.09 size: 5 time: 14
       op0 is compile time invariant
       op1 is compile time invariant
    ClockStartTimeout/215 function body not available
      loop depth: 0 freq:1.00 size: 5 time: 14
       op0 is compile time invariant
       op1 is compile time invariant
       op2 is compile time invariant
       op3 is compile time invariant

IPA function summary for CallEmptyCallbacks/76 inlinable
  global time:     275.000000
  self size:       84
  global size:     84
  min size:       130
  self stack:      0
  global stack:    0
    size:16.000000, time:16.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 5 time: 17
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16

IPA function summary for McMeEnterKey/75 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_HSE_CLK_B/74 inlinable fp_expression
  global time:     24.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:22.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_HSE_CLK_A/73 inlinable fp_expression
  global time:     44.500000
  self size:       36
  global size:     36
  min size:       0
  self stack:      0
  global stack:    0
    size:33.000000, time:42.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_AIPS_PLAT_CLK_B/72 inlinable fp_expression
  global time:     24.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:22.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_AIPS_PLAT_CLK_A/71 inlinable fp_expression
  global time:     44.500000
  self size:       36
  global size:     36
  min size:       0
  self stack:      0
  global stack:    0
    size:33.000000, time:42.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_CORE_CLK_B/70 inlinable fp_expression
  global time:     24.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:22.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_CORE_CLK_A/69 inlinable fp_expression
  global time:     44.500000
  self size:       36
  global size:     36
  min size:       0
  self stack:      0
  global stack:    0
    size:33.000000, time:42.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_FXOSC_CLK_B/68 inlinable fp_expression
  global time:     24.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:22.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_FXOSC_CLK_A/67 inlinable fp_expression
  global time:     44.500000
  self size:       36
  global size:     36
  min size:       0
  self stack:      0
  global stack:    0
    size:33.000000, time:42.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_E/66 inlinable
  global time:     33.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:31.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_D/65 inlinable
  global time:     130.409092
  self size:       21
  global size:     21
  min size:       0
  self stack:      0
  global stack:    0
    size:18.000000, time:128.409092
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_C/64 inlinable
  global time:     74.454546
  self size:       19
  global size:     19
  min size:       0
  self stack:      0
  global stack:    0
    size:16.000000, time:72.454546
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_B/63 inlinable
  global time:     41.745501
  self size:       31
  global size:     31
  min size:       0
  self stack:      48
  global stack:    48
    size:28.000000, time:39.745501
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_A/62 inlinable
  global time:     29.000000
  self size:       24
  global size:     24
  min size:       0
  self stack:      0
  global stack:    0
    size:21.000000, time:27.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 inlinable
  global time:     84.674325
  self size:       37
  global size:     37
  min size:       2
  self stack:      0
  global stack:    0
    size:33.000000, time:80.341131
    size:3.000000, time:1.999860,  executed if:(not inlined)
  calls:
    CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 function not considered for inlining
      loop depth: 0 freq:0.23 size: 1 time: 10callee size: 5 stack: 0

IPA function summary for IntegerDividers_K/60 inlinable
  global time:     45.000000
  self size:       49
  global size:     49
  min size:       0
  self stack:      0
  global stack:    0
    size:46.000000, time:43.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_J/59 inlinable
  global time:     45.000000
  self size:       49
  global size:     49
  min size:       0
  self stack:      0
  global stack:    0
    size:46.000000, time:43.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_I/58 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_H/57 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_G/56 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_F/55 inlinable
  global time:     46.000000
  self size:       50
  global size:     50
  min size:       0
  self stack:      0
  global stack:    0
    size:47.000000, time:44.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_E/54 inlinable
  global time:     45.000000
  self size:       49
  global size:     49
  min size:       0
  self stack:      0
  global stack:    0
    size:46.000000, time:43.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_D/53 inlinable
  global time:     45.000000
  self size:       49
  global size:     49
  min size:       0
  self stack:      0
  global stack:    0
    size:46.000000, time:43.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_C/52 inlinable
  global time:     46.000000
  self size:       50
  global size:     50
  min size:       0
  self stack:      0
  global stack:    0
    size:47.000000, time:44.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_B/51 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_A/50 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PLL_C/49 inlinable
  global time:     38.000000
  self size:       21
  global size:     21
  min size:       0
  self stack:      0
  global stack:    0
    size:18.000000, time:36.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PLL_B/48 inlinable
  global time:     25.000000
  self size:       17
  global size:     17
  min size:       0
  self stack:      0
  global stack:    0
    size:14.000000, time:23.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PLL_A/47 inlinable
  global time:     34.500000
  self size:       38
  global size:     38
  min size:       0
  self stack:      0
  global stack:    0
    size:35.000000, time:32.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 inlinable
  global time:     30.000000
  self size:       41
  global size:     41
  min size:       0
  self stack:      0
  global stack:    0
    size:38.000000, time:28.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for NOT_UNDER_MCU_CONTROL_B/45 inlinable
  global time:     27.500000
  self size:       45
  global size:     45
  min size:       0
  self stack:      0
  global stack:    0
    size:42.000000, time:25.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for NOT_UNDER_MCU_CONTROL_A/44 inlinable
  global time:     33.000000
  self size:       39
  global size:     39
  min size:       2
  self stack:      0
  global stack:    0
    size:35.000000, time:26.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    NOT_UNDER_MCU_CONTROL_A.part.0/230 function not considered for inlining
      loop depth: 0 freq:0.50 size: 1 time: 10callee size: 6 stack: 0

IPA function summary for CONFIG_ELEMENTS_MAPPINGS_02/43 inlinable
  global time:     1586.297791
  self size:       56
  global size:     56
  min size:       0
  self stack:      0
  global stack:    0
    size:53.000000, time:1584.297791
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CONFIG_ELEMENTS_MAPPINGS_01/42 inlinable
  global time:     101.954022
  self size:       8
  global size:     8
  min size:       2
  self stack:      0
  global stack:    0
    size:4.000000, time:89.954022
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 function not considered for inlining
      loop depth: 0 freq:1.00 size: 1 time: 10callee size:14 stack: 0

IPA function summary for UpdateFrequencies/41 inlinable
  global time:     66.000000
  self size:       67
  global size:     67
  min size:       0
  self stack:      0
  global stack:    0
    size:64.000000, time:64.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for GetProducerClockFreq/40 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  array index:(op0 changed)
  calls:

IPA function summary for SpecificPlatformInitClock/39 inlinable
  global time:     3.000000
  self size:       4
  global size:     4
  min size:       0
  self stack:      0
  global stack:    0
    size:1.000000, time:1.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for SpecificPeripheralClockInitialization/38 inlinable
  global time:     2.000000
  self size:       3
  global size:     3
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for GetClockState/37 inlinable
  global time:     5.000000
  self size:       7
  global size:     7
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
    size:2.000000, time:2.000000,  nonconst if:(op0 changed)
    size:1.000000, time:0.500000,  executed if:(op0 > 20)
    size:1.000000, time:0.500000,  executed if:(op0 <= 20)
  array index:(op0 changed)
  calls:

IPA function summary for UpdateClockState/36 inlinable
  global time:     4.500000
  self size:       6
  global size:     6
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
    size:2.000000, time:2.000000,  nonconst if:(op0 changed)
    size:1.000000, time:0.500000,  executed if:(op0 <= 20)
  array index:(op0 changed)
  calls:


Flattening functions:
Overall time estimate: 5475.853470 weighted by profile: 0.000000

Deciding on inlining of small functions.  Starting with size 0.
Enqueueing calls in CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231.
Enqueueing calls in NOT_UNDER_MCU_CONTROL_A.part.0/230.
Enqueueing calls in CONFIG_ELEMENTS_MAPPINGS_01.part.0/229.
Enqueueing calls in get_TRACE_CLK_Frequency/202.
Enqueueing calls in get_STM1_CLK_Frequency/201.
Enqueueing calls in get_STMB_CLK_Frequency/200.
Enqueueing calls in get_STM0_CLK_Frequency/199.
Enqueueing calls in get_STMA_CLK_Frequency/198.
Enqueueing calls in get_RTC0_CLK_Frequency/197.
Enqueueing calls in get_RTC_CLK_Frequency/196.
Enqueueing calls in get_QSPI0_SFCK_CLK_Frequency/195.
Enqueueing calls in get_QSPI_SFCK_CLK_Frequency/194.
Enqueueing calls in get_FLEXCAN5_CLK_Frequency/193.
Enqueueing calls in get_FLEXCAN4_CLK_Frequency/192.
Enqueueing calls in get_FLEXCAN3_CLK_Frequency/191.
Enqueueing calls in get_FLEXCANB_CLK_Frequency/190.
Enqueueing calls in get_FLEXCAN2_CLK_Frequency/189.
Enqueueing calls in get_FLEXCAN1_CLK_Frequency/188.
Enqueueing calls in get_FLEXCAN0_CLK_Frequency/187.
Enqueueing calls in get_FLEXCANA_CLK_Frequency/186.
Enqueueing calls in get_EMAC0_TX_CLK_Frequency/185.
Enqueueing calls in get_EMAC_TX_CLK_Frequency/184.
Enqueueing calls in get_EMAC0_TS_CLK_Frequency/183.
Enqueueing calls in get_EMAC_TS_CLK_Frequency/182.
Enqueueing calls in get_EMAC0_RX_CLK_Frequency/181.
Enqueueing calls in get_EMAC_RX_CLK_Frequency/180.
Enqueueing calls in get_CLKOUT_STANDBY_CLK_Frequency/179.
Enqueueing calls in get_SWT1_CLK_Frequency/178.
Enqueueing calls in get_SWT0_CLK_Frequency/177.
Enqueueing calls in get_SIUL0_CLK_Frequency/176.
Enqueueing calls in get_QSPI0_TX_MEM_CLK_Frequency/175.
Enqueueing calls in get_QSPI0_RAM_CLK_Frequency/174.
Enqueueing calls in get_DCM0_CLK_Frequency/173.
Enqueueing calls in get_SEMA42_CLK_Frequency/172.
Enqueueing calls in get_MSCM_CLK_Frequency/171.
Enqueueing calls in get_LPUART8_CLK_Frequency/170.
Enqueueing calls in get_LPUART0_CLK_Frequency/169.
Enqueueing calls in get_LPSPI0_CLK_Frequency/168.
Enqueueing calls in get_INTM_CLK_Frequency/167.
Enqueueing calls in get_FLEXIO0_CLK_Frequency/166.
Enqueueing calls in get_CRC0_CLK_Frequency/165.
Enqueueing calls in get_WKPU0_CLK_Frequency/164.
Enqueueing calls in get_TSENSE0_CLK_Frequency/163.
Enqueueing calls in get_TRGMUX0_CLK_Frequency/162.
Enqueueing calls in get_STCU0_CLK_Frequency/161.
Enqueueing calls in get_SAI1_CLK_Frequency/160.
Enqueueing calls in get_SAI0_CLK_Frequency/159.
Enqueueing calls in get_PIT2_CLK_Frequency/158.
Enqueueing calls in get_PIT1_CLK_Frequency/157.
Enqueueing calls in get_PIT0_CLK_Frequency/156.
Enqueueing calls in get_MUB_CLK_Frequency/155.
Enqueueing calls in get_MUA_CLK_Frequency/154.
Enqueueing calls in get_LPUART9_CLK_Frequency/153.
Enqueueing calls in get_LPUART7_CLK_Frequency/152.
Enqueueing calls in get_LPUART6_CLK_Frequency/151.
Enqueueing calls in get_LPUART5_CLK_Frequency/150.
Enqueueing calls in get_LPUART4_CLK_Frequency/149.
Enqueueing calls in get_LPUART3_CLK_Frequency/148.
Enqueueing calls in get_LPUART2_CLK_Frequency/147.
Enqueueing calls in get_LPUART1_CLK_Frequency/146.
Enqueueing calls in get_LPUART15_CLK_Frequency/145.
Enqueueing calls in get_LPUART14_CLK_Frequency/144.
Enqueueing calls in get_LPUART13_CLK_Frequency/143.
Enqueueing calls in get_LPUART12_CLK_Frequency/142.
Enqueueing calls in get_LPUART11_CLK_Frequency/141.
Enqueueing calls in get_LPUART10_CLK_Frequency/140.
Enqueueing calls in get_LPSPI5_CLK_Frequency/139.
Enqueueing calls in get_LPSPI4_CLK_Frequency/138.
Enqueueing calls in get_LPSPI3_CLK_Frequency/137.
Enqueueing calls in get_LPSPI2_CLK_Frequency/136.
Enqueueing calls in get_LPSPI1_CLK_Frequency/135.
Enqueueing calls in get_LPI2C1_CLK_Frequency/134.
Enqueueing calls in get_LPI2C0_CLK_Frequency/133.
Enqueueing calls in get_FLASH0_CLK_Frequency/132.
Enqueueing calls in get_ERM0_CLK_Frequency/131.
Enqueueing calls in get_EIM0_CLK_Frequency/130.
Enqueueing calls in get_CMP2_CLK_Frequency/129.
Enqueueing calls in get_CMP1_CLK_Frequency/128.
Enqueueing calls in get_CMP0_CLK_Frequency/127.
Enqueueing calls in get_TEMPSENSE_CLK_Frequency/126.
Enqueueing calls in get_TCM_CM7_1_CLK_Frequency/125.
Enqueueing calls in get_TCM_CM7_0_CLK_Frequency/124.
Enqueueing calls in get_LCU1_CLK_Frequency/123.
Enqueueing calls in get_LCU0_CLK_Frequency/122.
Enqueueing calls in get_EMIOS2_CLK_Frequency/121.
Enqueueing calls in get_EMIOS1_CLK_Frequency/120.
Enqueueing calls in get_EMIOS0_CLK_Frequency/119.
Enqueueing calls in get_EDMA0_TCD9_CLK_Frequency/118.
Enqueueing calls in get_EDMA0_TCD8_CLK_Frequency/117.
Enqueueing calls in get_EDMA0_TCD7_CLK_Frequency/116.
Enqueueing calls in get_EDMA0_TCD6_CLK_Frequency/115.
Enqueueing calls in get_EDMA0_TCD5_CLK_Frequency/114.
Enqueueing calls in get_EDMA0_TCD4_CLK_Frequency/113.
Enqueueing calls in get_EDMA0_TCD3_CLK_Frequency/112.
Enqueueing calls in get_EDMA0_TCD31_CLK_Frequency/111.
Enqueueing calls in get_EDMA0_TCD30_CLK_Frequency/110.
Enqueueing calls in get_EDMA0_TCD2_CLK_Frequency/109.
Enqueueing calls in get_EDMA0_TCD29_CLK_Frequency/108.
Enqueueing calls in get_EDMA0_TCD28_CLK_Frequency/107.
Enqueueing calls in get_EDMA0_TCD27_CLK_Frequency/106.
Enqueueing calls in get_EDMA0_TCD26_CLK_Frequency/105.
Enqueueing calls in get_EDMA0_TCD25_CLK_Frequency/104.
Enqueueing calls in get_EDMA0_TCD24_CLK_Frequency/103.
Enqueueing calls in get_EDMA0_TCD23_CLK_Frequency/102.
Enqueueing calls in get_EDMA0_TCD22_CLK_Frequency/101.
Enqueueing calls in get_EDMA0_TCD21_CLK_Frequency/100.
Enqueueing calls in get_EDMA0_TCD20_CLK_Frequency/99.
Enqueueing calls in get_EDMA0_TCD1_CLK_Frequency/98.
Enqueueing calls in get_EDMA0_TCD19_CLK_Frequency/97.
Enqueueing calls in get_EDMA0_TCD18_CLK_Frequency/96.
Enqueueing calls in get_EDMA0_TCD17_CLK_Frequency/95.
Enqueueing calls in get_EDMA0_TCD16_CLK_Frequency/94.
Enqueueing calls in get_EDMA0_TCD15_CLK_Frequency/93.
Enqueueing calls in get_EDMA0_TCD14_CLK_Frequency/92.
Enqueueing calls in get_EDMA0_TCD13_CLK_Frequency/91.
Enqueueing calls in get_EDMA0_TCD12_CLK_Frequency/90.
Enqueueing calls in get_EDMA0_TCD11_CLK_Frequency/89.
Enqueueing calls in get_EDMA0_TCD10_CLK_Frequency/88.
Enqueueing calls in get_EDMA0_TCD0_CLK_Frequency/87.
Enqueueing calls in get_EDMA0_CLK_Frequency/86.
Enqueueing calls in get_DMAMUX1_CLK_Frequency/85.
Enqueueing calls in get_DMAMUX0_CLK_Frequency/84.
Enqueueing calls in get_BCTU0_CLK_Frequency/83.
Enqueueing calls in get_ADC2_CLK_Frequency/82.
Enqueueing calls in get_ADC1_CLK_Frequency/81.
Enqueueing calls in get_ADC0_CLK_Frequency/80.
Enqueueing calls in CallbackDelay/77.
Enqueueing calls in CallEmptyCallbacks/76.
Enqueueing calls in McMeEnterKey/75.
Enqueueing calls in CMU_HSE_CLK_B/74.
Enqueueing calls in CMU_HSE_CLK_A/73.
Enqueueing calls in CMU_AIPS_PLAT_CLK_B/72.
Enqueueing calls in CMU_AIPS_PLAT_CLK_A/71.
Enqueueing calls in CMU_CORE_CLK_B/70.
Enqueueing calls in CMU_CORE_CLK_A/69.
Enqueueing calls in CMU_FXOSC_CLK_B/68.
Enqueueing calls in CMU_FXOSC_CLK_A/67.
Enqueueing calls in PCFS_PLL_PHI0_E/66.
Enqueueing calls in PCFS_PLL_PHI0_D/65.
Enqueueing calls in PCFS_PLL_PHI0_C/64.
Enqueueing calls in PCFS_PLL_PHI0_B/63.
Enqueueing calls in PCFS_PLL_PHI0_A/62.
Enqueueing calls in CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61.
Enqueueing calls in IntegerDividers_K/60.
Enqueueing calls in IntegerDividers_J/59.
Enqueueing calls in IntegerDividers_I/58.
Enqueueing calls in IntegerDividers_H/57.
Enqueueing calls in IntegerDividers_G/56.
Enqueueing calls in IntegerDividers_F/55.
Enqueueing calls in IntegerDividers_E/54.
Enqueueing calls in IntegerDividers_D/53.
Enqueueing calls in IntegerDividers_C/52.
Enqueueing calls in IntegerDividers_B/51.
Enqueueing calls in IntegerDividers_A/50.
Enqueueing calls in PLL_C/49.
Enqueueing calls in PLL_B/48.
Enqueueing calls in PLL_A/47.
Enqueueing calls in IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46.
Enqueueing calls in NOT_UNDER_MCU_CONTROL_B/45.
Enqueueing calls in NOT_UNDER_MCU_CONTROL_A/44.
Enqueueing calls in CONFIG_ELEMENTS_MAPPINGS_02/43.
Enqueueing calls in CONFIG_ELEMENTS_MAPPINGS_01/42.
Enqueueing calls in UpdateFrequencies/41.
Enqueueing calls in GetProducerClockFreq/40.
Enqueueing calls in SpecificPlatformInitClock/39.
Enqueueing calls in SpecificPeripheralClockInitialization/38.
Enqueueing calls in GetClockState/37.
Enqueueing calls in UpdateClockState/36.

Considering get_RTC_CLK_Frequency/196 with 3 size
 to be inlined into get_RTC0_CLK_Frequency/197 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_ADC1_CLK_Frequency/81 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_ADC2_CLK_Frequency/82 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_BCTU0_CLK_Frequency/83 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_DMAMUX0_CLK_Frequency/84 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_DMAMUX1_CLK_Frequency/85 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_CLK_Frequency/86 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD0_CLK_Frequency/87 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD10_CLK_Frequency/88 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD11_CLK_Frequency/89 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD12_CLK_Frequency/90 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD13_CLK_Frequency/91 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD14_CLK_Frequency/92 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD15_CLK_Frequency/93 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD16_CLK_Frequency/94 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD17_CLK_Frequency/95 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD18_CLK_Frequency/96 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD19_CLK_Frequency/97 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD1_CLK_Frequency/98 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD20_CLK_Frequency/99 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD21_CLK_Frequency/100 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD22_CLK_Frequency/101 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD23_CLK_Frequency/102 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD24_CLK_Frequency/103 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD25_CLK_Frequency/104 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD26_CLK_Frequency/105 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD27_CLK_Frequency/106 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD28_CLK_Frequency/107 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD29_CLK_Frequency/108 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD2_CLK_Frequency/109 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD30_CLK_Frequency/110 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD31_CLK_Frequency/111 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD3_CLK_Frequency/112 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD4_CLK_Frequency/113 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD5_CLK_Frequency/114 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD6_CLK_Frequency/115 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD7_CLK_Frequency/116 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD8_CLK_Frequency/117 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EDMA0_TCD9_CLK_Frequency/118 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EMIOS0_CLK_Frequency/119 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EMIOS1_CLK_Frequency/120 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_EMIOS2_CLK_Frequency/121 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_LCU0_CLK_Frequency/122 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_LCU1_CLK_Frequency/123 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_TCM_CM7_0_CLK_Frequency/124 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_TCM_CM7_1_CLK_Frequency/125 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_ADC0_CLK_Frequency/80 with 5 size
 to be inlined into get_TEMPSENSE_CLK_Frequency/126 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_CMP1_CLK_Frequency/128 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_CMP2_CLK_Frequency/129 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_EIM0_CLK_Frequency/130 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_ERM0_CLK_Frequency/131 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_FLASH0_CLK_Frequency/132 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPI2C0_CLK_Frequency/133 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPI2C1_CLK_Frequency/134 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPSPI1_CLK_Frequency/135 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPSPI2_CLK_Frequency/136 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPSPI3_CLK_Frequency/137 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPSPI4_CLK_Frequency/138 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPSPI5_CLK_Frequency/139 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART10_CLK_Frequency/140 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART11_CLK_Frequency/141 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART12_CLK_Frequency/142 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART13_CLK_Frequency/143 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART14_CLK_Frequency/144 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART15_CLK_Frequency/145 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART1_CLK_Frequency/146 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART2_CLK_Frequency/147 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART3_CLK_Frequency/148 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART4_CLK_Frequency/149 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART5_CLK_Frequency/150 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART6_CLK_Frequency/151 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART7_CLK_Frequency/152 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_LPUART9_CLK_Frequency/153 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_MUA_CLK_Frequency/154 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_MUB_CLK_Frequency/155 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_PIT0_CLK_Frequency/156 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_PIT1_CLK_Frequency/157 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_PIT2_CLK_Frequency/158 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_SAI0_CLK_Frequency/159 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_SAI1_CLK_Frequency/160 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_STCU0_CLK_Frequency/161 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_TRGMUX0_CLK_Frequency/162 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_TSENSE0_CLK_Frequency/163 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CMP0_CLK_Frequency/127 with 5 size
 to be inlined into get_WKPU0_CLK_Frequency/164 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CRC0_CLK_Frequency/165 with 5 size
 to be inlined into get_FLEXIO0_CLK_Frequency/166 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CRC0_CLK_Frequency/165 with 5 size
 to be inlined into get_INTM_CLK_Frequency/167 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CRC0_CLK_Frequency/165 with 5 size
 to be inlined into get_LPSPI0_CLK_Frequency/168 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CRC0_CLK_Frequency/165 with 5 size
 to be inlined into get_LPUART0_CLK_Frequency/169 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CRC0_CLK_Frequency/165 with 5 size
 to be inlined into get_LPUART8_CLK_Frequency/170 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CRC0_CLK_Frequency/165 with 5 size
 to be inlined into get_MSCM_CLK_Frequency/171 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_CRC0_CLK_Frequency/165 with 5 size
 to be inlined into get_SEMA42_CLK_Frequency/172 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_QSPI0_RAM_CLK_Frequency/174 with 5 size
 to be inlined into get_QSPI0_TX_MEM_CLK_Frequency/175 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering get_SWT0_CLK_Frequency/177 with 5 size
 to be inlined into get_SWT1_CLK_Frequency/178 in unknown:0
 Estimated badness is -inf, frequency 1.00.

Considering CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 with 28 size
 to be inlined into CONFIG_ELEMENTS_MAPPINGS_01/42 in unknown:0
 Estimated badness is -0.062500, frequency 1.00.

Considering NOT_UNDER_MCU_CONTROL_A.part.0/230 with 13 size
 to be inlined into NOT_UNDER_MCU_CONTROL_A/44 in unknown:0
 Estimated badness is -0.055556, frequency 0.50.

Considering CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 with 11 size
 to be inlined into CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 in unknown:0
 Estimated badness is -0.036364, frequency 0.23.

Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:

Deciding on functions to be inlined into all callers and removing useless speculations:
Overall time estimate: 4603.886795 weighted by profile: 0.000000

Why inlining failed?
function body not available                       :        2 calls, 10.090909 freq, 0 count
call is unlikely and code size would grow         :       12 calls, 12.000000 freq, 0 count
IPA function summary for get_TRACE_CLK_Frequency/202 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_STM1_CLK_Frequency/201 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_STMB_CLK_Frequency/200 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_STMB_CLK_Frequency/200 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       15
  self stack:      0
  global stack:    0
  estimated growth:13
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_STM0_CLK_Frequency/199 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_STMA_CLK_Frequency/198 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_STMA_CLK_Frequency/198 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       15
  self stack:      0
  global stack:    0
  estimated growth:13
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_RTC0_CLK_Frequency/197 inlinable
  global time:     2.000000
  self size:       5
  global size:     3
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_RTC_CLK_Frequency/232 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 1 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_RTC_CLK_Frequency/196 inlinable
  global time:     2.000000
  self size:       3
  global size:     3
  min size:       0
  self stack:      0
  global stack:    0
  estimated growth:-2
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_QSPI0_SFCK_CLK_Frequency/195 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_QSPI_SFCK_CLK_Frequency/194 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_QSPI_SFCK_CLK_Frequency/194 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       15
  self stack:      0
  global stack:    0
  estimated growth:13
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_FLEXCAN5_CLK_Frequency/193 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANB_CLK_Frequency/190 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCAN4_CLK_Frequency/192 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANB_CLK_Frequency/190 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCAN3_CLK_Frequency/191 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANB_CLK_Frequency/190 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCANB_CLK_Frequency/190 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       15
  self stack:      0
  global stack:    0
  estimated growth:39
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_FLEXCAN2_CLK_Frequency/189 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANA_CLK_Frequency/186 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCAN1_CLK_Frequency/188 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANA_CLK_Frequency/186 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCAN0_CLK_Frequency/187 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_FLEXCANA_CLK_Frequency/186 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_FLEXCANA_CLK_Frequency/186 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       15
  self stack:      0
  global stack:    0
  estimated growth:39
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_EMAC0_TX_CLK_Frequency/185 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_EMAC_TX_CLK_Frequency/184 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_EMAC_TX_CLK_Frequency/184 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       15
  self stack:      0
  global stack:    0
  estimated growth:13
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_EMAC0_TS_CLK_Frequency/183 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_EMAC_TS_CLK_Frequency/182 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_EMAC_TS_CLK_Frequency/182 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       15
  self stack:      0
  global stack:    0
  estimated growth:13
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_EMAC0_RX_CLK_Frequency/181 inlinable
  global time:     13.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_EMAC_RX_CLK_Frequency/180 call is unlikely and code size would grow
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 9 stack: 0

IPA function summary for get_EMAC_RX_CLK_Frequency/180 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       15
  self stack:      0
  global stack:    0
  estimated growth:13
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_CLKOUT_STANDBY_CLK_Frequency/179 inlinable
  global time:     26.000000
  self size:       18
  global size:     18
  min size:       0
  self stack:      0
  global stack:    0
    size:15.000000, time:24.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_SWT1_CLK_Frequency/178 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_SWT0_CLK_Frequency/324 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_SWT0_CLK_Frequency/177 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       2
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_SIUL0_CLK_Frequency/176 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_QSPI0_TX_MEM_CLK_Frequency/175 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_QSPI0_RAM_CLK_Frequency/323 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_QSPI0_RAM_CLK_Frequency/174 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       2
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_DCM0_CLK_Frequency/173 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_SEMA42_CLK_Frequency/172 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/322 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_MSCM_CLK_Frequency/171 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/321 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART8_CLK_Frequency/170 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/320 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART0_CLK_Frequency/169 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/319 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPSPI0_CLK_Frequency/168 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/318 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_INTM_CLK_Frequency/167 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/317 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_FLEXIO0_CLK_Frequency/166 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CRC0_CLK_Frequency/316 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_CRC0_CLK_Frequency/165 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       2
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_WKPU0_CLK_Frequency/164 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/315 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_TSENSE0_CLK_Frequency/163 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/314 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_TRGMUX0_CLK_Frequency/162 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/313 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_STCU0_CLK_Frequency/161 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/312 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_SAI1_CLK_Frequency/160 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/311 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_SAI0_CLK_Frequency/159 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/310 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_PIT2_CLK_Frequency/158 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/309 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_PIT1_CLK_Frequency/157 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/308 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_PIT0_CLK_Frequency/156 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/307 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_MUB_CLK_Frequency/155 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/306 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_MUA_CLK_Frequency/154 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/305 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART9_CLK_Frequency/153 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/304 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART7_CLK_Frequency/152 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/303 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART6_CLK_Frequency/151 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/302 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART5_CLK_Frequency/150 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/301 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART4_CLK_Frequency/149 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/300 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART3_CLK_Frequency/148 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/299 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART2_CLK_Frequency/147 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/298 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART1_CLK_Frequency/146 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/297 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART15_CLK_Frequency/145 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/296 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART14_CLK_Frequency/144 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/295 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART13_CLK_Frequency/143 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/294 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART12_CLK_Frequency/142 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/293 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART11_CLK_Frequency/141 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/292 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPUART10_CLK_Frequency/140 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/291 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPSPI5_CLK_Frequency/139 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/290 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPSPI4_CLK_Frequency/138 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/289 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPSPI3_CLK_Frequency/137 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/288 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPSPI2_CLK_Frequency/136 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/287 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPSPI1_CLK_Frequency/135 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/286 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPI2C1_CLK_Frequency/134 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/285 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LPI2C0_CLK_Frequency/133 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/284 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_FLASH0_CLK_Frequency/132 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/283 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_ERM0_CLK_Frequency/131 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/282 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EIM0_CLK_Frequency/130 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/281 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_CMP2_CLK_Frequency/129 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/280 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_CMP1_CLK_Frequency/128 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_CMP0_CLK_Frequency/279 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_CMP0_CLK_Frequency/127 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       2
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for get_TEMPSENSE_CLK_Frequency/126 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/278 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_TCM_CM7_1_CLK_Frequency/125 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/277 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_TCM_CM7_0_CLK_Frequency/124 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/276 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LCU1_CLK_Frequency/123 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/275 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_LCU0_CLK_Frequency/122 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/274 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EMIOS2_CLK_Frequency/121 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/273 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EMIOS1_CLK_Frequency/120 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/272 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EMIOS0_CLK_Frequency/119 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/271 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD9_CLK_Frequency/118 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/270 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD8_CLK_Frequency/117 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/269 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD7_CLK_Frequency/116 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/268 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD6_CLK_Frequency/115 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/267 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD5_CLK_Frequency/114 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/266 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD4_CLK_Frequency/113 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/265 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD3_CLK_Frequency/112 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/264 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD31_CLK_Frequency/111 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/263 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD30_CLK_Frequency/110 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/262 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD2_CLK_Frequency/109 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/261 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD29_CLK_Frequency/108 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/260 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD28_CLK_Frequency/107 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/259 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD27_CLK_Frequency/106 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/258 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD26_CLK_Frequency/105 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/257 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD25_CLK_Frequency/104 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/256 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD24_CLK_Frequency/103 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/255 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD23_CLK_Frequency/102 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/254 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD22_CLK_Frequency/101 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/253 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD21_CLK_Frequency/100 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/252 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD20_CLK_Frequency/99 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/251 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD1_CLK_Frequency/98 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/250 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD19_CLK_Frequency/97 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/249 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD18_CLK_Frequency/96 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/248 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD17_CLK_Frequency/95 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/247 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD16_CLK_Frequency/94 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/246 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD15_CLK_Frequency/93 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/245 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD14_CLK_Frequency/92 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/244 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD13_CLK_Frequency/91 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/243 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD12_CLK_Frequency/90 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/242 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD11_CLK_Frequency/89 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/241 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD10_CLK_Frequency/88 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/240 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_TCD0_CLK_Frequency/87 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/239 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_EDMA0_CLK_Frequency/86 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/238 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_DMAMUX1_CLK_Frequency/85 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/237 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_DMAMUX0_CLK_Frequency/84 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/236 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_BCTU0_CLK_Frequency/83 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/235 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_ADC2_CLK_Frequency/82 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/234 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_ADC1_CLK_Frequency/81 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       4
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    get_ADC0_CLK_Frequency/233 inlined
      loop depth: 0 freq:1.00 size: 2 time: 11callee size: 2 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for get_ADC0_CLK_Frequency/80 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       2
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CallbackDelay/77 inlinable
  global time:     170.545455
  self size:       16
  global size:     16
  min size:       20
  self stack:      12
  global stack:    12
    size:3.000000, time:27.272727
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    ClockTimeoutExpired/216 function body not available
      loop depth: 1 freq:9.09 size: 5 time: 14
       op0 is compile time invariant
       op1 is compile time invariant
    ClockStartTimeout/215 function body not available
      loop depth: 0 freq:1.00 size: 5 time: 14
       op0 is compile time invariant
       op1 is compile time invariant
       op2 is compile time invariant
       op3 is compile time invariant

IPA function summary for CallEmptyCallbacks/76 inlinable
  global time:     275.000000
  self size:       84
  global size:     84
  min size:       130
  self stack:      0
  global stack:    0
    size:16.000000, time:16.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 5 time: 17
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16
    indirect call loop depth: 0 freq:1.00 size: 4 time: 16

IPA function summary for McMeEnterKey/75 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_HSE_CLK_B/74 inlinable fp_expression
  global time:     24.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:22.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_HSE_CLK_A/73 inlinable fp_expression
  global time:     44.500000
  self size:       36
  global size:     36
  min size:       0
  self stack:      0
  global stack:    0
    size:33.000000, time:42.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_AIPS_PLAT_CLK_B/72 inlinable fp_expression
  global time:     24.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:22.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_AIPS_PLAT_CLK_A/71 inlinable fp_expression
  global time:     44.500000
  self size:       36
  global size:     36
  min size:       0
  self stack:      0
  global stack:    0
    size:33.000000, time:42.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_CORE_CLK_B/70 inlinable fp_expression
  global time:     24.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:22.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_CORE_CLK_A/69 inlinable fp_expression
  global time:     44.500000
  self size:       36
  global size:     36
  min size:       0
  self stack:      0
  global stack:    0
    size:33.000000, time:42.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_FXOSC_CLK_B/68 inlinable fp_expression
  global time:     24.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:22.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CMU_FXOSC_CLK_A/67 inlinable fp_expression
  global time:     44.500000
  self size:       36
  global size:     36
  min size:       0
  self stack:      0
  global stack:    0
    size:33.000000, time:42.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_E/66 inlinable
  global time:     33.000000
  self size:       25
  global size:     25
  min size:       0
  self stack:      0
  global stack:    0
    size:22.000000, time:31.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_D/65 inlinable
  global time:     130.409092
  self size:       21
  global size:     21
  min size:       0
  self stack:      0
  global stack:    0
    size:18.000000, time:128.409092
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_C/64 inlinable
  global time:     74.454546
  self size:       19
  global size:     19
  min size:       0
  self stack:      0
  global stack:    0
    size:16.000000, time:72.454546
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_B/63 inlinable
  global time:     41.745501
  self size:       31
  global size:     31
  min size:       0
  self stack:      48
  global stack:    48
    size:28.000000, time:39.745501
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PCFS_PLL_PHI0_A/62 inlinable
  global time:     29.000000
  self size:       24
  global size:     24
  min size:       0
  self stack:      0
  global stack:    0
    size:21.000000, time:27.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 inlinable
  global time:     84.207658
  self size:       37
  global size:     44
  min size:       2
  self stack:      0
  global stack:    0
    size:41.000000, time:82.207798
    size:3.000000, time:1.999860,  executed if:(not inlined)
  calls:
    CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 inlined
      loop depth: 0 freq:0.23 size: 1 time: 10callee size: 5 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for IntegerDividers_K/60 inlinable
  global time:     45.000000
  self size:       49
  global size:     49
  min size:       0
  self stack:      0
  global stack:    0
    size:46.000000, time:43.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_J/59 inlinable
  global time:     45.000000
  self size:       49
  global size:     49
  min size:       0
  self stack:      0
  global stack:    0
    size:46.000000, time:43.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_I/58 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_H/57 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_G/56 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_F/55 inlinable
  global time:     46.000000
  self size:       50
  global size:     50
  min size:       0
  self stack:      0
  global stack:    0
    size:47.000000, time:44.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_E/54 inlinable
  global time:     45.000000
  self size:       49
  global size:     49
  min size:       0
  self stack:      0
  global stack:    0
    size:46.000000, time:43.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_D/53 inlinable
  global time:     45.000000
  self size:       49
  global size:     49
  min size:       0
  self stack:      0
  global stack:    0
    size:46.000000, time:43.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_C/52 inlinable
  global time:     46.000000
  self size:       50
  global size:     50
  min size:       0
  self stack:      0
  global stack:    0
    size:47.000000, time:44.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_B/51 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IntegerDividers_A/50 inlinable
  global time:     47.000000
  self size:       51
  global size:     51
  min size:       0
  self stack:      0
  global stack:    0
    size:48.000000, time:45.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PLL_C/49 inlinable
  global time:     38.000000
  self size:       21
  global size:     21
  min size:       0
  self stack:      0
  global stack:    0
    size:18.000000, time:36.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PLL_B/48 inlinable
  global time:     25.000000
  self size:       17
  global size:     17
  min size:       0
  self stack:      0
  global stack:    0
    size:14.000000, time:23.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for PLL_A/47 inlinable
  global time:     34.500000
  self size:       38
  global size:     38
  min size:       0
  self stack:      0
  global stack:    0
    size:35.000000, time:32.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 inlinable
  global time:     30.000000
  self size:       41
  global size:     41
  min size:       0
  self stack:      0
  global stack:    0
    size:38.000000, time:28.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for NOT_UNDER_MCU_CONTROL_B/45 inlinable
  global time:     27.500000
  self size:       45
  global size:     45
  min size:       0
  self stack:      0
  global stack:    0
    size:42.000000, time:25.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for NOT_UNDER_MCU_CONTROL_A/44 inlinable
  global time:     31.500000
  self size:       39
  global size:     48
  min size:       2
  self stack:      0
  global stack:    0
    size:45.000000, time:29.500000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    NOT_UNDER_MCU_CONTROL_A.part.0/230 inlined
      loop depth: 0 freq:0.50 size: 1 time: 10callee size: 6 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for CONFIG_ELEMENTS_MAPPINGS_02/43 inlinable
  global time:     1586.297791
  self size:       56
  global size:     56
  min size:       0
  self stack:      0
  global stack:    0
    size:53.000000, time:1584.297791
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for CONFIG_ELEMENTS_MAPPINGS_01/42 inlinable
  global time:     307.226748
  self size:       8
  global size:     32
  min size:       2
  self stack:      0
  global stack:    0
    size:29.000000, time:305.226748
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 inlined
      loop depth: 0 freq:1.00 size: 1 time: 10callee size:14 stack: 0
      Stack frame offset 0, callee self size 0, callee size 0

IPA function summary for UpdateFrequencies/41 inlinable
  global time:     66.000000
  self size:       67
  global size:     67
  min size:       0
  self stack:      0
  global stack:    0
    size:64.000000, time:64.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for GetProducerClockFreq/40 inlinable
  global time:     4.000000
  self size:       5
  global size:     5
  min size:       0
  self stack:      0
  global stack:    0
    size:2.000000, time:2.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  array index:(op0 changed)
  calls:

IPA function summary for SpecificPlatformInitClock/39 inlinable
  global time:     3.000000
  self size:       4
  global size:     4
  min size:       0
  self stack:      0
  global stack:    0
    size:1.000000, time:1.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for SpecificPeripheralClockInitialization/38 inlinable
  global time:     2.000000
  self size:       3
  global size:     3
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

IPA function summary for GetClockState/37 inlinable
  global time:     5.000000
  self size:       7
  global size:     7
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
    size:2.000000, time:2.000000,  nonconst if:(op0 changed)
    size:1.000000, time:0.500000,  executed if:(op0 > 20)
    size:1.000000, time:0.500000,  executed if:(op0 <= 20)
  array index:(op0 changed)
  calls:

IPA function summary for UpdateClockState/36 inlinable
  global time:     4.500000
  self size:       6
  global size:     6
  min size:       0
  self stack:      0
  global stack:    0
    size:0.000000, time:0.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
    size:2.000000, time:2.000000,  nonconst if:(op0 changed)
    size:1.000000, time:0.500000,  executed if:(op0 <= 20)
  array index:(op0 changed)
  calls:

Symbol table:

get_SWT0_CLK_Frequency/324 (get_SWT0_CLK_Frequency) @07519c40
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 177
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_SWT0_CLK_Frequency/324 is inline copy in get_SWT1_CLK_Frequency/178
  Clone of get_SWT0_CLK_Frequency/177
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_SWT1_CLK_Frequency/178 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_QSPI0_RAM_CLK_Frequency/323 (get_QSPI0_RAM_CLK_Frequency) @07519b60
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 174
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_QSPI0_RAM_CLK_Frequency/323 is inline copy in get_QSPI0_TX_MEM_CLK_Frequency/175
  Clone of get_QSPI0_RAM_CLK_Frequency/174
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_QSPI0_TX_MEM_CLK_Frequency/175 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CRC0_CLK_Frequency/322 (get_CRC0_CLK_Frequency) @07519a80
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 321
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CRC0_CLK_Frequency/322 is inline copy in get_SEMA42_CLK_Frequency/172
  Clone of get_CRC0_CLK_Frequency/165
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_SEMA42_CLK_Frequency/172 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CRC0_CLK_Frequency/321 (get_CRC0_CLK_Frequency) @075199a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 320
  previous sharing asm name: 322
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CRC0_CLK_Frequency/321 is inline copy in get_MSCM_CLK_Frequency/171
  Clone of get_CRC0_CLK_Frequency/165
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_MSCM_CLK_Frequency/171 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CRC0_CLK_Frequency/320 (get_CRC0_CLK_Frequency) @075198c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 319
  previous sharing asm name: 321
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CRC0_CLK_Frequency/320 is inline copy in get_LPUART8_CLK_Frequency/170
  Clone of get_CRC0_CLK_Frequency/165
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART8_CLK_Frequency/170 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CRC0_CLK_Frequency/319 (get_CRC0_CLK_Frequency) @075197e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 318
  previous sharing asm name: 320
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CRC0_CLK_Frequency/319 is inline copy in get_LPUART0_CLK_Frequency/169
  Clone of get_CRC0_CLK_Frequency/165
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART0_CLK_Frequency/169 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CRC0_CLK_Frequency/318 (get_CRC0_CLK_Frequency) @07519700
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 317
  previous sharing asm name: 319
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CRC0_CLK_Frequency/318 is inline copy in get_LPSPI0_CLK_Frequency/168
  Clone of get_CRC0_CLK_Frequency/165
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPSPI0_CLK_Frequency/168 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CRC0_CLK_Frequency/317 (get_CRC0_CLK_Frequency) @07519620
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 316
  previous sharing asm name: 318
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CRC0_CLK_Frequency/317 is inline copy in get_INTM_CLK_Frequency/167
  Clone of get_CRC0_CLK_Frequency/165
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_INTM_CLK_Frequency/167 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CRC0_CLK_Frequency/316 (get_CRC0_CLK_Frequency) @07519540
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 165
  previous sharing asm name: 317
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CRC0_CLK_Frequency/316 is inline copy in get_FLEXIO0_CLK_Frequency/166
  Clone of get_CRC0_CLK_Frequency/165
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_FLEXIO0_CLK_Frequency/166 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/315 (get_CMP0_CLK_Frequency) @07519460
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 314
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/315 is inline copy in get_WKPU0_CLK_Frequency/164
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_WKPU0_CLK_Frequency/164 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/314 (get_CMP0_CLK_Frequency) @07519380
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 313
  previous sharing asm name: 315
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/314 is inline copy in get_TSENSE0_CLK_Frequency/163
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_TSENSE0_CLK_Frequency/163 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/313 (get_CMP0_CLK_Frequency) @075192a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 312
  previous sharing asm name: 314
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/313 is inline copy in get_TRGMUX0_CLK_Frequency/162
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_TRGMUX0_CLK_Frequency/162 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/312 (get_CMP0_CLK_Frequency) @075191c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 311
  previous sharing asm name: 313
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/312 is inline copy in get_STCU0_CLK_Frequency/161
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_STCU0_CLK_Frequency/161 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/311 (get_CMP0_CLK_Frequency) @075190e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 310
  previous sharing asm name: 312
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/311 is inline copy in get_SAI1_CLK_Frequency/160
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_SAI1_CLK_Frequency/160 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/310 (get_CMP0_CLK_Frequency) @07519000
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 309
  previous sharing asm name: 311
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/310 is inline copy in get_SAI0_CLK_Frequency/159
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_SAI0_CLK_Frequency/159 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/309 (get_CMP0_CLK_Frequency) @07516ee0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 308
  previous sharing asm name: 310
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/309 is inline copy in get_PIT2_CLK_Frequency/158
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_PIT2_CLK_Frequency/158 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/308 (get_CMP0_CLK_Frequency) @07516e00
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 307
  previous sharing asm name: 309
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/308 is inline copy in get_PIT1_CLK_Frequency/157
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_PIT1_CLK_Frequency/157 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/307 (get_CMP0_CLK_Frequency) @07516d20
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 306
  previous sharing asm name: 308
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/307 is inline copy in get_PIT0_CLK_Frequency/156
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_PIT0_CLK_Frequency/156 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/306 (get_CMP0_CLK_Frequency) @07516c40
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 305
  previous sharing asm name: 307
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/306 is inline copy in get_MUB_CLK_Frequency/155
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_MUB_CLK_Frequency/155 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/305 (get_CMP0_CLK_Frequency) @07516b60
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 304
  previous sharing asm name: 306
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/305 is inline copy in get_MUA_CLK_Frequency/154
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_MUA_CLK_Frequency/154 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/304 (get_CMP0_CLK_Frequency) @07516a80
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 303
  previous sharing asm name: 305
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/304 is inline copy in get_LPUART9_CLK_Frequency/153
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART9_CLK_Frequency/153 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/303 (get_CMP0_CLK_Frequency) @075169a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 302
  previous sharing asm name: 304
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/303 is inline copy in get_LPUART7_CLK_Frequency/152
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART7_CLK_Frequency/152 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/302 (get_CMP0_CLK_Frequency) @075168c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 301
  previous sharing asm name: 303
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/302 is inline copy in get_LPUART6_CLK_Frequency/151
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART6_CLK_Frequency/151 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/301 (get_CMP0_CLK_Frequency) @075167e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 300
  previous sharing asm name: 302
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/301 is inline copy in get_LPUART5_CLK_Frequency/150
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART5_CLK_Frequency/150 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/300 (get_CMP0_CLK_Frequency) @07516700
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 299
  previous sharing asm name: 301
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/300 is inline copy in get_LPUART4_CLK_Frequency/149
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART4_CLK_Frequency/149 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/299 (get_CMP0_CLK_Frequency) @07516620
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 298
  previous sharing asm name: 300
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/299 is inline copy in get_LPUART3_CLK_Frequency/148
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART3_CLK_Frequency/148 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/298 (get_CMP0_CLK_Frequency) @07516540
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 297
  previous sharing asm name: 299
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/298 is inline copy in get_LPUART2_CLK_Frequency/147
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART2_CLK_Frequency/147 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/297 (get_CMP0_CLK_Frequency) @07516460
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 296
  previous sharing asm name: 298
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/297 is inline copy in get_LPUART1_CLK_Frequency/146
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART1_CLK_Frequency/146 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/296 (get_CMP0_CLK_Frequency) @07516380
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 295
  previous sharing asm name: 297
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/296 is inline copy in get_LPUART15_CLK_Frequency/145
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART15_CLK_Frequency/145 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/295 (get_CMP0_CLK_Frequency) @075162a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 294
  previous sharing asm name: 296
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/295 is inline copy in get_LPUART14_CLK_Frequency/144
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART14_CLK_Frequency/144 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/294 (get_CMP0_CLK_Frequency) @075161c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 293
  previous sharing asm name: 295
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/294 is inline copy in get_LPUART13_CLK_Frequency/143
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART13_CLK_Frequency/143 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/293 (get_CMP0_CLK_Frequency) @075160e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 292
  previous sharing asm name: 294
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/293 is inline copy in get_LPUART12_CLK_Frequency/142
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART12_CLK_Frequency/142 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/292 (get_CMP0_CLK_Frequency) @07516000
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 291
  previous sharing asm name: 293
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/292 is inline copy in get_LPUART11_CLK_Frequency/141
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART11_CLK_Frequency/141 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/291 (get_CMP0_CLK_Frequency) @07510ee0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 290
  previous sharing asm name: 292
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/291 is inline copy in get_LPUART10_CLK_Frequency/140
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPUART10_CLK_Frequency/140 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/290 (get_CMP0_CLK_Frequency) @07510e00
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 289
  previous sharing asm name: 291
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/290 is inline copy in get_LPSPI5_CLK_Frequency/139
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPSPI5_CLK_Frequency/139 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/289 (get_CMP0_CLK_Frequency) @07510d20
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 288
  previous sharing asm name: 290
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/289 is inline copy in get_LPSPI4_CLK_Frequency/138
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPSPI4_CLK_Frequency/138 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/288 (get_CMP0_CLK_Frequency) @07510c40
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 287
  previous sharing asm name: 289
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/288 is inline copy in get_LPSPI3_CLK_Frequency/137
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPSPI3_CLK_Frequency/137 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/287 (get_CMP0_CLK_Frequency) @07510b60
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 286
  previous sharing asm name: 288
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/287 is inline copy in get_LPSPI2_CLK_Frequency/136
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPSPI2_CLK_Frequency/136 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/286 (get_CMP0_CLK_Frequency) @07510a80
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 285
  previous sharing asm name: 287
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/286 is inline copy in get_LPSPI1_CLK_Frequency/135
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPSPI1_CLK_Frequency/135 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/285 (get_CMP0_CLK_Frequency) @075109a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 284
  previous sharing asm name: 286
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/285 is inline copy in get_LPI2C1_CLK_Frequency/134
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPI2C1_CLK_Frequency/134 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/284 (get_CMP0_CLK_Frequency) @075108c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 283
  previous sharing asm name: 285
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/284 is inline copy in get_LPI2C0_CLK_Frequency/133
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LPI2C0_CLK_Frequency/133 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/283 (get_CMP0_CLK_Frequency) @075107e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 282
  previous sharing asm name: 284
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/283 is inline copy in get_FLASH0_CLK_Frequency/132
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_FLASH0_CLK_Frequency/132 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/282 (get_CMP0_CLK_Frequency) @07510700
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 281
  previous sharing asm name: 283
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/282 is inline copy in get_ERM0_CLK_Frequency/131
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_ERM0_CLK_Frequency/131 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/281 (get_CMP0_CLK_Frequency) @07510620
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 280
  previous sharing asm name: 282
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/281 is inline copy in get_EIM0_CLK_Frequency/130
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EIM0_CLK_Frequency/130 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/280 (get_CMP0_CLK_Frequency) @07510540
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 279
  previous sharing asm name: 281
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/280 is inline copy in get_CMP2_CLK_Frequency/129
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_CMP2_CLK_Frequency/129 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CMP0_CLK_Frequency/279 (get_CMP0_CLK_Frequency) @07510460
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 127
  previous sharing asm name: 280
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_CMP0_CLK_Frequency/279 is inline copy in get_CMP1_CLK_Frequency/128
  Clone of get_CMP0_CLK_Frequency/127
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_CMP1_CLK_Frequency/128 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/278 (get_ADC0_CLK_Frequency) @07510380
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 277
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/278 is inline copy in get_TEMPSENSE_CLK_Frequency/126
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_TEMPSENSE_CLK_Frequency/126 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/277 (get_ADC0_CLK_Frequency) @075102a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 276
  previous sharing asm name: 278
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/277 is inline copy in get_TCM_CM7_1_CLK_Frequency/125
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_TCM_CM7_1_CLK_Frequency/125 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/276 (get_ADC0_CLK_Frequency) @075101c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 275
  previous sharing asm name: 277
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/276 is inline copy in get_TCM_CM7_0_CLK_Frequency/124
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_TCM_CM7_0_CLK_Frequency/124 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/275 (get_ADC0_CLK_Frequency) @075100e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 274
  previous sharing asm name: 276
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/275 is inline copy in get_LCU1_CLK_Frequency/123
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LCU1_CLK_Frequency/123 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/274 (get_ADC0_CLK_Frequency) @07510000
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 273
  previous sharing asm name: 275
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/274 is inline copy in get_LCU0_CLK_Frequency/122
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_LCU0_CLK_Frequency/122 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/273 (get_ADC0_CLK_Frequency) @0750cee0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 272
  previous sharing asm name: 274
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/273 is inline copy in get_EMIOS2_CLK_Frequency/121
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EMIOS2_CLK_Frequency/121 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/272 (get_ADC0_CLK_Frequency) @0750ce00
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 271
  previous sharing asm name: 273
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/272 is inline copy in get_EMIOS1_CLK_Frequency/120
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EMIOS1_CLK_Frequency/120 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/271 (get_ADC0_CLK_Frequency) @0750cd20
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 270
  previous sharing asm name: 272
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/271 is inline copy in get_EMIOS0_CLK_Frequency/119
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EMIOS0_CLK_Frequency/119 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/270 (get_ADC0_CLK_Frequency) @0750cc40
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 269
  previous sharing asm name: 271
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/270 is inline copy in get_EDMA0_TCD9_CLK_Frequency/118
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD9_CLK_Frequency/118 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/269 (get_ADC0_CLK_Frequency) @0750cb60
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 268
  previous sharing asm name: 270
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/269 is inline copy in get_EDMA0_TCD8_CLK_Frequency/117
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD8_CLK_Frequency/117 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/268 (get_ADC0_CLK_Frequency) @0750ca80
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 267
  previous sharing asm name: 269
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/268 is inline copy in get_EDMA0_TCD7_CLK_Frequency/116
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD7_CLK_Frequency/116 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/267 (get_ADC0_CLK_Frequency) @0750c9a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 266
  previous sharing asm name: 268
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/267 is inline copy in get_EDMA0_TCD6_CLK_Frequency/115
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD6_CLK_Frequency/115 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/266 (get_ADC0_CLK_Frequency) @0750c8c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 265
  previous sharing asm name: 267
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/266 is inline copy in get_EDMA0_TCD5_CLK_Frequency/114
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD5_CLK_Frequency/114 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/265 (get_ADC0_CLK_Frequency) @0750c7e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 264
  previous sharing asm name: 266
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/265 is inline copy in get_EDMA0_TCD4_CLK_Frequency/113
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD4_CLK_Frequency/113 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/264 (get_ADC0_CLK_Frequency) @0750c700
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 263
  previous sharing asm name: 265
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/264 is inline copy in get_EDMA0_TCD3_CLK_Frequency/112
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD3_CLK_Frequency/112 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/263 (get_ADC0_CLK_Frequency) @0750c620
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 262
  previous sharing asm name: 264
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/263 is inline copy in get_EDMA0_TCD31_CLK_Frequency/111
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD31_CLK_Frequency/111 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/262 (get_ADC0_CLK_Frequency) @0750c540
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 261
  previous sharing asm name: 263
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/262 is inline copy in get_EDMA0_TCD30_CLK_Frequency/110
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD30_CLK_Frequency/110 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/261 (get_ADC0_CLK_Frequency) @0750c460
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 260
  previous sharing asm name: 262
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/261 is inline copy in get_EDMA0_TCD2_CLK_Frequency/109
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD2_CLK_Frequency/109 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/260 (get_ADC0_CLK_Frequency) @0750c380
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 259
  previous sharing asm name: 261
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/260 is inline copy in get_EDMA0_TCD29_CLK_Frequency/108
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD29_CLK_Frequency/108 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/259 (get_ADC0_CLK_Frequency) @0750c2a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 258
  previous sharing asm name: 260
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/259 is inline copy in get_EDMA0_TCD28_CLK_Frequency/107
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD28_CLK_Frequency/107 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/258 (get_ADC0_CLK_Frequency) @0750c1c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 257
  previous sharing asm name: 259
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/258 is inline copy in get_EDMA0_TCD27_CLK_Frequency/106
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD27_CLK_Frequency/106 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/257 (get_ADC0_CLK_Frequency) @0750c0e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 256
  previous sharing asm name: 258
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/257 is inline copy in get_EDMA0_TCD26_CLK_Frequency/105
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD26_CLK_Frequency/105 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/256 (get_ADC0_CLK_Frequency) @0750c000
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 255
  previous sharing asm name: 257
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/256 is inline copy in get_EDMA0_TCD25_CLK_Frequency/104
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD25_CLK_Frequency/104 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/255 (get_ADC0_CLK_Frequency) @07508ee0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 254
  previous sharing asm name: 256
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/255 is inline copy in get_EDMA0_TCD24_CLK_Frequency/103
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD24_CLK_Frequency/103 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/254 (get_ADC0_CLK_Frequency) @07508e00
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 253
  previous sharing asm name: 255
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/254 is inline copy in get_EDMA0_TCD23_CLK_Frequency/102
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD23_CLK_Frequency/102 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/253 (get_ADC0_CLK_Frequency) @07508d20
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 252
  previous sharing asm name: 254
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/253 is inline copy in get_EDMA0_TCD22_CLK_Frequency/101
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD22_CLK_Frequency/101 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/252 (get_ADC0_CLK_Frequency) @07508c40
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 251
  previous sharing asm name: 253
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/252 is inline copy in get_EDMA0_TCD21_CLK_Frequency/100
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD21_CLK_Frequency/100 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/251 (get_ADC0_CLK_Frequency) @07508b60
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 250
  previous sharing asm name: 252
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/251 is inline copy in get_EDMA0_TCD20_CLK_Frequency/99
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD20_CLK_Frequency/99 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/250 (get_ADC0_CLK_Frequency) @07508a80
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 249
  previous sharing asm name: 251
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/250 is inline copy in get_EDMA0_TCD1_CLK_Frequency/98
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD1_CLK_Frequency/98 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/249 (get_ADC0_CLK_Frequency) @075089a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 248
  previous sharing asm name: 250
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/249 is inline copy in get_EDMA0_TCD19_CLK_Frequency/97
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD19_CLK_Frequency/97 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/248 (get_ADC0_CLK_Frequency) @075088c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 247
  previous sharing asm name: 249
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/248 is inline copy in get_EDMA0_TCD18_CLK_Frequency/96
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD18_CLK_Frequency/96 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/247 (get_ADC0_CLK_Frequency) @075087e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 246
  previous sharing asm name: 248
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/247 is inline copy in get_EDMA0_TCD17_CLK_Frequency/95
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD17_CLK_Frequency/95 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/246 (get_ADC0_CLK_Frequency) @07508700
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 245
  previous sharing asm name: 247
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/246 is inline copy in get_EDMA0_TCD16_CLK_Frequency/94
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD16_CLK_Frequency/94 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/245 (get_ADC0_CLK_Frequency) @07508620
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 244
  previous sharing asm name: 246
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/245 is inline copy in get_EDMA0_TCD15_CLK_Frequency/93
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD15_CLK_Frequency/93 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/244 (get_ADC0_CLK_Frequency) @07508540
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 243
  previous sharing asm name: 245
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/244 is inline copy in get_EDMA0_TCD14_CLK_Frequency/92
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD14_CLK_Frequency/92 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/243 (get_ADC0_CLK_Frequency) @07508460
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 242
  previous sharing asm name: 244
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/243 is inline copy in get_EDMA0_TCD13_CLK_Frequency/91
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD13_CLK_Frequency/91 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/242 (get_ADC0_CLK_Frequency) @07508380
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 241
  previous sharing asm name: 243
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/242 is inline copy in get_EDMA0_TCD12_CLK_Frequency/90
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD12_CLK_Frequency/90 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/241 (get_ADC0_CLK_Frequency) @075082a0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 240
  previous sharing asm name: 242
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/241 is inline copy in get_EDMA0_TCD11_CLK_Frequency/89
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD11_CLK_Frequency/89 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/240 (get_ADC0_CLK_Frequency) @075081c0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 239
  previous sharing asm name: 241
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/240 is inline copy in get_EDMA0_TCD10_CLK_Frequency/88
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD10_CLK_Frequency/88 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/239 (get_ADC0_CLK_Frequency) @075080e0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 238
  previous sharing asm name: 240
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/239 is inline copy in get_EDMA0_TCD0_CLK_Frequency/87
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_TCD0_CLK_Frequency/87 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/238 (get_ADC0_CLK_Frequency) @07508000
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 237
  previous sharing asm name: 239
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/238 is inline copy in get_EDMA0_CLK_Frequency/86
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_EDMA0_CLK_Frequency/86 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/237 (get_ADC0_CLK_Frequency) @0715b380
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 236
  previous sharing asm name: 238
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/237 is inline copy in get_DMAMUX1_CLK_Frequency/85
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_DMAMUX1_CLK_Frequency/85 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/236 (get_ADC0_CLK_Frequency) @074afee0
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 235
  previous sharing asm name: 237
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/236 is inline copy in get_DMAMUX0_CLK_Frequency/84
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_DMAMUX0_CLK_Frequency/84 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/235 (get_ADC0_CLK_Frequency) @074afe00
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 234
  previous sharing asm name: 236
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/235 is inline copy in get_BCTU0_CLK_Frequency/83
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_BCTU0_CLK_Frequency/83 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/234 (get_ADC0_CLK_Frequency) @074afd20
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 233
  previous sharing asm name: 235
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/234 is inline copy in get_ADC2_CLK_Frequency/82
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_ADC2_CLK_Frequency/82 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_ADC0_CLK_Frequency/233 (get_ADC0_CLK_Frequency) @074afc40
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 80
  previous sharing asm name: 234
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Function get_ADC0_CLK_Frequency/233 is inline copy in get_ADC1_CLK_Frequency/81
  Clone of get_ADC0_CLK_Frequency/80
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_ADC1_CLK_Frequency/81 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_RTC_CLK_Frequency/232 (get_RTC_CLK_Frequency) @074afb60
  Type: function definition analyzed
  Visibility:
  next sharing asm name: 196
  References: 
  Referring: 
  Function get_RTC_CLK_Frequency/232 is inline copy in get_RTC0_CLK_Frequency/197
  Clone of get_RTC_CLK_Frequency/196
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local icf_merged optimize_size
  Called by: get_RTC0_CLK_Frequency/197 (inlined) (1073741824 (estimated locally),1.00 per call) 
  Calls: 
CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0) @0733a700
  Type: function definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: bufferFreqs/25 (read)configuredCoreClock/29 (write)bufferFreqs/25 (read)configuredAipsPlatClock/30 (write)bufferFreqs/25 (read)configuredAipsSlowClock/31 (write)bufferFreqs/25 (read)configuredHseClock/32 (write)
  Referring: 
  Function CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 is inline copy in CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61
  Availability: local
  Function flags: count:26801491 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (inlined) (26801491 (estimated locally),0.23 per call) 
  Calls: 
NOT_UNDER_MCU_CONTROL_A.part.0/230 (NOT_UNDER_MCU_CONTROL_A.part.0) @0733a9a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: clkState/27 (write)clkState/27 (write)
  Referring: 
  Function NOT_UNDER_MCU_CONTROL_A.part.0/230 is inline copy in NOT_UNDER_MCU_CONTROL_A/44
  Availability: local
  Function flags: count:536870912 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: NOT_UNDER_MCU_CONTROL_A/44 (inlined) (536870912 (estimated locally),0.50 per call) 
  Calls: 
CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (CONFIG_ELEMENTS_MAPPINGS_01.part.0) @0733a000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: freqPointers/26 (write)config_clock/33 (read)freqPointers/26 (write)freqPointers/26 (write)freqPointers/26 (write)
  Referring: 
  Function CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 is inline copy in CONFIG_ELEMENTS_MAPPINGS_01/42
  Availability: local
  Function flags: count:46707769 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: CONFIG_ELEMENTS_MAPPINGS_01/42 (inlined) (46707769 (estimated locally),1.00 per call) 
  Calls: 
*.LC1/228 (*.LC1) @067e9c18
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: 
  Referring: PCFS_PLL_PHI0_B/63 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
*.LC0/227 (*.LC0) @067e9b88
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly artificial
  References: 
  Referring: PCFS_PLL_PHI0_B/63 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
pcfsCallbacks/226 (pcfsCallbacks) @07090288
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
selectorCallbacks/225 (selectorCallbacks) @070901b0
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
pllCallbacks/224 (pllCallbacks) @07090048
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
intOscCallbacks/223 (intOscCallbacks) @0708ef30
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
gateCallbacks/222 (gateCallbacks) @0708edc8
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
fracDivCallbacks/221 (fracDivCallbacks) @0708ec60
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
extOscCallbacks/220 (extOscCallbacks) @0708eb88
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
dividerTriggerCallbacks/219 (dividerTriggerCallbacks) @0708eab0
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
dividerCallbacks/218 (dividerCallbacks) @0708e9d8
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
cmuCallbacks/217 (cmuCallbacks) @0708e750
  Type: variable
  Body removed by symtab_remove_unreachable_nodes
  Visibility: external public
  References: 
  Referring: CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)CallEmptyCallbacks/76 (read)
  Availability: not_available
  Varpool flags: read-only
ClockTimeoutExpired/216 (ClockTimeoutExpired) @07084b60
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: CallbackDelay/77 (1073741824 (estimated locally),9.09 per call) 
  Calls: 
ClockStartTimeout/215 (ClockStartTimeout) @07084a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: CallbackDelay/77 (118111600 (estimated locally),1.00 per call) 
  Calls: 
bufferFreqEntriesCLKOUT_RUN_CLK.5132/214 (bufferFreqEntriesCLKOUT_RUN_CLK) @0708e318
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntriesCLKOUT_RUN_CLK.5131/213 (selectorEntriesCLKOUT_RUN_CLK) @0708e2d0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesQSPI_MEM_CLK.5130/212 (bufferFreqEntriesQSPI_MEM_CLK) @0708e288
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesLBIST_CLK.5129/211 (bufferFreqEntriesLBIST_CLK) @0708e240
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesDCM_CLK.5128/210 (bufferFreqEntriesDCM_CLK) @0708e1f8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesHSE_CLK.5127/209 (bufferFreqEntriesHSE_CLK) @0708e1b0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesAIPS_SLOW_CLK.5126/208 (bufferFreqEntriesAIPS_SLOW_CLK) @0708e168
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesAIPS_PLAT_CLK.5125/207 (bufferFreqEntriesAIPS_PLAT_CLK) @0708e120
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesCORE_CLK.5124/206 (bufferFreqEntriesCORE_CLK) @0708e0d8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
bufferFreqEntriesSCS_CLK.5123/205 (bufferFreqEntriesSCS_CLK) @0708e090
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntriesSCS_CLK.5122/204 (selectorEntriesSCS_CLK) @0708e048
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
convertValueToClockState.5133/203 (convertValueToClockState) @0708e000
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
get_TRACE_CLK_Frequency/202 (get_TRACE_CLK_Frequency) @0707ab60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_STM1_CLK_Frequency/201 (get_STM1_CLK_Frequency) @0707a620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_STMB_CLK_Frequency/200 (1073741824 (estimated locally),1.00 per call) 
get_STMB_CLK_Frequency/200 (get_STMB_CLK_Frequency) @0707a0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_STM1_CLK_Frequency/201 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_STM0_CLK_Frequency/199 (get_STM0_CLK_Frequency) @0707ad20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_STMA_CLK_Frequency/198 (1073741824 (estimated locally),1.00 per call) 
get_STMA_CLK_Frequency/198 (get_STMA_CLK_Frequency) @0707aa80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_STM0_CLK_Frequency/199 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_RTC0_CLK_Frequency/197 (get_RTC0_CLK_Frequency) @0707a7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_RTC_CLK_Frequency/232 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_RTC_CLK_Frequency/196 (get_RTC_CLK_Frequency) @0707a540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  previous sharing asm name: 232
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: 
get_QSPI0_SFCK_CLK_Frequency/195 (get_QSPI0_SFCK_CLK_Frequency) @0707a2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_QSPI_SFCK_CLK_Frequency/194 (1073741824 (estimated locally),1.00 per call) 
get_QSPI_SFCK_CLK_Frequency/194 (get_QSPI_SFCK_CLK_Frequency) @0707a000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_QSPI0_SFCK_CLK_Frequency/195 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_FLEXCAN5_CLK_Frequency/193 (get_FLEXCAN5_CLK_Frequency) @0706db60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANB_CLK_Frequency/190 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCAN4_CLK_Frequency/192 (get_FLEXCAN4_CLK_Frequency) @0706d620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANB_CLK_Frequency/190 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCAN3_CLK_Frequency/191 (get_FLEXCAN3_CLK_Frequency) @0706d0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANB_CLK_Frequency/190 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCANB_CLK_Frequency/190 (get_FLEXCANB_CLK_Frequency) @0706dd20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_FLEXCAN5_CLK_Frequency/193 (1073741824 (estimated locally),1.00 per call) get_FLEXCAN4_CLK_Frequency/192 (1073741824 (estimated locally),1.00 per call) get_FLEXCAN3_CLK_Frequency/191 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_FLEXCAN2_CLK_Frequency/189 (get_FLEXCAN2_CLK_Frequency) @0706da80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANA_CLK_Frequency/186 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCAN1_CLK_Frequency/188 (get_FLEXCAN1_CLK_Frequency) @0706d7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANA_CLK_Frequency/186 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCAN0_CLK_Frequency/187 (get_FLEXCAN0_CLK_Frequency) @0706d540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_FLEXCANA_CLK_Frequency/186 (1073741824 (estimated locally),1.00 per call) 
get_FLEXCANA_CLK_Frequency/186 (get_FLEXCANA_CLK_Frequency) @0706d2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_FLEXCAN2_CLK_Frequency/189 (1073741824 (estimated locally),1.00 per call) get_FLEXCAN1_CLK_Frequency/188 (1073741824 (estimated locally),1.00 per call) get_FLEXCAN0_CLK_Frequency/187 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_EMAC0_TX_CLK_Frequency/185 (get_EMAC0_TX_CLK_Frequency) @0706d000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_EMAC_TX_CLK_Frequency/184 (1073741824 (estimated locally),1.00 per call) 
get_EMAC_TX_CLK_Frequency/184 (get_EMAC_TX_CLK_Frequency) @07064b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_EMAC0_TX_CLK_Frequency/185 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_EMAC0_TS_CLK_Frequency/183 (get_EMAC0_TS_CLK_Frequency) @07064620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_EMAC_TS_CLK_Frequency/182 (1073741824 (estimated locally),1.00 per call) 
get_EMAC_TS_CLK_Frequency/182 (get_EMAC_TS_CLK_Frequency) @070640e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_EMAC0_TS_CLK_Frequency/183 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_EMAC0_RX_CLK_Frequency/181 (get_EMAC0_RX_CLK_Frequency) @07064d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_EMAC_RX_CLK_Frequency/180 (1073741824 (estimated locally),1.00 per call) 
get_EMAC_RX_CLK_Frequency/180 (get_EMAC_RX_CLK_Frequency) @07064a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: get_EMAC0_RX_CLK_Frequency/181 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
get_CLKOUT_STANDBY_CLK_Frequency/179 (get_CLKOUT_STANDBY_CLK_Frequency) @070647e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: hardwareValue_selectorEntry/22 (read)freqPointers/26 (read)bufferFreqs/25 (read)enableDisableMask/12 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SWT1_CLK_Frequency/178 (get_SWT1_CLK_Frequency) @07064540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_SWT0_CLK_Frequency/324 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_SWT0_CLK_Frequency/177 (get_SWT0_CLK_Frequency) @070642a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  previous sharing asm name: 324
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: 
get_SIUL0_CLK_Frequency/176 (get_SIUL0_CLK_Frequency) @07064000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_QSPI0_TX_MEM_CLK_Frequency/175 (get_QSPI0_TX_MEM_CLK_Frequency) @07061b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_QSPI0_RAM_CLK_Frequency/323 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_QSPI0_RAM_CLK_Frequency/174 (get_QSPI0_RAM_CLK_Frequency) @07061620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  previous sharing asm name: 323
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: 
get_DCM0_CLK_Frequency/173 (get_DCM0_CLK_Frequency) @070610e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
get_SEMA42_CLK_Frequency/172 (get_SEMA42_CLK_Frequency) @07061d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/322 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_MSCM_CLK_Frequency/171 (get_MSCM_CLK_Frequency) @07061a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/321 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART8_CLK_Frequency/170 (get_LPUART8_CLK_Frequency) @070617e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/320 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART0_CLK_Frequency/169 (get_LPUART0_CLK_Frequency) @07061540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/319 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPSPI0_CLK_Frequency/168 (get_LPSPI0_CLK_Frequency) @070612a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/318 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_INTM_CLK_Frequency/167 (get_INTM_CLK_Frequency) @07061000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/317 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_FLEXIO0_CLK_Frequency/166 (get_FLEXIO0_CLK_Frequency) @0705eb60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CRC0_CLK_Frequency/316 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_CRC0_CLK_Frequency/165 (get_CRC0_CLK_Frequency) @0705e620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  previous sharing asm name: 316
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: 
get_WKPU0_CLK_Frequency/164 (get_WKPU0_CLK_Frequency) @0705e0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/315 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_TSENSE0_CLK_Frequency/163 (get_TSENSE0_CLK_Frequency) @0705ed20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/314 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_TRGMUX0_CLK_Frequency/162 (get_TRGMUX0_CLK_Frequency) @0705ea80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/313 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_STCU0_CLK_Frequency/161 (get_STCU0_CLK_Frequency) @0705e7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/312 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_SAI1_CLK_Frequency/160 (get_SAI1_CLK_Frequency) @0705e540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/311 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_SAI0_CLK_Frequency/159 (get_SAI0_CLK_Frequency) @0705e2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/310 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_PIT2_CLK_Frequency/158 (get_PIT2_CLK_Frequency) @0705e000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/309 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_PIT1_CLK_Frequency/157 (get_PIT1_CLK_Frequency) @07057b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/308 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_PIT0_CLK_Frequency/156 (get_PIT0_CLK_Frequency) @07057620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/307 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_MUB_CLK_Frequency/155 (get_MUB_CLK_Frequency) @070570e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/306 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_MUA_CLK_Frequency/154 (get_MUA_CLK_Frequency) @07057d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/305 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART9_CLK_Frequency/153 (get_LPUART9_CLK_Frequency) @07057a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/304 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART7_CLK_Frequency/152 (get_LPUART7_CLK_Frequency) @070577e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/303 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART6_CLK_Frequency/151 (get_LPUART6_CLK_Frequency) @07057540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/302 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART5_CLK_Frequency/150 (get_LPUART5_CLK_Frequency) @070572a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/301 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART4_CLK_Frequency/149 (get_LPUART4_CLK_Frequency) @07057000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/300 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART3_CLK_Frequency/148 (get_LPUART3_CLK_Frequency) @07054b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/299 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART2_CLK_Frequency/147 (get_LPUART2_CLK_Frequency) @07054620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/298 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART1_CLK_Frequency/146 (get_LPUART1_CLK_Frequency) @070540e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/297 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART15_CLK_Frequency/145 (get_LPUART15_CLK_Frequency) @07054d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/296 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART14_CLK_Frequency/144 (get_LPUART14_CLK_Frequency) @07054a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/295 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART13_CLK_Frequency/143 (get_LPUART13_CLK_Frequency) @070547e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/294 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART12_CLK_Frequency/142 (get_LPUART12_CLK_Frequency) @07054540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/293 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART11_CLK_Frequency/141 (get_LPUART11_CLK_Frequency) @070542a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/292 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPUART10_CLK_Frequency/140 (get_LPUART10_CLK_Frequency) @07054000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/291 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPSPI5_CLK_Frequency/139 (get_LPSPI5_CLK_Frequency) @07051b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/290 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPSPI4_CLK_Frequency/138 (get_LPSPI4_CLK_Frequency) @07051620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/289 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPSPI3_CLK_Frequency/137 (get_LPSPI3_CLK_Frequency) @070510e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/288 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPSPI2_CLK_Frequency/136 (get_LPSPI2_CLK_Frequency) @07051d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/287 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPSPI1_CLK_Frequency/135 (get_LPSPI1_CLK_Frequency) @07051a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/286 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPI2C1_CLK_Frequency/134 (get_LPI2C1_CLK_Frequency) @070517e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/285 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LPI2C0_CLK_Frequency/133 (get_LPI2C0_CLK_Frequency) @07051540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/284 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_FLASH0_CLK_Frequency/132 (get_FLASH0_CLK_Frequency) @070512a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/283 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_ERM0_CLK_Frequency/131 (get_ERM0_CLK_Frequency) @07051000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/282 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EIM0_CLK_Frequency/130 (get_EIM0_CLK_Frequency) @0704eb60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/281 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_CMP2_CLK_Frequency/129 (get_CMP2_CLK_Frequency) @0704e620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/280 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_CMP1_CLK_Frequency/128 (get_CMP1_CLK_Frequency) @0704e0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_CMP0_CLK_Frequency/279 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_CMP0_CLK_Frequency/127 (get_CMP0_CLK_Frequency) @0704ed20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  previous sharing asm name: 279
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: 
get_TEMPSENSE_CLK_Frequency/126 (get_TEMPSENSE_CLK_Frequency) @0704ea80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/278 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_TCM_CM7_1_CLK_Frequency/125 (get_TCM_CM7_1_CLK_Frequency) @0704e7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/277 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_TCM_CM7_0_CLK_Frequency/124 (get_TCM_CM7_0_CLK_Frequency) @0704e540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/276 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LCU1_CLK_Frequency/123 (get_LCU1_CLK_Frequency) @0704e2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/275 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_LCU0_CLK_Frequency/122 (get_LCU0_CLK_Frequency) @0704e000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/274 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EMIOS2_CLK_Frequency/121 (get_EMIOS2_CLK_Frequency) @07048b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/273 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EMIOS1_CLK_Frequency/120 (get_EMIOS1_CLK_Frequency) @07048620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/272 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EMIOS0_CLK_Frequency/119 (get_EMIOS0_CLK_Frequency) @070480e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/271 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD9_CLK_Frequency/118 (get_EDMA0_TCD9_CLK_Frequency) @07048d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/270 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD8_CLK_Frequency/117 (get_EDMA0_TCD8_CLK_Frequency) @07048a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/269 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD7_CLK_Frequency/116 (get_EDMA0_TCD7_CLK_Frequency) @070487e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/268 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD6_CLK_Frequency/115 (get_EDMA0_TCD6_CLK_Frequency) @07048540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/267 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD5_CLK_Frequency/114 (get_EDMA0_TCD5_CLK_Frequency) @070482a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/266 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD4_CLK_Frequency/113 (get_EDMA0_TCD4_CLK_Frequency) @07048000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/265 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD3_CLK_Frequency/112 (get_EDMA0_TCD3_CLK_Frequency) @07046b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/264 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD31_CLK_Frequency/111 (get_EDMA0_TCD31_CLK_Frequency) @07046620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/263 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD30_CLK_Frequency/110 (get_EDMA0_TCD30_CLK_Frequency) @070460e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/262 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD2_CLK_Frequency/109 (get_EDMA0_TCD2_CLK_Frequency) @07046d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/261 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD29_CLK_Frequency/108 (get_EDMA0_TCD29_CLK_Frequency) @07046a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/260 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD28_CLK_Frequency/107 (get_EDMA0_TCD28_CLK_Frequency) @070467e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/259 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD27_CLK_Frequency/106 (get_EDMA0_TCD27_CLK_Frequency) @07046540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/258 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD26_CLK_Frequency/105 (get_EDMA0_TCD26_CLK_Frequency) @070462a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/257 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD25_CLK_Frequency/104 (get_EDMA0_TCD25_CLK_Frequency) @07046000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/256 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD24_CLK_Frequency/103 (get_EDMA0_TCD24_CLK_Frequency) @07043b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/255 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD23_CLK_Frequency/102 (get_EDMA0_TCD23_CLK_Frequency) @07043620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/254 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD22_CLK_Frequency/101 (get_EDMA0_TCD22_CLK_Frequency) @070430e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/253 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD21_CLK_Frequency/100 (get_EDMA0_TCD21_CLK_Frequency) @07043d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/252 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD20_CLK_Frequency/99 (get_EDMA0_TCD20_CLK_Frequency) @07043a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/251 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD1_CLK_Frequency/98 (get_EDMA0_TCD1_CLK_Frequency) @070437e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/250 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD19_CLK_Frequency/97 (get_EDMA0_TCD19_CLK_Frequency) @07043540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/249 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD18_CLK_Frequency/96 (get_EDMA0_TCD18_CLK_Frequency) @070432a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/248 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD17_CLK_Frequency/95 (get_EDMA0_TCD17_CLK_Frequency) @07043000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/247 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD16_CLK_Frequency/94 (get_EDMA0_TCD16_CLK_Frequency) @0703eb60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/246 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD15_CLK_Frequency/93 (get_EDMA0_TCD15_CLK_Frequency) @0703e620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/245 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD14_CLK_Frequency/92 (get_EDMA0_TCD14_CLK_Frequency) @0703e0e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/244 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD13_CLK_Frequency/91 (get_EDMA0_TCD13_CLK_Frequency) @0703ed20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/243 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD12_CLK_Frequency/90 (get_EDMA0_TCD12_CLK_Frequency) @0703ea80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/242 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD11_CLK_Frequency/89 (get_EDMA0_TCD11_CLK_Frequency) @0703e7e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/241 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD10_CLK_Frequency/88 (get_EDMA0_TCD10_CLK_Frequency) @0703e540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/240 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_TCD0_CLK_Frequency/87 (get_EDMA0_TCD0_CLK_Frequency) @0703e2a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/239 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_EDMA0_CLK_Frequency/86 (get_EDMA0_CLK_Frequency) @0703e000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/238 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_DMAMUX1_CLK_Frequency/85 (get_DMAMUX1_CLK_Frequency) @07038a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/237 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_DMAMUX0_CLK_Frequency/84 (get_DMAMUX0_CLK_Frequency) @07038540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/236 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_BCTU0_CLK_Frequency/83 (get_BCTU0_CLK_Frequency) @07038ee0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/235 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_ADC2_CLK_Frequency/82 (get_ADC2_CLK_Frequency) @07038c40
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/234 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_ADC1_CLK_Frequency/81 (get_ADC1_CLK_Frequency) @070389a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: get_ADC0_CLK_Frequency/233 (inlined) (1073741824 (estimated locally),1.00 per call) 
get_ADC0_CLK_Frequency/80 (get_ADC0_CLK_Frequency) @07038700
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  previous sharing asm name: 233
  Address is taken.
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: consumerClockCallbacks/79 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body icf_merged optimize_size
  Called by: 
  Calls: 
consumerClockCallbacks/79 (consumerClockCallbacks) @07037240
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: get_ADC0_CLK_Frequency/80 (addr)get_ADC1_CLK_Frequency/81 (addr)get_ADC2_CLK_Frequency/82 (addr)get_BCTU0_CLK_Frequency/83 (addr)get_CLKOUT_STANDBY_CLK_Frequency/179 (addr)get_CMP0_CLK_Frequency/127 (addr)get_CMP1_CLK_Frequency/128 (addr)get_CMP2_CLK_Frequency/129 (addr)get_CRC0_CLK_Frequency/165 (addr)get_DCM0_CLK_Frequency/173 (addr)get_DMAMUX0_CLK_Frequency/84 (addr)get_DMAMUX1_CLK_Frequency/85 (addr)get_EDMA0_CLK_Frequency/86 (addr)get_EDMA0_TCD0_CLK_Frequency/87 (addr)get_EDMA0_TCD10_CLK_Frequency/88 (addr)get_EDMA0_TCD11_CLK_Frequency/89 (addr)get_EDMA0_TCD12_CLK_Frequency/90 (addr)get_EDMA0_TCD13_CLK_Frequency/91 (addr)get_EDMA0_TCD14_CLK_Frequency/92 (addr)get_EDMA0_TCD15_CLK_Frequency/93 (addr)get_EDMA0_TCD16_CLK_Frequency/94 (addr)get_EDMA0_TCD17_CLK_Frequency/95 (addr)get_EDMA0_TCD18_CLK_Frequency/96 (addr)get_EDMA0_TCD19_CLK_Frequency/97 (addr)get_EDMA0_TCD1_CLK_Frequency/98 (addr)get_EDMA0_TCD20_CLK_Frequency/99 (addr)get_EDMA0_TCD21_CLK_Frequency/100 (addr)get_EDMA0_TCD22_CLK_Frequency/101 (addr)get_EDMA0_TCD23_CLK_Frequency/102 (addr)get_EDMA0_TCD24_CLK_Frequency/103 (addr)get_EDMA0_TCD25_CLK_Frequency/104 (addr)get_EDMA0_TCD26_CLK_Frequency/105 (addr)get_EDMA0_TCD27_CLK_Frequency/106 (addr)get_EDMA0_TCD28_CLK_Frequency/107 (addr)get_EDMA0_TCD29_CLK_Frequency/108 (addr)get_EDMA0_TCD2_CLK_Frequency/109 (addr)get_EDMA0_TCD30_CLK_Frequency/110 (addr)get_EDMA0_TCD31_CLK_Frequency/111 (addr)get_EDMA0_TCD3_CLK_Frequency/112 (addr)get_EDMA0_TCD4_CLK_Frequency/113 (addr)get_EDMA0_TCD5_CLK_Frequency/114 (addr)get_EDMA0_TCD6_CLK_Frequency/115 (addr)get_EDMA0_TCD7_CLK_Frequency/116 (addr)get_EDMA0_TCD8_CLK_Frequency/117 (addr)get_EDMA0_TCD9_CLK_Frequency/118 (addr)get_EIM0_CLK_Frequency/130 (addr)get_EMAC_RX_CLK_Frequency/180 (addr)get_EMAC0_RX_CLK_Frequency/181 (addr)get_EMAC_TS_CLK_Frequency/182 (addr)get_EMAC0_TS_CLK_Frequency/183 (addr)get_EMAC_TX_CLK_Frequency/184 (addr)get_EMAC0_TX_CLK_Frequency/185 (addr)get_EMIOS0_CLK_Frequency/119 (addr)get_EMIOS1_CLK_Frequency/120 (addr)get_EMIOS2_CLK_Frequency/121 (addr)get_ERM0_CLK_Frequency/131 (addr)get_FLASH0_CLK_Frequency/132 (addr)get_FLEXCANA_CLK_Frequency/186 (addr)get_FLEXCAN0_CLK_Frequency/187 (addr)get_FLEXCAN1_CLK_Frequency/188 (addr)get_FLEXCAN2_CLK_Frequency/189 (addr)get_FLEXCANB_CLK_Frequency/190 (addr)get_FLEXCAN3_CLK_Frequency/191 (addr)get_FLEXCAN4_CLK_Frequency/192 (addr)get_FLEXCAN5_CLK_Frequency/193 (addr)get_FLEXIO0_CLK_Frequency/166 (addr)get_INTM_CLK_Frequency/167 (addr)get_LCU0_CLK_Frequency/122 (addr)get_LCU1_CLK_Frequency/123 (addr)get_LPI2C0_CLK_Frequency/133 (addr)get_LPI2C1_CLK_Frequency/134 (addr)get_LPSPI0_CLK_Frequency/168 (addr)get_LPSPI1_CLK_Frequency/135 (addr)get_LPSPI2_CLK_Frequency/136 (addr)get_LPSPI3_CLK_Frequency/137 (addr)get_LPSPI4_CLK_Frequency/138 (addr)get_LPSPI5_CLK_Frequency/139 (addr)get_LPUART0_CLK_Frequency/169 (addr)get_LPUART10_CLK_Frequency/140 (addr)get_LPUART11_CLK_Frequency/141 (addr)get_LPUART12_CLK_Frequency/142 (addr)get_LPUART13_CLK_Frequency/143 (addr)get_LPUART14_CLK_Frequency/144 (addr)get_LPUART15_CLK_Frequency/145 (addr)get_LPUART1_CLK_Frequency/146 (addr)get_LPUART2_CLK_Frequency/147 (addr)get_LPUART3_CLK_Frequency/148 (addr)get_LPUART4_CLK_Frequency/149 (addr)get_LPUART5_CLK_Frequency/150 (addr)get_LPUART6_CLK_Frequency/151 (addr)get_LPUART7_CLK_Frequency/152 (addr)get_LPUART8_CLK_Frequency/170 (addr)get_LPUART9_CLK_Frequency/153 (addr)get_MSCM_CLK_Frequency/171 (addr)get_MUA_CLK_Frequency/154 (addr)get_MUB_CLK_Frequency/155 (addr)get_PIT0_CLK_Frequency/156 (addr)get_PIT1_CLK_Frequency/157 (addr)get_PIT2_CLK_Frequency/158 (addr)get_QSPI0_RAM_CLK_Frequency/174 (addr)get_QSPI_SFCK_CLK_Frequency/194 (addr)get_QSPI0_SFCK_CLK_Frequency/195 (addr)get_QSPI0_TX_MEM_CLK_Frequency/175 (addr)get_RTC_CLK_Frequency/196 (addr)get_RTC0_CLK_Frequency/197 (addr)get_SAI0_CLK_Frequency/159 (addr)get_SAI1_CLK_Frequency/160 (addr)get_SEMA42_CLK_Frequency/172 (addr)get_SIUL0_CLK_Frequency/176 (addr)get_STCU0_CLK_Frequency/161 (addr)get_STMA_CLK_Frequency/198 (addr)get_STM0_CLK_Frequency/199 (addr)get_STMB_CLK_Frequency/200 (addr)get_STM1_CLK_Frequency/201 (addr)get_SWT0_CLK_Frequency/177 (addr)get_SWT1_CLK_Frequency/178 (addr)get_TCM_CM7_0_CLK_Frequency/124 (addr)get_TCM_CM7_1_CLK_Frequency/125 (addr)get_TEMPSENSE_CLK_Frequency/126 (addr)get_TRACE_CLK_Frequency/202 (addr)get_TRGMUX0_CLK_Frequency/162 (addr)get_TSENSE0_CLK_Frequency/163 (addr)get_WKPU0_CLK_Frequency/164 (addr)
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
calcFreqCallbacks/78 (calcFreqCallbacks) @06f84ea0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: CONFIG_ELEMENTS_MAPPINGS_01/42 (addr)CONFIG_ELEMENTS_MAPPINGS_02/43 (addr)NOT_UNDER_MCU_CONTROL_A/44 (addr)NOT_UNDER_MCU_CONTROL_B/45 (addr)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (addr)PLL_A/47 (addr)PLL_B/48 (addr)PLL_C/49 (addr)IntegerDividers_A/50 (addr)IntegerDividers_B/51 (addr)IntegerDividers_C/52 (addr)IntegerDividers_D/53 (addr)IntegerDividers_E/54 (addr)IntegerDividers_F/55 (addr)IntegerDividers_G/56 (addr)IntegerDividers_H/57 (addr)IntegerDividers_I/58 (addr)IntegerDividers_J/59 (addr)IntegerDividers_K/60 (addr)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (addr)PCFS_PLL_PHI0_A/62 (addr)PCFS_PLL_PHI0_B/63 (addr)PCFS_PLL_PHI0_C/64 (addr)PCFS_PLL_PHI0_D/65 (addr)PCFS_PLL_PHI0_E/66 (addr)CMU_FXOSC_CLK_A/67 (addr)CMU_FXOSC_CLK_B/68 (addr)CMU_CORE_CLK_A/69 (addr)CMU_CORE_CLK_B/70 (addr)CMU_AIPS_PLAT_CLK_A/71 (addr)CMU_AIPS_PLAT_CLK_B/72 (addr)CMU_HSE_CLK_A/73 (addr)CMU_HSE_CLK_B/74 (addr)CallEmptyCallbacks/76 (addr)CallbackDelay/77 (addr)
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
CallbackDelay/77 (CallbackDelay) @06fda460
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: 
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:118111600 (estimated locally) body optimize_size
  Called by: 
  Calls: ClockTimeoutExpired/216 (1073741824 (estimated locally),9.09 per call) ClockStartTimeout/215 (118111600 (estimated locally),1.00 per call) 
CallEmptyCallbacks/76 (CallEmptyCallbacks) @06fda1c0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuCallbacks/217 (read)cmuCallbacks/217 (read)cmuCallbacks/217 (read)cmuCallbacks/217 (read)dividerCallbacks/218 (read)dividerTriggerCallbacks/219 (read)extOscCallbacks/220 (read)fracDivCallbacks/221 (read)fracDivCallbacks/221 (read)gateCallbacks/222 (read)gateCallbacks/222 (read)intOscCallbacks/223 (read)pllCallbacks/224 (read)pllCallbacks/224 (read)selectorCallbacks/225 (read)pcfsCallbacks/226 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
   Indirect call(1073741824 (estimated locally),1.00 per call) 
McMeEnterKey/75 (McMeEnterKey) @06fd2e00
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_HSE_CLK_B/74 (CMU_HSE_CLK_B) @06fd2d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_HSE_CLK_A/73 (CMU_HSE_CLK_A) @06fd2a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)configuredHseClock/32 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_AIPS_PLAT_CLK_B/72 (CMU_AIPS_PLAT_CLK_B) @06fd27e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_AIPS_PLAT_CLK_A/71 (CMU_AIPS_PLAT_CLK_A) @06fd2540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)configuredAipsPlatClock/30 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_CORE_CLK_B/70 (CMU_CORE_CLK_B) @06fd22a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_CORE_CLK_A/69 (CMU_CORE_CLK_A) @06fd2000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)configuredCoreClock/29 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_FXOSC_CLK_B/68 (CMU_FXOSC_CLK_B) @06f86d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)cmuEntries/35 (read)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CMU_FXOSC_CLK_A/67 (CMU_FXOSC_CLK_A) @06f86a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: cmuEntries/35 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (read)configuredAipsSlowClock/31 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)cmuEntries/35 (write)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_E/66 (PCFS_PLL_PHI0_E) @06f867e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)pcfsEntries/34 (write)pcfsEntries/34 (write)pcfsEntries/34 (write)pcfsEntries/34 (write)pcfsEntries/34 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_D/65 (PCFS_PLL_PHI0_D) @06f86540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:118111600 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_C/64 (PCFS_PLL_PHI0_C) @06f862a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:118111600 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_B/63 (PCFS_PLL_PHI0_B) @06f86000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: *.LC0/227 (read)*.LC1/228 (read)tmpData/28 (read)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:357985524 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PCFS_PLL_PHI0_A/62 (PCFS_PLL_PHI0_A) @06f78d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: pcfsEntries/34 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS) @06f78a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: config_clock/33 (read)bufferFreqs/25 (read)configuredCoreClock/29 (write)bufferFreqs/25 (read)configuredAipsPlatClock/30 (write)bufferFreqs/25 (read)configuredAipsSlowClock/31 (write)bufferFreqs/25 (read)configuredHseClock/32 (write)configuredCoreClock/29 (write)configuredAipsPlatClock/30 (write)configuredAipsSlowClock/31 (write)configuredHseClock/32 (write)configuredCoreClock/29 (write)configuredAipsPlatClock/30 (write)configuredAipsSlowClock/31 (write)configuredHseClock/32 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:114863532 (estimated locally) body optimize_size
  Called by: 
  Calls: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (inlined) (26801491 (estimated locally),0.23 per call) 
IntegerDividers_K/60 (IntegerDividers_K) @06f787e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_J/59 (IntegerDividers_J) @06f78540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_I/58 (IntegerDividers_I) @06f782a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_H/57 (IntegerDividers_H) @06f78000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_G/56 (IntegerDividers_G) @06f20d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_F/55 (IntegerDividers_F) @06f20a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (read)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_E/54 (IntegerDividers_E) @06f207e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_D/53 (IntegerDividers_D) @06f20540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_C/52 (IntegerDividers_C) @06f202a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_B/51 (IntegerDividers_B) @06f20000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IntegerDividers_A/50 (IntegerDividers_A) @06f15d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PLL_C/49 (PLL_C) @06f15a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)bufferFreqs/25 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PLL_B/48 (PLL_B) @06f157e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: tmpData/28 (read)tmpData/28 (write)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
PLL_A/47 (PLL_A) @06f15540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: bufferFreqs/25 (read)tmpData/28 (write)freqPointers/26 (read)config_clock/33 (read)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (write)tmpData/28 (read)tmpData/28 (read)tmpData/28 (write)tmpData/28 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS) @06f152a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (write)freqPointers/26 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (read)config_clock/33 (read)bufferFreqs/25 (write)bufferFreqs/25 (write)freqPointers/26 (write)freqPointers/26 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
NOT_UNDER_MCU_CONTROL_B/45 (NOT_UNDER_MCU_CONTROL_B) @06f15000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (read)clkState/27 (write)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)clkState/27 (write)clkState/27 (write)clkState/27 (write)freqPointers/26 (read)selectorEntryIndex/23 (read)clkState/27 (write)freqPointers/26 (read)selectorEntryIndex/23 (read)clkState/27 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
NOT_UNDER_MCU_CONTROL_A/44 (NOT_UNDER_MCU_CONTROL_A) @06ebcee0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: clkState/27 (write)freqPointers/26 (read)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)clkState/27 (write)freqPointers/26 (read)clkState/27 (write)freqPointers/26 (read)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: NOT_UNDER_MCU_CONTROL_A.part.0/230 (inlined) (536870912 (estimated locally),0.50 per call) 
CONFIG_ELEMENTS_MAPPINGS_02/43 (CONFIG_ELEMENTS_MAPPINGS_02) @06ebcc40
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (write)config_clock/33 (read)freqPointers/26 (write)freqPointers/26 (write)pcfsEntries/34 (read)pcfsEntries/34 (write)cmuEntries/35 (read)cmuEntries/35 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:7299031 (estimated locally) body optimize_size
  Called by: 
  Calls: 
CONFIG_ELEMENTS_MAPPINGS_01/42 (CONFIG_ELEMENTS_MAPPINGS_01) @06ebc9a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  Address is taken.
  References: freqPointers/26 (write)
  Referring: calcFreqCallbacks/78 (addr)
  Availability: available
  Function flags: count:46707770 (estimated locally) body optimize_size
  Called by: 
  Calls: CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (inlined) (46707769 (estimated locally),1.00 per call) 
UpdateFrequencies/41 (UpdateFrequencies) @06ebc700
  Type: function definition analyzed
  Visibility: externally_visible public
  References: clkState/27 (read)freqPointers/26 (write)clkState/27 (read)freqPointers/26 (write)clkState/27 (read)clkState/27 (read)freqPointers/26 (write)clkState/27 (read)freqPointers/26 (write)freqPointers/26 (write)clkState/27 (read)convertValueToClockState.5133/203 (read)clkState/27 (write)clkState/27 (read)convertValueToClockState.5133/203 (read)clkState/27 (write)freqPointers/26 (write)freqPointers/26 (write)clkState/27 (read)selectorEntriesSCS_CLK.5122/204 (read)clkState/27 (read)bufferFreqEntriesSCS_CLK.5123/205 (read)freqPointers/26 (write)bufferFreqEntriesCORE_CLK.5124/206 (read)freqPointers/26 (write)bufferFreqEntriesAIPS_PLAT_CLK.5125/207 (read)freqPointers/26 (write)bufferFreqEntriesAIPS_SLOW_CLK.5126/208 (read)freqPointers/26 (write)bufferFreqEntriesHSE_CLK.5127/209 (read)freqPointers/26 (write)bufferFreqEntriesDCM_CLK.5128/210 (read)freqPointers/26 (write)bufferFreqEntriesLBIST_CLK.5129/211 (read)freqPointers/26 (write)bufferFreqEntriesQSPI_MEM_CLK.5130/212 (read)freqPointers/26 (write)selectorEntryIndex/23 (read)clkState/27 (write)selectorEntriesCLKOUT_RUN_CLK.5131/213 (read)clkState/27 (read)bufferFreqEntriesCLKOUT_RUN_CLK.5132/214 (read)freqPointers/26 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
GetProducerClockFreq/40 (GetProducerClockFreq) @06ebc000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: freqPointers/26 (read)bufferFreqs/25 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
SpecificPlatformInitClock/39 (SpecificPlatformInitClock) @06eb7a80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: config_clock/33 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
SpecificPeripheralClockInitialization/38 (SpecificPeripheralClockInitialization) @06eb7ee0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
GetClockState/37 (GetClockState) @06eb7c40
  Type: function definition analyzed
  Visibility: externally_visible public
  References: clkState/27 (read)clkState/27 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
UpdateClockState/36 (UpdateClockState) @06eb79a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: clkState/27 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
cmuEntries/35 (cmuEntries) @06eb4870
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: CMU_FXOSC_CLK_A/67 (write)CMU_AIPS_PLAT_CLK_B/72 (read)CMU_AIPS_PLAT_CLK_B/72 (write)CMU_AIPS_PLAT_CLK_B/72 (write)CMU_HSE_CLK_A/73 (read)CMU_AIPS_PLAT_CLK_A/71 (read)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (read)CMU_CORE_CLK_B/70 (read)CMU_CORE_CLK_B/70 (write)CMU_CORE_CLK_B/70 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CMU_CORE_CLK_A/69 (read)CMU_CORE_CLK_A/69 (write)CMU_CORE_CLK_A/69 (write)CMU_HSE_CLK_A/73 (write)CMU_FXOSC_CLK_B/68 (read)CMU_FXOSC_CLK_B/68 (write)CMU_FXOSC_CLK_B/68 (write)CMU_HSE_CLK_A/73 (write)CMU_FXOSC_CLK_A/67 (read)CMU_FXOSC_CLK_A/67 (write)CMU_HSE_CLK_B/74 (read)CMU_HSE_CLK_B/74 (write)CMU_HSE_CLK_B/74 (write)
  Availability: available
  Varpool flags: initialized
pcfsEntries/34 (pcfsEntries) @06eb4708
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CONFIG_ELEMENTS_MAPPINGS_02/43 (read)PCFS_PLL_PHI0_A/62 (read)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)PCFS_PLL_PHI0_E/66 (write)
  Availability: available
  Varpool flags: initialized
config_clock/33 (config_clock) @06eb4678
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CMU_AIPS_PLAT_CLK_A/71 (read)CMU_CORE_CLK_A/69 (read)CMU_FXOSC_CLK_A/67 (read)PCFS_PLL_PHI0_A/62 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)IntegerDividers_K/60 (read)IntegerDividers_J/59 (read)IntegerDividers_J/59 (read)IntegerDividers_J/59 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)IntegerDividers_F/55 (read)IntegerDividers_F/55 (read)IntegerDividers_F/55 (read)IntegerDividers_E/54 (read)IntegerDividers_E/54 (read)IntegerDividers_E/54 (read)IntegerDividers_D/53 (read)IntegerDividers_D/53 (read)IntegerDividers_D/53 (read)IntegerDividers_C/52 (read)IntegerDividers_C/52 (read)IntegerDividers_C/52 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)PLL_A/47 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (read)IntegerDividers_K/60 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)CONFIG_ELEMENTS_MAPPINGS_02/43 (read)IntegerDividers_K/60 (read)CMU_HSE_CLK_A/73 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)SpecificPlatformInitClock/39 (write)
  Availability: available
  Varpool flags: initialized
configuredHseClock/32 (configuredHseClock) @06eb4480
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_HSE_CLK_A/73 (read)
  Availability: available
  Varpool flags: initialized
configuredAipsSlowClock/31 (configuredAipsSlowClock) @06eb43f0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CMU_CORE_CLK_A/69 (read)CMU_FXOSC_CLK_A/67 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_AIPS_PLAT_CLK_A/71 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_HSE_CLK_A/73 (read)
  Availability: available
  Varpool flags: initialized
configuredAipsPlatClock/30 (configuredAipsPlatClock) @06eb4360
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_AIPS_PLAT_CLK_A/71 (read)
  Availability: available
  Varpool flags: initialized
configuredCoreClock/29 (configuredCoreClock) @06eb42d0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (write)CMU_CORE_CLK_A/69 (read)
  Availability: available
  Varpool flags: initialized
tmpData/28 (tmpData) @06eb4240
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CMU_AIPS_PLAT_CLK_B/72 (read)CMU_AIPS_PLAT_CLK_B/72 (read)CMU_CORE_CLK_A/69 (write)CMU_CORE_CLK_A/69 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_CORE_CLK_B/70 (read)CMU_CORE_CLK_B/70 (read)CMU_FXOSC_CLK_A/67 (write)CMU_FXOSC_CLK_A/67 (write)CMU_CORE_CLK_A/69 (write)CMU_CORE_CLK_A/69 (write)CMU_FXOSC_CLK_B/68 (read)CMU_FXOSC_CLK_B/68 (read)PCFS_PLL_PHI0_E/66 (read)PCFS_PLL_PHI0_E/66 (read)CMU_FXOSC_CLK_A/67 (write)CMU_FXOSC_CLK_A/67 (write)PCFS_PLL_PHI0_E/66 (read)PCFS_PLL_PHI0_E/66 (read)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_D/65 (write)PCFS_PLL_PHI0_D/65 (write)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_C/64 (read)PCFS_PLL_PHI0_C/64 (write)PCFS_PLL_PHI0_C/64 (write)PCFS_PLL_PHI0_C/64 (write)PCFS_PLL_PHI0_C/64 (read)PLL_A/47 (write)PCFS_PLL_PHI0_C/64 (read)PCFS_PLL_PHI0_C/64 (read)PCFS_PLL_PHI0_D/65 (write)CMU_AIPS_PLAT_CLK_A/71 (write)CMU_AIPS_PLAT_CLK_A/71 (write)PLL_C/49 (read)PLL_C/49 (read)PLL_C/49 (read)PLL_C/49 (read)PLL_C/49 (read)PCFS_PLL_PHI0_A/62 (write)PCFS_PLL_PHI0_A/62 (write)PCFS_PLL_PHI0_B/63 (read)PCFS_PLL_PHI0_B/63 (write)CMU_HSE_CLK_A/73 (write)CMU_HSE_CLK_A/73 (write)PLL_B/48 (read)PLL_B/48 (write)PLL_B/48 (read)PLL_C/49 (read)PLL_C/49 (read)PCFS_PLL_PHI0_A/62 (write)PCFS_PLL_PHI0_A/62 (write)PLL_C/49 (read)PLL_C/49 (write)PLL_B/48 (write)PLL_B/48 (write)PLL_B/48 (read)PLL_B/48 (write)PLL_A/47 (read)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (write)PLL_A/47 (read)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_D/65 (read)PCFS_PLL_PHI0_D/65 (write)PCFS_PLL_PHI0_E/66 (read)CMU_HSE_CLK_A/73 (write)CMU_HSE_CLK_A/73 (write)CMU_HSE_CLK_B/74 (read)CMU_HSE_CLK_B/74 (read)
  Availability: available
  Varpool flags:
clkState/27 (clkState) @06eb41b0
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_A.part.0/230 (write)NOT_UNDER_MCU_CONTROL_A.part.0/230 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_A/44 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)UpdateClockState/36 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)NOT_UNDER_MCU_CONTROL_B/45 (write)GetClockState/37 (read)GetClockState/37 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (read)UpdateFrequencies/41 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags:
freqPointers/26 (freqPointers) @06eb4120
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: NOT_UNDER_MCU_CONTROL_B/45 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)get_FLEXCANA_CLK_Frequency/186 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)get_EMAC_TX_CLK_Frequency/184 (read)get_EMAC_TS_CLK_Frequency/182 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)GetProducerClockFreq/40 (read)UpdateFrequencies/41 (write)get_TRACE_CLK_Frequency/202 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_SWT0_CLK_Frequency/177 (read)get_QSPI0_RAM_CLK_Frequency/174 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)IntegerDividers_I/58 (read)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)UpdateFrequencies/41 (write)NOT_UNDER_MCU_CONTROL_A/44 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)IntegerDividers_H/57 (read)get_ADC0_CLK_Frequency/80 (read)get_DCM0_CLK_Frequency/173 (read)UpdateFrequencies/41 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)IntegerDividers_G/56 (read)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)IntegerDividers_K/60 (read)IntegerDividers_F/55 (read)IntegerDividers_F/55 (read)IntegerDividers_J/59 (read)get_STMA_CLK_Frequency/198 (read)get_SIUL0_CLK_Frequency/176 (read)get_CRC0_CLK_Frequency/165 (read)CONFIG_ELEMENTS_MAPPINGS_01.part.0/229 (write)IntegerDividers_E/54 (read)CONFIG_ELEMENTS_MAPPINGS_01/42 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)IntegerDividers_D/53 (read)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)UpdateFrequencies/41 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (read)UpdateFrequencies/41 (write)get_FLEXCANB_CLK_Frequency/190 (read)get_CMP0_CLK_Frequency/127 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)IntegerDividers_B/51 (read)CONFIG_ELEMENTS_MAPPINGS_02/43 (write)get_STMB_CLK_Frequency/200 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IntegerDividers_A/50 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (read)PLL_A/47 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)NOT_UNDER_MCU_CONTROL_A/44 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)get_ADC0_CLK_Frequency/233 (read)get_ADC0_CLK_Frequency/234 (read)get_ADC0_CLK_Frequency/235 (read)get_ADC0_CLK_Frequency/236 (read)get_ADC0_CLK_Frequency/237 (read)get_ADC0_CLK_Frequency/238 (read)get_ADC0_CLK_Frequency/239 (read)get_ADC0_CLK_Frequency/240 (read)get_ADC0_CLK_Frequency/241 (read)get_ADC0_CLK_Frequency/242 (read)get_ADC0_CLK_Frequency/243 (read)get_ADC0_CLK_Frequency/244 (read)get_ADC0_CLK_Frequency/245 (read)get_ADC0_CLK_Frequency/246 (read)get_ADC0_CLK_Frequency/247 (read)get_ADC0_CLK_Frequency/248 (read)get_ADC0_CLK_Frequency/249 (read)get_ADC0_CLK_Frequency/250 (read)get_ADC0_CLK_Frequency/251 (read)get_ADC0_CLK_Frequency/252 (read)get_ADC0_CLK_Frequency/253 (read)get_ADC0_CLK_Frequency/254 (read)get_ADC0_CLK_Frequency/255 (read)get_ADC0_CLK_Frequency/256 (read)get_ADC0_CLK_Frequency/257 (read)get_ADC0_CLK_Frequency/258 (read)get_ADC0_CLK_Frequency/259 (read)get_ADC0_CLK_Frequency/260 (read)get_ADC0_CLK_Frequency/261 (read)get_ADC0_CLK_Frequency/262 (read)get_ADC0_CLK_Frequency/263 (read)get_ADC0_CLK_Frequency/264 (read)get_ADC0_CLK_Frequency/265 (read)get_ADC0_CLK_Frequency/266 (read)get_ADC0_CLK_Frequency/267 (read)get_ADC0_CLK_Frequency/268 (read)get_ADC0_CLK_Frequency/269 (read)get_ADC0_CLK_Frequency/270 (read)get_ADC0_CLK_Frequency/271 (read)get_ADC0_CLK_Frequency/272 (read)get_ADC0_CLK_Frequency/273 (read)get_ADC0_CLK_Frequency/274 (read)get_ADC0_CLK_Frequency/275 (read)get_ADC0_CLK_Frequency/276 (read)get_ADC0_CLK_Frequency/277 (read)get_ADC0_CLK_Frequency/278 (read)get_CMP0_CLK_Frequency/279 (read)get_CMP0_CLK_Frequency/280 (read)get_CMP0_CLK_Frequency/281 (read)get_CMP0_CLK_Frequency/282 (read)get_CMP0_CLK_Frequency/283 (read)get_CMP0_CLK_Frequency/284 (read)get_CMP0_CLK_Frequency/285 (read)get_CMP0_CLK_Frequency/286 (read)get_CMP0_CLK_Frequency/287 (read)get_CMP0_CLK_Frequency/288 (read)get_CMP0_CLK_Frequency/289 (read)get_CMP0_CLK_Frequency/290 (read)get_CMP0_CLK_Frequency/291 (read)get_CMP0_CLK_Frequency/292 (read)get_CMP0_CLK_Frequency/293 (read)get_CMP0_CLK_Frequency/294 (read)get_CMP0_CLK_Frequency/295 (read)get_CMP0_CLK_Frequency/296 (read)get_CMP0_CLK_Frequency/297 (read)get_CMP0_CLK_Frequency/298 (read)get_CMP0_CLK_Frequency/299 (read)get_CMP0_CLK_Frequency/300 (read)get_CMP0_CLK_Frequency/301 (read)get_CMP0_CLK_Frequency/302 (read)get_CMP0_CLK_Frequency/303 (read)get_CMP0_CLK_Frequency/304 (read)get_CMP0_CLK_Frequency/305 (read)get_CMP0_CLK_Frequency/306 (read)get_CMP0_CLK_Frequency/307 (read)get_CMP0_CLK_Frequency/308 (read)get_CMP0_CLK_Frequency/309 (read)get_CMP0_CLK_Frequency/310 (read)get_CMP0_CLK_Frequency/311 (read)get_CMP0_CLK_Frequency/312 (read)get_CMP0_CLK_Frequency/313 (read)get_CMP0_CLK_Frequency/314 (read)get_CMP0_CLK_Frequency/315 (read)get_CRC0_CLK_Frequency/316 (read)get_CRC0_CLK_Frequency/317 (read)get_CRC0_CLK_Frequency/318 (read)get_CRC0_CLK_Frequency/319 (read)get_CRC0_CLK_Frequency/320 (read)get_CRC0_CLK_Frequency/321 (read)get_CRC0_CLK_Frequency/322 (read)get_QSPI0_RAM_CLK_Frequency/323 (read)get_SWT0_CLK_Frequency/324 (read)
  Availability: available
  Varpool flags:
bufferFreqs/25 (bufferFreqs) @06eb4090
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)CMU_CORE_CLK_A/69 (read)CMU_FXOSC_CLK_A/67 (read)PCFS_PLL_PHI0_A/62 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)IntegerDividers_K/60 (write)IntegerDividers_K/60 (write)IntegerDividers_J/59 (write)IntegerDividers_J/59 (write)IntegerDividers_J/59 (read)IntegerDividers_J/59 (write)IntegerDividers_J/59 (write)IntegerDividers_J/59 (read)IntegerDividers_J/59 (write)IntegerDividers_J/59 (write)IntegerDividers_I/58 (read)IntegerDividers_I/58 (write)IntegerDividers_I/58 (write)IntegerDividers_I/58 (read)IntegerDividers_I/58 (write)IntegerDividers_I/58 (write)IntegerDividers_I/58 (read)IntegerDividers_I/58 (write)IntegerDividers_I/58 (write)IntegerDividers_H/57 (read)IntegerDividers_H/57 (write)IntegerDividers_H/57 (write)IntegerDividers_H/57 (read)IntegerDividers_H/57 (write)IntegerDividers_H/57 (write)IntegerDividers_H/57 (read)IntegerDividers_H/57 (write)IntegerDividers_H/57 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (write)IntegerDividers_G/56 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (write)IntegerDividers_G/56 (write)IntegerDividers_G/56 (read)IntegerDividers_G/56 (write)IntegerDividers_G/56 (write)IntegerDividers_F/55 (write)IntegerDividers_F/55 (write)IntegerDividers_F/55 (read)IntegerDividers_F/55 (write)IntegerDividers_F/55 (write)IntegerDividers_F/55 (read)IntegerDividers_F/55 (write)IntegerDividers_F/55 (read)IntegerDividers_F/55 (write)IntegerDividers_E/54 (read)IntegerDividers_E/54 (write)IntegerDividers_E/54 (write)IntegerDividers_E/54 (read)IntegerDividers_E/54 (write)IntegerDividers_E/54 (write)IntegerDividers_E/54 (read)IntegerDividers_E/54 (write)IntegerDividers_E/54 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IntegerDividers_D/53 (read)IntegerDividers_D/53 (write)IntegerDividers_D/53 (write)IntegerDividers_D/53 (read)IntegerDividers_D/53 (write)IntegerDividers_D/53 (write)IntegerDividers_D/53 (read)IntegerDividers_D/53 (write)IntegerDividers_D/53 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (write)IntegerDividers_C/52 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (write)IntegerDividers_C/52 (write)IntegerDividers_C/52 (read)IntegerDividers_C/52 (write)IntegerDividers_C/52 (write)IntegerDividers_B/51 (read)IntegerDividers_B/51 (write)IntegerDividers_B/51 (write)IntegerDividers_B/51 (read)IntegerDividers_B/51 (write)IntegerDividers_B/51 (write)IntegerDividers_B/51 (read)IntegerDividers_B/51 (write)IntegerDividers_B/51 (write)IntegerDividers_A/50 (read)IntegerDividers_A/50 (write)IntegerDividers_A/50 (write)IntegerDividers_A/50 (read)IntegerDividers_A/50 (write)IntegerDividers_A/50 (write)IntegerDividers_A/50 (read)IntegerDividers_A/50 (write)IntegerDividers_A/50 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)PLL_C/49 (write)IntegerDividers_J/59 (read)IntegerDividers_K/60 (write)IntegerDividers_K/60 (write)IntegerDividers_K/60 (read)IntegerDividers_K/60 (write)IntegerDividers_K/60 (write)IntegerDividers_K/60 (read)PCFS_PLL_PHI0_A/62 (read)PLL_A/47 (read)IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS/46 (write)get_TRACE_CLK_Frequency/202 (read)get_CRC0_CLK_Frequency/165 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_CMP0_CLK_Frequency/127 (read)get_FLEXCANB_CLK_Frequency/190 (read)IntegerDividers_K/60 (read)get_SWT0_CLK_Frequency/177 (read)GetProducerClockFreq/40 (read)get_ADC0_CLK_Frequency/80 (read)CMU_HSE_CLK_A/73 (read)CMU_AIPS_PLAT_CLK_A/71 (read)get_EMAC_TS_CLK_Frequency/182 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_STMB_CLK_Frequency/200 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)get_SIUL0_CLK_Frequency/176 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS.part.0/231 (read)get_DCM0_CLK_Frequency/173 (read)get_STMA_CLK_Frequency/198 (read)CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS/61 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)IntegerDividers_F/55 (read)get_QSPI0_RAM_CLK_Frequency/174 (read)CMU_FXOSC_CLK_A/67 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)get_ADC0_CLK_Frequency/233 (read)get_ADC0_CLK_Frequency/234 (read)get_ADC0_CLK_Frequency/235 (read)get_ADC0_CLK_Frequency/236 (read)get_ADC0_CLK_Frequency/237 (read)get_ADC0_CLK_Frequency/238 (read)get_ADC0_CLK_Frequency/239 (read)get_ADC0_CLK_Frequency/240 (read)get_ADC0_CLK_Frequency/241 (read)get_ADC0_CLK_Frequency/242 (read)get_ADC0_CLK_Frequency/243 (read)get_ADC0_CLK_Frequency/244 (read)get_ADC0_CLK_Frequency/245 (read)get_ADC0_CLK_Frequency/246 (read)get_ADC0_CLK_Frequency/247 (read)get_ADC0_CLK_Frequency/248 (read)get_ADC0_CLK_Frequency/249 (read)get_ADC0_CLK_Frequency/250 (read)get_ADC0_CLK_Frequency/251 (read)get_ADC0_CLK_Frequency/252 (read)get_ADC0_CLK_Frequency/253 (read)get_ADC0_CLK_Frequency/254 (read)get_ADC0_CLK_Frequency/255 (read)get_ADC0_CLK_Frequency/256 (read)get_ADC0_CLK_Frequency/257 (read)get_ADC0_CLK_Frequency/258 (read)get_ADC0_CLK_Frequency/259 (read)get_ADC0_CLK_Frequency/260 (read)get_ADC0_CLK_Frequency/261 (read)get_ADC0_CLK_Frequency/262 (read)get_ADC0_CLK_Frequency/263 (read)get_ADC0_CLK_Frequency/264 (read)get_ADC0_CLK_Frequency/265 (read)get_ADC0_CLK_Frequency/266 (read)get_ADC0_CLK_Frequency/267 (read)get_ADC0_CLK_Frequency/268 (read)get_ADC0_CLK_Frequency/269 (read)get_ADC0_CLK_Frequency/270 (read)get_ADC0_CLK_Frequency/271 (read)get_ADC0_CLK_Frequency/272 (read)get_ADC0_CLK_Frequency/273 (read)get_ADC0_CLK_Frequency/274 (read)get_ADC0_CLK_Frequency/275 (read)get_ADC0_CLK_Frequency/276 (read)get_ADC0_CLK_Frequency/277 (read)get_ADC0_CLK_Frequency/278 (read)get_CMP0_CLK_Frequency/279 (read)get_CMP0_CLK_Frequency/280 (read)get_CMP0_CLK_Frequency/281 (read)get_CMP0_CLK_Frequency/282 (read)get_CMP0_CLK_Frequency/283 (read)get_CMP0_CLK_Frequency/284 (read)get_CMP0_CLK_Frequency/285 (read)get_CMP0_CLK_Frequency/286 (read)get_CMP0_CLK_Frequency/287 (read)get_CMP0_CLK_Frequency/288 (read)get_CMP0_CLK_Frequency/289 (read)get_CMP0_CLK_Frequency/290 (read)get_CMP0_CLK_Frequency/291 (read)get_CMP0_CLK_Frequency/292 (read)get_CMP0_CLK_Frequency/293 (read)get_CMP0_CLK_Frequency/294 (read)get_CMP0_CLK_Frequency/295 (read)get_CMP0_CLK_Frequency/296 (read)get_CMP0_CLK_Frequency/297 (read)get_CMP0_CLK_Frequency/298 (read)get_CMP0_CLK_Frequency/299 (read)get_CMP0_CLK_Frequency/300 (read)get_CMP0_CLK_Frequency/301 (read)get_CMP0_CLK_Frequency/302 (read)get_CMP0_CLK_Frequency/303 (read)get_CMP0_CLK_Frequency/304 (read)get_CMP0_CLK_Frequency/305 (read)get_CMP0_CLK_Frequency/306 (read)get_CMP0_CLK_Frequency/307 (read)get_CMP0_CLK_Frequency/308 (read)get_CMP0_CLK_Frequency/309 (read)get_CMP0_CLK_Frequency/310 (read)get_CMP0_CLK_Frequency/311 (read)get_CMP0_CLK_Frequency/312 (read)get_CMP0_CLK_Frequency/313 (read)get_CMP0_CLK_Frequency/314 (read)get_CMP0_CLK_Frequency/315 (read)get_CRC0_CLK_Frequency/316 (read)get_CRC0_CLK_Frequency/317 (read)get_CRC0_CLK_Frequency/318 (read)get_CRC0_CLK_Frequency/319 (read)get_CRC0_CLK_Frequency/320 (read)get_CRC0_CLK_Frequency/321 (read)get_CRC0_CLK_Frequency/322 (read)get_QSPI0_RAM_CLK_Frequency/323 (read)get_SWT0_CLK_Frequency/324 (read)
  Availability: available
  Varpool flags:
HwPllName/24 (HwPllName) @06eb4000
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntryIndex/23 (selectorEntryIndex) @06e79f30
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: NOT_UNDER_MCU_CONTROL_B/45 (read)NOT_UNDER_MCU_CONTROL_B/45 (read)UpdateFrequencies/41 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
hardwareValue_selectorEntry/22 (hardwareValue_selectorEntry) @06e79ca8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: get_STMB_CLK_Frequency/200 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_STMA_CLK_Frequency/198 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_TRACE_CLK_Frequency/202 (read)get_FLEXCANB_CLK_Frequency/190 (read)get_EMAC_TS_CLK_Frequency/182 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
clockName_sourceType/21 (clockName_sourceType) @06e79f78
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
mcmeTriggerPartitions/20 (mcmeTriggerPartitions) @06e79ee8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
mcmeGetPartitions/19 (mcmeGetPartitions) @06e79ea0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
mcmeSetPartitions/18 (mcmeSetPartitions) @06e79e58
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cmu/17 (cmu) @06e79e10
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
pll/16 (pll) @06e79dc8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
xosc/15 (xosc) @06e79d80
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cgmPcfs/14 (cgmPcfs) @06e79d38
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cgm/13 (cgm) @06e79cf0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
enableDisableMask/12 (enableDisableMask) @06e79c60
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: get_STMB_CLK_Frequency/200 (read)get_EMAC_RX_CLK_Frequency/180 (read)get_STMA_CLK_Frequency/198 (read)get_FLEXCANA_CLK_Frequency/186 (read)get_QSPI_SFCK_CLK_Frequency/194 (read)get_CLKOUT_STANDBY_CLK_Frequency/179 (read)get_EMAC_TX_CLK_Frequency/184 (read)get_TRACE_CLK_Frequency/202 (read)get_FLEXCANB_CLK_Frequency/190 (read)get_EMAC_TS_CLK_Frequency/182 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorEntry_hardwareValue/11 (selectorEntry_hardwareValue) @06e79bd0
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
clockFeatures/10 (clockFeatures) @06e79b40
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
cmuCallbackIndex/9 (cmuCallbackIndex) @06e733a8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
pcfsCallbackIndex/8 (pcfsCallbackIndex) @06e73318
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
selectorCallbackIndex/7 (selectorCallbackIndex) @06e73288
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
pllCallbackIndex/6 (pllCallbackIndex) @06e731f8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
fractional_dividerCallbackIndex/5 (fractional_dividerCallbackIndex) @06e73168
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
gateCallbackIndex/4 (gateCallbackIndex) @06e730d8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
ircoscCallbackIndex/3 (ircoscCallbackIndex) @06e73048
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
xoscCallbackIndex/2 (xoscCallbackIndex) @06e5bf78
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
dividertriggerCallbackIndex/1 (dividertriggerCallbackIndex) @06e5bee8
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known
dividerCallbackIndex/0 (dividerCallbackIndex) @06e5bf30
  Type: variable definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Varpool flags: initialized read-only const-value-known

;; Function CONFIG_ELEMENTS_MAPPINGS_02 (CONFIG_ELEMENTS_MAPPINGS_02, funcdef_no=7, decl_uid=5155, cgraph_uid=8, symbol_order=43)

CONFIG_ELEMENTS_MAPPINGS_02 ()
{
  uint8 j;
  uint8 i;
  int _1;
  <unnamed type> _2;
  int _3;
  unsigned char _4;
  const struct Clock_Ip_ClockConfigType * config_clock.65_5;
  unsigned char _6;
  int _7;
  <unnamed type> _8;
  int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.65_11;
  unsigned char _12;
  int _13;
  <unnamed type> _14;
  int _15;
  unsigned char _16;
  unsigned char _17;
  <unnamed type> _19;
  int _20;
  <unnamed type> _21;
  unsigned char _22;
  unsigned char _23;
  int _24;
  <unnamed type> _25;
  int _26;
  <unnamed type> _27;
  unsigned char _28;
  unsigned char _29;

  <bb 2> [local count: 7299031]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG i => 0
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  _1 = (int) i_30;
  _2 = config_clock.65_5->selectors[_1].name;
  if (_2 <= 20)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 29527898]:
  # DEBUG BEGIN_STMT
  _3 = (int) _2;
  _4 = i_30 + 1;
  freqPointers[_3] = _4;

  <bb 5> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  i_60 = i_30 + 1;
  # DEBUG i => i_60

  <bb 6> [local count: 66354828]:
  # i_30 = PHI <0(2), i_60(5)>
  # DEBUG i => i_30
  # DEBUG BEGIN_STMT
  config_clock.65_5 = config_clock;
  _6 = config_clock.65_5->selectorsCount;
  if (_6 > i_30)
    goto <bb 3>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 7> [local count: 7299031]:
  # config_clock.65_11 = PHI <config_clock.65_5(6)>
  goto <bb 11>; [100.00%]

  <bb 8> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  _7 = (int) i_31;
  _8 = config_clock.65_11->dividers[_7].name;
  if (_8 <= 20)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 29527899]:
  # DEBUG BEGIN_STMT
  _9 = (int) _8;
  _10 = i_31 + 1;
  freqPointers[_9] = _10;

  <bb 10> [local count: 59055797]:
  # DEBUG BEGIN_STMT
  i_58 = i_31 + 1;
  # DEBUG i => i_58

  <bb 11> [local count: 66354828]:
  # i_31 = PHI <i_58(10), 0(7)>
  # DEBUG i => i_31
  # DEBUG BEGIN_STMT
  _12 = config_clock.65_11->dividersCount;
  if (_12 > i_31)
    goto <bb 8>; [89.00%]
  else
    goto <bb 34>; [11.00%]

  <bb 34> [local count: 7299031]:
  goto <bb 15>; [100.00%]

  <bb 12> [local count: 59055798]:
  # DEBUG BEGIN_STMT
  _13 = (int) i_32;
  _14 = config_clock.65_11->fracDivs[_13].name;
  if (_14 <= 20)
    goto <bb 13>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 13> [local count: 29527899]:
  # DEBUG BEGIN_STMT
  _15 = (int) _14;
  _16 = i_32 + 1;
  freqPointers[_15] = _16;

  <bb 14> [local count: 59055798]:
  # DEBUG BEGIN_STMT
  i_56 = i_32 + 1;
  # DEBUG i => i_56

  <bb 15> [local count: 66354829]:
  # i_32 = PHI <i_56(14), 0(34)>
  # DEBUG i => i_32
  # DEBUG BEGIN_STMT
  _17 = config_clock.65_11->fracDivsCount;
  if (_17 > i_32)
    goto <bb 12>; [89.00%]
  else
    goto <bb 32>; [11.00%]

  <bb 32> [local count: 7299031]:
  goto <bb 21>; [100.00%]

  <bb 16> [local count: 1014686024]:
  # DEBUG BEGIN_STMT
  _19 = pcfsEntries[0].name;
  _20 = (int) i_33;
  _21 = config_clock.65_11->pcfs[_20].name;
  if (_19 == _21)
    goto <bb 17>; [67.00%]
  else
    goto <bb 35>; [33.00%]

  <bb 35> [local count: 334846388]:
  goto <bb 29>; [100.00%]

  <bb 17> [local count: 679839636]:
  # DEBUG BEGIN_STMT
  _22 = i_33 + 1;
  pcfsEntries[0].configIndex = _22;

  <bb 19> [local count: 738895437]:
  # j_43 = PHI <1(17), 0(33)>

  <bb 29> [local count: 1073741824]:
  # j_35 = PHI <j_43(19), 1(35)>
  # DEBUG j => j_35
  # DEBUG BEGIN_STMT
  if (j_35 == 0)
    goto <bb 16>; [94.50%]
  else
    goto <bb 20>; [5.50%]

  <bb 20> [local count: 59055800]:
  # DEBUG BEGIN_STMT
  i_53 = i_33 + 1;
  # DEBUG i => i_53

  <bb 21> [local count: 66354831]:
  # i_33 = PHI <i_53(20), 0(32)>
  # DEBUG i => i_33
  # DEBUG BEGIN_STMT
  _23 = config_clock.65_11->pcfsCount;
  if (_23 > i_33)
    goto <bb 33>; [89.00%]
  else
    goto <bb 30>; [11.00%]

  <bb 33> [local count: 59055800]:
  goto <bb 19>; [100.00%]

  <bb 30> [local count: 7299031]:
  goto <bb 27>; [100.00%]

  <bb 22> [local count: 236223206]:
  # DEBUG BEGIN_STMT
  _24 = (int) j_36;
  _25 = cmuEntries[_24].name;
  _26 = (int) i_34;
  _27 = config_clock.65_11->cmus[_26].name;
  if (_25 == _27)
    goto <bb 23>; [34.00%]
  else
    goto <bb 24>; [66.00%]

  <bb 23> [local count: 80315890]:
  # DEBUG BEGIN_STMT
  _28 = i_34 + 1;
  cmuEntries[_24].configIndex = _28;

  <bb 24> [local count: 236223206]:
  # DEBUG BEGIN_STMT
  j_52 = j_36 + 1;
  # DEBUG j => j_52

  <bb 25> [local count: 295279007]:
  # j_36 = PHI <j_52(24), 0(31)>
  # DEBUG j => j_36
  # DEBUG BEGIN_STMT
  if (j_36 != 4)
    goto <bb 22>; [80.00%]
  else
    goto <bb 26>; [20.00%]

  <bb 26> [local count: 59055801]:
  # DEBUG BEGIN_STMT
  i_50 = i_34 + 1;
  # DEBUG i => i_50

  <bb 27> [local count: 66354833]:
  # i_34 = PHI <i_50(26), 0(30)>
  # DEBUG i => i_34
  # DEBUG BEGIN_STMT
  _29 = config_clock.65_11->cmusCount;
  if (_29 > i_34)
    goto <bb 31>; [89.00%]
  else
    goto <bb 28>; [11.00%]

  <bb 31> [local count: 59055801]:
  goto <bb 25>; [100.00%]

  <bb 28> [local count: 7299032]:
  return;

}



;; Function NOT_UNDER_MCU_CONTROL_B (NOT_UNDER_MCU_CONTROL_B, funcdef_no=9, decl_uid=5184, cgraph_uid=10, symbol_order=45)

NOT_UNDER_MCU_CONTROL_B ()
{
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  signed int _5;
  unsigned char _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  signed int _10;
  unsigned char _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  <unnamed type> _15;
  unsigned char _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  <unnamed type> _20;
  clock_element_state_t iftmp.55_21;
  clock_element_state_t iftmp.56_22;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[8];
  if (_1 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _2 ={v} MEM[(struct MC_ME_Type *)1076740096B].PRTN1_COFB1_STAT;
  _3 = _2 & 16777216;
  if (_3 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _4 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[0];
  _5 = (signed int) _4;
  if (_5 >= 0)
    goto <bb 6>; [59.00%]
  else
    goto <bb 5>; [41.00%]

  <bb 5> [local count: 110058537]:

  <bb 6> [local count: 268435456]:
  # iftmp.55_21 = PHI <0(4), 255(5)>
  clkState[8] = iftmp.55_21;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  clkState[8] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _6 = freqPointers[9];
  if (_6 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _7 ={v} MEM[(struct MC_ME_Type *)1076740096B].PRTN1_COFB1_STAT;
  _8 = _7 & 16777216;
  if (_8 != 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 10> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _9 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[1];
  _10 = (signed int) _9;
  if (_10 >= 0)
    goto <bb 12>; [59.00%]
  else
    goto <bb 11>; [41.00%]

  <bb 11> [local count: 110058537]:

  <bb 12> [local count: 268435456]:
  # iftmp.56_22 = PHI <0(10), 255(11)>
  clkState[9] = iftmp.56_22;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  clkState[9] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  clkState[10] = 255;
  # DEBUG BEGIN_STMT
  clkState[11] = 255;
  # DEBUG BEGIN_STMT
  _11 = freqPointers[12];
  if (_11 == 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _12 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].CSS;
  _13 = _12 >> 24;
  _14 = _13 & 63;
  _15 = selectorEntryIndex[_14];
  clkState[12] = _15;

  <bb 16> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _16 = freqPointers[20];
  if (_16 == 0)
    goto <bb 17>; [50.00%]
  else
    goto <bb 18>; [50.00%]

  <bb 17> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].CSS;
  _18 = _17 >> 24;
  _19 = _18 & 63;
  _20 = selectorEntryIndex[_19];
  clkState[20] = _20;

  <bb 18> [local count: 1073741824]:
  return;

}



;; Function IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS (IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS, funcdef_no=10, decl_uid=5187, cgraph_uid=11, symbol_order=46)

IRCOSCS_XOSCS_SERDES_EXTERNAL_CLOCKS ()
{
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.51_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  unsigned char _6;
  const struct Clock_Ip_ClockConfigType * config_clock.52_7;
  unsigned int _8;
  unsigned int _9;
  long unsigned int _10;
  unsigned char _11;
  const struct Clock_Ip_ClockConfigType * config_clock.53_12;
  unsigned int _13;
  unsigned int _14;
  long unsigned int _15;
  unsigned char _16;
  const struct Clock_Ip_ClockConfigType * config_clock.54_17;
  unsigned int _18;
  unsigned int _19;
  long unsigned int _20;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[4];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.51_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#1 => &config_clock.51_2->xoscs[_4]
  # DEBUG xoscConfig => D#1
  # DEBUG BEGIN_STMT
  _5 = MEM[(const struct Clock_Ip_XoscConfigType *)config_clock.51_2].xoscs[_4].freq;
  bufferFreqs[3] = _5;
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[3] = 16000000;

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _6 = freqPointers[5];
  if (_6 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.52_7 = config_clock;
  _8 = (unsigned int) _6;
  _9 = _8 + 4294967295;
  # DEBUG D#2 => &config_clock.52_7->xoscs[_9]
  # DEBUG xoscConfig => D#2
  # DEBUG BEGIN_STMT
  _10 = MEM[(const struct Clock_Ip_XoscConfigType *)config_clock.52_7].xoscs[_9].freq;
  bufferFreqs[4] = _10;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[4] = 32768;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  bufferFreqs[2] = 32000;
  # DEBUG BEGIN_STMT
  bufferFreqs[1] = 48000000;
  # DEBUG BEGIN_STMT
  freqPointers[0] = 1;
  # DEBUG BEGIN_STMT
  freqPointers[2] = 2;
  # DEBUG BEGIN_STMT
  _11 = freqPointers[10];
  if (_11 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.53_12 = config_clock;
  _13 = (unsigned int) _11;
  _14 = _13 + 4294967295;
  # DEBUG D#3 => &config_clock.53_12->extClks[_14]
  # DEBUG extClkConfig => D#3
  # DEBUG BEGIN_STMT
  _15 = MEM[(const struct Clock_Ip_ExtClkConfigType *)config_clock.53_12].extClks[_14].value;
  bufferFreqs[6] = _15;
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[6] = 0;

  <bb 11> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _16 = freqPointers[11];
  if (_16 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.54_17 = config_clock;
  _18 = (unsigned int) _16;
  _19 = _18 + 4294967295;
  # DEBUG D#4 => &config_clock.54_17->extClks[_19]
  # DEBUG extClkConfig => D#4
  # DEBUG BEGIN_STMT
  _20 = MEM[(const struct Clock_Ip_ExtClkConfigType *)config_clock.54_17].extClks[_19].value;
  bufferFreqs[7] = _20;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[7] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  freqPointers[10] = 6;
  # DEBUG BEGIN_STMT
  freqPointers[11] = 7;
  return;

}



;; Function PLL_A (PLL_A, funcdef_no=11, decl_uid=5192, cgraph_uid=12, symbol_order=47)

PLL_A ()
{
  long unsigned int _1;
  unsigned char _2;
  const struct Clock_Ip_ClockConfigType * config_clock.50_3;
  unsigned int _4;
  unsigned int _5;
  unsigned char _6;
  long unsigned int _7;
  unsigned char _8;
  long unsigned int _9;
  short unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  long unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = bufferFreqs[3];
  tmpData.input1 = _1;
  # DEBUG BEGIN_STMT
  _2 = freqPointers[6];
  if (_2 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.50_3 = config_clock;
  _4 = (unsigned int) _2;
  _5 = _4 + 4294967295;
  # DEBUG D#5 => &config_clock.50_3->plls[_5]
  # DEBUG pllConfig => D#5
  # DEBUG BEGIN_STMT
  _6 = MEM[(const struct Clock_Ip_PllConfigType *)config_clock.50_3].plls[_5].predivider;
  _7 = (long unsigned int) _6;
  tmpData.input2 = _7;
  # DEBUG BEGIN_STMT
  _8 = MEM[(const struct Clock_Ip_PllConfigType *)config_clock.50_3].plls[_5].mulFactorDiv;
  _9 = (long unsigned int) _8;
  tmpData.input3 = _9;
  # DEBUG BEGIN_STMT
  _10 = MEM[(const struct Clock_Ip_PllConfigType *)config_clock.50_3].plls[_5].numeratorFracLoopDiv;
  _11 = (long unsigned int) _10;
  tmpData.input4 = _11;
  # DEBUG BEGIN_STMT
  tmpData.input5 = 0;
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _12 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _13 = _12 >> 12;
  _14 = _13 & 7;
  tmpData.input2 = _14;
  # DEBUG BEGIN_STMT
  _15 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _16 = _15 & 255;
  tmpData.input3 = _16;
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLFD;
  _18 = _17 & 32767;
  tmpData.input4 = _18;
  # DEBUG BEGIN_STMT
  _19 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _20 = _19 >> 25;
  _21 = _20 & 63;
  tmpData.input5 = _21;

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _22 = tmpData.input3;
  _23 = tmpData.input2;
  _24 = _22 / _23;
  tmpData.aux1 = _24;
  # DEBUG BEGIN_STMT
  _25 = _23 * _24;
  _26 = _22 - _25;
  tmpData.aux2 = _26;
  return;

}



;; Function PLL_B (PLL_B, funcdef_no=12, decl_uid=5196, cgraph_uid=13, symbol_order=48)

PLL_B ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = tmpData.input2;
  _2 = _1 << 14;
  _3 = _1 << 11;
  _4 = _2 + _3;
  tmpData.aux3 = _4;
  # DEBUG BEGIN_STMT
  _5 = tmpData.input1;
  _6 = _5 / _4;
  tmpData.aux4 = _6;
  # DEBUG BEGIN_STMT
  _7 = _4 * _6;
  _8 = _5 - _7;
  tmpData.aux5 = _8;
  # DEBUG BEGIN_STMT
  _9 = tmpData.aux1;
  _10 = _5 * _9;
  tmpData.output = _10;
  return;

}



;; Function PLL_C (PLL_C, funcdef_no=13, decl_uid=5199, cgraph_uid=14, symbol_order=49)

PLL_C ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = tmpData.output;
  _2 = tmpData.input1;
  _3 = tmpData.input2;
  _4 = _2 / _3;
  _5 = tmpData.aux2;
  _6 = _4 * _5;
  _7 = _1 + _6;
  # DEBUG BEGIN_STMT
  _8 = tmpData.aux4;
  _9 = tmpData.input4;
  _10 = _8 * _9;
  _11 = _7 + _10;
  # DEBUG BEGIN_STMT
  _12 = tmpData.aux5;
  _13 = _9 * _12;
  _14 = tmpData.aux3;
  _15 = _13 / _14;
  _16 = _11 + _15;
  tmpData.output = _16;
  # DEBUG BEGIN_STMT
  bufferFreqs[5] = _16;
  return;

}



;; Function IntegerDividers_A (IntegerDividers_A, funcdef_no=14, decl_uid=5202, cgraph_uid=15, symbol_order=50)

IntegerDividers_A ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.47_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.48_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.49_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.47_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.47_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[1];
  _9 = _8 / dividerValue_28;
  bufferFreqs[8] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[8] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[14];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.48_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.48_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[1];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[1];
  _18 = _17 / dividerValue_29;
  bufferFreqs[9] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[9] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[15];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.49_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.49_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[2];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[1];
  _27 = _26 / dividerValue_30;
  bufferFreqs[10] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[10] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_B (IntegerDividers_B, funcdef_no=15, decl_uid=5206, cgraph_uid=16, symbol_order=51)

IntegerDividers_B ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.44_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.45_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.46_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[16];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.44_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.44_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[3];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[1];
  _9 = _8 / dividerValue_28;
  bufferFreqs[11] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[11] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[17];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.45_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.45_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[4];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[1];
  _18 = _17 / dividerValue_29;
  bufferFreqs[12] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[12] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[18];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.46_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.46_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[5];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[1];
  _27 = _26 / dividerValue_30;
  bufferFreqs[13] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[13] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_C (IntegerDividers_C, funcdef_no=16, decl_uid=5210, cgraph_uid=17, symbol_order=52)

IntegerDividers_C ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.41_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.42_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  const struct Clock_Ip_ClockConfigType * config_clock.43_19;
  unsigned int _20;
  unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[19];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.41_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_35 = config_clock.41_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_35
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[6];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_34 = _7 + 1;
  # DEBUG dividerValue => dividerValue_34

  <bb 5> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_35(3), dividerValue_34(4)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[1];
  _9 = _8 / dividerValue_27;
  bufferFreqs[14] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[14] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[20];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.42_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_39 = config_clock.42_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_39
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_38 = _16 + 1;
  # DEBUG dividerValue => dividerValue_38

  <bb 11> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_39(9), dividerValue_38(10)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[1];
  _18 = _17 / dividerValue_28;
  bufferFreqs[15] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[15] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_10 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.43_19 = config_clock;
  _20 = (unsigned int) _10;
  _21 = _20 + 4294967295;
  dividerValue_43 = config_clock.43_19->dividers[_21].value;
  # DEBUG dividerValue => dividerValue_43
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _22 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _23 = _22 >> 16;
  _24 = _23 & 63;
  dividerValue_42 = _24 + 1;
  # DEBUG dividerValue => dividerValue_42

  <bb 17> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_43(15), dividerValue_42(16)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _25 = bufferFreqs[2];
  _26 = _25 / dividerValue_29;
  bufferFreqs[16] = _26;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[16] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_D (IntegerDividers_D, funcdef_no=17, decl_uid=5214, cgraph_uid=18, symbol_order=53)

IntegerDividers_D ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.38_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.39_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.40_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.38_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.38_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[3];
  _9 = _8 / dividerValue_26;
  bufferFreqs[17] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[17] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.39_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.39_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[4];
  _17 = _16 / dividerValue_27;
  bufferFreqs[18] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[18] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.40_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.40_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[8];
  _25 = _24 / dividerValue_28;
  bufferFreqs[19] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[19] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_E (IntegerDividers_E, funcdef_no=18, decl_uid=5218, cgraph_uid=19, symbol_order=54)

IntegerDividers_E ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.35_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.36_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.37_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.35_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.35_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[11];
  _9 = _8 / dividerValue_26;
  bufferFreqs[20] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[20] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.36_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.36_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[9];
  _17 = _16 / dividerValue_27;
  bufferFreqs[21] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[21] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.37_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.37_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[10];
  _25 = _24 / dividerValue_28;
  bufferFreqs[22] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[22] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_F (IntegerDividers_F, funcdef_no=19, decl_uid=5222, cgraph_uid=20, symbol_order=55)

IntegerDividers_F ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.32_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.33_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  unsigned char _18;
  const struct Clock_Ip_ClockConfigType * config_clock.34_19;
  unsigned int _20;
  unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.32_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_35 = config_clock.32_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_35
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_34 = _7 + 1;
  # DEBUG dividerValue => dividerValue_34

  <bb 5> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_35(3), dividerValue_34(4)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[6];
  _9 = _8 / dividerValue_27;
  bufferFreqs[23] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[23] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.33_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_39 = config_clock.33_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_39
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_38 = _15 + 1;
  # DEBUG dividerValue => dividerValue_38

  <bb 11> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_39(9), dividerValue_38(10)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[7];
  _17 = _16 / dividerValue_28;
  bufferFreqs[24] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[24] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _18 = freqPointers[7];
  if (_18 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.34_19 = config_clock;
  _20 = (unsigned int) _18;
  _21 = _20 + 4294967295;
  dividerValue_43 = config_clock.34_19->dividers[_21].value;
  # DEBUG dividerValue => dividerValue_43
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _22 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLDV;
  _23 = _22 >> 25;
  dividerValue_42 = _23 & 63;
  # DEBUG dividerValue => dividerValue_42

  <bb 17> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_43(15), dividerValue_42(16)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[5];
  _25 = _24 / dividerValue_29;
  bufferFreqs[25] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[5];
  bufferFreqs[25] = _26;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_G (IntegerDividers_G, funcdef_no=20, decl_uid=5226, cgraph_uid=21, symbol_order=56)

IntegerDividers_G ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.29_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.30_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.31_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[8];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.29_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.29_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[0];
  _6 = _5 >> 16;
  _7 = _6 & 15;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[25];
  _9 = _8 / dividerValue_28;
  bufferFreqs[26] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[26] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[9];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.30_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.30_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLODIV[1];
  _15 = _14 >> 16;
  _16 = _15 & 15;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[25];
  _18 = _17 / dividerValue_29;
  bufferFreqs[27] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[27] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[13];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.31_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.31_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[0];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[26];
  _27 = _26 / dividerValue_30;
  bufferFreqs[28] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[28] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_H (IntegerDividers_H, funcdef_no=21, decl_uid=5230, cgraph_uid=22, symbol_order=57)

IntegerDividers_H ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.26_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.27_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.28_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.26_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.26_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[1];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[26];
  _9 = _8 / dividerValue_28;
  bufferFreqs[29] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[29] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[15];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.27_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.27_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[2];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[26];
  _18 = _17 / dividerValue_29;
  bufferFreqs[30] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[30] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[16];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.28_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.28_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[3];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[26];
  _27 = _26 / dividerValue_30;
  bufferFreqs[31] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[31] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_I (IntegerDividers_I, funcdef_no=22, decl_uid=5234, cgraph_uid=23, symbol_order=58)

IntegerDividers_I ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.23_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;
  const struct Clock_Ip_ClockConfigType * config_clock.24_11;
  unsigned int _12;
  unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  unsigned char _19;
  const struct Clock_Ip_ClockConfigType * config_clock.25_20;
  unsigned int _21;
  unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[17];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.23_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_36 = config_clock.23_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_36
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[4];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_35 = _7 + 1;
  # DEBUG dividerValue => dividerValue_35

  <bb 5> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_36(3), dividerValue_35(4)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[26];
  _9 = _8 / dividerValue_28;
  bufferFreqs[32] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[32] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = freqPointers[18];
  if (_10 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.24_11 = config_clock;
  _12 = (unsigned int) _10;
  _13 = _12 + 4294967295;
  dividerValue_40 = config_clock.24_11->dividers[_13].value;
  # DEBUG dividerValue => dividerValue_40
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[5];
  _15 = _14 >> 16;
  _16 = _15 & 63;
  dividerValue_39 = _16 + 1;
  # DEBUG dividerValue => dividerValue_39

  <bb 11> [local count: 1073741824]:
  # dividerValue_29 = PHI <dividerValue_40(9), dividerValue_39(10)>
  # DEBUG dividerValue => dividerValue_29
  # DEBUG BEGIN_STMT
  if (dividerValue_29 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _17 = bufferFreqs[26];
  _18 = _17 / dividerValue_29;
  bufferFreqs[33] = _18;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[33] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _19 = freqPointers[19];
  if (_19 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.25_20 = config_clock;
  _21 = (unsigned int) _19;
  _22 = _21 + 4294967295;
  dividerValue_44 = config_clock.25_20->dividers[_22].value;
  # DEBUG dividerValue => dividerValue_44
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(volatile struct cgmMux_Type *)1076724480B].divider[6];
  _24 = _23 >> 16;
  _25 = _24 & 63;
  dividerValue_43 = _25 + 1;
  # DEBUG dividerValue => dividerValue_43

  <bb 17> [local count: 1073741824]:
  # dividerValue_30 = PHI <dividerValue_44(15), dividerValue_43(16)>
  # DEBUG dividerValue => dividerValue_30
  # DEBUG BEGIN_STMT
  if (dividerValue_30 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _26 = bufferFreqs[26];
  _27 = _26 / dividerValue_30;
  bufferFreqs[34] = _27;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[34] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_J (IntegerDividers_J, funcdef_no=23, decl_uid=5238, cgraph_uid=24, symbol_order=59)

IntegerDividers_J ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.20_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.21_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.22_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.20_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.20_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[26];
  _9 = _8 / dividerValue_26;
  bufferFreqs[35] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[35] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.21_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.21_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[27];
  _17 = _16 / dividerValue_27;
  bufferFreqs[36] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[36] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.22_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.22_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[28];
  _25 = _24 / dividerValue_28;
  bufferFreqs[37] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[37] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function IntegerDividers_K (IntegerDividers_K, funcdef_no=24, decl_uid=5242, cgraph_uid=25, symbol_order=60)

IntegerDividers_K ()
{
  uint32 dividerValue;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.17_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  const struct Clock_Ip_ClockConfigType * config_clock.18_10;
  unsigned int _11;
  unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  const struct Clock_Ip_ClockConfigType * config_clock.19_18;
  unsigned int _19;
  unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = freqPointers[20];
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.17_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  dividerValue_34 = config_clock.17_2->dividers[_4].value;
  # DEBUG dividerValue => dividerValue_34
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _6 = _5 >> 16;
  _7 = _6 & 63;
  dividerValue_33 = _7 + 1;
  # DEBUG dividerValue => dividerValue_33

  <bb 5> [local count: 1073741824]:
  # dividerValue_26 = PHI <dividerValue_34(3), dividerValue_33(4)>
  # DEBUG dividerValue => dividerValue_26
  # DEBUG BEGIN_STMT
  if (dividerValue_26 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 6> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _8 = bufferFreqs[31];
  _9 = _8 / dividerValue_26;
  bufferFreqs[38] = _9;
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[38] = 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.18_10 = config_clock;
  _11 = (unsigned int) _1;
  _12 = _11 + 4294967295;
  dividerValue_38 = config_clock.18_10->dividers[_12].value;
  # DEBUG dividerValue => dividerValue_38
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _13 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _14 = _13 >> 16;
  _15 = _14 & 63;
  dividerValue_37 = _15 + 1;
  # DEBUG dividerValue => dividerValue_37

  <bb 11> [local count: 1073741824]:
  # dividerValue_27 = PHI <dividerValue_38(9), dividerValue_37(10)>
  # DEBUG dividerValue => dividerValue_27
  # DEBUG BEGIN_STMT
  if (dividerValue_27 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _16 = bufferFreqs[29];
  _17 = _16 / dividerValue_27;
  bufferFreqs[39] = _17;
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[39] = 0;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (_1 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.19_18 = config_clock;
  _19 = (unsigned int) _1;
  _20 = _19 + 4294967295;
  dividerValue_42 = config_clock.19_18->dividers[_20].value;
  # DEBUG dividerValue => dividerValue_42
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].divider[0];
  _22 = _21 >> 16;
  _23 = _22 & 63;
  dividerValue_41 = _23 + 1;
  # DEBUG dividerValue => dividerValue_41

  <bb 17> [local count: 1073741824]:
  # dividerValue_28 = PHI <dividerValue_42(15), dividerValue_41(16)>
  # DEBUG dividerValue => dividerValue_28
  # DEBUG BEGIN_STMT
  if (dividerValue_28 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _24 = bufferFreqs[30];
  _25 = _24 / dividerValue_28;
  bufferFreqs[40] = _25;
  goto <bb 20>; [100.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  bufferFreqs[40] = 0;

  <bb 20> [local count: 1073741824]:
  return;

}



;; Function PCFS_PLL_PHI0_A (PCFS_PLL_PHI0_A, funcdef_no=26, decl_uid=5258, cgraph_uid=27, symbol_order=62)

PCFS_PLL_PHI0_A ()
{
  uint32 amaxBrut;
  uint32 fsafe;
  uint32 finput;
  uint32 stepDuration;
  uint32 maxAllowableIDDchange;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.13_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = pcfsEntries[0].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.13_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#6 => &config_clock.13_2->pcfs[_4]
  # DEBUG pcfsConfig => D#6
  # DEBUG BEGIN_STMT
  maxAllowableIDDchange_15 = MEM[(const struct Clock_Ip_PcfsConfigType *)config_clock.13_2].pcfs[_4].maxAllowableIDDchange;
  # DEBUG maxAllowableIDDchange => maxAllowableIDDchange_15
  # DEBUG BEGIN_STMT
  stepDuration_16 = MEM[(const struct Clock_Ip_PcfsConfigType *)config_clock.13_2].pcfs[_4].stepDuration;
  # DEBUG stepDuration => stepDuration_16
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG maxAllowableIDDchange => 50
  # DEBUG BEGIN_STMT
  _5 ={v} MEM[(volatile struct cgmPcfs_Type *)1076723712B].PCFS_SDUR;
  stepDuration_14 = _5 & 65535;
  # DEBUG stepDuration => stepDuration_14

  <bb 5> [local count: 1073741824]:
  # maxAllowableIDDchange_11 = PHI <maxAllowableIDDchange_15(3), 50(4)>
  # stepDuration_12 = PHI <stepDuration_16(3), stepDuration_14(4)>
  # DEBUG stepDuration => stepDuration_12
  # DEBUG maxAllowableIDDchange => maxAllowableIDDchange_11
  # DEBUG BEGIN_STMT
  _6 = bufferFreqs[26];
  finput_17 = _6 / 1000000;
  # DEBUG finput => finput_17
  # DEBUG BEGIN_STMT
  _7 = bufferFreqs[1];
  fsafe_18 = _7 / 1000000;
  # DEBUG fsafe => fsafe_18
  # DEBUG BEGIN_STMT
  tmpData.input1 = stepDuration_12;
  # DEBUG BEGIN_STMT
  tmpData.input2 = finput_17;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fsafe_18;
  # DEBUG BEGIN_STMT
  _8 = maxAllowableIDDchange_11 * stepDuration_12;
  _9 = _8 * 100000;
  _10 = finput_17 * 2360;
  amaxBrut_22 = _9 / _10;
  # DEBUG amaxBrut => amaxBrut_22
  # DEBUG BEGIN_STMT
  tmpData.aux1 = amaxBrut_22;
  return;

}



;; Function PCFS_PLL_PHI0_B (PCFS_PLL_PHI0_B, funcdef_no=27, decl_uid=5267, cgraph_uid=28, symbol_order=63)

PCFS_PLL_PHI0_B ()
{
  uint8 i;
  uint32 RATE;
  uint32 amaxBrut;
  const uint32 pcfsRate[6];
  const uint32 aMax[6];
  unsigned int _1;
  unsigned int _2;
  long unsigned int _3;

  <bb 2> [local count: 357985524]:
  # DEBUG BEGIN_STMT
  aMax = *.LC0;
  # DEBUG BEGIN_STMT
  pcfsRate = *.LC1;
  # DEBUG BEGIN_STMT
  amaxBrut_11 = tmpData.aux1;
  # DEBUG amaxBrut => amaxBrut_11
  # DEBUG BEGIN_STMT
  # DEBUG RATE => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (amaxBrut_11 > 100)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 178992762]:
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 894749063]:
  # DEBUG BEGIN_STMT
  _1 = (unsigned int) i_7;
  _2 = _1 + 4294967295;
  _3 = aMax[_2];
  if (_3 < amaxBrut_11)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 447374531]:
  # DEBUG BEGIN_STMT
  RATE_12 = pcfsRate[_2];
  # DEBUG RATE => RATE_12

  <bb 5> [local count: 894749063]:
  # RATE_4 = PHI <RATE_5(3), RATE_12(4)>
  # DEBUG RATE => RATE_4
  # DEBUG BEGIN_STMT
  i_13 = i_7 + 1;
  # DEBUG i => i_13

  <bb 6> [local count: 1073741824]:
  # RATE_5 = PHI <RATE_4(5), 0(8)>
  # i_7 = PHI <i_13(5), 1(8)>
  # DEBUG i => i_7
  # DEBUG RATE => RATE_5
  # DEBUG BEGIN_STMT
  if (i_7 != 6)
    goto <bb 3>; [83.33%]
  else
    goto <bb 7>; [16.67%]

  <bb 7> [local count: 357985524]:
  # RATE_6 = PHI <RATE_5(6), 1000(2)>
  # DEBUG RATE => RATE_6
  # DEBUG BEGIN_STMT
  tmpData.aux1 = RATE_6;
  aMax ={v} {CLOBBER};
  pcfsRate ={v} {CLOBBER};
  return;

}



;; Function PCFS_PLL_PHI0_C (PCFS_PLL_PHI0_C, funcdef_no=28, decl_uid=5278, cgraph_uid=29, symbol_order=64)

PCFS_PLL_PHI0_C ()
{
  uint32 RATE;
  uint32 fsafe;
  uint32 finput;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;

  <bb 2> [local count: 118111600]:
  # DEBUG BEGIN_STMT
  finput_11 = tmpData.input2;
  # DEBUG finput => finput_11
  # DEBUG BEGIN_STMT
  fsafe_12 = tmpData.input3;
  # DEBUG fsafe => fsafe_12
  # DEBUG BEGIN_STMT
  RATE_13 = tmpData.aux1;
  # DEBUG RATE => RATE_13
  # DEBUG BEGIN_STMT
  _1 = finput_11 * 2048000;
  _2 = fsafe_12 * RATE_13;
  _3 = _1 / _2;
  _4 = 2048000 / RATE_13;
  _5 = _3 - _4;
  _6 = _5 + 256;
  tmpData.aux2 = _6;
  # DEBUG BEGIN_STMT
  tmpData.aux3 = 1073741824;
  # DEBUG BEGIN_STMT
  goto <bb 4>; [100.00%]

  <bb 3> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _7 = _8 >> 2;
  tmpData.aux3 = _7;

  <bb 4> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _8 = tmpData.aux3;
  if (_6 < _8)
    goto <bb 3>; [89.00%]
  else
    goto <bb 5>; [11.00%]

  <bb 5> [local count: 118111601]:
  return;

}



;; Function PCFS_PLL_PHI0_D (PCFS_PLL_PHI0_D, funcdef_no=29, decl_uid=5287, cgraph_uid=30, symbol_order=65)

PCFS_PLL_PHI0_D ()
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 118111600]:
  # DEBUG BEGIN_STMT
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _1 = tmpData.aux2;
  _2 = tmpData.aux4;
  _3 = _2 + _10;
  if (_1 >= _3)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 477815111]:
  # DEBUG BEGIN_STMT
  _4 = _1 - _3;
  tmpData.aux2 = _4;
  # DEBUG BEGIN_STMT
  _5 = _10 << 1;
  _6 = _2 + _5;
  tmpData.aux4 = _6;

  <bb 5> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _7 = tmpData.aux4;
  _8 = _7 >> 1;
  tmpData.aux4 = _8;
  # DEBUG BEGIN_STMT
  _9 = _10 >> 2;
  tmpData.aux3 = _9;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _10 = tmpData.aux3;
  if (_10 != 0)
    goto <bb 3>; [89.00%]
  else
    goto <bb 7>; [11.00%]

  <bb 7> [local count: 118111601]:
  return;

}



;; Function PCFS_PLL_PHI0_E (PCFS_PLL_PHI0_E, funcdef_no=30, decl_uid=5293, cgraph_uid=31, symbol_order=66)

PCFS_PLL_PHI0_E ()
{
  uint32 K;
  uint32 RATE;
  uint32 fsafe;
  uint32 finput;
  uint32 stepDuration;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  stepDuration_14 = tmpData.input1;
  # DEBUG stepDuration => stepDuration_14
  # DEBUG BEGIN_STMT
  finput_15 = tmpData.input2;
  # DEBUG finput => finput_15
  # DEBUG BEGIN_STMT
  fsafe_16 = tmpData.input3;
  # DEBUG fsafe => fsafe_16
  # DEBUG BEGIN_STMT
  RATE_17 = tmpData.aux1;
  # DEBUG RATE => RATE_17
  # DEBUG BEGIN_STMT
  _1 = tmpData.aux4;
  _2 = _1 << 2;
  _3 = _2 + 191;
  K_18 = _3 >> 7;
  # DEBUG K => K_18
  # DEBUG BEGIN_STMT
  _4 = stepDuration_14 * fsafe_16;
  pcfsEntries[0].sdur = _4;
  # DEBUG BEGIN_STMT
  _5 = RATE_17 * K_18;
  pcfsEntries[0].divc_init = _5;
  # DEBUG BEGIN_STMT
  pcfsEntries[0].divc_rate = RATE_17;
  # DEBUG BEGIN_STMT
  _6 = K_18 + 1;
  _7 = _5 * _6;
  _8 = _7 >> 1;
  _9 = _8 + 999;
  pcfsEntries[0].div_startValue = _9;
  # DEBUG BEGIN_STMT
  _10 = finput_15 * 1000;
  _11 = _10 / fsafe_16;
  _12 = _11 + 4294967295;
  pcfsEntries[0].div_endValue = _12;
  return;

}



;; Function CMU_FXOSC_CLK_A (CMU_FXOSC_CLK_A, funcdef_no=31, decl_uid=5301, cgraph_uid=32, symbol_order=67)

CMU_FXOSC_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.10_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int configuredAipsSlowClock.11_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[0].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.10_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#7 => &config_clock.10_2->cmus[_4]
  # DEBUG cmuConfig => D#7
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.10_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[1];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  _6 = bufferFreqs[3];
  fMonitoredClk_25 = _6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.11_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.11_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[0].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[0].refCount = _19;
  return;

}



;; Function CMU_FXOSC_CLK_B (CMU_FXOSC_CLK_B, funcdef_no=32, decl_uid=5311, cgraph_uid=33, symbol_order=68)

CMU_FXOSC_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[0].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[0].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[0].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}



;; Function CMU_CORE_CLK_A (CMU_CORE_CLK_A, funcdef_no=33, decl_uid=5316, cgraph_uid=34, symbol_order=69)

CMU_CORE_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.7_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int configuredCoreClock.8_6;
  long unsigned int configuredAipsSlowClock.9_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[1].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.7_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#8 => &config_clock.7_2->cmus[_4]
  # DEBUG cmuConfig => D#8
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.7_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[3];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  configuredCoreClock.8_6 = configuredCoreClock;
  fMonitoredClk_25 = configuredCoreClock.8_6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.9_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.9_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (configuredCoreClock.8_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[1].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[1].refCount = _19;
  return;

}



;; Function CMU_CORE_CLK_B (CMU_CORE_CLK_B, funcdef_no=34, decl_uid=5326, cgraph_uid=35, symbol_order=70)

CMU_CORE_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[1].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[1].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[1].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}



;; Function CMU_AIPS_PLAT_CLK_A (CMU_AIPS_PLAT_CLK_A, funcdef_no=35, decl_uid=5331, cgraph_uid=36, symbol_order=71)

CMU_AIPS_PLAT_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.4_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int configuredAipsPlatClock.5_6;
  long unsigned int configuredAipsSlowClock.6_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[2].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.4_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#9 => &config_clock.4_2->cmus[_4]
  # DEBUG cmuConfig => D#9
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.4_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[1];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  configuredAipsPlatClock.5_6 = configuredAipsPlatClock;
  fMonitoredClk_25 = configuredAipsPlatClock.5_6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.6_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.6_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (configuredAipsPlatClock.5_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[2].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[2].refCount = _19;
  return;

}



;; Function CMU_AIPS_PLAT_CLK_B (CMU_AIPS_PLAT_CLK_B, funcdef_no=36, decl_uid=5341, cgraph_uid=37, symbol_order=72)

CMU_AIPS_PLAT_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[2].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[2].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[2].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}



;; Function CMU_HSE_CLK_A (CMU_HSE_CLK_A, funcdef_no=37, decl_uid=5346, cgraph_uid=38, symbol_order=73)

CMU_HSE_CLK_A ()
{
  uint8 enable;
  uint32 cmp2;
  uint32 cmp1;
  uint32 fBusClk;
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  unsigned char _1;
  const struct Clock_Ip_ClockConfigType * config_clock.1_2;
  unsigned int _3;
  unsigned int _4;
  long unsigned int _5;
  long unsigned int configuredHseClock.2_6;
  long unsigned int configuredAipsSlowClock.3_7;
  long unsigned int _8;
  float _9;
  float _10;
  float _11;
  float _12;
  long unsigned int _13;
  float _14;
  float _15;
  float _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = cmuEntries[3].configIndex;
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  config_clock.1_2 = config_clock;
  _3 = (unsigned int) _1;
  _4 = _3 + 4294967295;
  # DEBUG D#10 => &config_clock.1_2->cmus[_4]
  # DEBUG cmuConfig => D#10
  # DEBUG BEGIN_STMT
  enable_23 = MEM[(const struct Clock_Ip_CmuConfigType *)config_clock.1_2].cmus[_4].enable;
  # DEBUG enable => enable_23

  <bb 4> [local count: 1073741824]:
  # enable_21 = PHI <enable_23(3), 0(2)>
  # DEBUG enable => enable_21
  # DEBUG BEGIN_STMT
  _5 = bufferFreqs[1];
  fReferenceClk_24 = _5 / 1000;
  # DEBUG fReferenceClk => fReferenceClk_24
  # DEBUG BEGIN_STMT
  configuredHseClock.2_6 = configuredHseClock;
  fMonitoredClk_25 = configuredHseClock.2_6 / 1000;
  # DEBUG fMonitoredClk => fMonitoredClk_25
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock.3_7 = configuredAipsSlowClock;
  fBusClk_26 = configuredAipsSlowClock.3_7 / 1000;
  # DEBUG fBusClk => fBusClk_26
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) enable_21;
  tmpData.input1 = _8;
  # DEBUG BEGIN_STMT
  tmpData.input2 = fReferenceClk_24;
  # DEBUG BEGIN_STMT
  tmpData.input3 = fMonitoredClk_25;
  # DEBUG BEGIN_STMT
  tmpData.input4 = fBusClk_26;
  # DEBUG BEGIN_STMT
  _9 = (float) fReferenceClk_24;
  _10 = _9 * 3.0e+0;
  _11 = (float) fBusClk_26;
  _12 = _10 / _11;
  _13 = (long unsigned int) _12;
  cmp1_31 = _13 + 1;
  # DEBUG cmp1 => cmp1_31
  # DEBUG BEGIN_STMT
  if (configuredHseClock.2_6 > 999)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _14 = _9 * 5.0e+0;
  _15 = (float) fMonitoredClk_25;
  _16 = _14 / _15;
  _17 = (long unsigned int) _16;
  cmp2_32 = _17 + 9;
  # DEBUG cmp2 => cmp2_32

  <bb 6> [local count: 1073741824]:
  # cmp2_20 = PHI <cmp2_32(5), 0(4)>
  # DEBUG cmp2 => cmp2_20
  # DEBUG BEGIN_STMT
  cmuEntries[3].enable = _8;
  # DEBUG BEGIN_STMT
  _18 = MAX_EXPR <cmp2_20, cmp1_31>;
  _19 = _18 * 10;
  cmuEntries[3].refCount = _19;
  return;

}



;; Function CMU_HSE_CLK_B (CMU_HSE_CLK_B, funcdef_no=38, decl_uid=5356, cgraph_uid=39, symbol_order=74)

CMU_HSE_CLK_B ()
{
  uint32 fMonitoredClk;
  uint32 fReferenceClk;
  float _1;
  float _2;
  float _3;
  float _4;
  float _5;
  long unsigned int _6;
  float _7;
  float _8;
  float _9;
  long unsigned int _10;
  float _11;
  float _12;
  float _13;
  float _14;
  float _15;
  long unsigned int _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  fReferenceClk_19 = tmpData.input2;
  # DEBUG fReferenceClk => fReferenceClk_19
  # DEBUG BEGIN_STMT
  fMonitoredClk_20 = tmpData.input3;
  # DEBUG fMonitoredClk => fMonitoredClk_20
  # DEBUG BEGIN_STMT
  if (fReferenceClk_19 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (float) fMonitoredClk_20;
  _2 = _1 * 1.011e+3;
  _3 = (float) fReferenceClk_19;
  _4 = _3 * 9.67e+2;
  _5 = _2 / _4;
  _6 = cmuEntries[3].refCount;
  _7 = (float) _6;
  _8 = _5 * _7;
  _9 = _8 + 3.0e+0;
  _10 = (long unsigned int) _9;
  cmuEntries[3].hfRef = _10;
  # DEBUG BEGIN_STMT
  _11 = _1 * 9.89e+2;
  _12 = _3 * 1.033e+3;
  _13 = _11 / _12;
  _14 = _7 * _13;
  _15 = _14 - 3.0e+0;
  _16 = (long unsigned int) _15;
  cmuEntries[3].lfRef = _16;

  <bb 4> [local count: 1073741824]:
  return;

}



;; Function CallEmptyCallbacks (CallEmptyCallbacks, funcdef_no=40, decl_uid=5364, cgraph_uid=41, symbol_order=76)

CallEmptyCallbacks ()
{
  void (*<T494>) (const struct Clock_Ip_CmuConfigType *) _1;
  void (*<T498>) (Clock_Ip_NameType) _2;
  void (*<T498>) (Clock_Ip_NameType) _3;
  Clock_Ip_CmuStatusType (*<T49c>) (Clock_Ip_NameType) _4;
  void (*<T43f>) (const struct Clock_Ip_DividerConfigType *) _5;
  void (*<T44a>) (const struct Clock_Ip_DividerTriggerConfigType *) _6;
  void (*<T433>) (const struct Clock_Ip_XoscConfigType *) _7;
  void (*<T456>) (const struct Clock_Ip_FracDivConfigType *) _8;
  clock_dfs_status_t (*<T45c>) (Clock_Ip_NameType) _9;
  void (*<T484>) (const struct Clock_Ip_GateConfigType *) _10;
  void (*<T489>) (Clock_Ip_NameType, boolean) _11;
  void (*<T428>) (const struct Clock_Ip_IrcoscConfigType *) _12;
  void (*<T467>) (const struct Clock_Ip_PllConfigType *) _13;
  clock_pll_status_t (*<T46d>) (Clock_Ip_NameType) _14;
  void (*<T478>) (const struct Clock_Ip_SelectorConfigType *) _15;
  void (*<T4a7>) (const struct Clock_Ip_PcfsConfigType *) _16;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = cmuCallbacks[0].Set;
  _1 (0B);
  # DEBUG BEGIN_STMT
  _2 = cmuCallbacks[0].Disable;
  _2 (145);
  # DEBUG BEGIN_STMT
  _3 = cmuCallbacks[0].Clear;
  _3 (145);
  # DEBUG BEGIN_STMT
  _4 = cmuCallbacks[0].GetStatus;
  _4 (145);
  # DEBUG BEGIN_STMT
  _5 = dividerCallbacks[0].Set;
  _5 (0B);
  # DEBUG BEGIN_STMT
  _6 = dividerTriggerCallbacks[0].Configure;
  _6 (0B);
  # DEBUG BEGIN_STMT
  _7 = extOscCallbacks[0].Reset;
  _7 (0B);
  # DEBUG BEGIN_STMT
  _8 = fracDivCallbacks[0].Set;
  _8 (0B);
  # DEBUG BEGIN_STMT
  _9 = fracDivCallbacks[0].Complete;
  _9 (145);
  # DEBUG BEGIN_STMT
  _10 = gateCallbacks[0].Set;
  _10 (0B);
  # DEBUG BEGIN_STMT
  _11 = gateCallbacks[0].Update;
  _11 (145, 0);
  # DEBUG BEGIN_STMT
  _12 = intOscCallbacks[0].Set;
  _12 (0B);
  # DEBUG BEGIN_STMT
  _13 = pllCallbacks[0].Set;
  _13 (0B);
  # DEBUG BEGIN_STMT
  _14 = pllCallbacks[0].Complete;
  _14 (145);
  # DEBUG BEGIN_STMT
  _15 = selectorCallbacks[0].Set;
  _15 (0B);
  # DEBUG BEGIN_STMT
  _16 = pcfsCallbacks[0].Set;
  _16 (0B);
  return;

}



;; Function get_ADC0_CLK_Frequency (get_ADC0_CLK_Frequency, funcdef_no=42, decl_uid=5377, cgraph_uid=43, symbol_order=80)


Saving body of get_ADC0_CLK_Frequency for later reuse
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1

Symbols to be put in SSA form
{ D.7322 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 4
Number of blocks to update: 3 ( 75%)


get_ADC0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[13];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}



;; Function get_CMP0_CLK_Frequency (get_CMP0_CLK_Frequency, funcdef_no=89, decl_uid=5387, cgraph_uid=90, symbol_order=127)


Saving body of get_CMP0_CLK_Frequency for later reuse
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1

Symbols to be put in SSA form
{ D.7327 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 4
Number of blocks to update: 3 ( 75%)


get_CMP0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[15];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}



;; Function get_CRC0_CLK_Frequency (get_CRC0_CLK_Frequency, funcdef_no=127, decl_uid=5393, cgraph_uid=128, symbol_order=165)


Saving body of get_CRC0_CLK_Frequency for later reuse
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1

Symbols to be put in SSA form
{ D.7332 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 4
Number of blocks to update: 3 ( 75%)


get_CRC0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[14];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}



;; Function get_DCM0_CLK_Frequency (get_DCM0_CLK_Frequency, funcdef_no=135, decl_uid=5395, cgraph_uid=136, symbol_order=173)

get_DCM0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[17];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}



;; Function get_QSPI0_RAM_CLK_Frequency (get_QSPI0_RAM_CLK_Frequency, funcdef_no=136, decl_uid=5575, cgraph_uid=137, symbol_order=174)


Saving body of get_QSPI0_RAM_CLK_Frequency for later reuse
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1

Symbols to be put in SSA form
{ D.7339 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 4
Number of blocks to update: 3 ( 75%)


get_QSPI0_RAM_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[19];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}



;; Function get_SIUL0_CLK_Frequency (get_SIUL0_CLK_Frequency, funcdef_no=138, decl_uid=5593, cgraph_uid=139, symbol_order=176)

get_SIUL0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[0];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}



;; Function get_SWT0_CLK_Frequency (get_SWT0_CLK_Frequency, funcdef_no=139, decl_uid=5605, cgraph_uid=140, symbol_order=177)


Saving body of get_SWT0_CLK_Frequency for later reuse
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1

Symbols to be put in SSA form
{ D.7346 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 4
Number of blocks to update: 3 ( 75%)


get_SWT0_CLK_Frequency ()
{
  unsigned char _1;
  int _2;
  uint32 _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = freqPointers[2];
  _2 = (int) _1;
  _4 = bufferFreqs[_2];
  return _4;

}



;; Function get_CLKOUT_STANDBY_CLK_Frequency (get_CLKOUT_STANDBY_CLK_Frequency, funcdef_no=141, decl_uid=5385, cgraph_uid=142, symbol_order=179)

get_CLKOUT_STANDBY_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724800B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724800B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724800B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function get_EMAC_RX_CLK_Frequency (get_EMAC_RX_CLK_Frequency, funcdef_no=142, decl_uid=5469, cgraph_uid=143, symbol_order=180)

get_EMAC_RX_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724928B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function get_EMAC0_RX_CLK_Frequency (get_EMAC0_RX_CLK_Frequency, funcdef_no=353, decl_uid=5471, cgraph_uid=144, symbol_order=181)

get_EMAC0_RX_CLK_Frequency ()
{
  uint32 retval.352;

  <bb 2> [local count: 1073741824]:
  retval.352_3 = get_EMAC_RX_CLK_Frequency (); [tail call]
  return retval.352_3;

}



;; Function get_EMAC_TS_CLK_Frequency (get_EMAC_TS_CLK_Frequency, funcdef_no=144, decl_uid=5473, cgraph_uid=145, symbol_order=182)

get_EMAC_TS_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725056B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function get_EMAC0_TS_CLK_Frequency (get_EMAC0_TS_CLK_Frequency, funcdef_no=355, decl_uid=5475, cgraph_uid=146, symbol_order=183)

get_EMAC0_TS_CLK_Frequency ()
{
  uint32 retval.353;

  <bb 2> [local count: 1073741824]:
  retval.353_3 = get_EMAC_TS_CLK_Frequency (); [tail call]
  return retval.353_3;

}



;; Function get_EMAC_TX_CLK_Frequency (get_EMAC_TX_CLK_Frequency, funcdef_no=146, decl_uid=5477, cgraph_uid=147, symbol_order=184)

get_EMAC_TX_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724992B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function get_EMAC0_TX_CLK_Frequency (get_EMAC0_TX_CLK_Frequency, funcdef_no=357, decl_uid=5479, cgraph_uid=148, symbol_order=185)

get_EMAC0_TX_CLK_Frequency ()
{
  uint32 retval.354;

  <bb 2> [local count: 1073741824]:
  retval.354_3 = get_EMAC_TX_CLK_Frequency (); [tail call]
  return retval.354_3;

}



;; Function get_FLEXCANA_CLK_Frequency (get_FLEXCANA_CLK_Frequency, funcdef_no=148, decl_uid=5491, cgraph_uid=149, symbol_order=186)

get_FLEXCANA_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724672B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function get_FLEXCAN0_CLK_Frequency (get_FLEXCAN0_CLK_Frequency, funcdef_no=359, decl_uid=5493, cgraph_uid=150, symbol_order=187)

get_FLEXCAN0_CLK_Frequency ()
{
  uint32 retval.355;

  <bb 2> [local count: 1073741824]:
  retval.355_3 = get_FLEXCANA_CLK_Frequency (); [tail call]
  return retval.355_3;

}



;; Function get_FLEXCAN1_CLK_Frequency (get_FLEXCAN1_CLK_Frequency, funcdef_no=361, decl_uid=5495, cgraph_uid=151, symbol_order=188)

get_FLEXCAN1_CLK_Frequency ()
{
  uint32 retval.356;

  <bb 2> [local count: 1073741824]:
  retval.356_3 = get_FLEXCANA_CLK_Frequency (); [tail call]
  return retval.356_3;

}



;; Function get_FLEXCAN2_CLK_Frequency (get_FLEXCAN2_CLK_Frequency, funcdef_no=363, decl_uid=5497, cgraph_uid=152, symbol_order=189)

get_FLEXCAN2_CLK_Frequency ()
{
  uint32 retval.357;

  <bb 2> [local count: 1073741824]:
  retval.357_3 = get_FLEXCANA_CLK_Frequency (); [tail call]
  return retval.357_3;

}



;; Function get_FLEXCANB_CLK_Frequency (get_FLEXCANB_CLK_Frequency, funcdef_no=152, decl_uid=5499, cgraph_uid=153, symbol_order=190)

get_FLEXCANB_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724736B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function get_FLEXCAN3_CLK_Frequency (get_FLEXCAN3_CLK_Frequency, funcdef_no=365, decl_uid=5501, cgraph_uid=154, symbol_order=191)

get_FLEXCAN3_CLK_Frequency ()
{
  uint32 retval.358;

  <bb 2> [local count: 1073741824]:
  retval.358_3 = get_FLEXCANB_CLK_Frequency (); [tail call]
  return retval.358_3;

}



;; Function get_FLEXCAN4_CLK_Frequency (get_FLEXCAN4_CLK_Frequency, funcdef_no=367, decl_uid=5503, cgraph_uid=155, symbol_order=192)

get_FLEXCAN4_CLK_Frequency ()
{
  uint32 retval.359;

  <bb 2> [local count: 1073741824]:
  retval.359_3 = get_FLEXCANB_CLK_Frequency (); [tail call]
  return retval.359_3;

}



;; Function get_FLEXCAN5_CLK_Frequency (get_FLEXCAN5_CLK_Frequency, funcdef_no=369, decl_uid=5505, cgraph_uid=156, symbol_order=193)

get_FLEXCAN5_CLK_Frequency ()
{
  uint32 retval.360;

  <bb 2> [local count: 1073741824]:
  retval.360_3 = get_FLEXCANB_CLK_Frequency (); [tail call]
  return retval.360_3;

}



;; Function get_QSPI_SFCK_CLK_Frequency (get_QSPI_SFCK_CLK_Frequency, funcdef_no=156, decl_uid=5577, cgraph_uid=157, symbol_order=194)

get_QSPI_SFCK_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725120B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function get_QSPI0_SFCK_CLK_Frequency (get_QSPI0_SFCK_CLK_Frequency, funcdef_no=371, decl_uid=5579, cgraph_uid=158, symbol_order=195)

get_QSPI0_SFCK_CLK_Frequency ()
{
  uint32 retval.361;

  <bb 2> [local count: 1073741824]:
  retval.361_3 = get_QSPI_SFCK_CLK_Frequency (); [tail call]
  return retval.361_3;

}



;; Function get_RTC_CLK_Frequency (get_RTC_CLK_Frequency, funcdef_no=158, decl_uid=5583, cgraph_uid=159, symbol_order=196)


Saving body of get_RTC_CLK_Frequency for later reuse
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1

Symbols to be put in SSA form
{ D.7385 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 4
Number of blocks to update: 3 ( 75%)


get_RTC_CLK_Frequency ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return 0;

}



;; Function get_STMA_CLK_Frequency (get_STMA_CLK_Frequency, funcdef_no=160, decl_uid=5597, cgraph_uid=161, symbol_order=198)

get_STMA_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724544B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function get_STM0_CLK_Frequency (get_STM0_CLK_Frequency, funcdef_no=375, decl_uid=5599, cgraph_uid=162, symbol_order=199)

get_STM0_CLK_Frequency ()
{
  uint32 retval.363;

  <bb 2> [local count: 1073741824]:
  retval.363_3 = get_STMA_CLK_Frequency (); [tail call]
  return retval.363_3;

}



;; Function get_STMB_CLK_Frequency (get_STMB_CLK_Frequency, funcdef_no=162, decl_uid=5601, cgraph_uid=163, symbol_order=200)

get_STMB_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076724608B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function get_STM1_CLK_Frequency (get_STM1_CLK_Frequency, funcdef_no=377, decl_uid=5603, cgraph_uid=164, symbol_order=201)

get_STM1_CLK_Frequency ()
{
  uint32 retval.364;

  <bb 2> [local count: 1073741824]:
  retval.364_3 = get_STMB_CLK_Frequency (); [tail call]
  return retval.364_3;

}



;; Function get_TRACE_CLK_Frequency (get_TRACE_CLK_Frequency, funcdef_no=164, decl_uid=5615, cgraph_uid=165, symbol_order=202)

get_TRACE_CLK_Frequency ()
{
  uint32 frequency;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  int _5;
  unsigned char _6;
  int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _15;
  long unsigned int _17;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 ={v} MEM[(volatile struct cgmMux_Type *)1076725184B].CSS;
  _2 = _1 >> 24;
  _3 = _2 & 63;
  _4 = hardwareValue_selectorEntry[_3];
  _5 = (int) _4;
  _6 = freqPointers[_5];
  _7 = (int) _6;
  frequency_14 = bufferFreqs[_7];
  # DEBUG frequency => frequency_14
  # DEBUG BEGIN_STMT
  _8 ={v} MEM[(volatile struct cgmMux_Type *)1076725184B].divider[0];
  _9 = _8 >> 31;
  _15 = enableDisableMask[_9];
  frequency_16 = frequency_14 & _15;
  # DEBUG frequency => frequency_16
  # DEBUG BEGIN_STMT
  _10 ={v} MEM[(volatile struct cgmMux_Type *)1076725184B].divider[0];
  _11 = _10 >> 16;
  _12 = _11 & 63;
  _17 = _12 + 1;
  frequency_18 = frequency_16 / _17;
  # DEBUG frequency => frequency_18
  # DEBUG BEGIN_STMT
  return frequency_18;

}



;; Function CallbackDelay (CallbackDelay, funcdef_no=41, decl_uid=5367, cgraph_uid=42, symbol_order=77)

CallbackDelay ()
{
  uint32 TimeoutTicks;
  uint32 ElapsedTime;
  uint32 StartTime;
  boolean TimeoutOccurred;
  long unsigned int TimeoutTicks.0_1;

  <bb 2> [local count: 118111600]:
  # DEBUG BEGIN_STMT
  # DEBUG TimeoutOccurred => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  ClockStartTimeout (&StartTime, &ElapsedTime, &TimeoutTicks, 10);

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  TimeoutTicks.0_1 = TimeoutTicks;
  TimeoutOccurred_6 = ClockTimeoutExpired (&StartTime, &ElapsedTime, TimeoutTicks.0_1);
  # DEBUG TimeoutOccurred => TimeoutOccurred_6
  # DEBUG BEGIN_STMT
  if (TimeoutOccurred_6 != 0)
    goto <bb 4>; [11.00%]
  else
    goto <bb 5>; [89.00%]

  <bb 5> [local count: 955630223]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 118111601]:
  StartTime ={v} {CLOBBER};
  ElapsedTime ={v} {CLOBBER};
  TimeoutTicks ={v} {CLOBBER};
  return;

}



;; Function CONFIG_ELEMENTS_MAPPINGS_01 (CONFIG_ELEMENTS_MAPPINGS_01, funcdef_no=6, decl_uid=5136, cgraph_uid=7, symbol_order=42)


Symbols to be put in SSA form
{ D.6647 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 20
Number of blocks to update: 19 ( 95%)


Merging blocks 5 and 7
Removing basic block 13
Removing basic block 16
Removing basic block 19
;; 10 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15
;;
;; Loop 6
;;  header 14, latch 13
;;  depth 1, outer 0
;;  nodes: 14 13
;;
;; Loop 7
;;  header 12, latch 11
;;  depth 1, outer 0
;;  nodes: 12 11
;;
;; Loop 8
;;  header 10, latch 9
;;  depth 1, outer 0
;;  nodes: 10 9
;;
;; Loop 9
;;  header 7, latch 6
;;  depth 1, outer 0
;;  nodes: 7 6
;;
;; Loop 1
;;  header 4, latch 3
;;  depth 1, outer 0
;;  nodes: 4 3
;; 2 succs { 4 }
;; 3 succs { 4 }
;; 4 succs { 3 5 }
;; 5 succs { 7 }
;; 6 succs { 7 }
;; 7 succs { 6 8 }
;; 8 succs { 10 }
;; 9 succs { 10 }
;; 10 succs { 9 12 }
;; 11 succs { 12 }
;; 12 succs { 11 14 }
;; 13 succs { 14 }
;; 14 succs { 13 15 }
;; 15 succs { 1 }
CONFIG_ELEMENTS_MAPPINGS_01 ()
{
  uint8 i;
  uint8 i;
  int _1;
  int _11;
  const struct Clock_Ip_ClockConfigType * config_clock.85_12;
  <unnamed type> _13;
  int _14;
  unsigned char _15;
  unsigned char _16;
  int _18;
  const struct Clock_Ip_ClockConfigType * config_clock.85_19;
  <unnamed type> _20;
  int _21;
  unsigned char _22;
  unsigned char _23;
  int _25;
  <unnamed type> _26;
  int _27;
  unsigned char _28;
  unsigned char _29;
  int _31;
  <unnamed type> _32;
  int _33;
  unsigned char _34;
  unsigned char _35;

  <bb 2> [local count: 46707770]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG i => 0
  goto <bb 4>; [100.00%]

  <bb 3> [local count: 1027034056]:
  # DEBUG BEGIN_STMT
  _1 = (int) i_3;
  freqPointers[_1] = 0;
  # DEBUG BEGIN_STMT
  i_9 = i_3 + 1;
  # DEBUG i => i_9

  <bb 4> [local count: 1073741824]:
  # i_3 = PHI <0(2), i_9(3)>
  # DEBUG i => i_3
  # DEBUG BEGIN_STMT
  if (i_3 != 22)
    goto <bb 3>; [95.65%]
  else
    goto <bb 5>; [4.35%]

  <bb 5> [local count: 46707769]:
  # i_4 = PHI <0(4)>
  # DEBUG INLINE_ENTRY CONFIG_ELEMENTS_MAPPINGS_01
  goto <bb 7>; [100.00%]

  <bb 6> [local count: 377908318]:
  # DEBUG BEGIN_STMT
  _11 = (int) i_10;
  _13 = config_clock.85_12->ircoscs[_11].name;
  _14 = (int) _13;
  _15 = i_10 + 1;
  freqPointers[_14] = _15;
  # DEBUG BEGIN_STMT
  # DEBUG i => _15

  <bb 7> [local count: 424616088]:
  # i_10 = PHI <0(5), _15(6)>
  # DEBUG i => i_10
  # DEBUG BEGIN_STMT
  config_clock.85_12 = config_clock;
  _16 = config_clock.85_12->ircoscsCount;
  if (i_10 < _16)
    goto <bb 6>; [89.00%]
  else
    goto <bb 8>; [11.00%]

  <bb 8> [local count: 46707770]:
  # config_clock.85_19 = PHI <config_clock.85_12(7)>
  goto <bb 10>; [100.00%]

  <bb 9> [local count: 377908321]:
  # DEBUG BEGIN_STMT
  _18 = (int) i_17;
  _20 = config_clock.85_19->xoscs[_18].name;
  _21 = (int) _20;
  _22 = i_17 + 1;
  freqPointers[_21] = _22;
  # DEBUG BEGIN_STMT
  # DEBUG i => _22

  <bb 10> [local count: 424616091]:
  # i_17 = PHI <0(8), _22(9)>
  # DEBUG i => i_17
  # DEBUG BEGIN_STMT
  _23 = config_clock.85_19->xoscsCount;
  if (i_17 < _23)
    goto <bb 9>; [89.00%]
  else
    goto <bb 12>; [11.00%]

  <bb 11> [local count: 377908323]:
  # DEBUG BEGIN_STMT
  _25 = (int) i_24;
  _26 = config_clock.85_19->plls[_25].name;
  _27 = (int) _26;
  _28 = i_24 + 1;
  freqPointers[_27] = _28;
  # DEBUG BEGIN_STMT
  # DEBUG i => _28

  <bb 12> [local count: 424616093]:
  # i_24 = PHI <0(10), _28(11)>
  # DEBUG i => i_24
  # DEBUG BEGIN_STMT
  _29 = config_clock.85_19->pllsCount;
  if (i_24 < _29)
    goto <bb 11>; [89.00%]
  else
    goto <bb 14>; [11.00%]

  <bb 13> [local count: 377908324]:
  # DEBUG BEGIN_STMT
  _31 = (int) i_30;
  _32 = config_clock.85_19->extClks[_31].name;
  _33 = (int) _32;
  _34 = i_30 + 1;
  freqPointers[_33] = _34;
  # DEBUG BEGIN_STMT
  # DEBUG i => _34

  <bb 14> [local count: 424616095]:
  # i_30 = PHI <0(12), _34(13)>
  # DEBUG i => i_30
  # DEBUG BEGIN_STMT
  _35 = config_clock.85_19->extClksCount;
  if (i_30 < _35)
    goto <bb 13>; [89.00%]
  else
    goto <bb 15>; [11.00%]

  <bb 15> [local count: 46707770]:
  # DEBUG i => NULL
  return;

}



;; Function NOT_UNDER_MCU_CONTROL_A (NOT_UNDER_MCU_CONTROL_A, funcdef_no=8, decl_uid=5181, cgraph_uid=9, symbol_order=44)


Symbols to be put in SSA form
{ D.6649 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 29
Number of blocks to update: 28 ( 97%)


Removing basic block 19
Removing basic block 21
Removing basic block 22
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25
;; 2 succs { 3 6 }
;; 3 succs { 5 4 }
;; 4 succs { 5 }
;; 5 succs { 6 }
;; 6 succs { 7 10 }
;; 7 succs { 9 8 }
;; 8 succs { 9 }
;; 9 succs { 10 }
;; 10 succs { 11 14 }
;; 11 succs { 13 12 }
;; 12 succs { 13 }
;; 13 succs { 14 }
;; 14 succs { 15 18 }
;; 15 succs { 17 16 }
;; 16 succs { 17 }
;; 17 succs { 18 }
;; 18 succs { 19 25 }
;; 19 succs { 20 23 }
;; 20 succs { 22 21 }
;; 21 succs { 22 }
;; 22 succs { 24 }
;; 23 succs { 24 }
;; 24 succs { 25 }
;; 25 succs { 1 }
NOT_UNDER_MCU_CONTROL_A ()
{
  unsigned char _1;
  long unsigned int _3;
  long unsigned int _4;
  unsigned char _5;
  long unsigned int _6;
  signed int _7;
  unsigned char _8;
  long unsigned int _9;
  long unsigned int _10;
  unsigned char _11;
  long unsigned int _12;
  signed int _13;
  unsigned char _14;
  clock_element_state_t iftmp.57_15;
  clock_element_state_t iftmp.58_16;
  clock_element_state_t iftmp.59_17;
  clock_element_state_t iftmp.60_18;
  long unsigned int _31;
  long unsigned int _32;
  long unsigned int _33;
  long unsigned int _34;
  <unnamed type> iftmp.61_35;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  clkState[0] = 255;
  # DEBUG BEGIN_STMT
  _1 = freqPointers[1];
  if (_1 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _3 ={v} MEM[(struct FIRC_Type *)1076690944B].STDBY_ENABLE;
  _4 = _3 & 1;
  if (_4 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 4> [local count: 268435456]:

  <bb 5> [local count: 536870913]:
  # iftmp.57_15 = PHI <0(3), 255(4)>
  clkState[1] = iftmp.57_15;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _5 = freqPointers[4];
  if (_5 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _6 ={v} MEM[(volatile struct ExtOSC_Type *)1076707328B].STAT;
  _7 = (signed int) _6;
  if (_7 >= 0)
    goto <bb 9>; [59.00%]
  else
    goto <bb 8>; [41.00%]

  <bb 8> [local count: 220117074]:

  <bb 9> [local count: 536870913]:
  # iftmp.58_16 = PHI <0(7), 255(8)>
  clkState[4] = iftmp.58_16;

  <bb 10> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _8 = freqPointers[3];
  if (_8 == 0)
    goto <bb 11>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 11> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _9 ={v} MEM[(struct SIRC_Type *)1076658176B].MISCELLANEOUS_IN;
  _10 = _9 & 256;
  if (_10 == 0)
    goto <bb 13>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 268435456]:

  <bb 13> [local count: 536870913]:
  # iftmp.59_17 = PHI <0(11), 255(12)>
  clkState[3] = iftmp.59_17;

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  clkState[2] = 255;
  # DEBUG BEGIN_STMT
  _11 = freqPointers[5];
  if (_11 == 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 18>; [50.00%]

  <bb 15> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _12 ={v} MEM[(struct SXOSC_Type *)1076674560B].SXOSC_STAT;
  _13 = (signed int) _12;
  if (_13 >= 0)
    goto <bb 17>; [59.00%]
  else
    goto <bb 16>; [41.00%]

  <bb 16> [local count: 220117074]:

  <bb 17> [local count: 536870913]:
  # iftmp.60_18 = PHI <0(15), 255(16)>
  clkState[5] = iftmp.60_18;

  <bb 18> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _14 = freqPointers[6];
  if (_14 == 0)
    goto <bb 19>; [50.00%]
  else
    goto <bb 25>; [50.00%]

  <bb 19> [local count: 536870913]:
  # DEBUG INLINE_ENTRY NOT_UNDER_MCU_CONTROL_A
  # DEBUG BEGIN_STMT
  _31 ={v} MEM[(struct MC_ME_Type *)1076740096B].PRTN1_COFB1_STAT;
  _32 = _31 & 16777216;
  if (_32 != 0)
    goto <bb 20>; [50.00%]
  else
    goto <bb 23>; [50.00%]

  <bb 20> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _33 ={v} MEM[(volatile struct PLL_Type *)1076756480B].PLLSR;
  _34 = _33 & 4;
  if (_34 == 0)
    goto <bb 22>; [50.00%]
  else
    goto <bb 21>; [50.00%]

  <bb 21> [local count: 134217728]:

  <bb 22> [local count: 268435456]:
  # iftmp.61_35 = PHI <0(20), 255(21)>
  clkState[6] = iftmp.61_35;
  goto <bb 24>; [100.00%]

  <bb 23> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  clkState[6] = 0;

  <bb 24> [local count: 536870913]:

  <bb 25> [local count: 1073741824]:
  return;

}



;; Function CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS (CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS, funcdef_no=25, decl_uid=5246, cgraph_uid=26, symbol_order=61)


Symbols to be put in SSA form
{ D.6666 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 18
Number of blocks to update: 17 ( 94%)


Removing basic block 9
Removing basic block 14
Removing basic block 15
Merging blocks 16 and 17
;; 2 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2 3 4 5 6 7 8 9 10 11 12 13
;;
;; Loop 1
;;  header 6, latch 5
;;  depth 1, outer 0
;;  nodes: 6 5 3
;; 2 succs { 6 }
;; 3 succs { 4 5 }
;; 4 succs { 7 }
;; 5 succs { 6 }
;; 6 succs { 3 7 }
;; 7 succs { 8 12 }
;; 8 succs { 11 9 10 }
;; 9 succs { 13 }
;; 10 succs { 13 }
;; 11 succs { 13 }
;; 12 succs { 13 }
;; 13 succs { 1 }
CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS ()
{
  const struct Clock_Ip_SelectorConfigType * selectorSCS_CLK;
  uint32 i;
  const struct Clock_Ip_ClockConfigType * config_clock.16_1;
  <unnamed type> _2;
  const struct Clock_Ip_ClockConfigType * config_clock.16_4;
  unsigned char _5;
  long unsigned int _6;
  <unnamed type> _7;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _31;
  long unsigned int _32;
  long unsigned int _33;
  long unsigned int _34;

  <bb 2> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG selectorSCS_CLK => 0B
  # DEBUG BEGIN_STMT
  # DEBUG i => 0
  goto <bb 6>; [100.00%]

  <bb 3> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _2 = config_clock.16_4->selectors[i_13].name;
  if (_2 == 12)
    goto <bb 4>; [5.50%]
  else
    goto <bb 5>; [94.50%]

  <bb 4> [local count: 55807731]:
  # config_clock.16_1 = PHI <config_clock.16_4(3)>
  # i_3 = PHI <i_13(3)>
  # DEBUG BEGIN_STMT
  selectorSCS_CLK_18 = &config_clock.16_1->selectors[i_3];
  # DEBUG selectorSCS_CLK => selectorSCS_CLK_18
  # DEBUG BEGIN_STMT
  goto <bb 7>; [100.00%]

  <bb 5> [local count: 958878293]:
  # DEBUG BEGIN_STMT
  i_17 = i_13 + 1;
  # DEBUG i => i_17

  <bb 6> [local count: 1073741824]:
  # i_13 = PHI <0(2), i_17(5)>
  # DEBUG i => i_13
  # DEBUG BEGIN_STMT
  config_clock.16_4 = config_clock;
  _5 = config_clock.16_4->selectorsCount;
  _6 = (long unsigned int) _5;
  if (_6 > i_13)
    goto <bb 3>; [94.50%]
  else
    goto <bb 7>; [5.50%]

  <bb 7> [local count: 114863532]:
  # selectorSCS_CLK_14 = PHI <selectorSCS_CLK_18(4), 0B(6)>
  # DEBUG selectorSCS_CLK => selectorSCS_CLK_14
  # DEBUG BEGIN_STMT
  if (selectorSCS_CLK_14 != 0B)
    goto <bb 8>; [70.00%]
  else
    goto <bb 12>; [30.00%]

  <bb 8> [local count: 80404472]:
  # DEBUG BEGIN_STMT
  _7 = selectorSCS_CLK_14->value;
  switch (_7) <default: <L8> [33.33%], case 0: <L12> [33.33%], case 8: <L7> [33.33%]>

  <bb 9> [local count: 26798811]:
<L12>:
  # DEBUG INLINE_ENTRY CALCULATE_CONFIGURED_CORE_AIPS_SLOW_PLAT_CLKS
  # DEBUG BEGIN_STMT
  _31 = bufferFreqs[8];
  configuredCoreClock = _31;
  # DEBUG BEGIN_STMT
  _32 = bufferFreqs[9];
  configuredAipsPlatClock = _32;
  # DEBUG BEGIN_STMT
  _33 = bufferFreqs[10];
  configuredAipsSlowClock = _33;
  # DEBUG BEGIN_STMT
  _34 = bufferFreqs[11];
  configuredHseClock = _34;
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  goto <bb 13>; [100.00%]

  <bb 10> [local count: 26798811]:
<L7>:
  # DEBUG BEGIN_STMT
  _9 = bufferFreqs[28];
  configuredCoreClock = _9;
  # DEBUG BEGIN_STMT
  _10 = bufferFreqs[29];
  configuredAipsPlatClock = _10;
  # DEBUG BEGIN_STMT
  _11 = bufferFreqs[30];
  configuredAipsSlowClock = _11;
  # DEBUG BEGIN_STMT
  _12 = bufferFreqs[31];
  configuredHseClock = _12;
  # DEBUG BEGIN_STMT
  goto <bb 13>; [100.00%]

  <bb 11> [local count: 26798811]:
<L8>:
  # DEBUG BEGIN_STMT
  configuredCoreClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsPlatClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock = 0;
  # DEBUG BEGIN_STMT
  configuredHseClock = 0;
  # DEBUG BEGIN_STMT
  goto <bb 13>; [100.00%]

  <bb 12> [local count: 34459060]:
  # DEBUG BEGIN_STMT
  configuredCoreClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsPlatClock = 0;
  # DEBUG BEGIN_STMT
  configuredAipsSlowClock = 0;
  # DEBUG BEGIN_STMT
  configuredHseClock = 0;

  <bb 13> [local count: 114855491]:
  # DEBUG i => NULL
  # DEBUG selectorSCS_CLK => NULL
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  return;

}



;; Function get_RTC0_CLK_Frequency (get_RTC0_CLK_Frequency, funcdef_no=373, decl_uid=5585, cgraph_uid=160, symbol_order=197)


Symbols to be put in SSA form
{ D.7431 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_RTC0_CLK_Frequency ()
{
  uint32 D.7431;
  uint32 retval.362;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = 0;
  retval.362_1 = _3;
  return retval.362_1;

}



;; Function get_ADC1_CLK_Frequency (get_ADC1_CLK_Frequency, funcdef_no=169, decl_uid=5379, cgraph_uid=44, symbol_order=81)


Symbols to be put in SSA form
{ D.6990 D.7434 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_ADC1_CLK_Frequency ()
{
  uint32 D.7434;
  uint32 retval.260;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.260_2 = _6;
  return retval.260_2;

}



;; Function get_ADC2_CLK_Frequency (get_ADC2_CLK_Frequency, funcdef_no=171, decl_uid=5381, cgraph_uid=45, symbol_order=82)


Symbols to be put in SSA form
{ D.6992 D.7437 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_ADC2_CLK_Frequency ()
{
  uint32 D.7437;
  uint32 retval.261;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.261_2 = _6;
  return retval.261_2;

}



;; Function get_BCTU0_CLK_Frequency (get_BCTU0_CLK_Frequency, funcdef_no=173, decl_uid=5383, cgraph_uid=46, symbol_order=83)


Symbols to be put in SSA form
{ D.6994 D.7440 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_BCTU0_CLK_Frequency ()
{
  uint32 D.7440;
  uint32 retval.262;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.262_2 = _6;
  return retval.262_2;

}



;; Function get_DMAMUX0_CLK_Frequency (get_DMAMUX0_CLK_Frequency, funcdef_no=175, decl_uid=5397, cgraph_uid=47, symbol_order=84)


Symbols to be put in SSA form
{ D.6996 D.7443 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_DMAMUX0_CLK_Frequency ()
{
  uint32 D.7443;
  uint32 retval.263;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.263_2 = _6;
  return retval.263_2;

}



;; Function get_DMAMUX1_CLK_Frequency (get_DMAMUX1_CLK_Frequency, funcdef_no=177, decl_uid=5399, cgraph_uid=48, symbol_order=85)


Symbols to be put in SSA form
{ D.6998 D.7446 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_DMAMUX1_CLK_Frequency ()
{
  uint32 D.7446;
  uint32 retval.264;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.264_2 = _6;
  return retval.264_2;

}



;; Function get_EDMA0_CLK_Frequency (get_EDMA0_CLK_Frequency, funcdef_no=179, decl_uid=5401, cgraph_uid=49, symbol_order=86)


Symbols to be put in SSA form
{ D.7000 D.7449 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_CLK_Frequency ()
{
  uint32 D.7449;
  uint32 retval.265;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.265_2 = _6;
  return retval.265_2;

}



;; Function get_EDMA0_TCD0_CLK_Frequency (get_EDMA0_TCD0_CLK_Frequency, funcdef_no=181, decl_uid=5403, cgraph_uid=50, symbol_order=87)


Symbols to be put in SSA form
{ D.7002 D.7452 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD0_CLK_Frequency ()
{
  uint32 D.7452;
  uint32 retval.266;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.266_2 = _6;
  return retval.266_2;

}



;; Function get_EDMA0_TCD10_CLK_Frequency (get_EDMA0_TCD10_CLK_Frequency, funcdef_no=183, decl_uid=5405, cgraph_uid=51, symbol_order=88)


Symbols to be put in SSA form
{ D.7004 D.7455 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD10_CLK_Frequency ()
{
  uint32 D.7455;
  uint32 retval.267;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.267_2 = _6;
  return retval.267_2;

}



;; Function get_EDMA0_TCD11_CLK_Frequency (get_EDMA0_TCD11_CLK_Frequency, funcdef_no=185, decl_uid=5407, cgraph_uid=52, symbol_order=89)


Symbols to be put in SSA form
{ D.7006 D.7458 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD11_CLK_Frequency ()
{
  uint32 D.7458;
  uint32 retval.268;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.268_2 = _6;
  return retval.268_2;

}



;; Function get_EDMA0_TCD12_CLK_Frequency (get_EDMA0_TCD12_CLK_Frequency, funcdef_no=187, decl_uid=5409, cgraph_uid=53, symbol_order=90)


Symbols to be put in SSA form
{ D.7008 D.7461 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD12_CLK_Frequency ()
{
  uint32 D.7461;
  uint32 retval.269;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.269_2 = _6;
  return retval.269_2;

}



;; Function get_EDMA0_TCD13_CLK_Frequency (get_EDMA0_TCD13_CLK_Frequency, funcdef_no=189, decl_uid=5411, cgraph_uid=54, symbol_order=91)


Symbols to be put in SSA form
{ D.7010 D.7464 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD13_CLK_Frequency ()
{
  uint32 D.7464;
  uint32 retval.270;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.270_2 = _6;
  return retval.270_2;

}



;; Function get_EDMA0_TCD14_CLK_Frequency (get_EDMA0_TCD14_CLK_Frequency, funcdef_no=191, decl_uid=5413, cgraph_uid=55, symbol_order=92)


Symbols to be put in SSA form
{ D.7012 D.7467 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD14_CLK_Frequency ()
{
  uint32 D.7467;
  uint32 retval.271;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.271_2 = _6;
  return retval.271_2;

}



;; Function get_EDMA0_TCD15_CLK_Frequency (get_EDMA0_TCD15_CLK_Frequency, funcdef_no=193, decl_uid=5415, cgraph_uid=56, symbol_order=93)


Symbols to be put in SSA form
{ D.7014 D.7470 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD15_CLK_Frequency ()
{
  uint32 D.7470;
  uint32 retval.272;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.272_2 = _6;
  return retval.272_2;

}



;; Function get_EDMA0_TCD16_CLK_Frequency (get_EDMA0_TCD16_CLK_Frequency, funcdef_no=195, decl_uid=5417, cgraph_uid=57, symbol_order=94)


Symbols to be put in SSA form
{ D.7016 D.7473 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD16_CLK_Frequency ()
{
  uint32 D.7473;
  uint32 retval.273;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.273_2 = _6;
  return retval.273_2;

}



;; Function get_EDMA0_TCD17_CLK_Frequency (get_EDMA0_TCD17_CLK_Frequency, funcdef_no=197, decl_uid=5419, cgraph_uid=58, symbol_order=95)


Symbols to be put in SSA form
{ D.7018 D.7476 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD17_CLK_Frequency ()
{
  uint32 D.7476;
  uint32 retval.274;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.274_2 = _6;
  return retval.274_2;

}



;; Function get_EDMA0_TCD18_CLK_Frequency (get_EDMA0_TCD18_CLK_Frequency, funcdef_no=199, decl_uid=5421, cgraph_uid=59, symbol_order=96)


Symbols to be put in SSA form
{ D.7020 D.7479 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD18_CLK_Frequency ()
{
  uint32 D.7479;
  uint32 retval.275;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.275_2 = _6;
  return retval.275_2;

}



;; Function get_EDMA0_TCD19_CLK_Frequency (get_EDMA0_TCD19_CLK_Frequency, funcdef_no=201, decl_uid=5423, cgraph_uid=60, symbol_order=97)


Symbols to be put in SSA form
{ D.7022 D.7482 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD19_CLK_Frequency ()
{
  uint32 D.7482;
  uint32 retval.276;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.276_2 = _6;
  return retval.276_2;

}



;; Function get_EDMA0_TCD1_CLK_Frequency (get_EDMA0_TCD1_CLK_Frequency, funcdef_no=203, decl_uid=5425, cgraph_uid=61, symbol_order=98)


Symbols to be put in SSA form
{ D.7024 D.7485 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD1_CLK_Frequency ()
{
  uint32 D.7485;
  uint32 retval.277;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.277_2 = _6;
  return retval.277_2;

}



;; Function get_EDMA0_TCD20_CLK_Frequency (get_EDMA0_TCD20_CLK_Frequency, funcdef_no=205, decl_uid=5427, cgraph_uid=62, symbol_order=99)


Symbols to be put in SSA form
{ D.7026 D.7488 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD20_CLK_Frequency ()
{
  uint32 D.7488;
  uint32 retval.278;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.278_2 = _6;
  return retval.278_2;

}



;; Function get_EDMA0_TCD21_CLK_Frequency (get_EDMA0_TCD21_CLK_Frequency, funcdef_no=207, decl_uid=5429, cgraph_uid=63, symbol_order=100)


Symbols to be put in SSA form
{ D.7028 D.7491 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD21_CLK_Frequency ()
{
  uint32 D.7491;
  uint32 retval.279;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.279_2 = _6;
  return retval.279_2;

}



;; Function get_EDMA0_TCD22_CLK_Frequency (get_EDMA0_TCD22_CLK_Frequency, funcdef_no=209, decl_uid=5431, cgraph_uid=64, symbol_order=101)


Symbols to be put in SSA form
{ D.7030 D.7494 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD22_CLK_Frequency ()
{
  uint32 D.7494;
  uint32 retval.280;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.280_2 = _6;
  return retval.280_2;

}



;; Function get_EDMA0_TCD23_CLK_Frequency (get_EDMA0_TCD23_CLK_Frequency, funcdef_no=211, decl_uid=5433, cgraph_uid=65, symbol_order=102)


Symbols to be put in SSA form
{ D.7032 D.7497 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD23_CLK_Frequency ()
{
  uint32 D.7497;
  uint32 retval.281;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.281_2 = _6;
  return retval.281_2;

}



;; Function get_EDMA0_TCD24_CLK_Frequency (get_EDMA0_TCD24_CLK_Frequency, funcdef_no=213, decl_uid=5435, cgraph_uid=66, symbol_order=103)


Symbols to be put in SSA form
{ D.7034 D.7500 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD24_CLK_Frequency ()
{
  uint32 D.7500;
  uint32 retval.282;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.282_2 = _6;
  return retval.282_2;

}



;; Function get_EDMA0_TCD25_CLK_Frequency (get_EDMA0_TCD25_CLK_Frequency, funcdef_no=215, decl_uid=5437, cgraph_uid=67, symbol_order=104)


Symbols to be put in SSA form
{ D.7036 D.7503 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD25_CLK_Frequency ()
{
  uint32 D.7503;
  uint32 retval.283;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.283_2 = _6;
  return retval.283_2;

}



;; Function get_EDMA0_TCD26_CLK_Frequency (get_EDMA0_TCD26_CLK_Frequency, funcdef_no=217, decl_uid=5439, cgraph_uid=68, symbol_order=105)


Symbols to be put in SSA form
{ D.7038 D.7506 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD26_CLK_Frequency ()
{
  uint32 D.7506;
  uint32 retval.284;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.284_2 = _6;
  return retval.284_2;

}



;; Function get_EDMA0_TCD27_CLK_Frequency (get_EDMA0_TCD27_CLK_Frequency, funcdef_no=219, decl_uid=5441, cgraph_uid=69, symbol_order=106)


Symbols to be put in SSA form
{ D.7040 D.7509 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD27_CLK_Frequency ()
{
  uint32 D.7509;
  uint32 retval.285;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.285_2 = _6;
  return retval.285_2;

}



;; Function get_EDMA0_TCD28_CLK_Frequency (get_EDMA0_TCD28_CLK_Frequency, funcdef_no=221, decl_uid=5443, cgraph_uid=70, symbol_order=107)


Symbols to be put in SSA form
{ D.7042 D.7512 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD28_CLK_Frequency ()
{
  uint32 D.7512;
  uint32 retval.286;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.286_2 = _6;
  return retval.286_2;

}



;; Function get_EDMA0_TCD29_CLK_Frequency (get_EDMA0_TCD29_CLK_Frequency, funcdef_no=223, decl_uid=5445, cgraph_uid=71, symbol_order=108)


Symbols to be put in SSA form
{ D.7044 D.7515 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD29_CLK_Frequency ()
{
  uint32 D.7515;
  uint32 retval.287;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.287_2 = _6;
  return retval.287_2;

}



;; Function get_EDMA0_TCD2_CLK_Frequency (get_EDMA0_TCD2_CLK_Frequency, funcdef_no=225, decl_uid=5447, cgraph_uid=72, symbol_order=109)


Symbols to be put in SSA form
{ D.7046 D.7518 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD2_CLK_Frequency ()
{
  uint32 D.7518;
  uint32 retval.288;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.288_2 = _6;
  return retval.288_2;

}



;; Function get_EDMA0_TCD30_CLK_Frequency (get_EDMA0_TCD30_CLK_Frequency, funcdef_no=227, decl_uid=5449, cgraph_uid=73, symbol_order=110)


Symbols to be put in SSA form
{ D.7048 D.7521 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD30_CLK_Frequency ()
{
  uint32 D.7521;
  uint32 retval.289;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.289_2 = _6;
  return retval.289_2;

}



;; Function get_EDMA0_TCD31_CLK_Frequency (get_EDMA0_TCD31_CLK_Frequency, funcdef_no=229, decl_uid=5451, cgraph_uid=74, symbol_order=111)


Symbols to be put in SSA form
{ D.7050 D.7524 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD31_CLK_Frequency ()
{
  uint32 D.7524;
  uint32 retval.290;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.290_2 = _6;
  return retval.290_2;

}



;; Function get_EDMA0_TCD3_CLK_Frequency (get_EDMA0_TCD3_CLK_Frequency, funcdef_no=231, decl_uid=5453, cgraph_uid=75, symbol_order=112)


Symbols to be put in SSA form
{ D.7052 D.7527 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD3_CLK_Frequency ()
{
  uint32 D.7527;
  uint32 retval.291;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.291_2 = _6;
  return retval.291_2;

}



;; Function get_EDMA0_TCD4_CLK_Frequency (get_EDMA0_TCD4_CLK_Frequency, funcdef_no=233, decl_uid=5455, cgraph_uid=76, symbol_order=113)


Symbols to be put in SSA form
{ D.7054 D.7530 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD4_CLK_Frequency ()
{
  uint32 D.7530;
  uint32 retval.292;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.292_2 = _6;
  return retval.292_2;

}



;; Function get_EDMA0_TCD5_CLK_Frequency (get_EDMA0_TCD5_CLK_Frequency, funcdef_no=235, decl_uid=5457, cgraph_uid=77, symbol_order=114)


Symbols to be put in SSA form
{ D.7056 D.7533 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD5_CLK_Frequency ()
{
  uint32 D.7533;
  uint32 retval.293;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.293_2 = _6;
  return retval.293_2;

}



;; Function get_EDMA0_TCD6_CLK_Frequency (get_EDMA0_TCD6_CLK_Frequency, funcdef_no=237, decl_uid=5459, cgraph_uid=78, symbol_order=115)


Symbols to be put in SSA form
{ D.7058 D.7536 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD6_CLK_Frequency ()
{
  uint32 D.7536;
  uint32 retval.294;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.294_2 = _6;
  return retval.294_2;

}



;; Function get_EDMA0_TCD7_CLK_Frequency (get_EDMA0_TCD7_CLK_Frequency, funcdef_no=239, decl_uid=5461, cgraph_uid=79, symbol_order=116)


Symbols to be put in SSA form
{ D.7060 D.7539 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD7_CLK_Frequency ()
{
  uint32 D.7539;
  uint32 retval.295;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.295_2 = _6;
  return retval.295_2;

}



;; Function get_EDMA0_TCD8_CLK_Frequency (get_EDMA0_TCD8_CLK_Frequency, funcdef_no=241, decl_uid=5463, cgraph_uid=80, symbol_order=117)


Symbols to be put in SSA form
{ D.7062 D.7542 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD8_CLK_Frequency ()
{
  uint32 D.7542;
  uint32 retval.296;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.296_2 = _6;
  return retval.296_2;

}



;; Function get_EDMA0_TCD9_CLK_Frequency (get_EDMA0_TCD9_CLK_Frequency, funcdef_no=243, decl_uid=5465, cgraph_uid=81, symbol_order=118)


Symbols to be put in SSA form
{ D.7064 D.7545 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EDMA0_TCD9_CLK_Frequency ()
{
  uint32 D.7545;
  uint32 retval.297;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.297_2 = _6;
  return retval.297_2;

}



;; Function get_EMIOS0_CLK_Frequency (get_EMIOS0_CLK_Frequency, funcdef_no=245, decl_uid=5481, cgraph_uid=82, symbol_order=119)


Symbols to be put in SSA form
{ D.7066 D.7548 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EMIOS0_CLK_Frequency ()
{
  uint32 D.7548;
  uint32 retval.298;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.298_2 = _6;
  return retval.298_2;

}



;; Function get_EMIOS1_CLK_Frequency (get_EMIOS1_CLK_Frequency, funcdef_no=247, decl_uid=5483, cgraph_uid=83, symbol_order=120)


Symbols to be put in SSA form
{ D.7068 D.7551 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EMIOS1_CLK_Frequency ()
{
  uint32 D.7551;
  uint32 retval.299;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.299_2 = _6;
  return retval.299_2;

}



;; Function get_EMIOS2_CLK_Frequency (get_EMIOS2_CLK_Frequency, funcdef_no=249, decl_uid=5485, cgraph_uid=84, symbol_order=121)


Symbols to be put in SSA form
{ D.7070 D.7554 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EMIOS2_CLK_Frequency ()
{
  uint32 D.7554;
  uint32 retval.300;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.300_2 = _6;
  return retval.300_2;

}



;; Function get_LCU0_CLK_Frequency (get_LCU0_CLK_Frequency, funcdef_no=251, decl_uid=5511, cgraph_uid=85, symbol_order=122)


Symbols to be put in SSA form
{ D.7072 D.7557 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LCU0_CLK_Frequency ()
{
  uint32 D.7557;
  uint32 retval.301;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.301_2 = _6;
  return retval.301_2;

}



;; Function get_LCU1_CLK_Frequency (get_LCU1_CLK_Frequency, funcdef_no=253, decl_uid=5513, cgraph_uid=86, symbol_order=123)


Symbols to be put in SSA form
{ D.7074 D.7560 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LCU1_CLK_Frequency ()
{
  uint32 D.7560;
  uint32 retval.302;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.302_2 = _6;
  return retval.302_2;

}



;; Function get_TCM_CM7_0_CLK_Frequency (get_TCM_CM7_0_CLK_Frequency, funcdef_no=255, decl_uid=5609, cgraph_uid=87, symbol_order=124)


Symbols to be put in SSA form
{ D.7076 D.7563 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_TCM_CM7_0_CLK_Frequency ()
{
  uint32 D.7563;
  uint32 retval.303;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.303_2 = _6;
  return retval.303_2;

}



;; Function get_TCM_CM7_1_CLK_Frequency (get_TCM_CM7_1_CLK_Frequency, funcdef_no=257, decl_uid=5611, cgraph_uid=88, symbol_order=125)


Symbols to be put in SSA form
{ D.7078 D.7566 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_TCM_CM7_1_CLK_Frequency ()
{
  uint32 D.7566;
  uint32 retval.304;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.304_2 = _6;
  return retval.304_2;

}



;; Function get_TEMPSENSE_CLK_Frequency (get_TEMPSENSE_CLK_Frequency, funcdef_no=259, decl_uid=5613, cgraph_uid=89, symbol_order=126)


Symbols to be put in SSA form
{ D.7080 D.7569 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_TEMPSENSE_CLK_Frequency ()
{
  uint32 D.7569;
  uint32 retval.305;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[13];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.305_2 = _6;
  return retval.305_2;

}



;; Function get_CMP1_CLK_Frequency (get_CMP1_CLK_Frequency, funcdef_no=261, decl_uid=5389, cgraph_uid=91, symbol_order=128)


Symbols to be put in SSA form
{ D.7082 D.7572 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_CMP1_CLK_Frequency ()
{
  uint32 D.7572;
  uint32 retval.306;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.306_2 = _6;
  return retval.306_2;

}



;; Function get_CMP2_CLK_Frequency (get_CMP2_CLK_Frequency, funcdef_no=263, decl_uid=5391, cgraph_uid=92, symbol_order=129)


Symbols to be put in SSA form
{ D.7084 D.7575 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_CMP2_CLK_Frequency ()
{
  uint32 D.7575;
  uint32 retval.307;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.307_2 = _6;
  return retval.307_2;

}



;; Function get_EIM0_CLK_Frequency (get_EIM0_CLK_Frequency, funcdef_no=265, decl_uid=5467, cgraph_uid=93, symbol_order=130)


Symbols to be put in SSA form
{ D.7086 D.7578 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_EIM0_CLK_Frequency ()
{
  uint32 D.7578;
  uint32 retval.308;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.308_2 = _6;
  return retval.308_2;

}



;; Function get_ERM0_CLK_Frequency (get_ERM0_CLK_Frequency, funcdef_no=267, decl_uid=5487, cgraph_uid=94, symbol_order=131)


Symbols to be put in SSA form
{ D.7088 D.7581 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_ERM0_CLK_Frequency ()
{
  uint32 D.7581;
  uint32 retval.309;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.309_2 = _6;
  return retval.309_2;

}



;; Function get_FLASH0_CLK_Frequency (get_FLASH0_CLK_Frequency, funcdef_no=269, decl_uid=5489, cgraph_uid=95, symbol_order=132)


Symbols to be put in SSA form
{ D.7090 D.7584 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_FLASH0_CLK_Frequency ()
{
  uint32 D.7584;
  uint32 retval.310;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.310_2 = _6;
  return retval.310_2;

}



;; Function get_LPI2C0_CLK_Frequency (get_LPI2C0_CLK_Frequency, funcdef_no=271, decl_uid=5515, cgraph_uid=96, symbol_order=133)


Symbols to be put in SSA form
{ D.7092 D.7587 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPI2C0_CLK_Frequency ()
{
  uint32 D.7587;
  uint32 retval.311;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.311_2 = _6;
  return retval.311_2;

}



;; Function get_LPI2C1_CLK_Frequency (get_LPI2C1_CLK_Frequency, funcdef_no=273, decl_uid=5517, cgraph_uid=97, symbol_order=134)


Symbols to be put in SSA form
{ D.7094 D.7590 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPI2C1_CLK_Frequency ()
{
  uint32 D.7590;
  uint32 retval.312;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.312_2 = _6;
  return retval.312_2;

}



;; Function get_LPSPI1_CLK_Frequency (get_LPSPI1_CLK_Frequency, funcdef_no=275, decl_uid=5521, cgraph_uid=98, symbol_order=135)


Symbols to be put in SSA form
{ D.7096 D.7593 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPSPI1_CLK_Frequency ()
{
  uint32 D.7593;
  uint32 retval.313;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.313_2 = _6;
  return retval.313_2;

}



;; Function get_LPSPI2_CLK_Frequency (get_LPSPI2_CLK_Frequency, funcdef_no=277, decl_uid=5523, cgraph_uid=99, symbol_order=136)


Symbols to be put in SSA form
{ D.7098 D.7596 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPSPI2_CLK_Frequency ()
{
  uint32 D.7596;
  uint32 retval.314;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.314_2 = _6;
  return retval.314_2;

}



;; Function get_LPSPI3_CLK_Frequency (get_LPSPI3_CLK_Frequency, funcdef_no=279, decl_uid=5525, cgraph_uid=100, symbol_order=137)


Symbols to be put in SSA form
{ D.7100 D.7599 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPSPI3_CLK_Frequency ()
{
  uint32 D.7599;
  uint32 retval.315;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.315_2 = _6;
  return retval.315_2;

}



;; Function get_LPSPI4_CLK_Frequency (get_LPSPI4_CLK_Frequency, funcdef_no=281, decl_uid=5527, cgraph_uid=101, symbol_order=138)


Symbols to be put in SSA form
{ D.7102 D.7602 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPSPI4_CLK_Frequency ()
{
  uint32 D.7602;
  uint32 retval.316;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.316_2 = _6;
  return retval.316_2;

}



;; Function get_LPSPI5_CLK_Frequency (get_LPSPI5_CLK_Frequency, funcdef_no=283, decl_uid=5529, cgraph_uid=102, symbol_order=139)


Symbols to be put in SSA form
{ D.7104 D.7605 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPSPI5_CLK_Frequency ()
{
  uint32 D.7605;
  uint32 retval.317;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.317_2 = _6;
  return retval.317_2;

}



;; Function get_LPUART10_CLK_Frequency (get_LPUART10_CLK_Frequency, funcdef_no=285, decl_uid=5533, cgraph_uid=103, symbol_order=140)


Symbols to be put in SSA form
{ D.7106 D.7608 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART10_CLK_Frequency ()
{
  uint32 D.7608;
  uint32 retval.318;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.318_2 = _6;
  return retval.318_2;

}



;; Function get_LPUART11_CLK_Frequency (get_LPUART11_CLK_Frequency, funcdef_no=287, decl_uid=5535, cgraph_uid=104, symbol_order=141)


Symbols to be put in SSA form
{ D.7108 D.7611 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART11_CLK_Frequency ()
{
  uint32 D.7611;
  uint32 retval.319;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.319_2 = _6;
  return retval.319_2;

}



;; Function get_LPUART12_CLK_Frequency (get_LPUART12_CLK_Frequency, funcdef_no=289, decl_uid=5537, cgraph_uid=105, symbol_order=142)


Symbols to be put in SSA form
{ D.7110 D.7614 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART12_CLK_Frequency ()
{
  uint32 D.7614;
  uint32 retval.320;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.320_2 = _6;
  return retval.320_2;

}



;; Function get_LPUART13_CLK_Frequency (get_LPUART13_CLK_Frequency, funcdef_no=291, decl_uid=5539, cgraph_uid=106, symbol_order=143)


Symbols to be put in SSA form
{ D.7112 D.7617 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART13_CLK_Frequency ()
{
  uint32 D.7617;
  uint32 retval.321;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.321_2 = _6;
  return retval.321_2;

}



;; Function get_LPUART14_CLK_Frequency (get_LPUART14_CLK_Frequency, funcdef_no=293, decl_uid=5541, cgraph_uid=107, symbol_order=144)


Symbols to be put in SSA form
{ D.7114 D.7620 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART14_CLK_Frequency ()
{
  uint32 D.7620;
  uint32 retval.322;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.322_2 = _6;
  return retval.322_2;

}



;; Function get_LPUART15_CLK_Frequency (get_LPUART15_CLK_Frequency, funcdef_no=295, decl_uid=5543, cgraph_uid=108, symbol_order=145)


Symbols to be put in SSA form
{ D.7116 D.7623 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART15_CLK_Frequency ()
{
  uint32 D.7623;
  uint32 retval.323;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.323_2 = _6;
  return retval.323_2;

}



;; Function get_LPUART1_CLK_Frequency (get_LPUART1_CLK_Frequency, funcdef_no=297, decl_uid=5545, cgraph_uid=109, symbol_order=146)


Symbols to be put in SSA form
{ D.7118 D.7626 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART1_CLK_Frequency ()
{
  uint32 D.7626;
  uint32 retval.324;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.324_2 = _6;
  return retval.324_2;

}



;; Function get_LPUART2_CLK_Frequency (get_LPUART2_CLK_Frequency, funcdef_no=299, decl_uid=5547, cgraph_uid=110, symbol_order=147)


Symbols to be put in SSA form
{ D.7120 D.7629 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART2_CLK_Frequency ()
{
  uint32 D.7629;
  uint32 retval.325;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.325_2 = _6;
  return retval.325_2;

}



;; Function get_LPUART3_CLK_Frequency (get_LPUART3_CLK_Frequency, funcdef_no=301, decl_uid=5549, cgraph_uid=111, symbol_order=148)


Symbols to be put in SSA form
{ D.7122 D.7632 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART3_CLK_Frequency ()
{
  uint32 D.7632;
  uint32 retval.326;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.326_2 = _6;
  return retval.326_2;

}



;; Function get_LPUART4_CLK_Frequency (get_LPUART4_CLK_Frequency, funcdef_no=303, decl_uid=5551, cgraph_uid=112, symbol_order=149)


Symbols to be put in SSA form
{ D.7124 D.7635 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART4_CLK_Frequency ()
{
  uint32 D.7635;
  uint32 retval.327;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.327_2 = _6;
  return retval.327_2;

}



;; Function get_LPUART5_CLK_Frequency (get_LPUART5_CLK_Frequency, funcdef_no=305, decl_uid=5553, cgraph_uid=113, symbol_order=150)


Symbols to be put in SSA form
{ D.7126 D.7638 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART5_CLK_Frequency ()
{
  uint32 D.7638;
  uint32 retval.328;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.328_2 = _6;
  return retval.328_2;

}



;; Function get_LPUART6_CLK_Frequency (get_LPUART6_CLK_Frequency, funcdef_no=307, decl_uid=5555, cgraph_uid=114, symbol_order=151)


Symbols to be put in SSA form
{ D.7128 D.7641 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART6_CLK_Frequency ()
{
  uint32 D.7641;
  uint32 retval.329;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.329_2 = _6;
  return retval.329_2;

}



;; Function get_LPUART7_CLK_Frequency (get_LPUART7_CLK_Frequency, funcdef_no=309, decl_uid=5557, cgraph_uid=115, symbol_order=152)


Symbols to be put in SSA form
{ D.7130 D.7644 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART7_CLK_Frequency ()
{
  uint32 D.7644;
  uint32 retval.330;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.330_2 = _6;
  return retval.330_2;

}



;; Function get_LPUART9_CLK_Frequency (get_LPUART9_CLK_Frequency, funcdef_no=311, decl_uid=5561, cgraph_uid=116, symbol_order=153)


Symbols to be put in SSA form
{ D.7132 D.7647 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART9_CLK_Frequency ()
{
  uint32 D.7647;
  uint32 retval.331;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.331_2 = _6;
  return retval.331_2;

}



;; Function get_MUA_CLK_Frequency (get_MUA_CLK_Frequency, funcdef_no=313, decl_uid=5565, cgraph_uid=117, symbol_order=154)


Symbols to be put in SSA form
{ D.7134 D.7650 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_MUA_CLK_Frequency ()
{
  uint32 D.7650;
  uint32 retval.332;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.332_2 = _6;
  return retval.332_2;

}



;; Function get_MUB_CLK_Frequency (get_MUB_CLK_Frequency, funcdef_no=315, decl_uid=5567, cgraph_uid=118, symbol_order=155)


Symbols to be put in SSA form
{ D.7136 D.7653 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_MUB_CLK_Frequency ()
{
  uint32 D.7653;
  uint32 retval.333;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.333_2 = _6;
  return retval.333_2;

}



;; Function get_PIT0_CLK_Frequency (get_PIT0_CLK_Frequency, funcdef_no=317, decl_uid=5569, cgraph_uid=119, symbol_order=156)


Symbols to be put in SSA form
{ D.7138 D.7656 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_PIT0_CLK_Frequency ()
{
  uint32 D.7656;
  uint32 retval.334;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.334_2 = _6;
  return retval.334_2;

}



;; Function get_PIT1_CLK_Frequency (get_PIT1_CLK_Frequency, funcdef_no=319, decl_uid=5571, cgraph_uid=120, symbol_order=157)


Symbols to be put in SSA form
{ D.7140 D.7659 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_PIT1_CLK_Frequency ()
{
  uint32 D.7659;
  uint32 retval.335;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.335_2 = _6;
  return retval.335_2;

}



;; Function get_PIT2_CLK_Frequency (get_PIT2_CLK_Frequency, funcdef_no=321, decl_uid=5573, cgraph_uid=121, symbol_order=158)


Symbols to be put in SSA form
{ D.7142 D.7662 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_PIT2_CLK_Frequency ()
{
  uint32 D.7662;
  uint32 retval.336;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.336_2 = _6;
  return retval.336_2;

}



;; Function get_SAI0_CLK_Frequency (get_SAI0_CLK_Frequency, funcdef_no=323, decl_uid=5587, cgraph_uid=122, symbol_order=159)


Symbols to be put in SSA form
{ D.7144 D.7665 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_SAI0_CLK_Frequency ()
{
  uint32 D.7665;
  uint32 retval.337;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.337_2 = _6;
  return retval.337_2;

}



;; Function get_SAI1_CLK_Frequency (get_SAI1_CLK_Frequency, funcdef_no=325, decl_uid=5589, cgraph_uid=123, symbol_order=160)


Symbols to be put in SSA form
{ D.7146 D.7668 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_SAI1_CLK_Frequency ()
{
  uint32 D.7668;
  uint32 retval.338;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.338_2 = _6;
  return retval.338_2;

}



;; Function get_STCU0_CLK_Frequency (get_STCU0_CLK_Frequency, funcdef_no=327, decl_uid=5595, cgraph_uid=124, symbol_order=161)


Symbols to be put in SSA form
{ D.7148 D.7671 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_STCU0_CLK_Frequency ()
{
  uint32 D.7671;
  uint32 retval.339;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.339_2 = _6;
  return retval.339_2;

}



;; Function get_TRGMUX0_CLK_Frequency (get_TRGMUX0_CLK_Frequency, funcdef_no=329, decl_uid=5617, cgraph_uid=125, symbol_order=162)


Symbols to be put in SSA form
{ D.7150 D.7674 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_TRGMUX0_CLK_Frequency ()
{
  uint32 D.7674;
  uint32 retval.340;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.340_2 = _6;
  return retval.340_2;

}



;; Function get_TSENSE0_CLK_Frequency (get_TSENSE0_CLK_Frequency, funcdef_no=331, decl_uid=5619, cgraph_uid=126, symbol_order=163)


Symbols to be put in SSA form
{ D.7152 D.7677 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_TSENSE0_CLK_Frequency ()
{
  uint32 D.7677;
  uint32 retval.341;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.341_2 = _6;
  return retval.341_2;

}



;; Function get_WKPU0_CLK_Frequency (get_WKPU0_CLK_Frequency, funcdef_no=333, decl_uid=5621, cgraph_uid=127, symbol_order=164)


Symbols to be put in SSA form
{ D.7154 D.7680 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_WKPU0_CLK_Frequency ()
{
  uint32 D.7680;
  uint32 retval.342;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[15];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.342_2 = _6;
  return retval.342_2;

}



;; Function get_FLEXIO0_CLK_Frequency (get_FLEXIO0_CLK_Frequency, funcdef_no=335, decl_uid=5507, cgraph_uid=129, symbol_order=166)


Symbols to be put in SSA form
{ D.7156 D.7683 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_FLEXIO0_CLK_Frequency ()
{
  uint32 D.7683;
  uint32 retval.343;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[14];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.343_2 = _6;
  return retval.343_2;

}



;; Function get_INTM_CLK_Frequency (get_INTM_CLK_Frequency, funcdef_no=337, decl_uid=5509, cgraph_uid=130, symbol_order=167)


Symbols to be put in SSA form
{ D.7158 D.7686 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_INTM_CLK_Frequency ()
{
  uint32 D.7686;
  uint32 retval.344;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[14];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.344_2 = _6;
  return retval.344_2;

}



;; Function get_LPSPI0_CLK_Frequency (get_LPSPI0_CLK_Frequency, funcdef_no=339, decl_uid=5519, cgraph_uid=131, symbol_order=168)


Symbols to be put in SSA form
{ D.7160 D.7689 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPSPI0_CLK_Frequency ()
{
  uint32 D.7689;
  uint32 retval.345;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[14];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.345_2 = _6;
  return retval.345_2;

}



;; Function get_LPUART0_CLK_Frequency (get_LPUART0_CLK_Frequency, funcdef_no=341, decl_uid=5531, cgraph_uid=132, symbol_order=169)


Symbols to be put in SSA form
{ D.7162 D.7692 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART0_CLK_Frequency ()
{
  uint32 D.7692;
  uint32 retval.346;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[14];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.346_2 = _6;
  return retval.346_2;

}



;; Function get_LPUART8_CLK_Frequency (get_LPUART8_CLK_Frequency, funcdef_no=343, decl_uid=5559, cgraph_uid=133, symbol_order=170)


Symbols to be put in SSA form
{ D.7164 D.7695 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_LPUART8_CLK_Frequency ()
{
  uint32 D.7695;
  uint32 retval.347;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[14];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.347_2 = _6;
  return retval.347_2;

}



;; Function get_MSCM_CLK_Frequency (get_MSCM_CLK_Frequency, funcdef_no=345, decl_uid=5563, cgraph_uid=134, symbol_order=171)


Symbols to be put in SSA form
{ D.7166 D.7698 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_MSCM_CLK_Frequency ()
{
  uint32 D.7698;
  uint32 retval.348;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[14];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.348_2 = _6;
  return retval.348_2;

}



;; Function get_SEMA42_CLK_Frequency (get_SEMA42_CLK_Frequency, funcdef_no=347, decl_uid=5591, cgraph_uid=135, symbol_order=172)


Symbols to be put in SSA form
{ D.7168 D.7701 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_SEMA42_CLK_Frequency ()
{
  uint32 D.7701;
  uint32 retval.349;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[14];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.349_2 = _6;
  return retval.349_2;

}



;; Function get_QSPI0_TX_MEM_CLK_Frequency (get_QSPI0_TX_MEM_CLK_Frequency, funcdef_no=349, decl_uid=5581, cgraph_uid=138, symbol_order=175)


Symbols to be put in SSA form
{ D.7170 D.7704 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_QSPI0_TX_MEM_CLK_Frequency ()
{
  uint32 D.7704;
  uint32 retval.350;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[19];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.350_2 = _6;
  return retval.350_2;

}



;; Function get_SWT1_CLK_Frequency (get_SWT1_CLK_Frequency, funcdef_no=351, decl_uid=5607, cgraph_uid=141, symbol_order=178)


Symbols to be put in SSA form
{ D.7172 D.7707 }
Incremental SSA update started at block: 0
Number of blocks in CFG: 6
Number of blocks to update: 5 ( 83%)


Merging blocks 2 and 4
Merging blocks 2 and 5
Merging blocks 2 and 3
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }
get_SWT1_CLK_Frequency ()
{
  uint32 D.7707;
  uint32 retval.351;
  unsigned char _3;
  int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _3 = freqPointers[2];
  _4 = (int) _3;
  _5 = bufferFreqs[_4];
  _6 = _5;
  retval.351_2 = _6;
  return retval.351_2;

}



;; Function UpdateClockState (UpdateClockState, funcdef_no=0, decl_uid=5029, cgraph_uid=1, symbol_order=36)

UpdateClockState (Clock_Ip_NameType name, clock_element_state_t state)
{
  int _1;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (name_3(D) <= 20)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (int) name_3(D);
  clkState[_1] = state_5(D);

  <bb 4> [local count: 1073741824]:
  return;

}



;; Function GetClockState (GetClockState, funcdef_no=1, decl_uid=5031, cgraph_uid=2, symbol_order=37)

GetClockState (Clock_Ip_NameType name)
{
  clock_element_state_t retValue;
  int _1;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (name_3(D) <= 20)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 = (int) name_3(D);
  retValue_6 = clkState[_1];
  # DEBUG retValue => retValue_6
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  retValue_5 = clkState[21];
  # DEBUG retValue => retValue_5

  <bb 5> [local count: 1073741824]:
  # retValue_2 = PHI <retValue_6(3), retValue_5(4)>
  # DEBUG retValue => retValue_2
  # DEBUG BEGIN_STMT
  return retValue_2;

}



;; Function SpecificPeripheralClockInitialization (SpecificPeripheralClockInitialization, funcdef_no=2, decl_uid=5033, cgraph_uid=3, symbol_order=38)

SpecificPeripheralClockInitialization (const struct Clock_IP_SpecificPeriphConfigType * config)
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}



;; Function SpecificPlatformInitClock (SpecificPlatformInitClock, funcdef_no=3, decl_uid=5035, cgraph_uid=4, symbol_order=39)

SpecificPlatformInitClock (const struct Clock_Ip_ClockConfigType * config)
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  config_clock = config_2(D);
  return;

}



;; Function GetProducerClockFreq (GetProducerClockFreq, funcdef_no=4, decl_uid=5037, cgraph_uid=5, symbol_order=40)

GetProducerClockFreq (Clock_Ip_NameType clockName)
{
  int _1;
  unsigned char _2;
  int _3;
  uint32 _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = (int) clockName_4(D);
  _2 = freqPointers[_1];
  _3 = (int) _2;
  _6 = bufferFreqs[_3];
  return _6;

}



;; Function UpdateFrequencies (UpdateFrequencies, funcdef_no=5, decl_uid=5041, cgraph_uid=6, symbol_order=41)

UpdateFrequencies (power_modes_t powerMode)
{
  uint8 pllEn;
  static const clock_element_state_t convertValueToClockState[256] = {0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 255};
  static const uint8 bufferFreqEntriesCLKOUT_RUN_CLK[3][13] = {"\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00", "\x00\x0f#\x10\x11\x12$\x13\x14\x15\x16\x17\x18", "\x00\x0f#\x10\x11\x12$%&\'(\x17\x18"};
  static const Clock_Ip_NameType selectorEntriesCLKOUT_RUN_CLK[13] = {21, 0, 8, 2, 4, 5, 9, 13, 16, 14, 15, 10, 11};
  static const uint8 bufferFreqEntriesQSPI_MEM_CLK[3] = "\x00\x0e\"";
  static const uint8 bufferFreqEntriesLBIST_CLK[3] = "\x00\r!";
  static const uint8 bufferFreqEntriesDCM_CLK[3] = "\x00\f ";
  static const uint8 bufferFreqEntriesHSE_CLK[3] = "\x00\v\x1f";
  static const uint8 bufferFreqEntriesAIPS_SLOW_CLK[3] = "\x00\n\x1e";
  static const uint8 bufferFreqEntriesAIPS_PLAT_CLK[3] = "\x00\t\x1d";
  static const uint8 bufferFreqEntriesCORE_CLK[3] = "\x00\b\x1c";
  static const uint8 bufferFreqEntriesSCS_CLK[3] = "\x00\x01\x1a";
  static const Clock_Ip_NameType selectorEntriesSCS_CLK[3] = {21, 0, 8};
  <unnamed type> _1;
  unsigned char _2;
  <unnamed type> _3;
  unsigned char _4;
  <unnamed type> _5;
  unsigned char _6;
  <unnamed type> _7;
  unsigned char _8;
  unsigned char _9;
  <unnamed type> _10;
  unsigned char _11;
  int _12;
  <unnamed type> _13;
  <unnamed type> _14;
  unsigned char _15;
  int _16;
  <unnamed type> _17;
  unsigned char _18;
  unsigned char _19;
  <unnamed type> _20;
  int _21;
  <unnamed type> _22;
  int _23;
  <unnamed type> _24;
  unsigned char _25;
  unsigned char _26;
  unsigned char _27;
  unsigned char _28;
  unsigned char _29;
  unsigned char _30;
  unsigned char _31;
  unsigned char _32;
  unsigned char _33;
  unsigned char _34;
  unsigned char _35;
  unsigned char _36;
  unsigned char _37;
  unsigned char _38;
  unsigned char _39;
  unsigned char _40;
  long unsigned int _41;
  long unsigned int _42;
  long unsigned int _43;
  <unnamed type> _44;
  int _45;
  <unnamed type> _46;
  int _47;
  <unnamed type> _48;
  unsigned char _49;
  unsigned char _50;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = clkState[1];
  _2 = _1 & 1;
  freqPointers[1] = _2;
  # DEBUG BEGIN_STMT
  _3 = clkState[3];
  _4 = _3 & 2;
  freqPointers[3] = _4;
  # DEBUG BEGIN_STMT
  pllEn_54 = clkState[6];
  # DEBUG pllEn => pllEn_54
  # DEBUG BEGIN_STMT
  _5 = clkState[4];
  _6 = _5 & 3;
  freqPointers[4] = _6;
  # DEBUG BEGIN_STMT
  _7 = clkState[5];
  _8 = _7 & 4;
  freqPointers[5] = _8;
  # DEBUG BEGIN_STMT
  _9 = pllEn_54 & 5;
  freqPointers[6] = _9;
  # DEBUG BEGIN_STMT
  _10 = clkState[8];
  _11 = _10 & pllEn_54;
  _12 = (int) _11;
  _13 = convertValueToClockState[_12];
  clkState[8] = _13;
  # DEBUG BEGIN_STMT
  _14 = clkState[9];
  _15 = _14 & pllEn_54;
  _16 = (int) _15;
  _17 = convertValueToClockState[_16];
  clkState[9] = _17;
  # DEBUG BEGIN_STMT
  _18 = _13 & 26;
  freqPointers[8] = _18;
  # DEBUG BEGIN_STMT
  _19 = _17 & 27;
  freqPointers[9] = _19;
  # DEBUG BEGIN_STMT
  _20 = clkState[12];
  _21 = (int) _20;
  _22 = selectorEntriesSCS_CLK[_21];
  _23 = (int) _22;
  _24 = clkState[_23];
  _25 = bufferFreqEntriesSCS_CLK[_21];
  _26 = _24 & _25;
  freqPointers[12] = _26;
  # DEBUG BEGIN_STMT
  _27 = bufferFreqEntriesCORE_CLK[_21];
  _28 = _24 & _27;
  freqPointers[13] = _28;
  # DEBUG BEGIN_STMT
  _29 = bufferFreqEntriesAIPS_PLAT_CLK[_21];
  _30 = _24 & _29;
  freqPointers[14] = _30;
  # DEBUG BEGIN_STMT
  _31 = bufferFreqEntriesAIPS_SLOW_CLK[_21];
  _32 = _24 & _31;
  freqPointers[15] = _32;
  # DEBUG BEGIN_STMT
  _33 = bufferFreqEntriesHSE_CLK[_21];
  _34 = _24 & _33;
  freqPointers[16] = _34;
  # DEBUG BEGIN_STMT
  _35 = bufferFreqEntriesDCM_CLK[_21];
  _36 = _24 & _35;
  freqPointers[17] = _36;
  # DEBUG BEGIN_STMT
  _37 = bufferFreqEntriesLBIST_CLK[_21];
  _38 = _24 & _37;
  freqPointers[18] = _38;
  # DEBUG BEGIN_STMT
  _39 = bufferFreqEntriesQSPI_MEM_CLK[_21];
  _40 = _24 & _39;
  freqPointers[19] = _40;
  # DEBUG BEGIN_STMT
  _41 ={v} MEM[(volatile struct cgmMux_Type *)1076724864B].CSS;
  _42 = _41 >> 24;
  _43 = _42 & 63;
  _44 = selectorEntryIndex[_43];
  clkState[20] = _44;
  # DEBUG BEGIN_STMT
  _45 = (int) _44;
  _46 = selectorEntriesCLKOUT_RUN_CLK[_45];
  _47 = (int) _46;
  _48 = clkState[_47];
  _49 = bufferFreqEntriesCLKOUT_RUN_CLK[_21][_45];
  _50 = _48 & _49;
  freqPointers[20] = _50;
  return;

}



;; Function McMeEnterKey (McMeEnterKey, funcdef_no=39, decl_uid=4863, cgraph_uid=40, symbol_order=75)

McMeEnterKey ()
{
  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  MEM[(struct MC_ME_Type *)1076740096B].CTL_KEY ={v} 23280;
  # DEBUG BEGIN_STMT
  MEM[(struct MC_ME_Type *)1076740096B].CTL_KEY ={v} 42255;
  return;

}


