
Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:
Symbol table:

FlexCAN_StartRxMessageFifoData.part.0/179 (FlexCAN_StartRxMessageFifoData.part.0) @06cc0a80
  Type: function definition analyzed
  Visibility: artificial
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: FlexCAN_StartRxMessageFifoData/60 (107374 (estimated locally),0.50 per call) 
  Calls: FlexCAN_SetMsgBuffIntCmd/132 (115158811 (estimated locally),0.11 per call) FlexCAN_SetMsgBuffIntCmd/132 (115158811 (estimated locally),0.11 per call) FlexCAN_SetMsgBuffIntCmd/132 (115158811 (estimated locally),0.11 per call) 
FlexCAN_GetMsgBuffIntStatusFlag.part.0/174 (FlexCAN_GetMsgBuffIntStatusFlag.part.0) @06d709a0
  Type: function definition analyzed
  Visibility: artificial
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: FlexCAN_GetMsgBuffIntStatusFlag/36 (134217728 (estimated locally),0.12 per call) 
  Calls: 
FlexCAN_SetEnhancedDataTimeSegments.part.0/172 (FlexCAN_SetEnhancedDataTimeSegments.part.0) @06d70620
  Type: function definition analyzed
  Visibility: artificial
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: FlexCAN_SetEnhancedDataTimeSegments/17 (107374 (estimated locally),0.50 per call) 
  Calls: 
FlexCAN_SetEnhancedNominalTimeSegments.part.0/170 (FlexCAN_SetEnhancedNominalTimeSegments.part.0) @06d702a0
  Type: function definition analyzed
  Visibility: artificial
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: FlexCAN_SetEnhancedNominalTimeSegments/15 (107374 (estimated locally),0.50 per call) 
  Calls: 
FlexCAN_SetExtendedTimeSegments.part.0/168 (FlexCAN_SetExtendedTimeSegments.part.0) @06cc2ee0
  Type: function definition analyzed
  Visibility: artificial
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: FlexCAN_SetExtendedTimeSegments/14 (107374 (estimated locally),0.50 per call) 
  Calls: 
FlexCAN_SetTimeSegments.part.0/166 (FlexCAN_SetTimeSegments.part.0) @06cc2b60
  Type: function definition analyzed
  Visibility: artificial
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: FlexCAN_SetTimeSegments/13 (107374 (estimated locally),0.50 per call) 
  Calls: 
FlexCAN_SetFDTimeSegments.part.0/164 (FlexCAN_SetFDTimeSegments.part.0) @06cc27e0
  Type: function definition analyzed
  Visibility: artificial
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) first_run:1 body local split_part optimize_size
  Called by: FlexCAN_SetFDTimeSegments/12 (107374 (estimated locally),0.50 per call) 
  Calls: 
FLEXCAN_ClearMsgBuffIntCmd/162 (FLEXCAN_ClearMsgBuffIntCmd) @0718e7e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_AbortTransfer/116 (12823 (estimated locally),0.06 per call) FlexCAN_AbortRxTransfer/68 (237404317 (estimated locally),0.22 per call) 
  Calls: 
FlexCAN_SetErrIntCmd/161 (FlexCAN_SetErrIntCmd) @0718e620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetErrorInt_Privileged/115 (5154 (estimated locally),0.02 per call) FlexCAN_Ip_SetErrorInt_Privileged/115 (5154 (estimated locally),0.02 per call) FlexCAN_Ip_SetErrorInt_Privileged/115 (15617 (estimated locally),0.07 per call) FlexCAN_Ip_SetErrorInt_Privileged/115 (15617 (estimated locally),0.07 per call) FlexCAN_Ip_SetErrorInt_Privileged/115 (15617 (estimated locally),0.07 per call) 
  Calls: 
FlexCAN_DisableInterrupts/160 (FlexCAN_DisableInterrupts) @0718e380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_DisableInterrupts_Privileged/114 (44539 (estimated locally),0.21 per call) 
  Calls: 
FlexCAN_EnableInterrupts/159 (FlexCAN_EnableInterrupts) @0718e1c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_EnableInterrupts_Privileged/113 (44539 (estimated locally),0.21 per call) 
  Calls: 
SchM_Exit_Can_CAN_EXCLUSIVE_AREA_17/158 (SchM_Exit_Can_CAN_EXCLUSIVE_AREA_17) @07179d20
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetTxArbitrationStartDelay_Privileged/110 (26575 (estimated locally),0.12 per call) 
  Calls: 
SchM_Enter_Can_CAN_EXCLUSIVE_AREA_17/157 (SchM_Enter_Can_CAN_EXCLUSIVE_AREA_17) @07179c40
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetTxArbitrationStartDelay_Privileged/110 (26575 (estimated locally),0.12 per call) 
  Calls: 
SchM_Exit_Can_CAN_EXCLUSIVE_AREA_16/156 (SchM_Exit_Can_CAN_EXCLUSIVE_AREA_16) @071798c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetTDCOffset_Privileged/109 (26575 (estimated locally),0.12 per call) 
  Calls: 
SchM_Enter_Can_CAN_EXCLUSIVE_AREA_16/155 (SchM_Enter_Can_CAN_EXCLUSIVE_AREA_16) @071797e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetTDCOffset_Privileged/109 (26575 (estimated locally),0.12 per call) 
  Calls: 
SchM_Exit_Can_CAN_EXCLUSIVE_AREA_15/154 (SchM_Exit_Can_CAN_EXCLUSIVE_AREA_15) @071792a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetBitrateCbt_Privileged/107 (6644 (estimated locally),0.03 per call) 
  Calls: 
SchM_Enter_Can_CAN_EXCLUSIVE_AREA_15/153 (SchM_Enter_Can_CAN_EXCLUSIVE_AREA_15) @071791c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetBitrateCbt_Privileged/107 (6644 (estimated locally),0.03 per call) 
  Calls: 
SchM_Exit_Can_CAN_EXCLUSIVE_AREA_14/152 (SchM_Exit_Can_CAN_EXCLUSIVE_AREA_14) @07165700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetBitrate_Privileged/102 (13288 (estimated locally),0.06 per call) 
  Calls: 
SchM_Enter_Can_CAN_EXCLUSIVE_AREA_14/151 (SchM_Enter_Can_CAN_EXCLUSIVE_AREA_14) @07165620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetBitrate_Privileged/102 (13288 (estimated locally),0.06 per call) 
  Calls: 
FlexCAN_GetMaxMbNum/150 (FlexCAN_GetMaxMbNum) @0714db60
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_SetRegDefaultVal/49 (1073741824 (estimated locally),1.00 per call) FlexCAN_SetRegDefaultVal/49 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
FlexCAN_ExitFreezeMode/149 (FlexCAN_ExitFreezeMode) @0714d540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetStartMode_Privileged/99 (107374 (estimated locally),0.50 per call) FlexCAN_Ip_ExitFreezeMode_Privileged/90 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
FlexCAN_GetMsgBuffRegion/148 (FlexCAN_GetMsgBuffRegion) @0714d0e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SendBlocking/87 (3012 (estimated locally),0.01 per call) FlexCAN_AbortRxTransfer/68 (354334802 (estimated locally),0.33 per call) FlexCAN_AbortRxTransfer/68 (237404317 (estimated locally),0.22 per call) FlexCAN_AbortTxTransfer/67 (114863532 (estimated locally),1.00 per call) 
  Calls: 
FlexCAN_GetMsgBuffTimestamp/147 (FlexCAN_GetMsgBuffTimestamp) @0712c380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_MainFunctionWrite/96 (35433 (estimated locally),0.16 per call) FlexCAN_IRQHandlerTxMB/62 (536870911 (estimated locally),0.50 per call) 
  Calls: 
FlexCAN_SetEnhancedRxFifoFilter/146 (FlexCAN_SetEnhancedRxFifoFilter) @07112d20
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_ConfigEnhancedRxFifo_Privileged/77 (6644 (estimated locally),0.03 per call) 
  Calls: 
FlexCAN_SetRxFifoFilter/145 (FlexCAN_SetRxFifoFilter) @07112a80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_ConfigRxFifo_Privileged/76 (26575 (estimated locally),0.12 per call) 
  Calls: 
FlexCAN_Enable/144 (FlexCAN_Enable) @071129a0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetListenOnlyMode_Privileged/119 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetRxMb15Mask_Privileged/118 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetRxMb14Mask_Privileged/117 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetErrorInt_Privileged/115 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetTxArbitrationStartDelay_Privileged/110 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetTDCOffset_Privileged/109 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetBitrateCbt_Privileged/107 (13690 (estimated locally),0.06 per call) FlexCAN_Ip_GetTDCValue_Privileged/106 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_GetTDCFail_Privileged/105 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_ClearTDCFail_Privileged/104 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetBitrate_Privileged/102 (13690 (estimated locally),0.06 per call) FlexCAN_Ip_SetRxMaskType_Privileged/101 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetRxFifoGlobalMask_Privileged/92 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetRxIndividualMask_Privileged/91 (11568 (estimated locally),0.05 per call) FlexCAN_Ip_SetRxMbGlobalMask_Privileged/88 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_ConfigEnhancedRxFifo_Privileged/77 (6845 (estimated locally),0.03 per call) FlexCAN_Ip_ConfigRxFifo_Privileged/76 (27380 (estimated locally),0.13 per call) 
  Calls: 
FlexCAN_ReadRxFifo/143 (FlexCAN_ReadRxFifo) @07112700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_IRQHandlerRxFIFO/63 (54331336 (estimated locally),0.05 per call) 
  Calls: 
FlexCAN_ReadEnhancedRxFifo/142 (FlexCAN_ReadEnhancedRxFifo) @071121c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_IRQHandlerEnhancedRxFIFO/66 (73014444 (estimated locally),0.07 per call) 
  Calls: 
FlexCAN_IsEnhancedRxFifoAvailable/141 (FlexCAN_IsEnhancedRxFifoAvailable) @070f97e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_DisableInterrupts_Privileged/114 (44539 (estimated locally),0.21 per call) FlexCAN_Ip_EnableInterrupts_Privileged/113 (14698 (estimated locally),0.07 per call) FlexCAN_Ip_MainFunctionRead/94 (10866 (estimated locally),0.05 per call) FlexCAN_Ip_ConfigEnhancedRxFifo_Privileged/77 (107374 (estimated locally),0.50 per call) FlexCAN_Ip_RxFifoBlocking/75 (107374 (estimated locally),0.50 per call) FlexCAN_Ip_RxFifo/74 (107374 (estimated locally),0.50 per call) FlexCAN_SetRegDefaultVal/49 (1073741824 (estimated locally),1.00 per call) FlexCAN_CompleteRxMessageEnhancedFifoData/54 (107374 (estimated locally),0.50 per call) 
  Calls: 
FlexCAN_GetMsgBuff/140 (FlexCAN_GetMsgBuff) @070f9540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_IRQHandlerTxMB/62 (536870911 (estimated locally),0.50 per call) FlexCAN_IRQHandlerRxMB/61 (1073741823 (estimated locally),1.00 per call) 
  Calls: 
FlexCAN_LockRxMsgBuff/139 (FlexCAN_LockRxMsgBuff) @070f9460
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_IRQHandlerTxMB/62 (536870911 (estimated locally),0.50 per call) FlexCAN_IRQHandlerRxMB/61 (1073741823 (estimated locally),1.00 per call) 
  Calls: 
OsIf_GetElapsed/138 (OsIf_GetElapsed) @070f91c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SendBlocking/87 (26606 (estimated locally),0.12 per call) FlexCAN_Ip_SendBlocking/87 (237131 (estimated locally),1.10 per call) FlexCAN_Ip_ReceiveBlocking/73 (313013 (estimated locally),1.46 per call) FlexCAN_AbortTxTransfer/67 (1014686025 (estimated locally),8.83 per call) FlexCAN_ProccessLegacyRxFIFO/57 (1014686025 (estimated locally),8.83 per call) FlexCAN_ProccessEnhancedRxFifo/56 (1014686025 (estimated locally),8.83 per call) 
  Calls: 
OsIf_GetCounter/137 (OsIf_GetCounter) @070f90e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SendBlocking/87 (3012 (estimated locally),0.01 per call) FlexCAN_Ip_SendBlocking/87 (214748 (estimated locally),1.00 per call) FlexCAN_Ip_ReceiveBlocking/73 (35433 (estimated locally),0.16 per call) FlexCAN_AbortTxTransfer/67 (114863532 (estimated locally),1.00 per call) FlexCAN_ProccessLegacyRxFIFO/57 (114863532 (estimated locally),1.00 per call) FlexCAN_ProccessEnhancedRxFifo/56 (114863532 (estimated locally),1.00 per call) 
  Calls: 
OsIf_MicrosToTicks/136 (OsIf_MicrosToTicks) @070f9000
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SendBlocking/87 (3012 (estimated locally),0.01 per call) FlexCAN_Ip_SendBlocking/87 (214748 (estimated locally),1.00 per call) FlexCAN_Ip_ReceiveBlocking/73 (214748 (estimated locally),1.00 per call) FlexCAN_AbortTxTransfer/67 (114863532 (estimated locally),1.00 per call) FlexCAN_ProccessLegacyRxFIFO/57 (114863532 (estimated locally),1.00 per call) FlexCAN_ProccessEnhancedRxFifo/56 (114863532 (estimated locally),1.00 per call) 
  Calls: 
FlexCAN_SetRxMsgBuff/135 (FlexCAN_SetRxMsgBuff) @070e1b60
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_ConfigRxMb/71 (25646 (estimated locally),0.12 per call) FlexCAN_Ip_ConfigRxMb/71 (25646 (estimated locally),0.12 per call) FlexCAN_Ip_ConfigRxMb/71 (25646 (estimated locally),0.12 per call) 
  Calls: 
FlexCAN_SetTxMsgBuff/134 (FlexCAN_SetTxMsgBuff) @070e18c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_ConfigRemoteResponseMb/78 (25646 (estimated locally),0.12 per call) FlexCAN_StartSendData/59 (16670 (estimated locally),0.08 per call) 
  Calls: 
FlexCAN_IsMbOutOfRange/133 (FlexCAN_IsMbOutOfRange) @070e17e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_ConfigRemoteResponseMb/78 (53687 (estimated locally),0.25 per call) FlexCAN_Ip_ConfigRxMb/71 (53687 (estimated locally),0.25 per call) FlexCAN_StartSendData/59 (53687 (estimated locally),0.25 per call) FlexCAN_StartRxMessageBufferData/58 (107374 (estimated locally),0.50 per call) 
  Calls: 
FlexCAN_SetMsgBuffIntCmd/132 (FlexCAN_SetMsgBuffIntCmd) @070e1540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_ConfigRemoteResponseMb/78 (8463 (estimated locally),0.04 per call) FlexCAN_Ip_ReceiveBlocking/73 (12047 (estimated locally),0.06 per call) FlexCAN_Ip_ReceiveBlocking/73 (17717 (estimated locally),0.08 per call) FlexCAN_Ip_Receive/72 (17717 (estimated locally),0.08 per call) FlexCAN_Ip_Send/70 (2923 (estimated locally),0.01 per call) FlexCAN_IRQHandlerTxMB/62 (147934780 (estimated locally),0.14 per call) FlexCAN_IRQHandlerTxMB/62 (177167401 (estimated locally),0.17 per call) FlexCAN_ProccessLegacyRxFIFO/57 (19089400 (estimated locally),0.17 per call) FlexCAN_ProccessLegacyRxFIFO/57 (19089400 (estimated locally),0.17 per call) FlexCAN_ProccessLegacyRxFIFO/57 (19089400 (estimated locally),0.17 per call) FlexCAN_IRQHandlerRxMB/61 (147934780 (estimated locally),0.14 per call) FlexCAN_IRQHandlerRxMB/61 (177167401 (estimated locally),0.17 per call) FlexCAN_CompleteRxMessageFifoData/80 (35433 (estimated locally),0.16 per call) FlexCAN_CompleteRxMessageFifoData/80 (35433 (estimated locally),0.16 per call) FlexCAN_CompleteRxMessageFifoData/80 (35433 (estimated locally),0.16 per call) FlexCAN_StartRxMessageFifoData.part.0/179 (115158811 (estimated locally),0.11 per call) FlexCAN_StartRxMessageFifoData.part.0/179 (115158811 (estimated locally),0.11 per call) FlexCAN_StartRxMessageFifoData.part.0/179 (115158811 (estimated locally),0.11 per call) 
  Calls: 
FlexCAN_EnableEnhancedRxFifo/131 (FlexCAN_EnableEnhancedRxFifo) @06795e00
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_InitRxFifo/52 (295869560 (estimated locally),0.28 per call) 
  Calls: 
FlexCAN_EnableRxFifo/130 (FlexCAN_EnableRxFifo) @06795d20
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_InitRxFifo/52 (354334802 (estimated locally),0.33 per call) 
  Calls: 
FlexCAN_SetMaxMsgBuffNum/129 (FlexCAN_SetMaxMsgBuffNum) @067957e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_InitController/53 (189246996 (estimated locally),0.18 per call) 
  Calls: 
FlexCAN_SetPayloadSize/128 (FlexCAN_SetPayloadSize) @06795700
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_InitController/53 (189246996 (estimated locally),0.18 per call) 
  Calls: 
FlexCAN_ConfigCtrlOptions/127 (FlexCAN_ConfigCtrlOptions) @06795620
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_InitController/53 (378493993 (estimated locally),0.35 per call) 
  Calls: 
FlexCAN_Init/126 (FlexCAN_Init) @06795540
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_InitController/53 (756987986 (estimated locally),0.71 per call) 
  Calls: 
FlexCAN_Disable/125 (FlexCAN_Disable) @06795460
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetListenOnlyMode_Privileged/119 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetRxMb15Mask_Privileged/118 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetRxMb14Mask_Privileged/117 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetErrorInt_Privileged/115 (25394 (estimated locally),0.12 per call) FlexCAN_Ip_SetTxArbitrationStartDelay_Privileged/110 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetTDCOffset_Privileged/109 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetBitrateCbt_Privileged/107 (13690 (estimated locally),0.06 per call) FlexCAN_Ip_GetTDCValue_Privileged/106 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_GetTDCFail_Privileged/105 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_ClearTDCFail_Privileged/104 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetBitrate_Privileged/102 (13690 (estimated locally),0.06 per call) FlexCAN_Ip_SetRxMaskType_Privileged/101 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetStopMode_Privileged/100 (35433 (estimated locally),0.16 per call) FlexCAN_Ip_Deinit_Privileged/93 (35433 (estimated locally),0.16 per call) FlexCAN_Ip_SetRxFifoGlobalMask_Privileged/92 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_SetRxIndividualMask_Privileged/91 (11568 (estimated locally),0.05 per call) FlexCAN_Ip_SetRxMbGlobalMask_Privileged/88 (27380 (estimated locally),0.13 per call) FlexCAN_Ip_ConfigEnhancedRxFifo_Privileged/77 (6845 (estimated locally),0.03 per call) FlexCAN_Ip_ConfigRxFifo_Privileged/76 (27380 (estimated locally),0.13 per call) FlexCAN_InitController/53 (62451509 (estimated locally),0.06 per call) FlexCAN_InitController/53 (189246996 (estimated locally),0.18 per call) FlexCAN_InitController/53 (378493993 (estimated locally),0.35 per call) FlexCAN_InitController/53 (209057533 (estimated locally),0.19 per call) 
  Calls: 
FlexCAN_EnterFreezeMode/124 (FlexCAN_EnterFreezeMode) @067951c0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_SetStopMode_Privileged/100 (107374 (estimated locally),0.50 per call) FlexCAN_Ip_Deinit_Privileged/93 (107374 (estimated locally),0.50 per call) FlexCAN_Ip_EnterFreezeMode_Privileged/89 (1073741824 (estimated locally),1.00 per call) FlexCAN_Ip_Init_Privileged/69 (17717 (estimated locally),0.08 per call) FlexCAN_InitController/53 (62451509 (estimated locally),0.06 per call) FlexCAN_InitController/53 (189246996 (estimated locally),0.18 per call) FlexCAN_InitController/53 (378493993 (estimated locally),0.35 per call) FlexCAN_InitController/53 (633507676 (estimated locally),0.59 per call) 
  Calls: 
FlexCAN_SetOperationMode/123 (FlexCAN_SetOperationMode) @067950e0
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_Init_Privileged/69 (17717 (estimated locally),0.08 per call) 
  Calls: 
SchM_Exit_Can_CAN_EXCLUSIVE_AREA_00/122 (SchM_Exit_Can_CAN_EXCLUSIVE_AREA_00) @06795000
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_Init_Privileged/69 (8858 (estimated locally),0.04 per call) FlexCAN_Ip_Init_Privileged/69 (8858 (estimated locally),0.04 per call) FlexCAN_InitController/53 (756987986 (estimated locally),0.71 per call) 
  Calls: 
SchM_Enter_Can_CAN_EXCLUSIVE_AREA_00/121 (SchM_Enter_Can_CAN_EXCLUSIVE_AREA_00) @070c5e00
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: FlexCAN_Ip_Init_Privileged/69 (8858 (estimated locally),0.04 per call) FlexCAN_Ip_Init_Privileged/69 (8858 (estimated locally),0.04 per call) FlexCAN_InitController/53 (756987986 (estimated locally),0.71 per call) 
  Calls: 
FlexCAN_Ip_GetListenOnlyMode/120 (FlexCAN_Ip_GetListenOnlyMode) @070c50e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
FlexCAN_Ip_SetListenOnlyMode_Privileged/119 (FlexCAN_Ip_SetListenOnlyMode_Privileged) @070c5d20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_SetListenOnlyMode/7 (26575 (estimated locally),0.12 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_SetRxMb15Mask_Privileged/118 (FlexCAN_Ip_SetRxMb15Mask_Privileged) @070c5a80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_SetRxMb14Mask_Privileged/117 (FlexCAN_Ip_SetRxMb14Mask_Privileged) @070c57e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_AbortTransfer/116 (FlexCAN_Ip_AbortTransfer) @070c5540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_AbortRxTransfer/68 (2595 (estimated locally),0.01 per call) FlexCAN_AbortTxTransfer/67 (2595 (estimated locally),0.01 per call) FLEXCAN_ClearMsgBuffIntCmd/162 (12823 (estimated locally),0.06 per call) 
FlexCAN_Ip_SetErrorInt_Privileged/115 (FlexCAN_Ip_SetErrorInt_Privileged) @070c52a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (25394 (estimated locally),0.12 per call) FlexCAN_SetErrIntCmd/161 (5154 (estimated locally),0.02 per call) FlexCAN_SetErrIntCmd/161 (5154 (estimated locally),0.02 per call) FlexCAN_SetErrIntCmd/161 (15617 (estimated locally),0.07 per call) FlexCAN_SetErrIntCmd/161 (15617 (estimated locally),0.07 per call) FlexCAN_SetErrIntCmd/161 (15617 (estimated locally),0.07 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_DisableInterrupts_Privileged/114 (FlexCAN_Ip_DisableInterrupts_Privileged) @070c5000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_IsEnhancedRxFifoAvailable/141 (44539 (estimated locally),0.21 per call) FlexCAN_DisableInterrupts/160 (44539 (estimated locally),0.21 per call) 
FlexCAN_Ip_EnableInterrupts_Privileged/113 (FlexCAN_Ip_EnableInterrupts_Privileged) @070b8b60
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_IsEnhancedRxFifoAvailable/141 (14698 (estimated locally),0.07 per call) FlexCAN_EnableInterrupts/159 (44539 (estimated locally),0.21 per call) 
FlexCAN_Ip_ClearBuffStatusFlag/112 (FlexCAN_Ip_ClearBuffStatusFlag) @070b8620
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_ClearMsgBuffIntStatusFlag/9 (52484 (estimated locally),0.24 per call) 
FlexCAN_Ip_GetBuffStatusFlag/111 (FlexCAN_Ip_GetBuffStatusFlag) @070b80e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_GetBuffStatusFlag/10 (52484 (estimated locally),0.24 per call) 
FlexCAN_Ip_SetTxArbitrationStartDelay_Privileged/110 (FlexCAN_Ip_SetTxArbitrationStartDelay_Privileged) @070b8d20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) SchM_Exit_Can_CAN_EXCLUSIVE_AREA_17/158 (26575 (estimated locally),0.12 per call) FlexCAN_SetTxArbitrationStartDelay/42 (26575 (estimated locally),0.12 per call) SchM_Enter_Can_CAN_EXCLUSIVE_AREA_17/157 (26575 (estimated locally),0.12 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_SetTDCOffset_Privileged/109 (FlexCAN_Ip_SetTDCOffset_Privileged) @070b8a80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) SchM_Exit_Can_CAN_EXCLUSIVE_AREA_16/156 (26575 (estimated locally),0.12 per call) FlexCAN_SetTDCOffset/2 (13288 (estimated locally),0.06 per call) FlexCAN_SetEnhancedTDCOffset/3 (13288 (estimated locally),0.06 per call) SchM_Enter_Can_CAN_EXCLUSIVE_AREA_16/155 (26575 (estimated locally),0.12 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_GetBitrateFD/108 (FlexCAN_Ip_GetBitrateFD) @070b87e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_GetFDTimeSegments/21 (26844 (estimated locally),0.13 per call) FlexCAN_GetEnhancedDataTimeSegments/18 (26844 (estimated locally),0.13 per call) 
FlexCAN_Ip_SetBitrateCbt_Privileged/107 (FlexCAN_Ip_SetBitrateCbt_Privileged) @070b8540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (13690 (estimated locally),0.06 per call) SchM_Exit_Can_CAN_EXCLUSIVE_AREA_15/154 (6644 (estimated locally),0.03 per call) FlexCAN_SetFDTimeSegments/12 (3322 (estimated locally),0.02 per call) FlexCAN_SetEnhancedDataTimeSegments/17 (3322 (estimated locally),0.02 per call) FlexCAN_SetFDEnabled/6 (6644 (estimated locally),0.03 per call) SchM_Enter_Can_CAN_EXCLUSIVE_AREA_15/153 (6644 (estimated locally),0.03 per call) FlexCAN_Enable/144 (13690 (estimated locally),0.06 per call) 
FlexCAN_Ip_GetTDCValue_Privileged/106 (FlexCAN_Ip_GetTDCValue_Privileged) @070b82a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_GetTDCFail_Privileged/105 (FlexCAN_Ip_GetTDCFail_Privileged) @070b8000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_ClearTDCFail_Privileged/104 (FlexCAN_Ip_ClearTDCFail_Privileged) @070abb60
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_GetBitrate/103 (FlexCAN_Ip_GetBitrate) @070ab620
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_GetTimeSegments/20 (21222 (estimated locally),0.10 per call) FlexCAN_GetExtendedTimeSegments/19 (14748 (estimated locally),0.07 per call) FlexCAN_GetEnhancedNominalTimeSegments/16 (17717 (estimated locally),0.08 per call) 
FlexCAN_Ip_SetBitrate_Privileged/102 (FlexCAN_Ip_SetBitrate_Privileged) @070ab0e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (13690 (estimated locally),0.06 per call) SchM_Exit_Can_CAN_EXCLUSIVE_AREA_14/152 (13288 (estimated locally),0.06 per call) FlexCAN_SetTimeSegments/13 (5253 (estimated locally),0.02 per call) FlexCAN_SetExtendedTimeSegments/14 (3650 (estimated locally),0.02 per call) FlexCAN_SetEnhancedNominalTimeSegments/15 (4385 (estimated locally),0.02 per call) FlexCAN_EnhCbtEnable/25 (13288 (estimated locally),0.06 per call) SchM_Enter_Can_CAN_EXCLUSIVE_AREA_14/151 (13288 (estimated locally),0.06 per call) FlexCAN_Enable/144 (13690 (estimated locally),0.06 per call) 
FlexCAN_Ip_SetRxMaskType_Privileged/101 (FlexCAN_Ip_SetRxMaskType_Privileged) @070abd20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_SetRxMaskType/43 (26575 (estimated locally),0.12 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_SetStopMode_Privileged/100 (FlexCAN_Ip_SetStopMode_Privileged) @070aba80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (35433 (estimated locally),0.16 per call) FlexCAN_EnterFreezeMode/124 (107374 (estimated locally),0.50 per call) 
FlexCAN_Ip_SetStartMode_Privileged/99 (FlexCAN_Ip_SetStartMode_Privileged) @070ab7e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_ExitFreezeMode/149 (107374 (estimated locally),0.50 per call) 
FlexCAN_Ip_GetStartMode_Privileged/98 (FlexCAN_Ip_GetStartMode_Privileged) @070ab540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
FlexCAN_Ip_GetStopMode_Privileged/97 (FlexCAN_Ip_GetStopMode_Privileged) @070ab2a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
FlexCAN_Ip_MainFunctionWrite/96 (FlexCAN_Ip_MainFunctionWrite) @070ab000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_ClearMsgBuffIntStatusFlag/9 (35433 (estimated locally),0.16 per call) FlexCAN_GetMsgBuffTimestamp/147 (35433 (estimated locally),0.16 per call) FlexCAN_GetBuffStatusFlag/10 (107374 (estimated locally),0.50 per call) 
FlexCAN_Ip_MainFunctionBusOff_Privileged/95 (FlexCAN_Ip_MainFunctionBusOff_Privileged) @0709eb60
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: 
   Indirect call(37581 (estimated locally),0.18 per call) 
FlexCAN_Ip_MainFunctionRead/94 (FlexCAN_Ip_MainFunctionRead) @0709e620
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_IRQHandlerRxMB/61 (2882 (estimated locally),0.01 per call) FlexCAN_GetBuffStatusFlag/10 (28476 (estimated locally),0.13 per call) FlexCAN_IRQHandlerRxFIFO/63 (2367 (estimated locally),0.01 per call) FlexCAN_IRQHandlerEnhancedRxFIFO/66 (735 (estimated locally),0.00 per call) FlexCAN_IsEnhancedRxFifoAvailable/141 (10866 (estimated locally),0.05 per call) 
FlexCAN_Ip_Deinit_Privileged/93 (FlexCAN_Ip_Deinit_Privileged) @0709e0e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (write)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (35433 (estimated locally),0.16 per call) FlexCAN_SetRegDefaultVal/49 (35433 (estimated locally),0.16 per call) FlexCAN_EnterFreezeMode/124 (107374 (estimated locally),0.50 per call) 
FlexCAN_Ip_SetRxFifoGlobalMask_Privileged/92 (FlexCAN_Ip_SetRxFifoGlobalMask_Privileged) @0709ed20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_SetRxIndividualMask_Privileged/91 (FlexCAN_Ip_SetRxIndividualMask_Privileged) @0709ea80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (11568 (estimated locally),0.05 per call) FlexCAN_Enable/144 (11568 (estimated locally),0.05 per call) 
FlexCAN_Ip_ExitFreezeMode_Privileged/90 (FlexCAN_Ip_ExitFreezeMode_Privileged) @0709e7e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_ExitFreezeMode/149 (1073741824 (estimated locally),1.00 per call) 
FlexCAN_Ip_EnterFreezeMode_Privileged/89 (FlexCAN_Ip_EnterFreezeMode_Privileged) @0709e540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_EnterFreezeMode/124 (1073741824 (estimated locally),1.00 per call) 
FlexCAN_Ip_SetRxMbGlobalMask_Privileged/88 (FlexCAN_Ip_SetRxMbGlobalMask_Privileged) @0709e2a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_SendBlocking/87 (FlexCAN_Ip_SendBlocking) @0709e000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_ClearMsgBuffIntStatusFlag/9 (26843 (estimated locally),0.12 per call) FlexCAN_GetBuffStatusFlag/10 (28155 (estimated locally),0.13 per call) OsIf_GetElapsed/138 (26606 (estimated locally),0.12 per call) OsIf_GetCounter/137 (3012 (estimated locally),0.01 per call) OsIf_MicrosToTicks/136 (3012 (estimated locally),0.01 per call) FlexCAN_GetMsgBuffRegion/148 (3012 (estimated locally),0.01 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (3012 (estimated locally),0.01 per call) FlexCAN_GetBuffStatusFlag/10 (250932 (estimated locally),1.17 per call) OsIf_GetElapsed/138 (237131 (estimated locally),1.10 per call) FlexCAN_StartSendData/59 (53687 (estimated locally),0.25 per call) OsIf_MicrosToTicks/136 (214748 (estimated locally),1.00 per call) OsIf_GetCounter/137 (214748 (estimated locally),1.00 per call) 
FlexCAN_Busoff_Error_IRQHandler/86 (FlexCAN_Busoff_Error_IRQHandler) @0708db60
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: 
   Indirect call(13153 (estimated locally),0.06 per call) 
   Indirect call(13153 (estimated locally),0.06 per call) 
   Indirect call(13153 (estimated locally),0.06 per call) 
   Indirect call(10786 (estimated locally),0.05 per call) 
   Indirect call(13153 (estimated locally),0.06 per call) 
FlexCAN_Ip_GetControllerRxErrorCounter/85 (FlexCAN_Ip_GetControllerRxErrorCounter) @0708d620
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: 
FlexCAN_Ip_GetControllerTxErrorCounter/84 (FlexCAN_Ip_GetControllerTxErrorCounter) @0708d0e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: 
FlexCAN_Ip_GetErrorStatus/83 (FlexCAN_Ip_GetErrorStatus) @0708dd20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: 
FlexCAN_Ip_ClearErrorStatus/82 (FlexCAN_Ip_ClearErrorStatus) @0708da80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: 
FlexCAN_IRQHandler/81 (FlexCAN_IRQHandler) @0708d7e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_ClearMsgBuffIntStatusFlag/9 (202115 (estimated locally),0.94 per call) FlexCAN_ProcessSpuriousInterruptMB/64 (9473 (estimated locally),0.04 per call) FlexCAN_ProcessIRQHandlerEnhancedRxFIFO/65 (1942 (estimated locally),0.01 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (2368 (estimated locally),0.01 per call) FlexCAN_GetMsgBuffIntStatusFlag/36 (14353 (estimated locally),0.07 per call) FlexCAN_IRQHandlerTxMB/62 (2905 (estimated locally),0.01 per call) FlexCAN_IRQHandlerRxMB/61 (2426 (estimated locally),0.01 per call) FlexCAN_IRQHandlerRxFIFO/63 (2368 (estimated locally),0.01 per call) FlexCAN_GetMsgBuffIntStatusFlag/36 (239641 (estimated locally),1.12 per call) FlexCAN_GetMsgBuffIntStatusFlag/36 (28706 (estimated locally),0.13 per call) 
FlexCAN_CompleteRxMessageFifoData/80 (FlexCAN_CompleteRxMessageFifoData) @0708d540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_IRQHandlerRxFIFO/63 (17929341 (estimated locally),0.02 per call) 
  Calls: FlexCAN_SetMsgBuffIntCmd/132 (35433 (estimated locally),0.16 per call) FlexCAN_SetMsgBuffIntCmd/132 (35433 (estimated locally),0.16 per call) FlexCAN_SetMsgBuffIntCmd/132 (35433 (estimated locally),0.16 per call) 
FlexCAN_Ip_GetTransferStatus/79 (FlexCAN_Ip_GetTransferStatus) @0708d2a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: 
FlexCAN_Ip_ConfigRemoteResponseMb/78 (FlexCAN_Ip_ConfigRemoteResponseMb) @0708d000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_SetMsgBuffIntCmd/132 (8463 (estimated locally),0.04 per call) FlexCAN_SetTxMsgBuff/134 (25646 (estimated locally),0.12 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (25646 (estimated locally),0.12 per call) FlexCAN_IsMbOutOfRange/133 (53687 (estimated locally),0.25 per call) 
FlexCAN_Ip_ConfigEnhancedRxFifo_Privileged/77 (FlexCAN_Ip_ConfigEnhancedRxFifo_Privileged) @0707db60
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (6845 (estimated locally),0.03 per call) FlexCAN_SetEnhancedRxFifoFilter/146 (6644 (estimated locally),0.03 per call) FlexCAN_Enable/144 (6845 (estimated locally),0.03 per call) FlexCAN_IsEnhancedRxFifoAvailable/141 (107374 (estimated locally),0.50 per call) 
FlexCAN_Ip_ConfigRxFifo_Privileged/76 (FlexCAN_Ip_ConfigRxFifo_Privileged) @0707d620
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_Disable/125 (27380 (estimated locally),0.13 per call) FlexCAN_SetRxFifoFilter/145 (26575 (estimated locally),0.12 per call) FlexCAN_Enable/144 (27380 (estimated locally),0.13 per call) 
FlexCAN_Ip_RxFifoBlocking/75 (FlexCAN_Ip_RxFifoBlocking) @0707d0e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_ProccessLegacyRxFIFO/57 (11693 (estimated locally),0.05 per call) FlexCAN_StartRxMessageFifoData/60 (35433 (estimated locally),0.16 per call) FlexCAN_ProccessLegacyRxFIFO/57 (14007 (estimated locally),0.07 per call) FlexCAN_StartRxMessageFifoData/60 (42445 (estimated locally),0.20 per call) FlexCAN_ProccessEnhancedRxFifo/56 (9734 (estimated locally),0.05 per call) FlexCAN_StartRxMessageEnhancedFifoData/55 (29496 (estimated locally),0.14 per call) FlexCAN_IsEnhancedRxFifoAvailable/141 (107374 (estimated locally),0.50 per call) 
FlexCAN_Ip_RxFifo/74 (FlexCAN_Ip_RxFifo) @0707dd20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_StartRxMessageFifoData/60 (35433 (estimated locally),0.16 per call) FlexCAN_StartRxMessageFifoData/60 (42445 (estimated locally),0.20 per call) FlexCAN_StartRxMessageEnhancedFifoData/55 (29496 (estimated locally),0.14 per call) FlexCAN_IsEnhancedRxFifoAvailable/141 (107374 (estimated locally),0.50 per call) 
FlexCAN_Ip_ReceiveBlocking/73 (FlexCAN_Ip_ReceiveBlocking) @0707da80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_flexcan_Ip_StatePtr/51 (read)g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_SetMsgBuffIntCmd/132 (12047 (estimated locally),0.06 per call) OsIf_GetElapsed/138 (313013 (estimated locally),1.46 per call) FlexCAN_IRQHandlerRxMB/61 (34087 (estimated locally),0.16 per call) FlexCAN_GetBuffStatusFlag/10 (103294 (estimated locally),0.48 per call) OsIf_GetCounter/137 (35433 (estimated locally),0.16 per call) FlexCAN_SetMsgBuffIntCmd/132 (17717 (estimated locally),0.08 per call) FlexCAN_StartRxMessageBufferData/58 (107374 (estimated locally),0.50 per call) OsIf_MicrosToTicks/136 (214748 (estimated locally),1.00 per call) 
FlexCAN_Ip_Receive/72 (FlexCAN_Ip_Receive) @0707d7e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_SetMsgBuffIntCmd/132 (17717 (estimated locally),0.08 per call) FlexCAN_StartRxMessageBufferData/58 (107374 (estimated locally),0.50 per call) 
FlexCAN_Ip_ConfigRxMb/71 (FlexCAN_Ip_ConfigRxMb) @0707d540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_SetRxMsgBuff/135 (25646 (estimated locally),0.12 per call) FlexCAN_SetRxMsgBuff/135 (25646 (estimated locally),0.12 per call) FlexCAN_SetRxMsgBuff/135 (25646 (estimated locally),0.12 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (25646 (estimated locally),0.12 per call) FlexCAN_IsMbOutOfRange/133 (53687 (estimated locally),0.25 per call) 
FlexCAN_Ip_Send/70 (FlexCAN_Ip_Send) @0707d2a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_SetMsgBuffIntCmd/132 (2923 (estimated locally),0.01 per call) FlexCAN_StartSendData/59 (17717 (estimated locally),0.08 per call) 
FlexCAN_Ip_Init_Privileged/69 (FlexCAN_Ip_Init_Privileged) @0707d000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (write)
  Referring: 
  Availability: available
  Function flags: count:214748 (estimated locally) body optimize_size
  Called by: 
  Calls: FlexCAN_EnterFreezeMode/124 (17717 (estimated locally),0.08 per call) FlexCAN_SetOperationMode/123 (17717 (estimated locally),0.08 per call) SchM_Exit_Can_CAN_EXCLUSIVE_AREA_00/122 (8858 (estimated locally),0.04 per call) FlexCAN_SetTimeSegments/13 (4429 (estimated locally),0.02 per call) FlexCAN_SetFDTimeSegments/12 (4429 (estimated locally),0.02 per call) FlexCAN_SetExtendedTimeSegments/14 (4429 (estimated locally),0.02 per call) SchM_Enter_Can_CAN_EXCLUSIVE_AREA_00/121 (8858 (estimated locally),0.04 per call) SchM_Exit_Can_CAN_EXCLUSIVE_AREA_00/122 (8858 (estimated locally),0.04 per call) FlexCAN_SetEnhancedDataTimeSegments/17 (2923 (estimated locally),0.01 per call) FlexCAN_SetEnhancedNominalTimeSegments/15 (8858 (estimated locally),0.04 per call) SchM_Enter_Can_CAN_EXCLUSIVE_AREA_00/121 (8858 (estimated locally),0.04 per call) FlexCAN_EnableExtCbt/24 (17717 (estimated locally),0.08 per call) FlexCAN_InitController/53 (53687 (estimated locally),0.25 per call) 
FlexCAN_AbortRxTransfer/68 (FlexCAN_AbortRxTransfer) @07062b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741823 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_AbortTransfer/116 (2595 (estimated locally),0.01 per call) 
  Calls: FlexCAN_ClearMsgBuffIntStatusFlag/9 (1073741824 (estimated locally),1.00 per call) FlexCAN_GetMsgBuffRegion/148 (354334802 (estimated locally),0.33 per call) FLEXCAN_ClearMsgBuffIntCmd/162 (237404317 (estimated locally),0.22 per call) FlexCAN_GetMsgBuffRegion/148 (237404317 (estimated locally),0.22 per call) RxFifoOcuppiedLastMsgBuff/29 (719407022 (estimated locally),0.67 per call) 
FlexCAN_AbortTxTransfer/67 (FlexCAN_AbortTxTransfer) @07062620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:114863532 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_AbortTransfer/116 (2595 (estimated locally),0.01 per call) 
  Calls: FlexCAN_ClearMsgBuffIntStatusFlag/9 (114863532 (estimated locally),1.00 per call) FlexCAN_GetBuffStatusFlag/10 (1073741824 (estimated locally),9.35 per call) OsIf_GetElapsed/138 (1014686025 (estimated locally),8.83 per call) OsIf_GetCounter/137 (114863532 (estimated locally),1.00 per call) OsIf_MicrosToTicks/136 (114863532 (estimated locally),1.00 per call) FlexCAN_GetMsgBuffRegion/148 (114863532 (estimated locally),1.00 per call) 
FlexCAN_IRQHandlerEnhancedRxFIFO/66 (FlexCAN_IRQHandlerEnhancedRxFIFO) @070620e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_MainFunctionRead/94 (735 (estimated locally),0.00 per call) FlexCAN_ProcessIRQHandlerEnhancedRxFIFO/65 (93544388 (estimated locally),0.44 per call) FlexCAN_ProccessEnhancedRxFifo/56 (214301689 (estimated locally),1.87 per call) 
  Calls: FlexCAN_CompleteRxMessageEnhancedFifoData/54 (24094767 (estimated locally),0.02 per call) FlexCAN_ReadEnhancedRxFifo/142 (73014444 (estimated locally),0.07 per call) 
   Indirect call(150323855 (estimated locally),0.14 per call) 
   Indirect call(150323855 (estimated locally),0.14 per call) 
   Indirect call(150323855 (estimated locally),0.14 per call) 
   Indirect call(51110111 (estimated locally),0.05 per call) 
FlexCAN_ProcessIRQHandlerEnhancedRxFIFO/65 (FlexCAN_ProcessIRQHandlerEnhancedRxFIFO) @07062d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:214748364 (estimated locally) body local optimize_size
  Called by: FlexCAN_IRQHandler/81 (1942 (estimated locally),0.01 per call) 
  Calls: FlexCAN_IRQHandlerEnhancedRxFIFO/66 (93544388 (estimated locally),0.44 per call) FlexCAN_GetEnhancedRxFIFOIntStatusFlag/48 (283467841 (estimated locally),1.32 per call) FlexCAN_GetEnhancedRxFIFOStatusFlag/46 (858993459 (estimated locally),4.00 per call) 
FlexCAN_ProcessSpuriousInterruptMB/64 (FlexCAN_ProcessSpuriousInterruptMB) @07062a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:118111602 (estimated locally) body local optimize_size
  Called by: FlexCAN_IRQHandler/81 (9473 (estimated locally),0.04 per call) 
  Calls: FlexCAN_ClearMsgBuffIntStatusFlag/9 (52034066 (estimated locally),0.44 per call) FlexCAN_GetBuffStatusImask/11 (315357973 (estimated locally),2.67 per call) FlexCAN_GetBuffStatusFlag/10 (955630223 (estimated locally),8.09 per call) 
FlexCAN_IRQHandlerRxFIFO/63 (FlexCAN_IRQHandlerRxFIFO) @070627e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741823 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_MainFunctionRead/94 (2367 (estimated locally),0.01 per call) FlexCAN_IRQHandler/81 (2368 (estimated locally),0.01 per call) FlexCAN_ProccessLegacyRxFIFO/57 (160726266 (estimated locally),1.40 per call) 
  Calls: FlexCAN_ClearMsgBuffIntStatusFlag/9 (268435456 (estimated locally),0.25 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (268435456 (estimated locally),0.25 per call) FlexCAN_CompleteRxMessageFifoData/80 (17929341 (estimated locally),0.02 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (54331336 (estimated locally),0.05 per call) FlexCAN_ReadRxFifo/143 (54331336 (estimated locally),0.05 per call) 
   Indirect call(187904819 (estimated locally),0.18 per call) 
   Indirect call(187904819 (estimated locally),0.18 per call) 
   Indirect call(38031935 (estimated locally),0.04 per call) 
FlexCAN_IRQHandlerTxMB/62 (FlexCAN_IRQHandlerTxMB) @07062540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741823 (estimated locally) body local optimize_size
  Called by: FlexCAN_IRQHandler/81 (2905 (estimated locally),0.01 per call) 
  Calls: FlexCAN_SetMsgBuffIntCmd/132 (147934780 (estimated locally),0.14 per call) FlexCAN_SetMsgBuffIntCmd/132 (177167401 (estimated locally),0.17 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (536870911 (estimated locally),0.50 per call) FlexCAN_GetMsgBuffTimestamp/147 (536870911 (estimated locally),0.50 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (108662672 (estimated locally),0.10 per call) FlexCAN_GetMsgBuff/140 (536870911 (estimated locally),0.50 per call) FlexCAN_LockRxMsgBuff/139 (536870911 (estimated locally),0.50 per call) 
   Indirect call(751619278 (estimated locally),0.70 per call) 
FlexCAN_IRQHandlerRxMB/61 (FlexCAN_IRQHandlerRxMB) @070622a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:1073741823 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_MainFunctionRead/94 (2882 (estimated locally),0.01 per call) FlexCAN_IRQHandler/81 (2426 (estimated locally),0.01 per call) FlexCAN_Ip_ReceiveBlocking/73 (34087 (estimated locally),0.16 per call) 
  Calls: FlexCAN_SetMsgBuffIntCmd/132 (147934780 (estimated locally),0.14 per call) FlexCAN_SetMsgBuffIntCmd/132 (177167401 (estimated locally),0.17 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (1073741823 (estimated locally),1.00 per call) FlexCAN_GetMsgBuff/140 (1073741823 (estimated locally),1.00 per call) FlexCAN_LockRxMsgBuff/139 (1073741823 (estimated locally),1.00 per call) 
   Indirect call(751619277 (estimated locally),0.70 per call) 
FlexCAN_StartRxMessageFifoData/60 (FlexCAN_StartRxMessageFifoData) @07062000
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_RxFifoBlocking/75 (35433 (estimated locally),0.16 per call) FlexCAN_Ip_RxFifoBlocking/75 (42445 (estimated locally),0.20 per call) FlexCAN_Ip_RxFifo/74 (35433 (estimated locally),0.16 per call) FlexCAN_Ip_RxFifo/74 (42445 (estimated locally),0.20 per call) 
  Calls: FlexCAN_StartRxMessageFifoData.part.0/179 (107374 (estimated locally),0.50 per call) 
FlexCAN_StartSendData/59 (FlexCAN_StartSendData) @06cd2b60
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_flexcan_Ip_StatePtr/51 (read)g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SendBlocking/87 (53687 (estimated locally),0.25 per call) FlexCAN_Ip_Send/70 (17717 (estimated locally),0.08 per call) 
  Calls: FlexCAN_SetTxMsgBuff/134 (16670 (estimated locally),0.08 per call) FlexCAN_ClearMsgBuffIntStatusFlag/9 (16670 (estimated locally),0.08 per call) FlexCAN_IsMbOutOfRange/133 (53687 (estimated locally),0.25 per call) 
FlexCAN_StartRxMessageBufferData/58 (FlexCAN_StartRxMessageBufferData) @06cd2620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_ReceiveBlocking/73 (107374 (estimated locally),0.50 per call) FlexCAN_Ip_Receive/72 (107374 (estimated locally),0.50 per call) 
  Calls: FlexCAN_IsMbOutOfRange/133 (107374 (estimated locally),0.50 per call) 
FlexCAN_ProccessLegacyRxFIFO/57 (FlexCAN_ProccessLegacyRxFIFO) @06cd20e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_flexcan_Ip_StatePtr/51 (read)g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: local
  Function flags: count:114863532 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_RxFifoBlocking/75 (11693 (estimated locally),0.05 per call) FlexCAN_Ip_RxFifoBlocking/75 (14007 (estimated locally),0.07 per call) 
  Calls: FlexCAN_SetMsgBuffIntCmd/132 (19089400 (estimated locally),0.17 per call) FlexCAN_SetMsgBuffIntCmd/132 (19089400 (estimated locally),0.17 per call) FlexCAN_SetMsgBuffIntCmd/132 (19089400 (estimated locally),0.17 per call) OsIf_GetElapsed/138 (1014686025 (estimated locally),8.83 per call) FlexCAN_IRQHandlerRxFIFO/63 (160726266 (estimated locally),1.40 per call) FlexCAN_GetBuffStatusFlag/10 (487049291 (estimated locally),4.24 per call) OsIf_GetCounter/137 (114863532 (estimated locally),1.00 per call) OsIf_MicrosToTicks/136 (114863532 (estimated locally),1.00 per call) 
FlexCAN_ProccessEnhancedRxFifo/56 (FlexCAN_ProccessEnhancedRxFifo) @06cd2d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_flexcan_Ip_StatePtr/51 (read)g_Flexcan_Ip_aBase/50 (read)
  Referring: 
  Availability: local
  Function flags: count:114863532 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_RxFifoBlocking/75 (9734 (estimated locally),0.05 per call) 
  Calls: OsIf_GetElapsed/138 (1014686025 (estimated locally),8.83 per call) FlexCAN_IRQHandlerEnhancedRxFIFO/66 (214301689 (estimated locally),1.87 per call) FlexCAN_GetEnhancedRxFIFOStatusFlag/46 (649399059 (estimated locally),5.65 per call) OsIf_GetCounter/137 (114863532 (estimated locally),1.00 per call) OsIf_MicrosToTicks/136 (114863532 (estimated locally),1.00 per call) 
FlexCAN_StartRxMessageEnhancedFifoData/55 (FlexCAN_StartRxMessageEnhancedFifoData) @06cd2a80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_RxFifoBlocking/75 (29496 (estimated locally),0.14 per call) FlexCAN_Ip_RxFifo/74 (29496 (estimated locally),0.14 per call) 
  Calls: 
FlexCAN_CompleteRxMessageEnhancedFifoData/54 (FlexCAN_CompleteRxMessageEnhancedFifoData) @06cd27e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: g_Flexcan_Ip_aBase/50 (read)g_flexcan_Ip_StatePtr/51 (read)
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_IRQHandlerEnhancedRxFIFO/66 (24094767 (estimated locally),0.02 per call) 
  Calls: FlexCAN_IsEnhancedRxFifoAvailable/141 (107374 (estimated locally),0.50 per call) 
FlexCAN_InitController/53 (FlexCAN_InitController) @06cd2540
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741823 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_Init_Privileged/69 (53687 (estimated locally),0.25 per call) 
  Calls: FlexCAN_Disable/125 (62451509 (estimated locally),0.06 per call) FlexCAN_EnterFreezeMode/124 (62451509 (estimated locally),0.06 per call) FlexCAN_SetMaxMsgBuffNum/129 (189246996 (estimated locally),0.18 per call) FlexCAN_SetPayloadSize/128 (189246996 (estimated locally),0.18 per call) FlexCAN_Disable/125 (189246996 (estimated locally),0.18 per call) FlexCAN_EnterFreezeMode/124 (189246996 (estimated locally),0.18 per call) FlexCAN_InitRxFifo/52 (378493993 (estimated locally),0.35 per call) FlexCAN_ConfigCtrlOptions/127 (378493993 (estimated locally),0.35 per call) FlexCAN_SetFDEnabled/6 (378493993 (estimated locally),0.35 per call) FlexCAN_DisableMemErrorDetection/5 (378493993 (estimated locally),0.35 per call) FlexCAN_Disable/125 (378493993 (estimated locally),0.35 per call) FlexCAN_EnterFreezeMode/124 (378493993 (estimated locally),0.35 per call) FlexCAN_Init/126 (756987986 (estimated locally),0.71 per call) SchM_Exit_Can_CAN_EXCLUSIVE_AREA_00/122 (756987986 (estimated locally),0.71 per call) SchM_Enter_Can_CAN_EXCLUSIVE_AREA_00/121 (756987986 (estimated locally),0.71 per call) FlexCAN_Disable/125 (209057533 (estimated locally),0.19 per call) FlexCAN_EnterFreezeMode/124 (633507676 (estimated locally),0.59 per call) 
FlexCAN_InitRxFifo/52 (FlexCAN_InitRxFifo) @06cd22a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_InitController/53 (378493993 (estimated locally),0.35 per call) 
  Calls: FlexCAN_EnableEnhancedRxFifo/131 (295869560 (estimated locally),0.28 per call) FlexCAN_EnableRxFifo/130 (354334802 (estimated locally),0.33 per call) 
g_flexcan_Ip_StatePtr/51 (g_flexcan_Ip_StatePtr) @06cc9678
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: FlexCAN_AbortTxTransfer/67 (read)FlexCAN_AbortRxTransfer/68 (read)FlexCAN_CompleteRxMessageFifoData/80 (read)FlexCAN_Ip_Init_Privileged/69 (write)FlexCAN_Ip_Send/70 (read)FlexCAN_StartRxMessageFifoData.part.0/179 (read)FlexCAN_Ip_ConfigRxMb/71 (read)FlexCAN_StartRxMessageBufferData/58 (read)FlexCAN_IRQHandlerTxMB/62 (read)FlexCAN_StartRxMessageEnhancedFifoData/55 (read)FlexCAN_CompleteRxMessageEnhancedFifoData/54 (read)FlexCAN_IRQHandlerRxMB/61 (read)FlexCAN_StartSendData/59 (read)FlexCAN_ProcessIRQHandlerEnhancedRxFIFO/65 (read)FlexCAN_ProccessEnhancedRxFifo/56 (read)FlexCAN_ProcessSpuriousInterruptMB/64 (read)FlexCAN_Ip_Receive/72 (read)FlexCAN_Ip_ReceiveBlocking/73 (read)FlexCAN_Ip_ConfigRemoteResponseMb/78 (read)FlexCAN_IRQHandlerRxFIFO/63 (read)FlexCAN_IRQHandlerEnhancedRxFIFO/66 (read)FlexCAN_Ip_DisableInterrupts_Privileged/114 (read)FlexCAN_Ip_GetTransferStatus/79 (read)FlexCAN_IRQHandler/81 (read)FlexCAN_Busoff_Error_IRQHandler/86 (read)FlexCAN_Ip_SendBlocking/87 (read)FlexCAN_Ip_Deinit_Privileged/93 (write)FlexCAN_Ip_MainFunctionRead/94 (read)FlexCAN_Ip_MainFunctionBusOff_Privileged/95 (read)FlexCAN_Ip_MainFunctionWrite/96 (read)FlexCAN_Ip_EnableInterrupts_Privileged/113 (read)FlexCAN_ProccessLegacyRxFIFO/57 (read)FlexCAN_Ip_AbortTransfer/116 (read)
  Availability: available
  Varpool flags:
g_Flexcan_Ip_aBase/50 (g_Flexcan_Ip_aBase) @06cc95e8
  Type: variable definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: FlexCAN_AbortTxTransfer/67 (read)FlexCAN_AbortRxTransfer/68 (read)FlexCAN_CompleteRxMessageFifoData/80 (read)FlexCAN_Ip_Init_Privileged/69 (read)FlexCAN_Ip_Send/70 (read)FlexCAN_StartRxMessageFifoData.part.0/179 (read)FlexCAN_Ip_ConfigRxMb/71 (read)FlexCAN_StartRxMessageBufferData/58 (read)FlexCAN_Ip_Receive/72 (read)FlexCAN_Ip_SetRxMb15Mask_Privileged/118 (read)FlexCAN_StartRxMessageEnhancedFifoData/55 (read)FlexCAN_Ip_ReceiveBlocking/73 (read)FlexCAN_CompleteRxMessageEnhancedFifoData/54 (read)FlexCAN_IRQHandlerRxMB/61 (read)FlexCAN_StartSendData/59 (read)FlexCAN_ProcessIRQHandlerEnhancedRxFIFO/65 (read)FlexCAN_ProccessEnhancedRxFifo/56 (read)FlexCAN_ProcessSpuriousInterruptMB/64 (read)FlexCAN_Ip_RxFifo/74 (read)FlexCAN_Ip_RxFifoBlocking/75 (read)FlexCAN_Ip_ConfigRxFifo_Privileged/76 (read)FlexCAN_Ip_ConfigEnhancedRxFifo_Privileged/77 (read)FlexCAN_IRQHandlerRxFIFO/63 (read)FlexCAN_IRQHandlerEnhancedRxFIFO/66 (read)FlexCAN_Ip_SetListenOnlyMode_Privileged/119 (read)FlexCAN_Ip_ConfigRemoteResponseMb/78 (read)FlexCAN_IRQHandler/81 (read)FlexCAN_Ip_ClearErrorStatus/82 (read)FlexCAN_Ip_GetErrorStatus/83 (read)FlexCAN_Ip_GetControllerTxErrorCounter/84 (read)FlexCAN_Ip_GetControllerRxErrorCounter/85 (read)FlexCAN_Busoff_Error_IRQHandler/86 (read)FlexCAN_Ip_SendBlocking/87 (read)FlexCAN_Ip_SetRxMbGlobalMask_Privileged/88 (read)FlexCAN_Ip_EnterFreezeMode_Privileged/89 (read)FlexCAN_Ip_ExitFreezeMode_Privileged/90 (read)FlexCAN_Ip_SetRxIndividualMask_Privileged/91 (read)FlexCAN_Ip_SetRxFifoGlobalMask_Privileged/92 (read)FlexCAN_Ip_Deinit_Privileged/93 (read)FlexCAN_Ip_MainFunctionRead/94 (read)FlexCAN_Ip_MainFunctionBusOff_Privileged/95 (read)FlexCAN_Ip_MainFunctionWrite/96 (read)FlexCAN_Ip_GetStopMode_Privileged/97 (read)FlexCAN_Ip_GetStartMode_Privileged/98 (read)FlexCAN_Ip_SetStartMode_Privileged/99 (read)FlexCAN_Ip_SetStopMode_Privileged/100 (read)FlexCAN_Ip_SetRxMaskType_Privileged/101 (read)FlexCAN_Ip_SetBitrate_Privileged/102 (read)FlexCAN_Ip_GetBitrate/103 (read)FlexCAN_Ip_ClearTDCFail_Privileged/104 (read)FlexCAN_Ip_GetTDCFail_Privileged/105 (read)FlexCAN_Ip_GetTDCValue_Privileged/106 (read)FlexCAN_Ip_SetBitrateCbt_Privileged/107 (read)FlexCAN_Ip_GetBitrateFD/108 (read)FlexCAN_Ip_SetTDCOffset_Privileged/109 (read)FlexCAN_Ip_SetTxArbitrationStartDelay_Privileged/110 (read)FlexCAN_Ip_GetBuffStatusFlag/111 (read)FlexCAN_Ip_ClearBuffStatusFlag/112 (read)FlexCAN_Ip_EnableInterrupts_Privileged/113 (read)FlexCAN_Ip_DisableInterrupts_Privileged/114 (read)FlexCAN_ProccessLegacyRxFIFO/57 (read)FlexCAN_IRQHandlerTxMB/62 (read)FlexCAN_Ip_SetErrorInt_Privileged/115 (read)FlexCAN_Ip_AbortTransfer/116 (read)FlexCAN_Ip_SetRxMb14Mask_Privileged/117 (read)FlexCAN_Ip_GetListenOnlyMode/120 (read)
  Availability: available
  Varpool flags: initialized read-only const-value-known
FlexCAN_SetRegDefaultVal/49 (FlexCAN_SetRegDefaultVal) @06d809a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_Deinit_Privileged/93 (35433 (estimated locally),0.16 per call) 
  Calls: FlexCAN_GetMaxMbNum/150 (1073741824 (estimated locally),1.00 per call) FlexCAN_GetMaxMbNum/150 (1073741824 (estimated locally),1.00 per call) FlexCAN_IsEnhancedRxFifoAvailable/141 (1073741824 (estimated locally),1.00 per call) 
FlexCAN_GetEnhancedRxFIFOIntStatusFlag/48 (FlexCAN_GetEnhancedRxFIFOIntStatusFlag) @06d7cee0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_ProcessIRQHandlerEnhancedRxFIFO/65 (283467841 (estimated locally),1.32 per call) 
  Calls: 
FlexCAN_GetEnhancedRxFIFOStatusFlag/46 (FlexCAN_GetEnhancedRxFIFOStatusFlag) @06d7c9a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_ProcessIRQHandlerEnhancedRxFIFO/65 (858993459 (estimated locally),4.00 per call) FlexCAN_ProccessEnhancedRxFifo/56 (649399059 (estimated locally),5.65 per call) 
  Calls: 
FlexCAN_SetRxMaskType/43 (FlexCAN_SetRxMaskType) @06d7c1c0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetRxMaskType_Privileged/101 (26575 (estimated locally),0.12 per call) 
  Calls: 
FlexCAN_SetTxArbitrationStartDelay/42 (FlexCAN_SetTxArbitrationStartDelay) @06d78d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetTxArbitrationStartDelay_Privileged/110 (26575 (estimated locally),0.12 per call) 
  Calls: 
FlexCAN_GetMsgBuffIntStatusFlag/36 (FlexCAN_GetMsgBuffIntStatusFlag) @06d70c40
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_IRQHandler/81 (14353 (estimated locally),0.07 per call) FlexCAN_IRQHandler/81 (239641 (estimated locally),1.12 per call) FlexCAN_IRQHandler/81 (28706 (estimated locally),0.13 per call) 
  Calls: FlexCAN_GetMsgBuffIntStatusFlag.part.0/174 (134217728 (estimated locally),0.12 per call) 
RxFifoOcuppiedLastMsgBuff/29 (RxFifoOcuppiedLastMsgBuff) @06cc22a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_AbortRxTransfer/68 (719407022 (estimated locally),0.67 per call) 
  Calls: 
FlexCAN_EnhCbtEnable/25 (FlexCAN_EnhCbtEnable) @06cc0620
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetBitrate_Privileged/102 (13288 (estimated locally),0.06 per call) 
  Calls: 
FlexCAN_EnableExtCbt/24 (FlexCAN_EnableExtCbt) @06cc02a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_Init_Privileged/69 (17717 (estimated locally),0.08 per call) 
  Calls: 
FlexCAN_GetFDTimeSegments/21 (FlexCAN_GetFDTimeSegments) @06cba9a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_GetBitrateFD/108 (26844 (estimated locally),0.13 per call) 
  Calls: 
FlexCAN_GetTimeSegments/20 (FlexCAN_GetTimeSegments) @06cba700
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_GetBitrate/103 (21222 (estimated locally),0.10 per call) 
  Calls: 
FlexCAN_GetExtendedTimeSegments/19 (FlexCAN_GetExtendedTimeSegments) @06cba460
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_GetBitrate/103 (14748 (estimated locally),0.07 per call) 
  Calls: 
FlexCAN_GetEnhancedDataTimeSegments/18 (FlexCAN_GetEnhancedDataTimeSegments) @06cba1c0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_GetBitrateFD/108 (26844 (estimated locally),0.13 per call) 
  Calls: 
FlexCAN_SetEnhancedDataTimeSegments/17 (FlexCAN_SetEnhancedDataTimeSegments) @06c31ee0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetBitrateCbt_Privileged/107 (3322 (estimated locally),0.02 per call) FlexCAN_Ip_Init_Privileged/69 (2923 (estimated locally),0.01 per call) 
  Calls: FlexCAN_SetEnhancedDataTimeSegments.part.0/172 (107374 (estimated locally),0.50 per call) 
FlexCAN_GetEnhancedNominalTimeSegments/16 (FlexCAN_GetEnhancedNominalTimeSegments) @06c319a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_GetBitrate/103 (17717 (estimated locally),0.08 per call) 
  Calls: 
FlexCAN_SetEnhancedNominalTimeSegments/15 (FlexCAN_SetEnhancedNominalTimeSegments) @06c31700
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetBitrate_Privileged/102 (4385 (estimated locally),0.02 per call) FlexCAN_Ip_Init_Privileged/69 (8858 (estimated locally),0.04 per call) 
  Calls: FlexCAN_SetEnhancedNominalTimeSegments.part.0/170 (107374 (estimated locally),0.50 per call) 
FlexCAN_SetExtendedTimeSegments/14 (FlexCAN_SetExtendedTimeSegments) @06c311c0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetBitrate_Privileged/102 (3650 (estimated locally),0.02 per call) FlexCAN_Ip_Init_Privileged/69 (4429 (estimated locally),0.02 per call) 
  Calls: FlexCAN_SetExtendedTimeSegments.part.0/168 (107374 (estimated locally),0.50 per call) 
FlexCAN_SetTimeSegments/13 (FlexCAN_SetTimeSegments) @06c2ca80
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetBitrate_Privileged/102 (5253 (estimated locally),0.02 per call) FlexCAN_Ip_Init_Privileged/69 (4429 (estimated locally),0.02 per call) 
  Calls: FlexCAN_SetTimeSegments.part.0/166 (107374 (estimated locally),0.50 per call) 
FlexCAN_SetFDTimeSegments/12 (FlexCAN_SetFDTimeSegments) @06c2c380
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:214748 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetBitrateCbt_Privileged/107 (3322 (estimated locally),0.02 per call) FlexCAN_Ip_Init_Privileged/69 (4429 (estimated locally),0.02 per call) 
  Calls: FlexCAN_SetFDTimeSegments.part.0/164 (107374 (estimated locally),0.50 per call) 
FlexCAN_GetBuffStatusImask/11 (FlexCAN_GetBuffStatusImask) @06c26c40
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_ProcessSpuriousInterruptMB/64 (315357973 (estimated locally),2.67 per call) 
  Calls: 
FlexCAN_GetBuffStatusFlag/10 (FlexCAN_GetBuffStatusFlag) @06c269a0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_GetBuffStatusFlag/111 (52484 (estimated locally),0.24 per call) FlexCAN_Ip_MainFunctionWrite/96 (107374 (estimated locally),0.50 per call) FlexCAN_Ip_MainFunctionRead/94 (28476 (estimated locally),0.13 per call) FlexCAN_Ip_SendBlocking/87 (28155 (estimated locally),0.13 per call) FlexCAN_Ip_SendBlocking/87 (250932 (estimated locally),1.17 per call) FlexCAN_Ip_ReceiveBlocking/73 (103294 (estimated locally),0.48 per call) FlexCAN_AbortTxTransfer/67 (1073741824 (estimated locally),9.35 per call) FlexCAN_ProccessLegacyRxFIFO/57 (487049291 (estimated locally),4.24 per call) FlexCAN_ProcessSpuriousInterruptMB/64 (955630223 (estimated locally),8.09 per call) 
  Calls: 
FlexCAN_ClearMsgBuffIntStatusFlag/9 (FlexCAN_ClearMsgBuffIntStatusFlag) @06c26700
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_ClearBuffStatusFlag/112 (52484 (estimated locally),0.24 per call) FlexCAN_Ip_MainFunctionWrite/96 (35433 (estimated locally),0.16 per call) FlexCAN_Ip_SendBlocking/87 (26843 (estimated locally),0.12 per call) FlexCAN_Ip_SendBlocking/87 (3012 (estimated locally),0.01 per call) FlexCAN_IRQHandler/81 (202115 (estimated locally),0.94 per call) FlexCAN_IRQHandler/81 (2368 (estimated locally),0.01 per call) FlexCAN_Ip_ConfigRemoteResponseMb/78 (25646 (estimated locally),0.12 per call) FlexCAN_Ip_ConfigRxMb/71 (25646 (estimated locally),0.12 per call) FlexCAN_AbortRxTransfer/68 (1073741824 (estimated locally),1.00 per call) FlexCAN_AbortTxTransfer/67 (114863532 (estimated locally),1.00 per call) FlexCAN_IRQHandlerTxMB/62 (536870911 (estimated locally),0.50 per call) FlexCAN_IRQHandlerTxMB/62 (108662672 (estimated locally),0.10 per call) FlexCAN_IRQHandlerRxFIFO/63 (268435456 (estimated locally),0.25 per call) FlexCAN_IRQHandlerRxFIFO/63 (268435456 (estimated locally),0.25 per call) FlexCAN_IRQHandlerRxFIFO/63 (54331336 (estimated locally),0.05 per call) FlexCAN_IRQHandlerRxMB/61 (1073741823 (estimated locally),1.00 per call) FlexCAN_StartSendData/59 (16670 (estimated locally),0.08 per call) FlexCAN_ProcessSpuriousInterruptMB/64 (52034066 (estimated locally),0.44 per call) 
  Calls: 
FlexCAN_SetListenOnlyMode/7 (FlexCAN_SetListenOnlyMode) @06c260e0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetListenOnlyMode_Privileged/119 (26575 (estimated locally),0.12 per call) 
  Calls: 
FlexCAN_SetFDEnabled/6 (FlexCAN_SetFDEnabled) @06c24d20
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetBitrateCbt_Privileged/107 (6644 (estimated locally),0.03 per call) FlexCAN_InitController/53 (378493993 (estimated locally),0.35 per call) 
  Calls: 
FlexCAN_DisableMemErrorDetection/5 (FlexCAN_DisableMemErrorDetection) @06c248c0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_InitController/53 (378493993 (estimated locally),0.35 per call) 
  Calls: 
FlexCAN_SetEnhancedTDCOffset/3 (FlexCAN_SetEnhancedTDCOffset) @06c1dc40
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetTDCOffset_Privileged/109 (13288 (estimated locally),0.06 per call) 
  Calls: 
FlexCAN_SetTDCOffset/2 (FlexCAN_SetTDCOffset) @06c1d8c0
  Type: function definition analyzed
  Visibility: prevailing_def_ironly
  References: 
  Referring: 
  Availability: local
  Function flags: count:1073741824 (estimated locally) body local optimize_size
  Called by: FlexCAN_Ip_SetTDCOffset_Privileged/109 (13288 (estimated locally),0.06 per call) 
  Calls: 
FlexCAN_StartRxMessageFifoData.part.0 (uint8 instance, struct Flexcan_Ip_MsgBuffType * data)
{
  struct FLEXCAN_Type * base;
  struct Flexcan_Ip_StateType * state;
  Flexcan_Ip_StatusType eResult;
  volatile boolean x;
  int _2;
  _Bool _5;
  <unnamed type> _6;
  <unnamed type> _7;
  _Bool _9;
  _Bool _10;
  _Bool _11;

  <bb 9> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = (int) instance_1(D);
  base_3 = g_Flexcan_Ip_aBase[_2];
  # DEBUG base => base_3
  # DEBUG BEGIN_STMT
  state_4 = g_flexcan_Ip_StatePtr[_2];
  # DEBUG state => state_4
  # DEBUG BEGIN_STMT
  _5 = state_4->bIsLegacyFifoEn;
  if (_5 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _6 ={v} state_4->mbs[0].state;
  if (_6 != 0)
    goto <bb 8>; [35.00%]
  else
    goto <bb 4>; [65.00%]

  <bb 4> [local count: 348966093]:
  # DEBUG BEGIN_STMT
  state_4->mbs[0].state ={v} 1;
  # DEBUG BEGIN_STMT
  _7 = state_4->transferType;
  if (_7 == 1)
    goto <bb 5>; [34.00%]
  else
    goto <bb 6>; [66.00%]

  <bb 5> [local count: 118648472]:
  # DEBUG BEGIN_STMT
  state_4->mbs[0].isPolling = 1;

  <bb 6> [local count: 348966093]:
  # DEBUG BEGIN_STMT
  state_4->mbs[0].pMBmessage = data_8(D);
  # DEBUG BEGIN_STMT
  if (_7 == 0)
    goto <bb 7>; [33.00%]
  else
    goto <bb 8>; [67.00%]

  <bb 7> [local count: 115158811]:
  # DEBUG BEGIN_STMT
  state_4->mbs[0].isPolling = 0;
  # DEBUG BEGIN_STMT
  _9 = state_4->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (base_3, instance_1(D), 6, 1, _9);
  # DEBUG BEGIN_STMT
  _10 = state_4->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (base_3, instance_1(D), 7, 1, _10);
  # DEBUG BEGIN_STMT
  _11 = state_4->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (base_3, instance_1(D), 5, 1, _11);

  <bb 8> [local count: 1073741824]:
  # eResult_12 = PHI <1(2), 2(3), 0(6), 0(7)>
  # DEBUG eResult => eResult_12
  # DEBUG BEGIN_STMT
  return eResult_12;

}


FlexCAN_GetMsgBuffIntStatusFlag.part.0 (const struct FLEXCAN_Type * base, uint32 msgBuffIdx)
{
  uint8 flag;
  uint32 mask;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _6;
  long unsigned int _7;
  unsigned char _8;

  <bb 4> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  mask_2 ={v} base_1(D)->IMASK3;
  # DEBUG mask => mask_2
  # DEBUG BEGIN_STMT
  _3 ={v} base_1(D)->IFLAG3;
  _4 = mask_2 & _3;
  _6 = msgBuffIdx_5(D) & 31;
  _7 = _4 >> _6;
  _8 = (unsigned char) _7;
  flag_9 = _8 & 1;
  # DEBUG flag => flag_9

  <bb 3> [local count: 1073741824]:
  # flag_10 = PHI <flag_9(2)>
  # DEBUG flag => flag_10
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  return flag_10;

}


FlexCAN_SetEnhancedDataTimeSegments.part.0 (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  long unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 3> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 ={v} base_1(D)->EDCBT;
  _3 = _2 & 4231991264;
  base_1(D)->EDCBT ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_1(D)->EDCBT;
  _6 = timeSeg_5(D)->phaseSeg1;
  _7 = timeSeg_5(D)->propSeg;
  _8 = _6 + _7;
  _9 = _8 & 31;
  _10 = timeSeg_5(D)->phaseSeg2;
  _11 = _10 << 12;
  _12 = _11 & 65535;
  _13 = _9 | _12;
  _14 = timeSeg_5(D)->rJumpwidth;
  _15 = _14 << 22;
  _16 = _15 & 62914560;
  _17 = _13 | _16;
  _18 = _4 | _17;
  base_1(D)->EDCBT ={v} _18;
  # DEBUG BEGIN_STMT
  _19 ={v} base_1(D)->EPRS;
  _20 = _19 & 4227923967;
  base_1(D)->EPRS ={v} _20;
  # DEBUG BEGIN_STMT
  _21 ={v} base_1(D)->EPRS;
  _22 = timeSeg_5(D)->preDivider;
  _23 = _22 << 16;
  _24 = _23 & 67043328;
  _25 = _21 | _24;
  base_1(D)->EPRS ={v} _25;
  return;

}


FlexCAN_SetEnhancedNominalTimeSegments.part.0 (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  long unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 3> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 ={v} base_1(D)->ENCBT;
  _3 = _2 & 3761770240;
  base_1(D)->ENCBT ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_1(D)->ENCBT;
  _6 = timeSeg_5(D)->phaseSeg1;
  _7 = timeSeg_5(D)->propSeg;
  _8 = _6 + _7;
  _9 = _8 + 1;
  _10 = _9 & 255;
  _11 = timeSeg_5(D)->phaseSeg2;
  _12 = _11 << 12;
  _13 = _12 & 520192;
  _14 = _10 | _13;
  _15 = timeSeg_5(D)->rJumpwidth;
  _16 = _15 << 22;
  _17 = _16 & 532676608;
  _18 = _14 | _17;
  _19 = _4 | _18;
  base_1(D)->ENCBT ={v} _19;
  # DEBUG BEGIN_STMT
  _20 ={v} base_1(D)->EPRS;
  _21 = _20 & 4294966272;
  base_1(D)->EPRS ={v} _21;
  # DEBUG BEGIN_STMT
  _22 ={v} base_1(D)->EPRS;
  _23 = timeSeg_5(D)->preDivider;
  _24 = _23 & 1023;
  _25 = _22 | _24;
  base_1(D)->EPRS ={v} _25;
  return;

}


FlexCAN_SetExtendedTimeSegments.part.0 (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  long unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;

  <bb 3> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 ={v} base_1(D)->CBT;
  _3 = _2 & 2147483648;
  base_1(D)->CBT ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_1(D)->CBT;
  _6 = timeSeg_5(D)->propSeg;
  _7 = _6 << 10;
  _8 = _7 & 65535;
  _9 = timeSeg_5(D)->phaseSeg2;
  _10 = _9 & 31;
  _11 = _8 | _10;
  _12 = timeSeg_5(D)->phaseSeg1;
  _13 = _12 << 5;
  _14 = _13 & 992;
  _15 = _11 | _14;
  _16 = timeSeg_5(D)->preDivider;
  _17 = _16 << 21;
  _18 = _17 & 2145386496;
  _19 = _15 | _18;
  _20 = timeSeg_5(D)->rJumpwidth;
  _21 = _20 << 16;
  _22 = _21 & 2031616;
  _23 = _19 | _22;
  _24 = _4 | _23;
  base_1(D)->CBT ={v} _24;
  return;

}


FlexCAN_SetTimeSegments.part.0 (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  long unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;

  <bb 3> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 ={v} base_1(D)->CTRL1;
  _3 = _2 & 65528;
  base_1(D)->CTRL1 ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_1(D)->CTRL1;
  _6 = timeSeg_5(D)->propSeg;
  _7 = _6 & 7;
  _8 = timeSeg_5(D)->phaseSeg2;
  _9 = _8 << 16;
  _10 = _9 & 458752;
  _11 = _7 | _10;
  _12 = timeSeg_5(D)->phaseSeg1;
  _13 = _12 << 19;
  _14 = _13 & 3670016;
  _15 = _11 | _14;
  _16 = timeSeg_5(D)->preDivider;
  _17 = _16 << 24;
  _18 = _15 | _17;
  _19 = timeSeg_5(D)->rJumpwidth;
  _20 = _19 << 22;
  _21 = _20 & 12582912;
  _22 = _18 | _21;
  _23 = _4 | _22;
  base_1(D)->CTRL1 ={v} _23;
  return;

}


FlexCAN_SetFDTimeSegments.part.0 (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  long unsigned int _18;
  long unsigned int _19;
  long unsigned int _20;
  long unsigned int _21;
  long unsigned int _22;
  long unsigned int _23;
  long unsigned int _24;

  <bb 3> [local count: 1073741824]:

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 ={v} base_1(D)->FDCBT;
  _3 = _2 & 3221783320;
  base_1(D)->FDCBT ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_1(D)->FDCBT;
  _6 = timeSeg_5(D)->propSeg;
  _7 = _6 << 10;
  _8 = _7 & 31744;
  _9 = timeSeg_5(D)->phaseSeg2;
  _10 = _9 & 7;
  _11 = _8 | _10;
  _12 = timeSeg_5(D)->phaseSeg1;
  _13 = _12 << 5;
  _14 = _13 & 255;
  _15 = _11 | _14;
  _16 = timeSeg_5(D)->preDivider;
  _17 = _16 << 20;
  _18 = _17 & 1072693248;
  _19 = _15 | _18;
  _20 = timeSeg_5(D)->rJumpwidth;
  _21 = _20 << 16;
  _22 = _21 & 458752;
  _23 = _19 | _22;
  _24 = _4 | _23;
  base_1(D)->FDCBT ={v} _24;
  return;

}


FlexCAN_Ip_GetListenOnlyMode (uint8 instance)
{
  const struct FLEXCAN_Type * base;
  int _1;
  long unsigned int _5;
  long unsigned int _6;
  _Bool _7;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_2(D);
  base_4 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_4
  # DEBUG BEGIN_STMT
  # DEBUG base => base_4
  # DEBUG INLINE_ENTRY FlexCAN_IsListenOnlyModeEnabled
  # DEBUG BEGIN_STMT
  _5 ={v} base_4->CTRL1;
  _6 = _5 & 8;
  _7 = _6 != 0;
  # DEBUG base => NULL
  return _7;

}


FlexCAN_Ip_SetListenOnlyMode_Privileged (uint8 instance, const boolean enable)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _18;
  signed int _19;
  _Bool x.0_20;
  long unsigned int _21;
  long unsigned int _22;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_8(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_20 ={v} x;
  if (x.0_20 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _2 = (int) instance_8(D);
  pBase_11 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _18 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _19 = (signed int) _18;
  # DEBUG pBase => NULL
  # DEBUG disabled => _19 < 0
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13

  <bb 6> [local count: 107374]:
  # result_3 = PHI <0(4), result_13(5)>
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _22 = _21 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _22 != 0
  # DEBUG BEGIN_STMT
  if (_22 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 53687]:
  if (result_3 == 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 80531]:
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  if (result_3 == 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 10>; [67.00%]

  <bb 9> [local count: 26575]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetListenOnlyMode (pBase_11, enable_14(D));

  <bb 10> [local count: 107374]:
  # result_10 = PHI <result_3(8), 0(9), 1(7)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 11>; [25.50%]
  else
    goto <bb 13>; [74.50%]

  <bb 11> [local count: 27380]:
  # DEBUG BEGIN_STMT
  status_17 = FlexCAN_Disable (pBase_11);
  # DEBUG status => status_17
  # DEBUG BEGIN_STMT
  if (status_17 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 13690]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_17

  <bb 13> [local count: 107374]:
  # result_4 = PHI <result_10(10), result_10(11), status_17(12)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_SetRxMb15Mask_Privileged (uint8 instance, uint32 mask)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _18;
  signed int _19;
  _Bool x.0_20;
  long unsigned int _21;
  long unsigned int _22;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_8(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_20 ={v} x;
  if (x.0_20 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _2 = (int) instance_8(D);
  pBase_11 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG freeze => 0
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _18 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _19 = (signed int) _18;
  # DEBUG pBase => NULL
  # DEBUG disabled => _19 < 0
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13

  <bb 6> [local count: 107374]:
  # result_3 = PHI <0(4), result_13(5)>
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _22 = _21 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _22 != 0
  # DEBUG BEGIN_STMT
  if (_22 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 53687]:
  if (result_3 == 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 80531]:
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  if (result_3 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 40265]:
  # DEBUG BEGIN_STMT
  pBase_11->RX15MASK ={v} mask_14(D);

  <bb 10> [local count: 107374]:
  # result_10 = PHI <result_3(8), 0(9), 1(7)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 11>; [25.50%]
  else
    goto <bb 13>; [74.50%]

  <bb 11> [local count: 27380]:
  # DEBUG BEGIN_STMT
  status_17 = FlexCAN_Disable (pBase_11);
  # DEBUG status => status_17
  # DEBUG BEGIN_STMT
  if (status_17 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 13690]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_17

  <bb 13> [local count: 107374]:
  # result_4 = PHI <result_10(10), result_10(11), status_17(12)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_SetRxMb14Mask_Privileged (uint8 instance, uint32 mask)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _18;
  signed int _19;
  _Bool x.0_20;
  long unsigned int _21;
  long unsigned int _22;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_8(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_20 ={v} x;
  if (x.0_20 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _2 = (int) instance_8(D);
  pBase_11 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG freeze => 0
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _18 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _19 = (signed int) _18;
  # DEBUG pBase => NULL
  # DEBUG disabled => _19 < 0
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13

  <bb 6> [local count: 107374]:
  # result_3 = PHI <0(4), result_13(5)>
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _22 = _21 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _22 != 0
  # DEBUG BEGIN_STMT
  if (_22 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 53687]:
  if (result_3 == 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 80531]:
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  if (result_3 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 40265]:
  # DEBUG BEGIN_STMT
  pBase_11->RX14MASK ={v} mask_14(D);

  <bb 10> [local count: 107374]:
  # result_10 = PHI <result_3(8), 0(9), 1(7)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 11>; [25.50%]
  else
    goto <bb 13>; [74.50%]

  <bb 11> [local count: 27380]:
  # DEBUG BEGIN_STMT
  status_17 = FlexCAN_Disable (pBase_11);
  # DEBUG status => status_17
  # DEBUG BEGIN_STMT
  if (status_17 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 13690]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_17

  <bb 13> [local count: 107374]:
  # result_4 = PHI <result_10(10), result_10(11), status_17(12)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_AbortTransfer (uint8 u8Instance, uint8 mb_idx)
{
  volatile boolean x;
  volatile boolean x;
  Flexcan_Ip_StatusType result;
  const struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * pBase;
  _Bool _1;
  unsigned char _2;
  _Bool _3;
  int _4;
  int _5;
  <unnamed type> _6;
  long unsigned int _7;
  _Bool _8;
  <unnamed type> _9;
  <unnamed type> _10;
  _Bool x.0_24;
  _Bool x.0_25;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = u8Instance_15(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_25 ={v} x;
  if (x.0_25 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 16> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = mb_idx_17(D) + 160;
  _3 = _2 > 158;
  x ={v} _3;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_24 ={v} x;
  if (x.0_24 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 13> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _4 = (int) u8Instance_15(D);
  pBase_18 = g_Flexcan_Ip_aBase[_4];
  # DEBUG pBase => pBase_18
  # DEBUG BEGIN_STMT
  state_19 = g_flexcan_Ip_StatePtr[_4];
  # DEBUG state => state_19
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  if (mb_idx_17(D) <= 95)
    goto <bb 7>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 7> [local count: 26844]:
  # DEBUG BEGIN_STMT
  _5 = (int) mb_idx_17(D);
  _6 ={v} state_19->mbs[_5].state;
  if (_6 == 0)
    goto <bb 12>; [52.23%]
  else
    goto <bb 8>; [47.77%]

  <bb 8> [local count: 12823]:
  # DEBUG BEGIN_STMT
  _7 = (long unsigned int) mb_idx_17(D);
  _8 = state_19->isIntActive;
  FLEXCAN_ClearMsgBuffIntCmd (pBase_18, u8Instance_15(D), _7, _8);
  # DEBUG BEGIN_STMT
  _9 ={v} state_19->mbs[_5].state;
  if (_9 == 2)
    goto <bb 9>; [20.24%]
  else
    goto <bb 10>; [79.76%]

  <bb 9> [local count: 2595]:
  # DEBUG BEGIN_STMT
  result_22 = FlexCAN_AbortTxTransfer (u8Instance_15(D), mb_idx_17(D));
  # DEBUG result => result_22

  <bb 10> [local count: 12823]:
  # result_11 = PHI <0(8), result_22(9)>
  # DEBUG result => result_11
  # DEBUG BEGIN_STMT
  _10 ={v} state_19->mbs[_5].state;
  if (_10 == 1)
    goto <bb 11>; [20.24%]
  else
    goto <bb 12>; [79.76%]

  <bb 11> [local count: 2595]:
  # DEBUG BEGIN_STMT
  FlexCAN_AbortRxTransfer (u8Instance_15(D), mb_idx_17(D));

  <bb 12> [local count: 53687]:
  # result_12 = PHI <0(6), 5(7), result_11(10), result_11(11)>
  # DEBUG result => result_12
  # DEBUG BEGIN_STMT
  return result_12;

}


FlexCAN_Ip_SetErrorInt_Privileged (uint8 u8Instance, Flexcan_Ip_ErrorIntType type, boolean enable)
{
  volatile boolean x;
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _23;
  signed int _24;
  _Bool x.0_25;
  long unsigned int _26;
  long unsigned int _27;
  long unsigned int _28;
  long unsigned int _29;
  _Bool x.0_30;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = u8Instance_7(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_25 ={v} x;
  if (x.0_25 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 21>; [50.00%]

  <bb 21> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 23> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _2 = (int) u8Instance_7(D);
  pBase_11 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _24 = (signed int) _23;
  # DEBUG pBase => NULL
  # DEBUG disabled => _24 < 0
  # DEBUG BEGIN_STMT
  if (_24 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13
  # DEBUG BEGIN_STMT
  if (result_13 == 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 6> [local count: 93684]:
  # result_9 = PHI <result_13(5), 0(4)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  switch (type_14(D)) <default: <L14> [16.67%], case 0: <L22> [16.67%], case 1: <L23> [16.67%], case 2: <L4> [16.67%], case 3: <L5> [16.67%], case 4: <L3> [16.67%]>

  <bb 7> [local count: 15617]:
<L3>:
  # DEBUG BEGIN_STMT
  FlexCAN_SetErrIntCmd (pBase_11, 32768, enable_15(D));
  # DEBUG BEGIN_STMT
  goto <bb 16>; [100.00%]

  <bb 8> [local count: 15617]:
<L4>:
  # DEBUG BEGIN_STMT
  FlexCAN_SetErrIntCmd (pBase_11, 16384, enable_15(D));
  # DEBUG BEGIN_STMT
  goto <bb 16>; [100.00%]

  <bb 9> [local count: 15617]:
<L5>:
  # DEBUG BEGIN_STMT
  FlexCAN_SetErrIntCmd (pBase_11, 16385, enable_15(D));
  # DEBUG BEGIN_STMT
  goto <bb 16>; [100.00%]

  <bb 10> [local count: 15617]:
<L22>:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _26 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _27 = _26 & 16777216;
  # DEBUG base => NULL
  if (_27 == 0)
    goto <bb 16>; [67.00%]
  else
    goto <bb 11>; [33.00%]

  <bb 11> [local count: 5154]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetErrIntCmd (pBase_11, 1024, enable_15(D));
  goto <bb 16>; [100.00%]

  <bb 12> [local count: 15617]:
<L23>:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _28 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _29 = _28 & 16777216;
  # DEBUG base => NULL
  if (_29 == 0)
    goto <bb 16>; [67.00%]
  else
    goto <bb 13>; [33.00%]

  <bb 13> [local count: 5154]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetErrIntCmd (pBase_11, 2048, enable_15(D));
  goto <bb 16>; [100.00%]

  <bb 14> [local count: 15617]:
<L14>:
  # DEBUG BEGIN_STMT
  x ={v} 0;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_30 ={v} x;
  if (x.0_30 != 0)
    goto <bb 16>; [50.00%]
  else
    goto <bb 20>; [50.00%]

  <bb 20> [local count: 7809]:

  <bb 15> [local count: 78085593]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 22> [local count: 78085593]:
  goto <bb 15>; [100.00%]

  <bb 16> [local count: 99584]:
  # result_3 = PHI <result_13(5), result_9(7), result_9(8), result_9(9), result_9(11), result_9(13), result_9(14), 1(10), 1(12)>
  # DEBUG x => NULL
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  if (_24 < 0)
    goto <bb 17>; [25.50%]
  else
    goto <bb 19>; [74.50%]

  <bb 17> [local count: 25394]:
  # DEBUG BEGIN_STMT
  status_22 = FlexCAN_Disable (pBase_11);
  # DEBUG status => status_22
  # DEBUG BEGIN_STMT
  if (status_22 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 12697]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_22

  <bb 19> [local count: 99584]:
  # result_4 = PHI <result_3(16), result_3(17), status_22(18)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_DisableInterrupts_Privileged (uint8 u8Instance)
{
  volatile boolean x;
  struct Flexcan_Ip_StateType * state;
  Flexcan_Ip_StatusType result;
  struct FLEXCAN_Type * pBase;
  int _1;
  _Bool _2;
  _Bool _3;
  long unsigned int _14;
  signed int _15;
  _Bool x.0_16;
  long unsigned int _17;
  signed int _18;
  long unsigned int _19;
  long unsigned int _20;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) u8Instance_7(D);
  pBase_9 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_9
  # DEBUG BEGIN_STMT
  # DEBUG result => 1
  # DEBUG BEGIN_STMT
  state_10 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_10
  # DEBUG BEGIN_STMT
  _2 = u8Instance_7(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_16 ={v} x;
  if (x.0_16 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 10> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 11> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_9
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _14 ={v} MEM[(const struct FLEXCAN_Type *)pBase_9].MCR;
  _15 = (signed int) _14;
  # DEBUG pBase => NULL
  if (_15 >= 0)
    goto <bb 5>; [41.48%]
  else
    goto <bb 9>; [58.52%]

  <bb 5> [local count: 44539]:
  # DEBUG BEGIN_STMT
  FlexCAN_DisableInterrupts (pBase_9);
  # DEBUG BEGIN_STMT
  _3 = FlexCAN_IsEnhancedRxFifoAvailable (pBase_9);
  if (_3 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 6> [local count: 22269]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_9
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhancedRxFifoEnabled
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(const struct FLEXCAN_Type *)pBase_9].ERFCR;
  _18 = (signed int) _17;
  # DEBUG base => NULL
  if (_18 < 0)
    goto <bb 7>; [41.00%]
  else
    goto <bb 8>; [59.00%]

  <bb 7> [local count: 9130]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_9
  # DEBUG enable => 0
  # DEBUG INLINE_ENTRY FlexCAN_SetEnhancedRxFifoIntAll
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _19 ={v} pBase_9->ERFIER;
  _20 = _19 & 268435455;
  pBase_9->ERFIER ={v} _20;

  <bb 8> [local count: 44539]:
  # DEBUG base => NULL
  # DEBUG enable => NULL
  # DEBUG BEGIN_STMT
  state_10->isIntActive = 0;
  # DEBUG BEGIN_STMT
  # DEBUG result => 0

  <bb 9> [local count: 107374]:
  # result_4 = PHI <1(4), 0(8)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_EnableInterrupts_Privileged (uint8 u8Instance)
{
  volatile boolean x;
  struct Flexcan_Ip_StateType * state;
  Flexcan_Ip_StatusType result;
  struct FLEXCAN_Type * pBase;
  int _1;
  _Bool _2;
  _Bool _3;
  _Bool _4;
  long unsigned int _15;
  signed int _16;
  _Bool x.0_17;
  long unsigned int _18;
  signed int _19;
  long unsigned int _20;
  long unsigned int _21;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) u8Instance_8(D);
  pBase_10 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_10
  # DEBUG BEGIN_STMT
  # DEBUG result => 1
  # DEBUG BEGIN_STMT
  state_11 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_11
  # DEBUG BEGIN_STMT
  _2 = u8Instance_8(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_17 ={v} x;
  if (x.0_17 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 11> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 12> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_10
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _15 ={v} MEM[(const struct FLEXCAN_Type *)pBase_10].MCR;
  _16 = (signed int) _15;
  # DEBUG pBase => NULL
  if (_16 >= 0)
    goto <bb 5>; [41.48%]
  else
    goto <bb 10>; [58.52%]

  <bb 5> [local count: 44539]:
  # DEBUG BEGIN_STMT
  FlexCAN_EnableInterrupts (pBase_10, u8Instance_8(D));
  # DEBUG BEGIN_STMT
  _3 = state_11->enhancedFifoOutput.isPolling;
  if (_3 != 0)
    goto <bb 9>; [67.00%]
  else
    goto <bb 6>; [33.00%]

  <bb 6> [local count: 14698]:
  _4 = FlexCAN_IsEnhancedRxFifoAvailable (pBase_10);
  if (_4 != 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 7> [local count: 7349]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_10
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhancedRxFifoEnabled
  # DEBUG BEGIN_STMT
  _18 ={v} MEM[(const struct FLEXCAN_Type *)pBase_10].ERFCR;
  _19 = (signed int) _18;
  # DEBUG base => NULL
  if (_19 < 0)
    goto <bb 8>; [41.00%]
  else
    goto <bb 9>; [59.00%]

  <bb 8> [local count: 3013]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_10
  # DEBUG enable => 1
  # DEBUG INLINE_ENTRY FlexCAN_SetEnhancedRxFifoIntAll
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _20 ={v} pBase_10->ERFIER;
  _21 = _20 | 4026531840;
  pBase_10->ERFIER ={v} _21;

  <bb 9> [local count: 44539]:
  # DEBUG base => NULL
  # DEBUG enable => NULL
  # DEBUG BEGIN_STMT
  state_11->isIntActive = 1;
  # DEBUG BEGIN_STMT
  # DEBUG result => 0

  <bb 10> [local count: 107374]:
  # result_5 = PHI <1(4), 0(9)>
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  return result_5;

}


FlexCAN_Ip_ClearBuffStatusFlag (uint8 instance, uint8 msgBuffIdx)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  _Bool _1;
  int _2;
  long unsigned int _3;
  _Bool x.0_10;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_5(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_10 ={v} x;
  if (x.0_10 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 9> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = (int) instance_5(D);
  pBase_7 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_7
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_8(D) == 255)
    goto <bb 5>; [51.12%]
  else
    goto <bb 6>; [48.88%]

  <bb 5> [local count: 54890]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_7
  # DEBUG intFlag => 30
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  pBase_7->ERFSR ={v} 1073741824;
  goto <bb 7>; [100.00%]

  <bb 6> [local count: 52484]:
  # DEBUG BEGIN_STMT
  _3 = (long unsigned int) msgBuffIdx_8(D);
  FlexCAN_ClearMsgBuffIntStatusFlag (pBase_7, _3);

  <bb 7> [local count: 107374]:
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  return;

}


FlexCAN_Ip_GetBuffStatusFlag (uint8 instance, uint8 msgBuffIdx)
{
  volatile boolean x;
  const struct FLEXCAN_Type * pBase;
  boolean returnResult;
  _Bool _1;
  int _2;
  long unsigned int _3;
  unsigned char _4;
  long unsigned int _13;
  _Bool x.0_15;
  long unsigned int _16;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG returnResult => 1
  # DEBUG BEGIN_STMT
  _1 = instance_7(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_15 ={v} x;
  if (x.0_15 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 9> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = (int) instance_7(D);
  pBase_9 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_9
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_10(D) == 255)
    goto <bb 5>; [51.12%]
  else
    goto <bb 6>; [48.88%]

  <bb 5> [local count: 54890]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_9
  # DEBUG intFlag => 30
  # DEBUG INLINE_ENTRY FlexCAN_GetEnhancedRxFIFOStatusFlag
  # DEBUG BEGIN_STMT
  _16 ={v} pBase_9->ERFSR;
  _13 = _16 >> 30;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  returnResult_14 = (boolean) _13;
  # DEBUG returnResult => returnResult_14
  goto <bb 7>; [100.00%]

  <bb 6> [local count: 52484]:
  # DEBUG BEGIN_STMT
  _3 = (long unsigned int) msgBuffIdx_10(D);
  _4 = FlexCAN_GetBuffStatusFlag (pBase_9, _3);
  returnResult_12 = _4 == 1;
  # DEBUG returnResult => returnResult_12

  <bb 7> [local count: 107374]:
  # returnResult_5 = PHI <returnResult_14(5), returnResult_12(6)>
  # DEBUG returnResult => returnResult_5
  # DEBUG BEGIN_STMT
  return returnResult_5;

}


FlexCAN_Ip_SetTxArbitrationStartDelay_Privileged (uint8 instance, uint8 value)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _20;
  signed int _21;
  _Bool x.0_22;
  long unsigned int _23;
  long unsigned int _24;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_8(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_22 ={v} x;
  if (x.0_22 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _2 = (int) instance_8(D);
  pBase_11 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _20 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _21 = (signed int) _20;
  # DEBUG pBase => NULL
  # DEBUG disabled => _21 < 0
  # DEBUG BEGIN_STMT
  if (_21 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13

  <bb 6> [local count: 107374]:
  # result_3 = PHI <0(4), result_13(5)>
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _23 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _24 = _23 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _24 != 0
  # DEBUG BEGIN_STMT
  if (_24 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 53687]:
  if (result_3 == 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 80531]:
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  if (result_3 == 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 10>; [67.00%]

  <bb 9> [local count: 26575]:
  # DEBUG BEGIN_STMT
  SchM_Enter_Can_CAN_EXCLUSIVE_AREA_17 ();
  # DEBUG BEGIN_STMT
  FlexCAN_SetTxArbitrationStartDelay (pBase_11, value_15(D));
  # DEBUG BEGIN_STMT
  SchM_Exit_Can_CAN_EXCLUSIVE_AREA_17 ();

  <bb 10> [local count: 107374]:
  # result_10 = PHI <result_3(8), 0(9), 1(7)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_21 < 0)
    goto <bb 11>; [25.50%]
  else
    goto <bb 13>; [74.50%]

  <bb 11> [local count: 27380]:
  # DEBUG BEGIN_STMT
  status_19 = FlexCAN_Disable (pBase_11);
  # DEBUG status => status_19
  # DEBUG BEGIN_STMT
  if (status_19 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 13690]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_19

  <bb 13> [local count: 107374]:
  # result_4 = PHI <result_10(10), result_10(11), status_19(12)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_SetTDCOffset_Privileged (uint8 instance, boolean enable, uint8 offset)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _25;
  signed int _26;
  _Bool x.0_27;
  long unsigned int _28;
  long unsigned int _29;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_11(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_27 ={v} x;
  if (x.0_27 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 17>; [50.00%]

  <bb 17> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 18> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _2 = (int) instance_11(D);
  pBase_14 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_14
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _25 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].MCR;
  _26 = (signed int) _25;
  # DEBUG pBase => NULL
  # DEBUG disabled => _26 < 0
  # DEBUG BEGIN_STMT
  if (_26 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_16 = FlexCAN_Enable (pBase_14);
  # DEBUG result => result_16

  <bb 6> [local count: 107374]:
  # result_5 = PHI <0(4), result_16(5)>
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _28 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].MCR;
  _29 = _28 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _29 != 0
  # DEBUG BEGIN_STMT
  if (_29 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 53687]:
  if (result_5 == 0)
    goto <bb 13>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 80531]:
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  if (result_5 == 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 13>; [67.00%]

  <bb 9> [local count: 26575]:
  # DEBUG BEGIN_STMT
  SchM_Enter_Can_CAN_EXCLUSIVE_AREA_16 ();
  # DEBUG BEGIN_STMT
  _3 ={v} pBase_14->CTRL2;
  _4 = _3 & 8192;
  if (_4 != 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 10> [local count: 13288]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetEnhancedTDCOffset (pBase_14, enable_18(D), offset_19(D));
  goto <bb 12>; [100.00%]

  <bb 11> [local count: 13288]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetTDCOffset (pBase_14, enable_18(D), offset_19(D));

  <bb 12> [local count: 26575]:
  # DEBUG BEGIN_STMT
  SchM_Exit_Can_CAN_EXCLUSIVE_AREA_16 ();

  <bb 13> [local count: 107374]:
  # result_13 = PHI <result_5(8), 0(12), 1(7)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_26 < 0)
    goto <bb 14>; [25.50%]
  else
    goto <bb 16>; [74.50%]

  <bb 14> [local count: 27380]:
  # DEBUG BEGIN_STMT
  status_24 = FlexCAN_Disable (pBase_14);
  # DEBUG status => status_24
  # DEBUG BEGIN_STMT
  if (status_24 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 15> [local count: 13690]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_24

  <bb 16> [local count: 107374]:
  # result_6 = PHI <result_13(13), result_13(14), status_24(15)>
  # DEBUG result => result_6
  # DEBUG BEGIN_STMT
  return result_6;

}


FlexCAN_Ip_GetBitrateFD (uint8 instance, struct Flexcan_Ip_TimeSegmentType * bitrate)
{
  volatile boolean x;
  volatile boolean x;
  const struct FLEXCAN_Type * pBase;
  _Bool _1;
  _Bool _2;
  int _3;
  long unsigned int _11;
  long unsigned int _12;
  _Bool _13;
  _Bool x.0_14;
  _Bool x.0_15;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_5(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_15 ={v} x;
  if (x.0_15 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 11> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 13> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = bitrate_7(D) != 0B;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_14 ={v} x;
  if (x.0_14 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 10> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 12> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = (int) instance_5(D);
  pBase_8 = g_Flexcan_Ip_aBase[_3];
  # DEBUG pBase => pBase_8
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_8
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhCbtEnabled
  # DEBUG BEGIN_STMT
  _11 ={v} pBase_8->CTRL2;
  _12 = _11 & 8192;
  _13 = _12 != 0;
  # DEBUG pBase => NULL
  # DEBUG enhCbt => _13
  # DEBUG BEGIN_STMT
  if (_12 != 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 26844]:
  # DEBUG BEGIN_STMT
  FlexCAN_GetEnhancedDataTimeSegments (pBase_8, bitrate_7(D));
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 26844]:
  # DEBUG BEGIN_STMT
  FlexCAN_GetFDTimeSegments (pBase_8, bitrate_7(D));

  <bb 9> [local count: 53687]:
  # DEBUG BEGIN_STMT
  return _13;

}


FlexCAN_Ip_SetBitrateCbt_Privileged (uint8 instance, const struct Flexcan_Ip_TimeSegmentType * bitrate, boolean bitRateSwitch)
{
  volatile boolean x;
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  _Bool _2;
  int _3;
  long unsigned int _25;
  long unsigned int _26;
  _Bool _27;
  long unsigned int _28;
  signed int _29;
  _Bool x.0_30;
  _Bool x.0_31;
  long unsigned int _32;
  long unsigned int _33;
  long unsigned int _34;
  long unsigned int _35;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_11(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_31 ={v} x;
  if (x.0_31 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 21>; [50.00%]

  <bb 21> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 23> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = bitrate_13(D) != 0B;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_30 ={v} x;
  if (x.0_30 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 20>; [50.00%]

  <bb 20> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 22> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _3 = (int) instance_11(D);
  pBase_14 = g_Flexcan_Ip_aBase[_3];
  # DEBUG pBase => pBase_14
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _28 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].MCR;
  _29 = (signed int) _28;
  # DEBUG pBase => NULL
  # DEBUG disabled => _29 < 0
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsFDEnabled
  # DEBUG BEGIN_STMT
  _25 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].MCR;
  _26 = _25 & 2048;
  _27 = _26 != 0;
  # DEBUG base => NULL
  # DEBUG fd_enable => _27
  # DEBUG BEGIN_STMT
  if (_29 < 0)
    goto <bb 7>; [25.50%]
  else
    goto <bb 8>; [74.50%]

  <bb 7> [local count: 13690]:
  # DEBUG BEGIN_STMT
  result_16 = FlexCAN_Enable (pBase_14);
  # DEBUG result => result_16

  <bb 8> [local count: 53687]:
  # result_5 = PHI <0(6), result_16(7)>
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _32 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].MCR;
  _33 = _32 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _33 != 0
  # DEBUG BEGIN_STMT
  if (_26 == 0)
    goto <bb 16>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 9> [local count: 26844]:
  if (_33 == 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 10> [local count: 13422]:
  if (result_5 == 0)
    goto <bb 16>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 11> [local count: 20133]:
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  if (result_5 == 0)
    goto <bb 12>; [33.00%]
  else
    goto <bb 16>; [67.00%]

  <bb 12> [local count: 6644]:
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhCbtEnabled
  # DEBUG BEGIN_STMT
  _34 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].CTRL2;
  _35 = _34 & 8192;
  # DEBUG pBase => NULL
  # DEBUG enhCbt => _35 != 0
  # DEBUG BEGIN_STMT
  SchM_Enter_Can_CAN_EXCLUSIVE_AREA_15 ();
  # DEBUG BEGIN_STMT
  FlexCAN_SetFDEnabled (pBase_14, _27, bitRateSwitch_18(D));
  # DEBUG BEGIN_STMT
  if (_35 != 0)
    goto <bb 13>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 13> [local count: 3322]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetEnhancedDataTimeSegments (pBase_14, bitrate_13(D));
  goto <bb 15>; [100.00%]

  <bb 14> [local count: 3322]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetFDTimeSegments (pBase_14, bitrate_13(D));

  <bb 15> [local count: 6644]:
  # DEBUG BEGIN_STMT
  SchM_Exit_Can_CAN_EXCLUSIVE_AREA_15 ();

  <bb 16> [local count: 53687]:
  # result_4 = PHI <result_5(11), 0(15), 1(8), 1(10)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_29 < 0)
    goto <bb 17>; [25.50%]
  else
    goto <bb 19>; [74.50%]

  <bb 17> [local count: 13690]:
  # DEBUG BEGIN_STMT
  status_24 = FlexCAN_Disable (pBase_14);
  # DEBUG status => status_24
  # DEBUG BEGIN_STMT
  if (status_24 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 18> [local count: 6845]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_24

  <bb 19> [local count: 53687]:
  # result_6 = PHI <result_4(16), result_4(17), status_24(18)>
  # DEBUG result => result_6
  # DEBUG BEGIN_STMT
  return result_6;

}


FlexCAN_Ip_GetTDCValue_Privileged (uint8 u8Instance)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType result;
  uint8 value;
  _Bool _1;
  int _2;
  long unsigned int _3;
  long unsigned int _4;
  unsigned char _5;
  long unsigned int _18;
  signed int _19;
  _Bool x.0_20;
  long unsigned int _21;
  long unsigned int _22;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG value => 0
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  _1 = u8Instance_10(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_20 ={v} x;
  if (x.0_20 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 13> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = (int) u8Instance_10(D);
  pBase_12 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_12
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_12
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _18 ={v} MEM[(const struct FLEXCAN_Type *)pBase_12].MCR;
  _19 = (signed int) _18;
  # DEBUG pBase => NULL
  # DEBUG disabled => _19 < 0
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_14 = FlexCAN_Enable (pBase_12);
  # DEBUG result => result_14
  # DEBUG BEGIN_STMT
  if (result_14 == 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 6> [local count: 93684]:
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_12
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhCbtEnabled
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(const struct FLEXCAN_Type *)pBase_12].CTRL2;
  _22 = _21 & 8192;
  # DEBUG pBase => NULL
  if (_22 != 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 46842]:
  # DEBUG BEGIN_STMT
  _3 ={v} pBase_12->ETDC;
  value_16 = (uint8) _3;
  # DEBUG value => value_16
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 46842]:
  # DEBUG BEGIN_STMT
  _4 ={v} pBase_12->FDCTRL;
  _5 = (unsigned char) _4;
  value_15 = _5 & 63;
  # DEBUG value => value_15

  <bb 9> [local count: 107374]:
  # value_6 = PHI <0(5), value_16(7), value_15(8)>
  # DEBUG value => value_6
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 10>; [25.50%]
  else
    goto <bb 11>; [74.50%]

  <bb 10> [local count: 27380]:
  # DEBUG BEGIN_STMT
  FlexCAN_Disable (pBase_12);

  <bb 11> [local count: 107374]:
  # DEBUG BEGIN_STMT
  return value_6;

}


FlexCAN_Ip_GetTDCFail_Privileged (uint8 u8Instance)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType result;
  boolean value;
  _Bool _1;
  int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _19;
  signed int _20;
  _Bool x.0_21;
  long unsigned int _22;
  long unsigned int _23;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG value => 0
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  _1 = u8Instance_11(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_21 ={v} x;
  if (x.0_21 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 13> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = (int) u8Instance_11(D);
  pBase_13 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_13
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_13
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _19 ={v} MEM[(const struct FLEXCAN_Type *)pBase_13].MCR;
  _20 = (signed int) _19;
  # DEBUG pBase => NULL
  # DEBUG disabled => _20 < 0
  # DEBUG BEGIN_STMT
  if (_20 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_15 = FlexCAN_Enable (pBase_13);
  # DEBUG result => result_15
  # DEBUG BEGIN_STMT
  if (result_15 == 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 6> [local count: 93684]:
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_13
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhCbtEnabled
  # DEBUG BEGIN_STMT
  _22 ={v} MEM[(const struct FLEXCAN_Type *)pBase_13].CTRL2;
  _23 = _22 & 8192;
  # DEBUG pBase => NULL
  if (_23 != 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 46842]:
  # DEBUG BEGIN_STMT
  _3 ={v} pBase_13->ETDC;
  _4 = _3 & 32768;
  value_17 = _4 != 0;
  # DEBUG value => value_17
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 46842]:
  # DEBUG BEGIN_STMT
  _5 ={v} pBase_13->FDCTRL;
  _6 = _5 & 16384;
  value_16 = _6 != 0;
  # DEBUG value => value_16

  <bb 9> [local count: 107374]:
  # value_7 = PHI <0(5), value_17(7), value_16(8)>
  # DEBUG value => value_7
  # DEBUG BEGIN_STMT
  if (_20 < 0)
    goto <bb 10>; [25.50%]
  else
    goto <bb 11>; [74.50%]

  <bb 10> [local count: 27380]:
  # DEBUG BEGIN_STMT
  FlexCAN_Disable (pBase_13);

  <bb 11> [local count: 107374]:
  # DEBUG BEGIN_STMT
  return value_7;

}


FlexCAN_Ip_ClearTDCFail_Privileged (uint8 u8Instance)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _17;
  signed int _18;
  _Bool x.0_19;
  long unsigned int _20;
  long unsigned int _21;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  _1 = u8Instance_9(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_19 ={v} x;
  if (x.0_19 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 13> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = (int) u8Instance_9(D);
  pBase_11 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _18 = (signed int) _17;
  # DEBUG pBase => NULL
  # DEBUG disabled => _18 < 0
  # DEBUG BEGIN_STMT
  if (_18 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13
  # DEBUG BEGIN_STMT
  if (result_13 == 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 6> [local count: 93684]:
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhCbtEnabled
  # DEBUG BEGIN_STMT
  _20 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].CTRL2;
  _21 = _20 & 8192;
  # DEBUG pBase => NULL
  if (_21 != 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 46842]:
  # DEBUG BEGIN_STMT
  _3 ={v} pBase_11->ETDC;
  _4 = _3 | 32768;
  pBase_11->ETDC ={v} _4;
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 46842]:
  # DEBUG BEGIN_STMT
  _5 ={v} pBase_11->FDCTRL;
  _6 = _5 | 16384;
  pBase_11->FDCTRL ={v} _6;

  <bb 9> [local count: 107374]:
  # DEBUG BEGIN_STMT
  if (_18 < 0)
    goto <bb 10>; [25.50%]
  else
    goto <bb 11>; [74.50%]

  <bb 10> [local count: 27380]:
  # DEBUG BEGIN_STMT
  FlexCAN_Disable (pBase_11);

  <bb 11> [local count: 107374]:
  return;

}


FlexCAN_Ip_GetBitrate (uint8 instance, struct Flexcan_Ip_TimeSegmentType * bitrate)
{
  volatile boolean x;
  volatile boolean x;
  const struct FLEXCAN_Type * pBase;
  _Bool _1;
  _Bool _2;
  int _3;
  long unsigned int _12;
  long unsigned int _13;
  _Bool _14;
  _Bool x.0_15;
  _Bool x.0_16;
  long unsigned int _17;
  signed int _18;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_5(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_16 ={v} x;
  if (x.0_16 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 13> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = bitrate_7(D) != 0B;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_15 ={v} x;
  if (x.0_15 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 14> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = (int) instance_5(D);
  pBase_8 = g_Flexcan_Ip_aBase[_3];
  # DEBUG pBase => pBase_8
  # DEBUG BEGIN_STMT
  # DEBUG enhCbt => 0
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_8
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhCbtEnabled
  # DEBUG BEGIN_STMT
  _12 ={v} pBase_8->CTRL2;
  _13 = _12 & 8192;
  _14 = _13 != 0;
  # DEBUG pBase => NULL
  # DEBUG enhCbt => _14
  # DEBUG BEGIN_STMT
  if (_13 != 0)
    goto <bb 7>; [33.00%]
  else
    goto <bb 8>; [67.00%]

  <bb 7> [local count: 17717]:
  # DEBUG BEGIN_STMT
  FlexCAN_GetEnhancedNominalTimeSegments (pBase_8, bitrate_7(D));
  goto <bb 11>; [100.00%]

  <bb 8> [local count: 35970]:
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_8
  # DEBUG INLINE_ENTRY FlexCAN_IsExCbtEnabled
  # DEBUG BEGIN_STMT
  _17 ={v} pBase_8->CBT;
  _18 = (signed int) _17;
  # DEBUG pBase => NULL
  if (_18 < 0)
    goto <bb 9>; [41.00%]
  else
    goto <bb 10>; [59.00%]

  <bb 9> [local count: 14748]:
  # DEBUG BEGIN_STMT
  FlexCAN_GetExtendedTimeSegments (pBase_8, bitrate_7(D));
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 21222]:
  # DEBUG BEGIN_STMT
  FlexCAN_GetTimeSegments (pBase_8, bitrate_7(D));

  <bb 11> [local count: 53687]:
  # DEBUG BEGIN_STMT
  return _14;

}


FlexCAN_Ip_SetBitrate_Privileged (uint8 instance, const struct Flexcan_Ip_TimeSegmentType * bitrate, boolean enhExt)
{
  volatile boolean x;
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  _Bool _2;
  int _3;
  long unsigned int _26;
  signed int _27;
  _Bool x.0_28;
  _Bool x.0_29;
  long unsigned int _30;
  long unsigned int _31;
  long unsigned int _32;
  signed int _33;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_11(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_29 ={v} x;
  if (x.0_29 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 22>; [50.00%]

  <bb 22> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 24> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = bitrate_13(D) != 0B;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_28 ={v} x;
  if (x.0_28 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 21>; [50.00%]

  <bb 21> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 23> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _3 = (int) instance_11(D);
  pBase_14 = g_Flexcan_Ip_aBase[_3];
  # DEBUG pBase => pBase_14
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _26 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].MCR;
  _27 = (signed int) _26;
  # DEBUG pBase => NULL
  # DEBUG disabled => _27 < 0
  # DEBUG BEGIN_STMT
  if (_27 < 0)
    goto <bb 7>; [25.50%]
  else
    goto <bb 8>; [74.50%]

  <bb 7> [local count: 13690]:
  # DEBUG BEGIN_STMT
  result_16 = FlexCAN_Enable (pBase_14);
  # DEBUG result => result_16

  <bb 8> [local count: 53687]:
  # result_5 = PHI <0(6), result_16(7)>
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _30 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].MCR;
  _31 = _30 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _31 != 0
  # DEBUG BEGIN_STMT
  if (_31 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 26844]:
  if (result_5 == 0)
    goto <bb 17>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 10> [local count: 40265]:
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  if (result_5 == 0)
    goto <bb 11>; [33.00%]
  else
    goto <bb 17>; [67.00%]

  <bb 11> [local count: 13288]:
  # DEBUG BEGIN_STMT
  SchM_Enter_Can_CAN_EXCLUSIVE_AREA_14 ();
  # DEBUG BEGIN_STMT
  FlexCAN_EnhCbtEnable (pBase_14, enhExt_18(D));
  # DEBUG BEGIN_STMT
  if (enhExt_18(D) != 0)
    goto <bb 12>; [33.00%]
  else
    goto <bb 13>; [67.00%]

  <bb 12> [local count: 4385]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetEnhancedNominalTimeSegments (pBase_14, bitrate_13(D));
  goto <bb 16>; [100.00%]

  <bb 13> [local count: 8903]:
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsExCbtEnabled
  # DEBUG BEGIN_STMT
  _32 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].CBT;
  _33 = (signed int) _32;
  # DEBUG pBase => NULL
  if (_33 < 0)
    goto <bb 14>; [41.00%]
  else
    goto <bb 15>; [59.00%]

  <bb 14> [local count: 3650]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetExtendedTimeSegments (pBase_14, bitrate_13(D));
  goto <bb 16>; [100.00%]

  <bb 15> [local count: 5253]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetTimeSegments (pBase_14, bitrate_13(D));

  <bb 16> [local count: 13288]:
  # DEBUG BEGIN_STMT
  SchM_Exit_Can_CAN_EXCLUSIVE_AREA_14 ();

  <bb 17> [local count: 53687]:
  # result_4 = PHI <result_5(10), 0(16), 1(9)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_27 < 0)
    goto <bb 18>; [25.50%]
  else
    goto <bb 20>; [74.50%]

  <bb 18> [local count: 13690]:
  # DEBUG BEGIN_STMT
  status_25 = FlexCAN_Disable (pBase_14);
  # DEBUG status => status_25
  # DEBUG BEGIN_STMT
  if (status_25 != 0)
    goto <bb 19>; [50.00%]
  else
    goto <bb 20>; [50.00%]

  <bb 19> [local count: 6845]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_25

  <bb 20> [local count: 53687]:
  # result_6 = PHI <result_4(17), result_4(18), status_25(19)>
  # DEBUG result => result_6
  # DEBUG BEGIN_STMT
  return result_6;

}


FlexCAN_Ip_SetRxMaskType_Privileged (uint8 instance, Flexcan_Ip_RxMaskType type)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _18;
  signed int _19;
  _Bool x.0_20;
  long unsigned int _21;
  long unsigned int _22;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_8(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_20 ={v} x;
  if (x.0_20 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _2 = (int) instance_8(D);
  pBase_11 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _18 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _19 = (signed int) _18;
  # DEBUG pBase => NULL
  # DEBUG disabled => _19 < 0
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13

  <bb 6> [local count: 107374]:
  # result_3 = PHI <0(4), result_13(5)>
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _22 = _21 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _22 != 0
  # DEBUG BEGIN_STMT
  if (_22 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 53687]:
  if (result_3 == 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 80531]:
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  if (result_3 == 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 10>; [67.00%]

  <bb 9> [local count: 26575]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetRxMaskType (pBase_11, type_14(D));

  <bb 10> [local count: 107374]:
  # result_10 = PHI <result_3(8), 0(9), 1(7)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_19 < 0)
    goto <bb 11>; [25.50%]
  else
    goto <bb 13>; [74.50%]

  <bb 11> [local count: 27380]:
  # DEBUG BEGIN_STMT
  status_17 = FlexCAN_Disable (pBase_11);
  # DEBUG status => status_17
  # DEBUG BEGIN_STMT
  if (status_17 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 13690]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_17

  <bb 13> [local count: 107374]:
  # result_4 = PHI <result_10(10), result_10(11), status_17(12)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_SetStopMode_Privileged (uint8 instance)
{
  volatile boolean x;
  Flexcan_Ip_StatusType status;
  struct FLEXCAN_Type * pBase;
  _Bool _1;
  int _2;
  _Bool x.0_12;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_5(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_12 ={v} x;
  if (x.0_12 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 7> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 8> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = (int) instance_5(D);
  pBase_7 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_7
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  status_9 = FlexCAN_EnterFreezeMode (pBase_7);
  # DEBUG status => status_9
  # DEBUG BEGIN_STMT
  if (status_9 == 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 35433]:
  # DEBUG BEGIN_STMT
  status_11 = FlexCAN_Disable (pBase_7);
  # DEBUG status => status_11

  <bb 6> [local count: 107374]:
  # status_3 = PHI <status_9(4), status_11(5)>
  # DEBUG status => status_3
  # DEBUG BEGIN_STMT
  return status_3;

}


FlexCAN_Ip_SetStartMode_Privileged (uint8 instance)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  _Bool _1;
  int _2;
  long unsigned int _3;
  long unsigned int _4;
  Flexcan_Ip_StatusType _10;
  _Bool x.0_11;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_5(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_11 ={v} x;
  if (x.0_11 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 5> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 6> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = (int) instance_5(D);
  pBase_7 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_7
  # DEBUG BEGIN_STMT
  _3 ={v} pBase_7->MCR;
  _4 = _3 & 2147483647;
  pBase_7->MCR ={v} _4;
  # DEBUG BEGIN_STMT
  _10 = FlexCAN_ExitFreezeMode (pBase_7);
  return _10;

}


FlexCAN_Ip_GetStartMode_Privileged (uint8 instance)
{
  const struct FLEXCAN_Type * base;
  int _1;
  long unsigned int _2;
  long unsigned int _3;
  boolean _7;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_4(D);
  base_6 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_6
  # DEBUG BEGIN_STMT
  _2 ={v} base_6->MCR;
  _3 = _2 & 17825792;
  _7 = _3 == 0;
  return _7;

}


FlexCAN_Ip_GetStopMode_Privileged (uint8 instance)
{
  const struct FLEXCAN_Type * base;
  int _1;
  long unsigned int _2;
  long unsigned int _3;
  boolean _7;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_4(D);
  base_6 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_6
  # DEBUG BEGIN_STMT
  _2 ={v} base_6->MCR;
  _3 = _2 & 1048576;
  _7 = _3 != 0;
  return _7;

}


FlexCAN_Ip_MainFunctionWrite (uint8 instance, uint8 mb_idx)
{
  volatile boolean x;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  long unsigned int _3;
  unsigned char _4;
  int _5;
  long unsigned int _6;
  _Bool x.0_18;
  long unsigned int vol.5_19;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_8(D);
  base_10 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_10
  # DEBUG BEGIN_STMT
  state_11 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_11
  # DEBUG BEGIN_STMT
  _2 = instance_8(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_18 ={v} x;
  if (x.0_18 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 7> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 8> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = (long unsigned int) mb_idx_12(D);
  _4 = FlexCAN_GetBuffStatusFlag (base_10, _3);
  if (_4 != 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 35433]:
  # DEBUG BEGIN_STMT
  _5 = (int) mb_idx_12(D);
  _6 = FlexCAN_GetMsgBuffTimestamp (base_10, _3);
  state_11->mbs[_5].time_stamp = _6;
  # DEBUG BEGIN_STMT
  # DEBUG base => base_10
  # DEBUG INLINE_ENTRY FlexCAN_UnlockRxMsgBuff
  # DEBUG BEGIN_STMT
  vol.5_19 ={v} MEM[(const struct FLEXCAN_Type *)base_10].TIMER;
  # DEBUG base => NULL
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_10, _3);
  # DEBUG BEGIN_STMT
  state_11->mbs[_5].state ={v} 0;

  <bb 6> [local count: 107374]:
  return;

}


FlexCAN_Ip_MainFunctionBusOff_Privileged (uint8 instance)
{
  volatile boolean x;
  uint32 u32ErrStatus;
  const struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  Flexcan_Ip_StatusType eRetVal;
  int _1;
  _Bool _2;
  long unsigned int _3;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _4;
  _Bool x.0_15;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG eRetVal => 1
  # DEBUG BEGIN_STMT
  _1 = (int) instance_8(D);
  base_10 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_10
  # DEBUG BEGIN_STMT
  state_11 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_11
  # DEBUG BEGIN_STMT
  # DEBUG u32ErrStatus => 0
  # DEBUG BEGIN_STMT
  _2 = instance_8(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_15 ={v} x;
  if (x.0_15 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 9> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 10> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  u32ErrStatus_12 ={v} base_10->ESR1;
  # DEBUG u32ErrStatus => u32ErrStatus_12
  # DEBUG BEGIN_STMT
  _3 = u32ErrStatus_12 & 4;
  if (_3 != 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 5> [local count: 53687]:
  # DEBUG BEGIN_STMT
  _4 = state_11->error_callback;
  if (_4 != 0B)
    goto <bb 6>; [70.00%]
  else
    goto <bb 7>; [30.00%]

  <bb 6> [local count: 37581]:
  # DEBUG BEGIN_STMT
  _4 (instance_8(D), 11, u32ErrStatus_12, state_11);

  <bb 7> [local count: 53687]:
  # DEBUG BEGIN_STMT
  base_10->ESR1 ={v} 4;
  # DEBUG BEGIN_STMT
  # DEBUG eRetVal => 0

  <bb 8> [local count: 107374]:
  # eRetVal_5 = PHI <1(4), 0(7)>
  # DEBUG eRetVal => eRetVal_5
  # DEBUG BEGIN_STMT
  return eRetVal_5;

}


FlexCAN_Ip_MainFunctionRead (uint8 instance, uint8 mb_idx)
{
  uint32 flag;
  volatile boolean x;
  volatile boolean x;
  const struct Flexcan_Ip_StateType * state;
  const struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  unsigned char _3;
  _Bool _4;
  _Bool _5;
  _Bool _6;
  long unsigned int _7;
  unsigned char _8;
  int _9;
  <unnamed type> _10;
  _Bool x.0_22;
  _Bool x.0_23;
  long unsigned int _24;
  signed int _25;
  long unsigned int _26;
  long unsigned int _27;
  unsigned char _28;
  long unsigned int _29;
  long unsigned int _31;
  long unsigned int _32;
  unsigned char _33;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_12(D);
  base_14 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_14
  # DEBUG BEGIN_STMT
  state_15 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_15
  # DEBUG BEGIN_STMT
  _2 = instance_12(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_23 ={v} x;
  if (x.0_23 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 21>; [50.00%]

  <bb 21> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 23> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = mb_idx_16(D) + 160;
  _4 = _3 > 158;
  x ={v} _4;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_22 ={v} x;
  if (x.0_22 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 20>; [50.00%]

  <bb 20> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 22> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  if (mb_idx_16(D) == 255)
    goto <bb 7>; [20.24%]
  else
    goto <bb 11>; [79.76%]

  <bb 7> [local count: 10866]:
  # DEBUG BEGIN_STMT
  _5 = FlexCAN_IsEnhancedRxFifoAvailable (base_14);
  if (_5 != 0)
    goto <bb 8>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 8> [local count: 5433]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_14
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhancedRxFifoEnabled
  # DEBUG BEGIN_STMT
  _24 ={v} base_14->ERFCR;
  _25 = (signed int) _24;
  # DEBUG base => NULL
  if (_25 < 0)
    goto <bb 9>; [41.00%]
  else
    goto <bb 19>; [59.00%]

  <bb 9> [local count: 2228]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_14
  # DEBUG intFlag => 28
  # DEBUG INLINE_ENTRY FlexCAN_GetEnhancedRxFIFOStatusFlag
  # DEBUG BEGIN_STMT
  _26 ={v} base_14->ERFSR;
  _31 = _26 >> 28;
  _27 = _31 & 1;
  _28 = (unsigned char) _27;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  if (_28 != 0)
    goto <bb 10>; [33.00%]
  else
    goto <bb 19>; [67.00%]

  <bb 10> [local count: 735]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerEnhancedRxFIFO (instance_12(D), 28);
  goto <bb 19>; [100.00%]

  <bb 11> [local count: 42821]:
  # DEBUG BEGIN_STMT
  _6 = state_15->bIsLegacyFifoEn;
  if (_6 != 0)
    goto <bb 12>; [67.00%]
  else
    goto <bb 16>; [33.00%]

  <bb 12> [local count: 28690]:
  if (mb_idx_16(D) <= 7)
    goto <bb 13>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 13> [local count: 14345]:
  # DEBUG BEGIN_STMT
  if (mb_idx_16(D) == 0)
    goto <bb 14>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 14> [local count: 7172]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_14
  # DEBUG msgBuffIdx => 5
  # DEBUG INLINE_ENTRY FlexCAN_GetBuffStatusFlag
  # DEBUG BEGIN_STMT
  # DEBUG flag => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _29 ={v} base_14->IFLAG1;
  _32 = _29 >> 5;
  flag_30 = _32 & 1;
  # DEBUG flag => flag_30
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _33 = (unsigned char) flag_30;
  # DEBUG base => NULL
  # DEBUG msgBuffIdx => NULL
  # DEBUG flag => NULL
  if (_33 != 0)
    goto <bb 15>; [33.00%]
  else
    goto <bb 19>; [67.00%]

  <bb 15> [local count: 2367]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerRxFIFO (instance_12(D), 5);
  goto <bb 19>; [100.00%]

  <bb 16> [local count: 28476]:
  # DEBUG BEGIN_STMT
  _7 = (long unsigned int) mb_idx_16(D);
  _8 = FlexCAN_GetBuffStatusFlag (base_14, _7);
  if (_8 != 0)
    goto <bb 17>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 17> [local count: 14238]:
  # DEBUG BEGIN_STMT
  _9 = (int) mb_idx_16(D);
  _10 ={v} state_15->mbs[_9].state;
  if (_10 == 1)
    goto <bb 18>; [20.24%]
  else
    goto <bb 19>; [79.76%]

  <bb 18> [local count: 2882]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerRxMB (instance_12(D), _7);

  <bb 19> [local count: 53687]:
  return;

}


FlexCAN_Ip_Deinit_Privileged (uint8 instance)
{
  volatile boolean x;
  Flexcan_Ip_StatusType result;
  struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  _Bool x.0_12;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_4(D);
  base_6 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_6
  # DEBUG BEGIN_STMT
  # DEBUG result => 1
  # DEBUG BEGIN_STMT
  _2 = instance_4(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_12 ={v} x;
  if (x.0_12 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 7> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 8> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  result_8 = FlexCAN_EnterFreezeMode (base_6);
  # DEBUG result => result_8
  # DEBUG BEGIN_STMT
  if (result_8 == 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 35433]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetRegDefaultVal (base_6);
  # DEBUG BEGIN_STMT
  FlexCAN_Disable (base_6);
  # DEBUG BEGIN_STMT
  g_flexcan_Ip_StatePtr[_1] = 0B;

  <bb 6> [local count: 107374]:
  # DEBUG BEGIN_STMT
  return result_8;

}


FlexCAN_Ip_SetRxFifoGlobalMask_Privileged (uint8 instance, uint32 mask)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _17;
  signed int _18;
  _Bool x.0_19;
  long unsigned int _20;
  long unsigned int _21;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_8(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_19 ={v} x;
  if (x.0_19 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _2 = (int) instance_8(D);
  pBase_11 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _18 = (signed int) _17;
  # DEBUG pBase => NULL
  # DEBUG disabled => _18 < 0
  # DEBUG BEGIN_STMT
  if (_18 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13

  <bb 6> [local count: 107374]:
  # result_3 = PHI <0(4), result_13(5)>
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _20 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _21 = _20 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _21 != 0
  # DEBUG BEGIN_STMT
  if (_21 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 53687]:
  if (result_3 == 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 80531]:
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  if (result_3 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 40265]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG Mask => mask_14(D)
  # DEBUG INLINE_ENTRY FlexCAN_SetRxFifoGlobalMask
  # DEBUG BEGIN_STMT
  pBase_11->RXFGMASK ={v} mask_14(D);

  <bb 10> [local count: 107374]:
  # result_10 = PHI <result_3(8), 0(9), 1(7)>
  # DEBUG result => NULL
  # DEBUG base => NULL
  # DEBUG Mask => NULL
  # DEBUG BEGIN_STMT
  if (_18 < 0)
    goto <bb 11>; [25.50%]
  else
    goto <bb 13>; [74.50%]

  <bb 11> [local count: 27380]:
  # DEBUG BEGIN_STMT
  status_16 = FlexCAN_Disable (pBase_11);
  # DEBUG status => status_16
  # DEBUG BEGIN_STMT
  if (status_16 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 13690]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_16

  <bb 13> [local count: 107374]:
  # result_4 = PHI <result_10(10), result_10(11), status_16(12)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_SetRxIndividualMask_Privileged (uint8 instance, uint8 mb_idx, uint32 mask)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  int _1;
  _Bool _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  _Bool x.0_21;
  long unsigned int _22;
  signed int _23;
  long unsigned int _24;
  long unsigned int _25;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _1 = (int) instance_12(D);
  pBase_14 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_14
  # DEBUG BEGIN_STMT
  # DEBUG freeze => 0
  # DEBUG BEGIN_STMT
  _2 = instance_12(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_21 ={v} x;
  if (x.0_21 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 16>; [50.00%]

  <bb 16> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 17> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = (long unsigned int) mb_idx_15(D);
  _4 ={v} pBase_14->MCR;
  _5 = _4 & 127;
  if (_3 > _5)
    goto <bb 15>; [35.00%]
  else
    goto <bb 5>; [65.00%]

  <bb 5> [local count: 69793]:
  if (mb_idx_15(D) > 95)
    goto <bb 15>; [35.00%]
  else
    goto <bb 6>; [65.00%]

  <bb 6> [local count: 45366]:
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _22 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].MCR;
  _23 = (signed int) _22;
  # DEBUG pBase => NULL
  # DEBUG disabled => _23 < 0
  # DEBUG BEGIN_STMT
  if (_23 < 0)
    goto <bb 7>; [25.50%]
  else
    goto <bb 8>; [74.50%]

  <bb 7> [local count: 11568]:
  # DEBUG BEGIN_STMT
  result_17 = FlexCAN_Enable (pBase_14);
  # DEBUG result => result_17

  <bb 8> [local count: 45366]:
  # result_6 = PHI <0(6), result_17(7)>
  # DEBUG result => result_6
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_14
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _24 ={v} MEM[(const struct FLEXCAN_Type *)pBase_14].MCR;
  _25 = _24 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _25 != 0
  # DEBUG BEGIN_STMT
  if (_25 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 22683]:
  if (result_6 == 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 10> [local count: 34024]:
  # DEBUG result => result_6
  # DEBUG BEGIN_STMT
  if (result_6 == 0)
    goto <bb 11>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 11> [local count: 17012]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_14
  # DEBUG msgBuffIdx => _3
  # DEBUG mask => mask_18(D)
  # DEBUG INLINE_ENTRY FlexCAN_SetRxIndividualMask
  # DEBUG BEGIN_STMT
  pBase_14->RXIMR[_3] ={v} mask_18(D);

  <bb 12> [local count: 45366]:
  # result_11 = PHI <result_6(10), 0(11), 1(9)>
  # DEBUG result => NULL
  # DEBUG base => NULL
  # DEBUG msgBuffIdx => NULL
  # DEBUG mask => NULL
  # DEBUG BEGIN_STMT
  if (_23 < 0)
    goto <bb 13>; [25.50%]
  else
    goto <bb 15>; [74.50%]

  <bb 13> [local count: 11568]:
  # DEBUG BEGIN_STMT
  status_20 = FlexCAN_Disable (pBase_14);
  # DEBUG status => status_20
  # DEBUG BEGIN_STMT
  if (status_20 != 0)
    goto <bb 14>; [50.00%]
  else
    goto <bb 15>; [50.00%]

  <bb 14> [local count: 5784]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_20

  <bb 15> [local count: 107374]:
  # result_7 = PHI <4(5), result_11(12), result_11(13), status_20(14), 4(4)>
  # DEBUG result => result_7
  # DEBUG BEGIN_STMT
  return result_7;

}


FlexCAN_Ip_ExitFreezeMode_Privileged (uint8 instance)
{
  struct FLEXCAN_Type * base;
  int _1;
  Flexcan_Ip_StatusType _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_2(D);
  base_4 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_4
  # DEBUG BEGIN_STMT
  _6 = FlexCAN_ExitFreezeMode (base_4);
  return _6;

}


FlexCAN_Ip_EnterFreezeMode_Privileged (uint8 instance)
{
  struct FLEXCAN_Type * base;
  int _1;
  Flexcan_Ip_StatusType _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_2(D);
  base_4 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_4
  # DEBUG BEGIN_STMT
  _6 = FlexCAN_EnterFreezeMode (base_4);
  return _6;

}


FlexCAN_Ip_SetRxMbGlobalMask_Privileged (uint8 instance, uint32 mask)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  int _1;
  _Bool _2;
  long unsigned int _17;
  signed int _18;
  _Bool x.0_19;
  long unsigned int _20;
  long unsigned int _21;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _1 = (int) instance_9(D);
  pBase_11 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG freeze => 0
  # DEBUG BEGIN_STMT
  _2 = instance_9(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_19 ={v} x;
  if (x.0_19 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _17 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _18 = (signed int) _17;
  # DEBUG pBase => NULL
  # DEBUG disabled => _18 < 0
  # DEBUG BEGIN_STMT
  if (_18 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13

  <bb 6> [local count: 107374]:
  # result_3 = PHI <0(4), result_13(5)>
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _20 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _21 = _20 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _21 != 0
  # DEBUG BEGIN_STMT
  if (_21 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 53687]:
  if (result_3 == 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 80531]:
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  if (result_3 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 40265]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG Mask => mask_14(D)
  # DEBUG INLINE_ENTRY FlexCAN_SetRxMsgBuffGlobalMask
  # DEBUG BEGIN_STMT
  pBase_11->RXMGMASK ={v} mask_14(D);

  <bb 10> [local count: 107374]:
  # result_8 = PHI <result_3(8), 0(9), 1(7)>
  # DEBUG result => NULL
  # DEBUG base => NULL
  # DEBUG Mask => NULL
  # DEBUG BEGIN_STMT
  if (_18 < 0)
    goto <bb 11>; [25.50%]
  else
    goto <bb 13>; [74.50%]

  <bb 11> [local count: 27380]:
  # DEBUG BEGIN_STMT
  status_16 = FlexCAN_Disable (pBase_11);
  # DEBUG status => status_16
  # DEBUG BEGIN_STMT
  if (status_16 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 13690]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_16

  <bb 13> [local count: 107374]:
  # result_4 = PHI <result_8(10), result_8(11), status_16(12)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_SendBlocking (uint8 instance, uint8 mb_idx, const struct Flexcan_Ip_DataInfoType * tx_info, uint32 msg_id, const uint8 * mb_data, uint32 timeout_ms)
{
  volatile boolean x;
  volatile boolean x;
  volatile uint32 * flexcan_mb;
  uint32 flexcan_mb_config;
  uint32 uS2Ticks;
  uint32 mS2Ticks;
  uint32 timeElapsed;
  uint32 timeStart;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  Flexcan_Ip_StatusType result;
  int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  _Bool _5;
  _Bool _6;
  long unsigned int _7;
  unsigned char _8;
  int _9;
  <unnamed type> _10;
  long unsigned int _11;
  unsigned char _12;
  long unsigned int _13;
  long unsigned int _14;
  int _15;
  long unsigned int _45;
  long unsigned int _60;
  _Bool x.0_66;
  _Bool x.0_67;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = (int) instance_28(D);
  base_30 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_30
  # DEBUG BEGIN_STMT
  state_31 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_31
  # DEBUG BEGIN_STMT
  _3 = OsIf_GetCounter (0);
  timeStart = _3;
  # DEBUG BEGIN_STMT
  # DEBUG timeElapsed => 0
  # DEBUG BEGIN_STMT
  _4 = timeout_ms_34(D) * 1000;
  mS2Ticks_36 = OsIf_MicrosToTicks (_4, 0);
  # DEBUG mS2Ticks => mS2Ticks_36
  # DEBUG BEGIN_STMT
  # DEBUG uS2Ticks => 0
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb_config => 0
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb => 0B
  # DEBUG BEGIN_STMT
  _5 = instance_28(D) <= 5;
  x ={v} _5;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_67 ={v} x;
  if (x.0_67 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 22>; [50.00%]

  <bb 22> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 26> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _6 = tx_info_37(D) != 0B;
  x ={v} _6;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_66 ={v} x;
  if (x.0_66 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 21>; [50.00%]

  <bb 21> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 25> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  result_42 = FlexCAN_StartSendData (instance_28(D), mb_idx_38(D), tx_info_37(D), msg_id_39(D), mb_data_40(D));
  # DEBUG result => result_42
  # DEBUG BEGIN_STMT
  if (result_42 == 0)
    goto <bb 20>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 20> [local count: 26844]:
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 237131]:
  # DEBUG BEGIN_STMT
  _45 = OsIf_GetElapsed (&timeStart, 0);
  timeElapsed_46 = timeElapsed_20 + _45;
  # DEBUG timeElapsed => timeElapsed_46
  # DEBUG BEGIN_STMT
  if (mS2Ticks_36 <= timeElapsed_46)
    goto <bb 9>; [5.50%]
  else
    goto <bb 24>; [94.50%]

  <bb 24> [local count: 224089]:

  <bb 8> [local count: 250932]:
  # timeElapsed_20 = PHI <0(20), timeElapsed_46(24)>
  # DEBUG timeElapsed => timeElapsed_20
  # DEBUG BEGIN_STMT
  _7 = (long unsigned int) mb_idx_38(D);
  _8 = FlexCAN_GetBuffStatusFlag (base_30, _7);
  if (_8 != 1)
    goto <bb 7>; [94.50%]
  else
    goto <bb 9>; [5.50%]

  <bb 9> [local count: 26843]:
  # result_16 = PHI <3(7), 0(8)>
  # _2 = PHI <_7(7), _7(8)>
  # DEBUG result => result_16
  # DEBUG BEGIN_STMT
  if (result_16 == 3)
    goto <bb 10>; [34.00%]
  else
    goto <bb 18>; [66.00%]

  <bb 10> [local count: 9127]:
  _9 = (int) mb_idx_38(D);
  _10 ={v} state_31->mbs[_9].state;
  if (_10 != 0)
    goto <bb 11>; [33.00%]
  else
    goto <bb 18>; [67.00%]

  <bb 11> [local count: 3012]:
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_30, _2);
  # DEBUG BEGIN_STMT
  flexcan_mb_49 = FlexCAN_GetMsgBuffRegion (base_30, _2);
  # DEBUG flexcan_mb => flexcan_mb_49
  # DEBUG BEGIN_STMT
  flexcan_mb_config_50 ={v} *flexcan_mb_49;
  # DEBUG flexcan_mb_config => flexcan_mb_config_50
  # DEBUG BEGIN_STMT
  flexcan_mb_config_51 = flexcan_mb_config_50 & 4043309055;
  # DEBUG flexcan_mb_config => flexcan_mb_config_51
  # DEBUG BEGIN_STMT
  flexcan_mb_config_52 = flexcan_mb_config_51 | 150994944;
  # DEBUG flexcan_mb_config => flexcan_mb_config_52
  # DEBUG BEGIN_STMT
  *flexcan_mb_49 ={v} flexcan_mb_config_52;
  # DEBUG BEGIN_STMT
  uS2Ticks_55 = OsIf_MicrosToTicks (100, 0);
  # DEBUG uS2Ticks => uS2Ticks_55
  # DEBUG BEGIN_STMT
  _11 = OsIf_GetCounter (0);
  timeStart = _11;
  # DEBUG BEGIN_STMT
  # DEBUG timeElapsed => 0
  # DEBUG BEGIN_STMT
  goto <bb 13>; [100.00%]

  <bb 12> [local count: 26606]:
  # DEBUG BEGIN_STMT
  _60 = OsIf_GetElapsed (&timeStart, 0);
  timeElapsed_61 = timeElapsed_21 + _60;
  # DEBUG timeElapsed => timeElapsed_61
  # DEBUG BEGIN_STMT
  if (uS2Ticks_55 <= timeElapsed_61)
    goto <bb 14>; [5.50%]
  else
    goto <bb 23>; [94.50%]

  <bb 23> [local count: 25143]:

  <bb 13> [local count: 28155]:
  # timeElapsed_21 = PHI <0(11), timeElapsed_61(23)>
  # DEBUG timeElapsed => timeElapsed_21
  # DEBUG BEGIN_STMT
  _12 = FlexCAN_GetBuffStatusFlag (base_30, _2);
  if (_12 == 0)
    goto <bb 12>; [94.50%]
  else
    goto <bb 14>; [5.50%]

  <bb 14> [local count: 3012]:
  # DEBUG result => 3
  # DEBUG BEGIN_STMT
  flexcan_mb_config_62 ={v} *flexcan_mb_49;
  # DEBUG flexcan_mb_config => flexcan_mb_config_62
  # DEBUG BEGIN_STMT
  _13 = flexcan_mb_config_62 >> 24;
  _14 = _13 & 15;
  if (_14 == 8)
    goto <bb 15>; [34.00%]
  else
    goto <bb 16>; [66.00%]

  <bb 15> [local count: 1024]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0

  <bb 16> [local count: 3012]:
  # result_17 = PHI <3(14), 0(15)>
  # DEBUG result => result_17
  # DEBUG BEGIN_STMT
  if (_14 == 9)
    goto <bb 17>; [34.00%]
  else
    goto <bb 18>; [66.00%]

  <bb 17> [local count: 1024]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 3

  <bb 18> [local count: 26843]:
  # result_18 = PHI <result_16(9), 3(10), result_17(16), 3(17)>
  # DEBUG result => result_18
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_30, _2);
  # DEBUG BEGIN_STMT
  _15 = (int) mb_idx_38(D);
  state_31->mbs[_15].state ={v} 0;

  <bb 19> [local count: 53687]:
  # result_19 = PHI <result_42(6), result_18(18)>
  # DEBUG result => result_19
  # DEBUG BEGIN_STMT
  timeStart ={v} {CLOBBER};
  return result_19;

}


FlexCAN_Busoff_Error_IRQHandler (uint8 instance)
{
  volatile boolean x;
  boolean isSpuriousInt;
  uint32 u32ErrStatus;
  const struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * pBase;
  int _1;
  _Bool _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _6;
  long unsigned int _7;
  long unsigned int _8;
  signed int _9;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _14;
  long unsigned int _15;
  long unsigned int _16;
  long unsigned int _17;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _18;
  long unsigned int _19;
  long unsigned int _20;
  long unsigned int _21;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _22;
  _Bool x.0_57;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_36(D);
  pBase_38 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_38
  # DEBUG BEGIN_STMT
  state_39 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_39
  # DEBUG BEGIN_STMT
  # DEBUG u32ErrStatus => 0
  # DEBUG BEGIN_STMT
  # DEBUG isSpuriousInt => 1
  # DEBUG BEGIN_STMT
  _2 = instance_36(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_57 ={v} x;
  if (x.0_57 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 28>; [50.00%]

  <bb 28> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 29> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  if (state_39 != 0B)
    goto <bb 5>; [70.00%]
  else
    goto <bb 26>; [30.00%]

  <bb 5> [local count: 75162]:
  # DEBUG BEGIN_STMT
  u32ErrStatus_40 ={v} pBase_38->ESR1;
  # DEBUG u32ErrStatus => u32ErrStatus_40
  # DEBUG BEGIN_STMT
  _3 = u32ErrStatus_40 & 2;
  if (_3 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 6> [local count: 37581]:
  _4 ={v} pBase_38->CTRL1;
  _5 = _4 & 16384;
  if (_5 != 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 7> [local count: 18790]:
  # DEBUG BEGIN_STMT
  pBase_38->ESR1 ={v} 2;
  # DEBUG BEGIN_STMT
  _6 = state_39->error_callback;
  if (_6 != 0B)
    goto <bb 8>; [70.00%]
  else
    goto <bb 9>; [30.00%]

  <bb 8> [local count: 13153]:
  # DEBUG BEGIN_STMT
  _6 (instance_36(D), 9, u32ErrStatus_40, state_39);
  # DEBUG BEGIN_STMT
  u32ErrStatus_43 ={v} pBase_38->ESR1;
  # DEBUG u32ErrStatus => u32ErrStatus_43

  <bb 9> [local count: 75162]:
  # u32ErrStatus_23 = PHI <u32ErrStatus_40(5), u32ErrStatus_40(6), u32ErrStatus_43(8), u32ErrStatus_40(7)>
  # isSpuriousInt_27 = PHI <1(5), 1(6), 0(8), 0(7)>
  # DEBUG isSpuriousInt => isSpuriousInt_27
  # DEBUG u32ErrStatus => u32ErrStatus_23
  # DEBUG BEGIN_STMT
  _7 = u32ErrStatus_23 & 1048576;
  if (_7 != 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 10> [local count: 37581]:
  _8 ={v} pBase_38->CTRL2;
  _9 = (signed int) _8;
  if (_9 < 0)
    goto <bb 11>; [41.00%]
  else
    goto <bb 13>; [59.00%]

  <bb 11> [local count: 15408]:
  # DEBUG BEGIN_STMT
  pBase_38->ESR1 ={v} 1048576;
  # DEBUG BEGIN_STMT
  _10 = state_39->error_callback;
  if (_10 != 0B)
    goto <bb 12>; [70.00%]
  else
    goto <bb 13>; [30.00%]

  <bb 12> [local count: 10786]:
  # DEBUG BEGIN_STMT
  _10 (instance_36(D), 10, u32ErrStatus_23, state_39);
  # DEBUG BEGIN_STMT
  u32ErrStatus_46 ={v} pBase_38->ESR1;
  # DEBUG u32ErrStatus => u32ErrStatus_46

  <bb 13> [local count: 75162]:
  # u32ErrStatus_24 = PHI <u32ErrStatus_23(9), u32ErrStatus_23(10), u32ErrStatus_46(12), u32ErrStatus_23(11)>
  # isSpuriousInt_28 = PHI <isSpuriousInt_27(9), isSpuriousInt_27(10), 0(12), 0(11)>
  # DEBUG isSpuriousInt => isSpuriousInt_28
  # DEBUG u32ErrStatus => u32ErrStatus_24
  # DEBUG BEGIN_STMT
  _11 = u32ErrStatus_24 & 131072;
  if (_11 != 0)
    goto <bb 14>; [50.00%]
  else
    goto <bb 17>; [50.00%]

  <bb 14> [local count: 37581]:
  _12 ={v} pBase_38->CTRL1;
  _13 = _12 & 2048;
  if (_13 != 0)
    goto <bb 15>; [50.00%]
  else
    goto <bb 17>; [50.00%]

  <bb 15> [local count: 18790]:
  # DEBUG BEGIN_STMT
  pBase_38->ESR1 ={v} 131072;
  # DEBUG BEGIN_STMT
  _14 = state_39->error_callback;
  if (_14 != 0B)
    goto <bb 16>; [70.00%]
  else
    goto <bb 17>; [30.00%]

  <bb 16> [local count: 13153]:
  # DEBUG BEGIN_STMT
  _14 (instance_36(D), 13, u32ErrStatus_24, state_39);
  # DEBUG BEGIN_STMT
  u32ErrStatus_49 ={v} pBase_38->ESR1;
  # DEBUG u32ErrStatus => u32ErrStatus_49

  <bb 17> [local count: 75162]:
  # u32ErrStatus_25 = PHI <u32ErrStatus_24(13), u32ErrStatus_24(14), u32ErrStatus_49(16), u32ErrStatus_24(15)>
  # isSpuriousInt_29 = PHI <isSpuriousInt_28(13), isSpuriousInt_28(14), 0(16), 0(15)>
  # DEBUG isSpuriousInt => isSpuriousInt_29
  # DEBUG u32ErrStatus => u32ErrStatus_25
  # DEBUG BEGIN_STMT
  _15 = u32ErrStatus_25 & 65536;
  if (_15 != 0)
    goto <bb 18>; [50.00%]
  else
    goto <bb 21>; [50.00%]

  <bb 18> [local count: 37581]:
  _16 ={v} pBase_38->CTRL1;
  _17 = _16 & 1024;
  if (_17 != 0)
    goto <bb 19>; [50.00%]
  else
    goto <bb 21>; [50.00%]

  <bb 19> [local count: 18790]:
  # DEBUG BEGIN_STMT
  pBase_38->ESR1 ={v} 65536;
  # DEBUG BEGIN_STMT
  _18 = state_39->error_callback;
  if (_18 != 0B)
    goto <bb 20>; [70.00%]
  else
    goto <bb 21>; [30.00%]

  <bb 20> [local count: 13153]:
  # DEBUG BEGIN_STMT
  _18 (instance_36(D), 12, u32ErrStatus_25, state_39);
  # DEBUG BEGIN_STMT
  u32ErrStatus_53 ={v} pBase_38->ESR1;
  # DEBUG u32ErrStatus => u32ErrStatus_53

  <bb 21> [local count: 75162]:
  # u32ErrStatus_26 = PHI <u32ErrStatus_25(17), u32ErrStatus_25(18), u32ErrStatus_53(20), u32ErrStatus_25(19)>
  # isSpuriousInt_30 = PHI <isSpuriousInt_29(17), isSpuriousInt_29(18), 0(20), 0(19)>
  # DEBUG isSpuriousInt => isSpuriousInt_30
  # DEBUG u32ErrStatus => u32ErrStatus_26
  # DEBUG BEGIN_STMT
  _19 = u32ErrStatus_26 & 4;
  if (_19 != 0)
    goto <bb 22>; [50.00%]
  else
    goto <bb 25>; [50.00%]

  <bb 22> [local count: 37581]:
  _20 ={v} pBase_38->CTRL1;
  _21 = _20 & 32768;
  if (_21 != 0)
    goto <bb 23>; [50.00%]
  else
    goto <bb 25>; [50.00%]

  <bb 23> [local count: 18790]:
  # DEBUG BEGIN_STMT
  pBase_38->ESR1 ={v} 4;
  # DEBUG BEGIN_STMT
  _22 = state_39->error_callback;
  if (_22 != 0B)
    goto <bb 24>; [70.00%]
  else
    goto <bb 27>; [30.00%]

  <bb 24> [local count: 13153]:
  # DEBUG BEGIN_STMT
  _22 (instance_36(D), 11, u32ErrStatus_26, state_39);
  goto <bb 27>; [100.00%]

  <bb 25> [local count: 56371]:
  # DEBUG isSpuriousInt => isSpuriousInt_30
  # DEBUG BEGIN_STMT
  if (isSpuriousInt_30 != 0)
    goto <bb 26>; [50.00%]
  else
    goto <bb 27>; [50.00%]

  <bb 26> [local count: 60398]:
  # DEBUG isSpuriousInt => NULL
  # DEBUG BEGIN_STMT
  pBase_38->ESR1 ={v} 3866630;

  <bb 27> [local count: 107374]:
  # DEBUG isSpuriousInt => NULL
  return;

}


FlexCAN_Ip_GetControllerRxErrorCounter (uint8 instance)
{
  volatile boolean x;
  const struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  long unsigned int _3;
  long unsigned int _4;
  uint8 _8;
  _Bool x.0_9;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_5(D);
  base_7 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_7
  # DEBUG BEGIN_STMT
  _2 = instance_5(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_9 ={v} x;
  if (x.0_9 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 5> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 6> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 ={v} base_7->ECR;
  _4 = _3 >> 8;
  _8 = (uint8) _4;
  return _8;

}


FlexCAN_Ip_GetControllerTxErrorCounter (uint8 instance)
{
  volatile boolean x;
  const struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  long unsigned int _3;
  uint8 _7;
  _Bool x.0_8;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_4(D);
  base_6 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_6
  # DEBUG BEGIN_STMT
  _2 = instance_4(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_8 ={v} x;
  if (x.0_8 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 5> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 6> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 ={v} base_6->ECR;
  _7 = (uint8) _3;
  return _7;

}


FlexCAN_Ip_GetErrorStatus (uint8 instance)
{
  volatile boolean x;
  const struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  uint32 _6;
  _Bool x.0_7;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_3(D);
  base_5 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_5
  # DEBUG BEGIN_STMT
  _2 = instance_3(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_7 ={v} x;
  if (x.0_7 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 5> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 6> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _6 ={v} base_5->ESR1;
  return _6;

}


FlexCAN_Ip_ClearErrorStatus (uint8 instance, uint32 error)
{
  volatile boolean x;
  struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  _Bool x.0_8;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_3(D);
  base_5 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_5
  # DEBUG BEGIN_STMT
  _2 = instance_3(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_8 ={v} x;
  if (x.0_8 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 5> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 6> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  base_5->ESR1 ={v} error_6(D);
  return;

}


FlexCAN_IRQHandler (uint8 instance, uint32 startMbIdx, uint32 endMbIdx, boolean bEnhancedFifoExisted)
{
  volatile boolean x;
  volatile boolean x;
  uint32 mb_idx;
  boolean bIsSpuriousInt;
  const struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  uint32 flag_reg;
  uint32 u32MbHandle;
  int _1;
  _Bool _3;
  _Bool _4;
  unsigned char _5;
  unsigned char _6;
  _Bool _7;
  <unnamed type> _8;
  <unnamed type> _9;
  unsigned char _10;
  <unnamed type> _11;
  <unnamed type> _12;
  _Bool x.0_49;
  _Bool x.0_50;
  long unsigned int _51;
  signed int _52;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG u32MbHandle => 0
  # DEBUG BEGIN_STMT
  # DEBUG flag_reg => 0
  # DEBUG BEGIN_STMT
  _1 = (int) instance_26(D);
  base_28 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_28
  # DEBUG BEGIN_STMT
  state_29 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_29
  # DEBUG BEGIN_STMT
  # DEBUG bIsSpuriousInt => 1
  # DEBUG BEGIN_STMT
  # DEBUG mb_idx => endMbIdx_30(D)
  # DEBUG BEGIN_STMT
  _3 = instance_26(D) <= 5;
  x ={v} _3;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_50 ={v} x;
  if (x.0_50 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 35>; [50.00%]

  <bb 35> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 37> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _4 = endMbIdx_30(D) <= 95;
  x ={v} _4;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_49 ={v} x;
  if (x.0_49 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 34>; [50.00%]

  <bb 34> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 36> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  if (state_29 != 0B)
    goto <bb 7>; [53.47%]
  else
    goto <bb 33>; [46.53%]

  <bb 33> [local count: 24981]:
  goto <bb 29>; [100.00%]

  <bb 7> [local count: 28706]:
  # DEBUG BEGIN_STMT
  _5 = FlexCAN_GetMsgBuffIntStatusFlag (base_28, endMbIdx_30(D));
  flag_reg_36 = (uint32) _5;
  # DEBUG flag_reg => flag_reg_36
  # DEBUG BEGIN_STMT
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 239641]:
  # DEBUG BEGIN_STMT
  mb_idx_37 = mb_idx_17 + 4294967295;
  # DEBUG mb_idx => mb_idx_37
  # DEBUG BEGIN_STMT
  _6 = FlexCAN_GetMsgBuffIntStatusFlag (base_28, mb_idx_37);
  flag_reg_39 = (uint32) _6;
  # DEBUG flag_reg => flag_reg_39

  <bb 9> [local count: 268347]:
  # flag_reg_14 = PHI <flag_reg_36(7), flag_reg_39(8)>
  # mb_idx_17 = PHI <endMbIdx_30(D)(7), mb_idx_37(8)>
  # DEBUG mb_idx => mb_idx_17
  # DEBUG flag_reg => flag_reg_14
  # DEBUG BEGIN_STMT
  if (flag_reg_14 == 0)
    goto <bb 10>; [94.50%]
  else
    goto <bb 11>; [5.50%]

  <bb 10> [local count: 253588]:
  if (mb_idx_17 > startMbIdx_31(D))
    goto <bb 8>; [94.50%]
  else
    goto <bb 11>; [5.50%]

  <bb 11> [local count: 28706]:
  # flag_reg_2 = PHI <flag_reg_14(9), 0(10)>
  # mb_idx_40 = PHI <mb_idx_17(9), mb_idx_17(10)>
  # DEBUG BEGIN_STMT
  if (flag_reg_2 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 22>; [50.00%]

  <bb 12> [local count: 14353]:
  # DEBUG BEGIN_STMT
  # DEBUG bIsSpuriousInt => 0
  # DEBUG BEGIN_STMT
  # DEBUG u32MbHandle => mb_idx_40
  # DEBUG BEGIN_STMT
  _7 = state_29->bIsLegacyFifoEn;
  if (_7 != 0)
    goto <bb 13>; [50.00%]
  else
    goto <bb 15>; [50.00%]

  <bb 13> [local count: 7177]:
  if (mb_idx_40 <= 7)
    goto <bb 14>; [33.00%]
  else
    goto <bb 15>; [67.00%]

  <bb 14> [local count: 2368]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerRxFIFO (instance_26(D), mb_idx_40);
  # DEBUG BEGIN_STMT
  # DEBUG u32MbHandle => 0
  goto <bb 17>; [100.00%]

  <bb 15> [local count: 11985]:
  # DEBUG BEGIN_STMT
  _8 ={v} state_29->mbs[mb_idx_40].state;
  if (_8 == 1)
    goto <bb 16>; [20.24%]
  else
    goto <bb 17>; [79.76%]

  <bb 16> [local count: 2426]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerRxMB (instance_26(D), mb_idx_40);

  <bb 17> [local count: 14353]:
  # u32MbHandle_13 = PHI <0(14), mb_idx_40(15), mb_idx_40(16)>
  # DEBUG u32MbHandle => u32MbHandle_13
  # DEBUG BEGIN_STMT
  _9 ={v} state_29->mbs[u32MbHandle_13].state;
  if (_9 == 2)
    goto <bb 18>; [20.24%]
  else
    goto <bb 19>; [79.76%]

  <bb 18> [local count: 2905]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerTxMB (instance_26(D), mb_idx_40);

  <bb 19> [local count: 14353]:
  # DEBUG BEGIN_STMT
  _10 = FlexCAN_GetMsgBuffIntStatusFlag (base_28, mb_idx_40);
  if (_10 != 0)
    goto <bb 20>; [50.00%]
  else
    goto <bb 22>; [50.00%]

  <bb 20> [local count: 7177]:
  # DEBUG BEGIN_STMT
  _11 ={v} state_29->mbs[u32MbHandle_13].state;
  if (_11 == 0)
    goto <bb 21>; [33.00%]
  else
    goto <bb 22>; [67.00%]

  <bb 21> [local count: 2368]:
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_28, mb_idx_40);

  <bb 22> [local count: 28706]:
  # bIsSpuriousInt_15 = PHI <1(11), 0(19), 0(20), 0(21)>
  # DEBUG bIsSpuriousInt => bIsSpuriousInt_15
  # DEBUG BEGIN_STMT
  if (bEnhancedFifoExisted_32(D) != 0)
    goto <bb 23>; [50.00%]
  else
    goto <bb 26>; [50.00%]

  <bb 23> [local count: 14353]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_28
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhancedRxFifoEnabled
  # DEBUG BEGIN_STMT
  _51 ={v} MEM[(const struct FLEXCAN_Type *)base_28].ERFCR;
  _52 = (signed int) _51;
  # DEBUG base => NULL
  if (_52 < 0)
    goto <bb 24>; [41.00%]
  else
    goto <bb 26>; [59.00%]

  <bb 24> [local count: 5885]:
  _12 = state_29->transferType;
  if (_12 == 0)
    goto <bb 25>; [33.00%]
  else
    goto <bb 26>; [67.00%]

  <bb 25> [local count: 1942]:
  # DEBUG BEGIN_STMT
  bIsSpuriousInt_47 = FlexCAN_ProcessIRQHandlerEnhancedRxFIFO (instance_26(D), bIsSpuriousInt_15);
  # DEBUG bIsSpuriousInt => bIsSpuriousInt_47

  <bb 26> [local count: 28706]:
  # bIsSpuriousInt_16 = PHI <bIsSpuriousInt_15(22), bIsSpuriousInt_15(23), bIsSpuriousInt_15(24), bIsSpuriousInt_47(25)>
  # DEBUG bIsSpuriousInt => bIsSpuriousInt_16
  # DEBUG BEGIN_STMT
  if (bIsSpuriousInt_16 != 0)
    goto <bb 27>; [33.00%]
  else
    goto <bb 32>; [67.00%]

  <bb 27> [local count: 9473]:
  # DEBUG BEGIN_STMT
  FlexCAN_ProcessSpuriousInterruptMB (instance_26(D), startMbIdx_31(D), endMbIdx_30(D));
  goto <bb 32>; [100.00%]

  <bb 28> [local count: 202115]:
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_28, mb_idx_18);
  # DEBUG BEGIN_STMT
  mb_idx_34 = mb_idx_18 + 1;
  # DEBUG mb_idx => mb_idx_34

  <bb 29> [local count: 227096]:
  # mb_idx_18 = PHI <mb_idx_34(28), startMbIdx_31(D)(33)>
  # DEBUG mb_idx => mb_idx_18
  # DEBUG BEGIN_STMT
  if (mb_idx_18 <= endMbIdx_30(D))
    goto <bb 28>; [89.00%]
  else
    goto <bb 30>; [11.00%]

  <bb 30> [local count: 24981]:
  # DEBUG BEGIN_STMT
  if (bEnhancedFifoExisted_32(D) != 0)
    goto <bb 31>; [50.00%]
  else
    goto <bb 32>; [50.00%]

  <bb 31> [local count: 12490]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_28
  # DEBUG intFlag => 28
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  base_28->ERFSR ={v} 268435456;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG BEGIN_STMT
  # DEBUG base => base_28
  # DEBUG intFlag => 29
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  base_28->ERFSR ={v} 536870912;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG BEGIN_STMT
  # DEBUG base => base_28
  # DEBUG intFlag => 30
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  base_28->ERFSR ={v} 1073741824;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG BEGIN_STMT
  # DEBUG base => base_28
  # DEBUG intFlag => 31
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  base_28->ERFSR ={v} 2147483648;

  <bb 32> [local count: 53687]:
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  return;

}


FlexCAN_CompleteRxMessageFifoData (uint8 instance)
{
  volatile boolean x;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  <unnamed type> _3;
  _Bool _4;
  _Bool _5;
  _Bool _6;
  _Bool x.0_17;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_8(D);
  base_10 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_10
  # DEBUG BEGIN_STMT
  state_11 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_11
  # DEBUG BEGIN_STMT
  _2 = instance_8(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_17 ={v} x;
  if (x.0_17 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 7> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 8> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = state_11->transferType;
  if (_3 == 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 35433]:
  # DEBUG BEGIN_STMT
  _4 = state_11->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (base_10, instance_8(D), 5, 0, _4);
  # DEBUG BEGIN_STMT
  _5 = state_11->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (base_10, instance_8(D), 6, 0, _5);
  # DEBUG BEGIN_STMT
  _6 = state_11->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (base_10, instance_8(D), 7, 0, _6);

  <bb 6> [local count: 107374]:
  # DEBUG BEGIN_STMT
  state_11->mbs[0].pMBmessage = 0B;
  # DEBUG BEGIN_STMT
  state_11->mbs[0].state ={v} 0;
  return;

}


FlexCAN_Ip_GetTransferStatus (uint8 instance, uint8 mb_idx)
{
  volatile boolean x;
  volatile boolean x;
  Flexcan_Ip_StatusType status;
  const struct Flexcan_Ip_StateType * state;
  int _1;
  _Bool _2;
  unsigned char _3;
  _Bool _4;
  int _5;
  <unnamed type> _6;
  <unnamed type> _7;
  _Bool x.0_13;
  _Bool x.0_14;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_9(D);
  state_11 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_11
  # DEBUG BEGIN_STMT
  # DEBUG status => 1
  # DEBUG BEGIN_STMT
  _2 = instance_9(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_14 ={v} x;
  if (x.0_14 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 13> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = mb_idx_12(D) + 160;
  _4 = _3 > 158;
  x ={v} _4;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_13 ={v} x;
  if (x.0_13 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 14> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  if (mb_idx_12(D) <= 95)
    goto <bb 7>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 7> [local count: 26844]:
  # DEBUG BEGIN_STMT
  _5 = (int) mb_idx_12(D);
  _6 ={v} state_11->mbs[_5].state;
  if (_6 == 0)
    goto <bb 11>; [65.00%]
  else
    goto <bb 8>; [35.00%]

  <bb 8> [local count: 9395]:
  # DEBUG BEGIN_STMT
  # DEBUG status => 2
  goto <bb 11>; [100.00%]

  <bb 9> [local count: 26844]:
  # DEBUG BEGIN_STMT
  _7 ={v} state_11->enhancedFifoOutput.state;
  if (_7 == 0)
    goto <bb 11>; [65.00%]
  else
    goto <bb 10>; [35.00%]

  <bb 10> [local count: 9395]:
  # DEBUG BEGIN_STMT
  # DEBUG status => 2

  <bb 11> [local count: 53687]:
  # status_8 = PHI <2(8), 0(9), 2(10), 0(7)>
  # DEBUG status => status_8
  # DEBUG BEGIN_STMT
  return status_8;

}


FlexCAN_Ip_ConfigRemoteResponseMb (uint8 instance, uint8 mb_idx, const struct Flexcan_Ip_DataInfoType * tx_info, uint32 msg_id, const uint8 * mb_data)
{
  volatile boolean x;
  volatile boolean x;
  const struct Flexcan_Ip_StateType * const state;
  struct FLEXCAN_Type * pBase;
  struct Flexcan_Ip_MsbuffCodeStatusType cs;
  Flexcan_Ip_StatusType result;
  int _1;
  _Bool _2;
  _Bool _3;
  _Bool _4;
  long unsigned int _5;
  _Bool _6;
  long unsigned int _7;
  <unnamed type> _8;
  long unsigned int _9;
  _Bool _10;
  _Bool _11;
  _Bool _12;
  _Bool x.0_33;
  _Bool x.0_34;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = (int) instance_15(D);
  pBase_17 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_17
  # DEBUG BEGIN_STMT
  state_18 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_18
  # DEBUG BEGIN_STMT
  _2 = instance_15(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_34 ={v} x;
  if (x.0_34 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 11> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 13> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = tx_info_19(D) != 0B;
  x ={v} _3;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_33 ={v} x;
  if (x.0_33 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 10> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 12> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _4 = state_18->bIsLegacyFifoEn;
  _5 = state_18->u32MaxMbNum;
  _6 = FlexCAN_IsMbOutOfRange (pBase_17, mb_idx_20(D), _4, _5);
  if (_6 != 0)
    goto <bb 9>; [52.23%]
  else
    goto <bb 7>; [47.77%]

  <bb 7> [local count: 25646]:
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _7 = tx_info_19(D)->data_length;
  cs.dataLen = _7;
  # DEBUG BEGIN_STMT
  _8 = tx_info_19(D)->msg_id_type;
  cs.msgIdType = _8;
  # DEBUG BEGIN_STMT
  cs.code = 10;
  # DEBUG BEGIN_STMT
  cs.fd_enable = 0;
  # DEBUG BEGIN_STMT
  _9 = (long unsigned int) mb_idx_20(D);
  FlexCAN_ClearMsgBuffIntStatusFlag (pBase_17, _9);
  # DEBUG BEGIN_STMT
  _10 = tx_info_19(D)->is_remote;
  FlexCAN_SetTxMsgBuff (pBase_17, _9, &cs, msg_id_27(D), mb_data_28(D), _10);
  # DEBUG BEGIN_STMT
  _11 = tx_info_19(D)->is_polling;
  if (_11 != 0)
    goto <bb 9>; [67.00%]
  else
    goto <bb 8>; [33.00%]

  <bb 8> [local count: 8463]:
  # DEBUG BEGIN_STMT
  _12 = state_18->isIntActive;
  result_31 = FlexCAN_SetMsgBuffIntCmd (pBase_17, instance_15(D), _9, 1, _12);
  # DEBUG result => result_31

  <bb 9> [local count: 53687]:
  # result_13 = PHI <4(6), 0(7), result_31(8)>
  # DEBUG result => result_13
  # DEBUG BEGIN_STMT
  cs ={v} {CLOBBER};
  return result_13;

}


FlexCAN_Ip_ConfigEnhancedRxFifo_Privileged (uint8 instance, const struct Flexcan_Ip_EnhancedIdTableType * id_filter_table)
{
  volatile boolean x;
  volatile boolean x;
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  int _1;
  _Bool _2;
  _Bool _3;
  _Bool _4;
  _Bool x.0_21;
  _Bool x.0_22;
  _Bool x.0_23;
  long unsigned int _24;
  signed int _25;
  long unsigned int _26;
  long unsigned int _27;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _1 = (int) instance_11(D);
  pBase_13 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_13
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_13
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _24 ={v} MEM[(const struct FLEXCAN_Type *)pBase_13].MCR;
  _25 = (signed int) _24;
  # DEBUG pBase => NULL
  # DEBUG disabled => _25 < 0
  # DEBUG BEGIN_STMT
  _2 = instance_11(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_23 ={v} x;
  if (x.0_23 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 20>; [50.00%]

  <bb 20> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 23> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = FlexCAN_IsEnhancedRxFifoAvailable (pBase_13);
  x ={v} _3;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_22 ={v} x;
  if (x.0_22 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 19> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 22> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _4 = id_filter_table_15(D) != 0B;
  x ={v} _4;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_21 ={v} x;
  if (x.0_21 != 0)
    goto <bb 8>; [50.00%]
  else
    goto <bb 18>; [50.00%]

  <bb 18> [local count: 26844]:

  <bb 7> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 21> [local count: 268435456]:
  goto <bb 7>; [100.00%]

  <bb 8> [local count: 26844]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  if (_25 < 0)
    goto <bb 9>; [25.50%]
  else
    goto <bb 10>; [74.50%]

  <bb 9> [local count: 6845]:
  # DEBUG BEGIN_STMT
  result_17 = FlexCAN_Enable (pBase_13);
  # DEBUG result => result_17

  <bb 10> [local count: 26844]:
  # result_5 = PHI <0(8), result_17(9)>
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_13
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _26 ={v} MEM[(const struct FLEXCAN_Type *)pBase_13].MCR;
  _27 = _26 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _27 != 0
  # DEBUG BEGIN_STMT
  if (_27 == 0)
    goto <bb 11>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 11> [local count: 13422]:
  if (result_5 == 0)
    goto <bb 14>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 20133]:
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  if (result_5 == 0)
    goto <bb 13>; [33.00%]
  else
    goto <bb 14>; [67.00%]

  <bb 13> [local count: 6644]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetEnhancedRxFifoFilter (pBase_13, id_filter_table_15(D));

  <bb 14> [local count: 26843]:
  # result_10 = PHI <result_5(12), 0(13), 1(11)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_25 < 0)
    goto <bb 15>; [25.50%]
  else
    goto <bb 17>; [74.50%]

  <bb 15> [local count: 6845]:
  # DEBUG BEGIN_STMT
  status_20 = FlexCAN_Disable (pBase_13);
  # DEBUG status => status_20
  # DEBUG BEGIN_STMT
  if (status_20 != 0)
    goto <bb 16>; [50.00%]
  else
    goto <bb 17>; [50.00%]

  <bb 16> [local count: 3423]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_20

  <bb 17> [local count: 26843]:
  # result_6 = PHI <result_10(14), result_10(15), status_20(16)>
  # DEBUG result => result_6
  # DEBUG BEGIN_STMT
  return result_6;

}


FlexCAN_Ip_ConfigRxFifo_Privileged (uint8 instance, Flexcan_Ip_RxFifoIdElementFormatType id_format, const struct Flexcan_Ip_IdTableType * id_filter_table)
{
  volatile boolean x;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType status;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  long unsigned int _19;
  signed int _20;
  _Bool x.0_21;
  long unsigned int _22;
  long unsigned int _23;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = instance_8(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_21 ={v} x;
  if (x.0_21 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  # DEBUG status => 0
  # DEBUG BEGIN_STMT
  _2 = (int) instance_8(D);
  pBase_11 = g_Flexcan_Ip_aBase[_2];
  # DEBUG pBase => pBase_11
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _19 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _20 = (signed int) _19;
  # DEBUG pBase => NULL
  # DEBUG disabled => _20 < 0
  # DEBUG BEGIN_STMT
  if (_20 < 0)
    goto <bb 5>; [25.50%]
  else
    goto <bb 6>; [74.50%]

  <bb 5> [local count: 27380]:
  # DEBUG BEGIN_STMT
  result_13 = FlexCAN_Enable (pBase_11);
  # DEBUG result => result_13

  <bb 6> [local count: 107374]:
  # result_3 = PHI <0(4), result_13(5)>
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_11
  # DEBUG INLINE_ENTRY FlexCAN_IsFreezeMode
  # DEBUG BEGIN_STMT
  _22 ={v} MEM[(const struct FLEXCAN_Type *)pBase_11].MCR;
  _23 = _22 & 16777216;
  # DEBUG base => NULL
  # DEBUG freeze => _23 != 0
  # DEBUG BEGIN_STMT
  if (_23 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 53687]:
  if (result_3 == 0)
    goto <bb 10>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 80531]:
  # DEBUG result => result_3
  # DEBUG BEGIN_STMT
  if (result_3 == 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 10>; [67.00%]

  <bb 9> [local count: 26575]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetRxFifoFilter (pBase_11, id_format_14(D), id_filter_table_15(D));

  <bb 10> [local count: 107374]:
  # result_10 = PHI <result_3(8), 0(9), 1(7)>
  # DEBUG result => NULL
  # DEBUG BEGIN_STMT
  if (_20 < 0)
    goto <bb 11>; [25.50%]
  else
    goto <bb 13>; [74.50%]

  <bb 11> [local count: 27380]:
  # DEBUG BEGIN_STMT
  status_18 = FlexCAN_Disable (pBase_11);
  # DEBUG status => status_18
  # DEBUG BEGIN_STMT
  if (status_18 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 13690]:
  # DEBUG BEGIN_STMT
  # DEBUG result => status_18

  <bb 13> [local count: 107374]:
  # result_4 = PHI <result_10(10), result_10(11), status_18(12)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_RxFifoBlocking (uint8 instance, struct Flexcan_Ip_MsgBuffType * data, uint32 timeout)
{
  volatile boolean x;
  const struct FLEXCAN_Type * base;
  Flexcan_Ip_StatusType result;
  int _1;
  _Bool _2;
  _Bool _3;
  _Bool x.0_24;
  long unsigned int _25;
  signed int _26;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  _1 = (int) instance_6(D);
  base_8 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_8
  # DEBUG BEGIN_STMT
  _2 = instance_6(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_24 ={v} x;
  if (x.0_24 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 13> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 14> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = FlexCAN_IsEnhancedRxFifoAvailable (base_8);
  if (_3 != 0)
    goto <bb 5>; [67.00%]
  else
    goto <bb 10>; [33.00%]

  <bb 5> [local count: 71941]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_8
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhancedRxFifoEnabled
  # DEBUG BEGIN_STMT
  _25 ={v} base_8->ERFCR;
  _26 = (signed int) _25;
  # DEBUG base => NULL
  if (_26 < 0)
    goto <bb 6>; [41.00%]
  else
    goto <bb 8>; [59.00%]

  <bb 6> [local count: 29496]:
  # DEBUG BEGIN_STMT
  result_21 = FlexCAN_StartRxMessageEnhancedFifoData (instance_6(D), data_10(D));
  # DEBUG result => result_21
  # DEBUG BEGIN_STMT
  if (result_21 == 0)
    goto <bb 7>; [33.00%]
  else
    goto <bb 12>; [67.00%]

  <bb 7> [local count: 9734]:
  # DEBUG BEGIN_STMT
  result_23 = FlexCAN_ProccessEnhancedRxFifo (instance_6(D), timeout_13(D));
  # DEBUG result => result_23
  goto <bb 12>; [100.00%]

  <bb 8> [local count: 42445]:
  # DEBUG BEGIN_STMT
  result_17 = FlexCAN_StartRxMessageFifoData (instance_6(D), data_10(D));
  # DEBUG result => result_17
  # DEBUG BEGIN_STMT
  if (result_17 == 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 12>; [67.00%]

  <bb 9> [local count: 14007]:
  # DEBUG BEGIN_STMT
  result_19 = FlexCAN_ProccessLegacyRxFIFO (instance_6(D), timeout_13(D));
  # DEBUG result => result_19
  goto <bb 12>; [100.00%]

  <bb 10> [local count: 35433]:
  # DEBUG BEGIN_STMT
  result_12 = FlexCAN_StartRxMessageFifoData (instance_6(D), data_10(D));
  # DEBUG result => result_12
  # DEBUG BEGIN_STMT
  if (result_12 == 0)
    goto <bb 11>; [33.00%]
  else
    goto <bb 12>; [67.00%]

  <bb 11> [local count: 11693]:
  # DEBUG BEGIN_STMT
  result_15 = FlexCAN_ProccessLegacyRxFIFO (instance_6(D), timeout_13(D));
  # DEBUG result => result_15

  <bb 12> [local count: 107374]:
  # result_4 = PHI <result_17(8), result_12(10), result_15(11), result_23(7), result_21(6), result_19(9)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_RxFifo (uint8 instance, struct Flexcan_Ip_MsgBuffType * data)
{
  volatile boolean x;
  const struct FLEXCAN_Type * base;
  Flexcan_Ip_StatusType result;
  _Bool _1;
  int _2;
  _Bool _3;
  _Bool x.0_17;
  long unsigned int _18;
  signed int _19;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  _1 = instance_6(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_17 ={v} x;
  if (x.0_17 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 10> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 11> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _2 = (int) instance_6(D);
  base_8 = g_Flexcan_Ip_aBase[_2];
  # DEBUG base => base_8
  # DEBUG BEGIN_STMT
  _3 = FlexCAN_IsEnhancedRxFifoAvailable (base_8);
  if (_3 != 0)
    goto <bb 5>; [67.00%]
  else
    goto <bb 8>; [33.00%]

  <bb 5> [local count: 71941]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_8
  # DEBUG INLINE_ENTRY FlexCAN_IsEnhancedRxFifoEnabled
  # DEBUG BEGIN_STMT
  _18 ={v} base_8->ERFCR;
  _19 = (signed int) _18;
  # DEBUG base => NULL
  if (_19 < 0)
    goto <bb 6>; [41.00%]
  else
    goto <bb 7>; [59.00%]

  <bb 6> [local count: 29496]:
  # DEBUG BEGIN_STMT
  result_16 = FlexCAN_StartRxMessageEnhancedFifoData (instance_6(D), data_10(D));
  # DEBUG result => result_16
  goto <bb 9>; [100.00%]

  <bb 7> [local count: 42445]:
  # DEBUG BEGIN_STMT
  result_14 = FlexCAN_StartRxMessageFifoData (instance_6(D), data_10(D));
  # DEBUG result => result_14
  goto <bb 9>; [100.00%]

  <bb 8> [local count: 35433]:
  # DEBUG BEGIN_STMT
  result_12 = FlexCAN_StartRxMessageFifoData (instance_6(D), data_10(D));
  # DEBUG result => result_12

  <bb 9> [local count: 107374]:
  # result_4 = PHI <result_14(7), result_12(8), result_16(6)>
  # DEBUG result => result_4
  # DEBUG BEGIN_STMT
  return result_4;

}


FlexCAN_Ip_ReceiveBlocking (uint8 instance, uint8 mb_idx, struct Flexcan_Ip_MsgBuffType * data, boolean isPolling, uint32 u32TimeoutMs)
{
  volatile boolean x;
  struct FLEXCAN_Type * base;
  struct Flexcan_Ip_StateType * state;
  uint32 mS2Ticks;
  uint32 timeElapsed;
  uint32 timeStart;
  Flexcan_Ip_StatusType result;
  long unsigned int _1;
  _Bool _2;
  int _3;
  long unsigned int _4;
  _Bool _5;
  long unsigned int _6;
  long unsigned int _7;
  unsigned char _8;
  int _9;
  <unnamed type> _10;
  long unsigned int _11;
  _Bool _12;
  int _13;
  <unnamed type> _14;
  long unsigned int _45;
  _Bool x.0_50;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  timeStart = 0;
  # DEBUG BEGIN_STMT
  # DEBUG timeElapsed => 0
  # DEBUG BEGIN_STMT
  _1 = u32TimeoutMs_27(D) * 1000;
  mS2Ticks_29 = OsIf_MicrosToTicks (_1, 0);
  # DEBUG mS2Ticks => mS2Ticks_29
  # DEBUG BEGIN_STMT
  _2 = instance_30(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_50 ={v} x;
  if (x.0_50 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 22>; [50.00%]

  <bb 22> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 24> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = (int) instance_30(D);
  state_31 = g_flexcan_Ip_StatePtr[_3];
  # DEBUG state => state_31
  # DEBUG BEGIN_STMT
  base_32 = g_Flexcan_Ip_aBase[_3];
  # DEBUG base => base_32
  # DEBUG BEGIN_STMT
  result_37 = FlexCAN_StartRxMessageBufferData (instance_30(D), mb_idx_33(D), data_34(D), isPolling_35(D));
  # DEBUG result => result_37
  # DEBUG BEGIN_STMT
  if (result_37 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 5> [local count: 53687]:
  if (isPolling_35(D) != 0)
    goto <bb 7>; [67.00%]
  else
    goto <bb 6>; [33.00%]

  <bb 6> [local count: 17717]:
  # DEBUG BEGIN_STMT
  _4 = (long unsigned int) mb_idx_33(D);
  _5 = state_31->isIntActive;
  result_39 = FlexCAN_SetMsgBuffIntCmd (base_32, instance_30(D), _4, 1, _5);
  # DEBUG result => result_39

  <bb 7> [local count: 107374]:
  # result_15 = PHI <result_37(4), 0(5), result_39(6)>
  # DEBUG result => result_15
  # DEBUG BEGIN_STMT
  if (result_15 == 0)
    goto <bb 8>; [33.00%]
  else
    goto <bb 14>; [67.00%]

  <bb 8> [local count: 35433]:
  # DEBUG BEGIN_STMT
  _6 = OsIf_GetCounter (0);
  timeStart = _6;
  # DEBUG BEGIN_STMT
  goto <bb 13>; [100.00%]

  <bb 9> [local count: 313013]:
  # DEBUG BEGIN_STMT
  if (isPolling_35(D) != 0)
    goto <bb 10>; [33.00%]
  else
    goto <bb 12>; [67.00%]

  <bb 10> [local count: 103294]:
  # DEBUG BEGIN_STMT
  _7 = (long unsigned int) mb_idx_33(D);
  _8 = FlexCAN_GetBuffStatusFlag (base_32, _7);
  if (_8 != 0)
    goto <bb 11>; [33.00%]
  else
    goto <bb 12>; [67.00%]

  <bb 11> [local count: 34087]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerRxMB (instance_30(D), _7);

  <bb 12> [local count: 313013]:
  # DEBUG BEGIN_STMT
  _45 = OsIf_GetElapsed (&timeStart, 0);
  timeElapsed_46 = timeElapsed_18 + _45;
  # DEBUG timeElapsed => timeElapsed_46
  # DEBUG BEGIN_STMT
  if (mS2Ticks_29 <= timeElapsed_46)
    goto <bb 14>; [5.50%]
  else
    goto <bb 23>; [94.50%]

  <bb 23> [local count: 295797]:

  <bb 13> [local count: 331231]:
  # timeElapsed_18 = PHI <0(8), timeElapsed_46(23)>
  # DEBUG timeElapsed => timeElapsed_18
  # DEBUG BEGIN_STMT
  _9 = (int) mb_idx_33(D);
  _10 ={v} state_31->mbs[_9].state;
  if (_10 == 1)
    goto <bb 9>; [94.50%]
  else
    goto <bb 14>; [5.50%]

  <bb 14> [local count: 107374]:
  # result_16 = PHI <result_15(7), 3(12), 0(13)>
  # DEBUG result => result_16
  # DEBUG BEGIN_STMT
  if (result_16 == 3)
    goto <bb 15>; [34.00%]
  else
    goto <bb 17>; [66.00%]

  <bb 15> [local count: 36507]:
  if (isPolling_35(D) != 0)
    goto <bb 17>; [67.00%]
  else
    goto <bb 16>; [33.00%]

  <bb 16> [local count: 12047]:
  # DEBUG BEGIN_STMT
  _11 = (long unsigned int) mb_idx_33(D);
  _12 = state_31->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (base_32, instance_30(D), _11, 0, _12);

  <bb 17> [local count: 107374]:
  # DEBUG BEGIN_STMT
  if (result_16 != 4)
    goto <bb 18>; [66.00%]
  else
    goto <bb 21>; [34.00%]

  <bb 18> [local count: 70867]:
  if (result_16 != 2)
    goto <bb 19>; [66.00%]
  else
    goto <bb 21>; [34.00%]

  <bb 19> [local count: 46772]:
  # DEBUG BEGIN_STMT
  _13 = (int) mb_idx_33(D);
  _14 ={v} state_31->mbs[_13].state;
  if (_14 == 0)
    goto <bb 21>; [65.00%]
  else
    goto <bb 20>; [35.00%]

  <bb 20> [local count: 16370]:
  # DEBUG BEGIN_STMT
  state_31->mbs[_13].state ={v} 0;
  # DEBUG BEGIN_STMT
  # DEBUG result => 3

  <bb 21> [local count: 107374]:
  # result_17 = PHI <result_16(17), result_16(18), 0(19), 3(20)>
  # DEBUG result => result_17
  # DEBUG BEGIN_STMT
  timeStart ={v} {CLOBBER};
  return result_17;

}


FlexCAN_Ip_Receive (uint8 instance, uint8 mb_idx, struct Flexcan_Ip_MsgBuffType * data, boolean isPolling)
{
  volatile boolean x;
  const struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  Flexcan_Ip_StatusType result;
  int _1;
  _Bool _2;
  long unsigned int _3;
  _Bool _4;
  _Bool x.0_18;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = (int) instance_7(D);
  base_9 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_9
  # DEBUG BEGIN_STMT
  state_10 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_10
  # DEBUG BEGIN_STMT
  _2 = instance_7(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_18 ={v} x;
  if (x.0_18 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 9> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  result_15 = FlexCAN_StartRxMessageBufferData (instance_7(D), mb_idx_11(D), data_12(D), isPolling_13(D));
  # DEBUG result => result_15
  # DEBUG BEGIN_STMT
  if (result_15 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 5> [local count: 53687]:
  if (isPolling_13(D) != 0)
    goto <bb 7>; [67.00%]
  else
    goto <bb 6>; [33.00%]

  <bb 6> [local count: 17717]:
  # DEBUG BEGIN_STMT
  _3 = (long unsigned int) mb_idx_11(D);
  _4 = state_10->isIntActive;
  result_17 = FlexCAN_SetMsgBuffIntCmd (base_9, instance_7(D), _3, 1, _4);
  # DEBUG result => result_17

  <bb 7> [local count: 107374]:
  # result_5 = PHI <result_15(4), 0(5), result_17(6)>
  # DEBUG result => result_5
  # DEBUG BEGIN_STMT
  return result_5;

}


FlexCAN_Ip_ConfigRxMb (uint8 instance, uint8 mb_idx, const struct Flexcan_Ip_DataInfoType * rx_info, uint32 msg_id)
{
  volatile boolean x;
  volatile boolean x;
  const struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  struct Flexcan_Ip_MsbuffCodeStatusType cs;
  Flexcan_Ip_StatusType eResult;
  int _1;
  _Bool _2;
  _Bool _3;
  _Bool _4;
  long unsigned int _5;
  _Bool _6;
  long unsigned int _7;
  long unsigned int _8;
  <unnamed type> _9;
  _Bool _10;
  _Bool x.0_32;
  _Bool x.0_33;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = (int) instance_13(D);
  base_15 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_15
  # DEBUG BEGIN_STMT
  state_16 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_16
  # DEBUG BEGIN_STMT
  _2 = instance_13(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_33 ={v} x;
  if (x.0_33 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 10> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 12> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = rx_info_17(D) != 0B;
  x ={v} _3;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_32 ={v} x;
  if (x.0_32 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 9> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 11> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _4 = state_16->bIsLegacyFifoEn;
  _5 = state_16->u32MaxMbNum;
  _6 = FlexCAN_IsMbOutOfRange (base_15, mb_idx_18(D), _4, _5);
  if (_6 != 0)
    goto <bb 8>; [52.23%]
  else
    goto <bb 7>; [47.77%]

  <bb 7> [local count: 25646]:
  # DEBUG BEGIN_STMT
  _7 = (long unsigned int) mb_idx_18(D);
  FlexCAN_ClearMsgBuffIntStatusFlag (base_15, _7);
  # DEBUG BEGIN_STMT
  _8 = rx_info_17(D)->data_length;
  cs.dataLen = _8;
  # DEBUG BEGIN_STMT
  _9 = rx_info_17(D)->msg_id_type;
  cs.msgIdType = _9;
  # DEBUG BEGIN_STMT
  _10 = rx_info_17(D)->fd_enable;
  cs.fd_enable = _10;
  # DEBUG BEGIN_STMT
  cs.code = 15;
  # DEBUG BEGIN_STMT
  FlexCAN_SetRxMsgBuff (base_15, _7, &cs, msg_id_25(D));
  # DEBUG BEGIN_STMT
  cs.code = 0;
  # DEBUG BEGIN_STMT
  FlexCAN_SetRxMsgBuff (base_15, _7, &cs, msg_id_25(D));
  # DEBUG BEGIN_STMT
  cs.code = 4;
  # DEBUG BEGIN_STMT
  FlexCAN_SetRxMsgBuff (base_15, _7, &cs, msg_id_25(D));

  <bb 8> [local count: 53687]:
  # eResult_11 = PHI <4(6), 0(7)>
  # DEBUG eResult => eResult_11
  # DEBUG BEGIN_STMT
  cs ={v} {CLOBBER};
  return eResult_11;

}


FlexCAN_Ip_Send (uint8 instance, uint8 mb_idx, const struct Flexcan_Ip_DataInfoType * tx_info, uint32 msg_id, const uint8 * mb_data)
{
  volatile boolean x;
  volatile boolean x;
  const struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  Flexcan_Ip_StatusType result;
  int _1;
  _Bool _2;
  _Bool _3;
  _Bool _4;
  long unsigned int _5;
  _Bool _6;
  long unsigned int _21;
  long unsigned int _22;
  _Bool x.0_23;
  _Bool x.0_24;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 1
  # DEBUG BEGIN_STMT
  _1 = (int) instance_9(D);
  base_11 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_11
  # DEBUG BEGIN_STMT
  state_12 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_12
  # DEBUG BEGIN_STMT
  _2 = instance_9(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_24 ={v} x;
  if (x.0_24 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 14> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = tx_info_13(D) != 0B;
  x ={v} _3;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_23 ={v} x;
  if (x.0_23 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 11> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 13> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  # DEBUG base => base_11
  # DEBUG INLINE_ENTRY FlexCAN_IsListenOnlyModeEnabled
  # DEBUG BEGIN_STMT
  _21 ={v} MEM[(const struct FLEXCAN_Type *)base_11].CTRL1;
  _22 = _21 & 8;
  # DEBUG base => NULL
  if (_22 == 0)
    goto <bb 7>; [33.00%]
  else
    goto <bb 10>; [67.00%]

  <bb 7> [local count: 17717]:
  # DEBUG BEGIN_STMT
  result_18 = FlexCAN_StartSendData (instance_9(D), mb_idx_14(D), tx_info_13(D), msg_id_15(D), mb_data_16(D));
  # DEBUG result => result_18
  # DEBUG BEGIN_STMT
  if (result_18 == 0)
    goto <bb 8>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 8> [local count: 8858]:
  _4 = tx_info_13(D)->is_polling;
  if (_4 != 0)
    goto <bb 10>; [67.00%]
  else
    goto <bb 9>; [33.00%]

  <bb 9> [local count: 2923]:
  # DEBUG BEGIN_STMT
  _5 = (long unsigned int) mb_idx_14(D);
  _6 = state_12->isIntActive;
  result_20 = FlexCAN_SetMsgBuffIntCmd (base_11, instance_9(D), _5, 1, _6);
  # DEBUG result => result_20

  <bb 10> [local count: 53687]:
  # result_7 = PHI <1(6), result_18(7), 0(8), result_20(9)>
  # DEBUG result => result_7
  # DEBUG BEGIN_STMT
  return result_7;

}


FlexCAN_Ip_Init_Privileged (uint8 Flexcan_Ip_u8Instance, struct Flexcan_Ip_StateType * Flexcan_Ip_pState, const struct Flexcan_Ip_ConfigType * Flexcan_Ip_pData)
{
  volatile boolean x;
  volatile boolean x;
  uint32 i;
  struct FLEXCAN_Type * pBase;
  Flexcan_Ip_StatusType eResult;
  int _1;
  _Bool _2;
  _Bool _3;
  _Bool _4;
  _Bool _5;
  long unsigned int _6;
  long unsigned int _7;
  const struct Flexcan_Ip_TimeSegmentType * _8;
  _Bool _9;
  const struct Flexcan_Ip_TimeSegmentType * _10;
  long unsigned int _11;
  long unsigned int _12;
  _Bool _13;
  const struct Flexcan_Ip_TimeSegmentType * _14;
  const struct Flexcan_Ip_TimeSegmentType * _15;
  const struct Flexcan_Ip_TimeSegmentType * _16;
  <unnamed type> _17;
  <unnamed type> _18;
  void (*<T341>) (uint8, Flexcan_Ip_EventType, uint32, const struct Flexcan_Ip_StateType *) _19;
  void (*<T341>) (uint8, Flexcan_Ip_EventType, uint32, const struct Flexcan_Ip_StateType *) _20;
  _Bool _21;
  long unsigned int _22;
  _Bool x.0_68;
  _Bool x.0_69;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 0
  # DEBUG BEGIN_STMT
  _1 = (int) Flexcan_Ip_u8Instance_30(D);
  pBase_32 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_32
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _2 = Flexcan_Ip_u8Instance_30(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_69 ={v} x;
  if (x.0_69 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 22>; [50.00%]

  <bb 22> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 24> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = Flexcan_Ip_pData_33(D) != 0B;
  x ={v} _3;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_68 ={v} x;
  if (x.0_68 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 21>; [50.00%]

  <bb 21> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 23> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  eResult_35 = FlexCAN_InitController (pBase_32, Flexcan_Ip_pData_33(D));
  # DEBUG eResult => eResult_35
  # DEBUG BEGIN_STMT
  if (eResult_35 == 0)
    goto <bb 7>; [33.00%]
  else
    goto <bb 19>; [67.00%]

  <bb 7> [local count: 17717]:
  # DEBUG BEGIN_STMT
  _4 = Flexcan_Ip_pData_33(D)->fd_enable;
  FlexCAN_EnableExtCbt (pBase_32, _4);
  # DEBUG BEGIN_STMT
  _5 = Flexcan_Ip_pData_33(D)->enhCbtEnable;
  if (_5 != 0)
    goto <bb 8>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 8> [local count: 8858]:
  # DEBUG BEGIN_STMT
  SchM_Enter_Can_CAN_EXCLUSIVE_AREA_00 ();
  # DEBUG BEGIN_STMT
  _6 ={v} pBase_32->CTRL2;
  _7 = _6 | 8192;
  pBase_32->CTRL2 ={v} _7;
  # DEBUG BEGIN_STMT
  _8 = &Flexcan_Ip_pData_33(D)->bitrate;
  FlexCAN_SetEnhancedNominalTimeSegments (pBase_32, _8);
  # DEBUG BEGIN_STMT
  _9 = Flexcan_Ip_pData_33(D)->fd_enable;
  if (_9 != 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 10>; [67.00%]

  <bb 9> [local count: 2923]:
  # DEBUG BEGIN_STMT
  _10 = &Flexcan_Ip_pData_33(D)->bitrate_cbt;
  FlexCAN_SetEnhancedDataTimeSegments (pBase_32, _10);

  <bb 10> [local count: 8858]:
  # DEBUG BEGIN_STMT
  SchM_Exit_Can_CAN_EXCLUSIVE_AREA_00 ();
  goto <bb 15>; [100.00%]

  <bb 11> [local count: 8858]:
  # DEBUG BEGIN_STMT
  SchM_Enter_Can_CAN_EXCLUSIVE_AREA_00 ();
  # DEBUG BEGIN_STMT
  _11 ={v} pBase_32->CTRL2;
  _12 = _11 & 4294959103;
  pBase_32->CTRL2 ={v} _12;
  # DEBUG BEGIN_STMT
  _13 = Flexcan_Ip_pData_33(D)->fd_enable;
  if (_13 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 4429]:
  # DEBUG BEGIN_STMT
  _14 = &Flexcan_Ip_pData_33(D)->bitrate;
  FlexCAN_SetExtendedTimeSegments (pBase_32, _14);
  # DEBUG BEGIN_STMT
  _15 = &Flexcan_Ip_pData_33(D)->bitrate_cbt;
  FlexCAN_SetFDTimeSegments (pBase_32, _15);
  goto <bb 14>; [100.00%]

  <bb 13> [local count: 4429]:
  # DEBUG BEGIN_STMT
  _16 = &Flexcan_Ip_pData_33(D)->bitrate;
  FlexCAN_SetTimeSegments (pBase_32, _16);

  <bb 14> [local count: 8858]:
  # DEBUG BEGIN_STMT
  SchM_Exit_Can_CAN_EXCLUSIVE_AREA_00 ();

  <bb 15> [local count: 17717]:
  # DEBUG BEGIN_STMT
  _17 = Flexcan_Ip_pData_33(D)->flexcanMode;
  FlexCAN_SetOperationMode (pBase_32, _17);
  # DEBUG BEGIN_STMT
  eResult_50 = FlexCAN_EnterFreezeMode (pBase_32);
  # DEBUG eResult => eResult_50
  # DEBUG BEGIN_STMT
  if (eResult_50 == 0)
    goto <bb 20>; [50.00%]
  else
    goto <bb 19>; [50.00%]

  <bb 20> [local count: 8858]:
  goto <bb 17>; [100.00%]

  <bb 16> [local count: 851176]:
  # DEBUG BEGIN_STMT
  Flexcan_Ip_pState_51(D)->mbs[i_24].isPolling = 1;
  # DEBUG BEGIN_STMT
  Flexcan_Ip_pState_51(D)->mbs[i_24].pMBmessage = 0B;
  # DEBUG BEGIN_STMT
  Flexcan_Ip_pState_51(D)->mbs[i_24].state ={v} 0;
  # DEBUG BEGIN_STMT
  Flexcan_Ip_pState_51(D)->mbs[i_24].time_stamp = 0;
  # DEBUG BEGIN_STMT
  i_67 = i_24 + 1;
  # DEBUG i => i_67

  <bb 17> [local count: 860035]:
  # i_24 = PHI <i_67(16), 0(20)>
  # DEBUG i => i_24
  # DEBUG BEGIN_STMT
  if (i_24 != 96)
    goto <bb 16>; [98.97%]
  else
    goto <bb 18>; [1.03%]

  <bb 18> [local count: 8858]:
  # DEBUG BEGIN_STMT
  Flexcan_Ip_pState_51(D)->enhancedFifoOutput.isPolling = 1;
  # DEBUG BEGIN_STMT
  Flexcan_Ip_pState_51(D)->enhancedFifoOutput.state ={v} 0;
  # DEBUG BEGIN_STMT
  _18 = Flexcan_Ip_pData_33(D)->transfer_type;
  Flexcan_Ip_pState_51(D)->transferType = _18;
  # DEBUG BEGIN_STMT
  _19 = Flexcan_Ip_pData_33(D)->Callback;
  Flexcan_Ip_pState_51(D)->callback = _19;
  # DEBUG BEGIN_STMT
  Flexcan_Ip_pState_51(D)->callbackParam = 0B;
  # DEBUG BEGIN_STMT
  _20 = Flexcan_Ip_pData_33(D)->ErrorCallback;
  Flexcan_Ip_pState_51(D)->error_callback = _20;
  # DEBUG BEGIN_STMT
  Flexcan_Ip_pState_51(D)->errorCallbackParam = 0B;
  # DEBUG BEGIN_STMT
  _21 = Flexcan_Ip_pData_33(D)->is_rx_fifo_needed;
  Flexcan_Ip_pState_51(D)->bIsLegacyFifoEn = _21;
  # DEBUG BEGIN_STMT
  _22 = Flexcan_Ip_pData_33(D)->max_num_mb;
  Flexcan_Ip_pState_51(D)->u32MaxMbNum = _22;
  # DEBUG BEGIN_STMT
  Flexcan_Ip_pState_51(D)->isIntActive = 1;
  # DEBUG BEGIN_STMT
  g_flexcan_Ip_StatePtr[_1] = Flexcan_Ip_pState_51(D);

  <bb 19> [local count: 53687]:
  # eResult_23 = PHI <eResult_35(6), eResult_50(15), 0(18)>
  # DEBUG eResult => eResult_23
  # DEBUG BEGIN_STMT
  return eResult_23;

}


FlexCAN_AbortRxTransfer (uint8 u8Instance, uint8 mb_idx)
{
  volatile uint32 * flexcan_mb;
  uint32 flexcan_mb_config;
  uint32 val2;
  uint32 val1;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * pBase;
  int _1;
  int _2;
  _Bool _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  _Bool _7;
  long unsigned int _8;
  long unsigned int _9;

  <bb 2> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  _1 = (int) u8Instance_12(D);
  pBase_14 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_14
  # DEBUG BEGIN_STMT
  state_15 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_15
  # DEBUG BEGIN_STMT
  # DEBUG val1 => 0
  # DEBUG BEGIN_STMT
  # DEBUG val2 => 0
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb_config => 0
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb => 0B
  # DEBUG BEGIN_STMT
  _2 = (int) mb_idx_16(D);
  state_15->mbs[_2].state ={v} 0;
  # DEBUG BEGIN_STMT
  _3 = state_15->bIsLegacyFifoEn;
  if (_3 != 0)
    goto <bb 3>; [67.00%]
  else
    goto <bb 7>; [33.00%]

  <bb 3> [local count: 719407022]:
  # DEBUG BEGIN_STMT
  _4 ={v} pBase_14->CTRL2;
  _5 = _4 >> 24;
  val1_25 = _5 & 15;
  # DEBUG val1 => val1_25
  # DEBUG BEGIN_STMT
  val2_26 = RxFifoOcuppiedLastMsgBuff (val1_25);
  # DEBUG val2 => val2_26
  # DEBUG BEGIN_STMT
  _6 = (long unsigned int) mb_idx_16(D);
  if (_6 > val2_26)
    goto <bb 4>; [33.00%]
  else
    goto <bb 5>; [67.00%]

  <bb 4> [local count: 237404317]:
  # DEBUG BEGIN_STMT
  flexcan_mb_28 = FlexCAN_GetMsgBuffRegion (pBase_14, _6);
  # DEBUG flexcan_mb => flexcan_mb_28
  # DEBUG BEGIN_STMT
  flexcan_mb_config_29 ={v} *flexcan_mb_28;
  # DEBUG flexcan_mb_config => flexcan_mb_config_29
  # DEBUG BEGIN_STMT
  flexcan_mb_config_30 = flexcan_mb_config_29 & 4043309055;
  # DEBUG flexcan_mb_config => flexcan_mb_config_30
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb_config => flexcan_mb_config_30
  # DEBUG BEGIN_STMT
  *flexcan_mb_28 ={v} flexcan_mb_config_30;
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb_config => flexcan_mb_config_30
  # DEBUG BEGIN_STMT
  flexcan_mb_config_32 = flexcan_mb_config_30 | 67108864;
  # DEBUG flexcan_mb_config => flexcan_mb_config_32
  # DEBUG BEGIN_STMT
  *flexcan_mb_28 ={v} flexcan_mb_config_32;

  <bb 5> [local count: 719407022]:
  # DEBUG BEGIN_STMT
  if (mb_idx_16(D) == 0)
    goto <bb 6>; [33.00%]
  else
    goto <bb 8>; [67.00%]

  <bb 6> [local count: 237404317]:
  # DEBUG BEGIN_STMT
  _7 = state_15->isIntActive;
  FLEXCAN_ClearMsgBuffIntCmd (pBase_14, u8Instance_12(D), 5, _7);
  goto <bb 8>; [100.00%]

  <bb 7> [local count: 354334802]:
  # DEBUG BEGIN_STMT
  _8 = (long unsigned int) mb_idx_16(D);
  flexcan_mb_19 = FlexCAN_GetMsgBuffRegion (pBase_14, _8);
  # DEBUG flexcan_mb => flexcan_mb_19
  # DEBUG BEGIN_STMT
  flexcan_mb_config_20 ={v} *flexcan_mb_19;
  # DEBUG flexcan_mb_config => flexcan_mb_config_20
  # DEBUG BEGIN_STMT
  flexcan_mb_config_21 = flexcan_mb_config_20 & 4043309055;
  # DEBUG flexcan_mb_config => flexcan_mb_config_21
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb_config => flexcan_mb_config_21
  # DEBUG BEGIN_STMT
  *flexcan_mb_19 ={v} flexcan_mb_config_21;
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb_config => flexcan_mb_config_21
  # DEBUG BEGIN_STMT
  flexcan_mb_config_23 = flexcan_mb_config_21 | 67108864;
  # DEBUG flexcan_mb_config => flexcan_mb_config_23
  # DEBUG BEGIN_STMT
  *flexcan_mb_19 ={v} flexcan_mb_config_23;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _9 = (long unsigned int) mb_idx_16(D);
  FlexCAN_ClearMsgBuffIntStatusFlag (pBase_14, _9);
  return;

}


FlexCAN_AbortTxTransfer (uint8 u8Instance, uint8 mb_idx)
{
  volatile uint32 * flexcan_mb;
  uint32 uS2Ticks;
  uint32 flexcan_mb_config;
  uint32 timeElapsed;
  uint32 timeStart;
  Flexcan_Ip_StatusType result;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * pBase;
  int _1;
  long unsigned int _2;
  long unsigned int _3;
  unsigned char _4;
  long unsigned int _5;
  long unsigned int _6;
  int _7;
  long unsigned int _32;

  <bb 2> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  _1 = (int) u8Instance_14(D);
  pBase_16 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_16
  # DEBUG BEGIN_STMT
  state_17 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_17
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  timeStart = 0;
  # DEBUG BEGIN_STMT
  # DEBUG timeElapsed => 0
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb_config => 0
  # DEBUG BEGIN_STMT
  # DEBUG uS2Ticks => 0
  # DEBUG BEGIN_STMT
  # DEBUG flexcan_mb => 0B
  # DEBUG BEGIN_STMT
  _2 = (long unsigned int) mb_idx_19(D);
  flexcan_mb_21 = FlexCAN_GetMsgBuffRegion (pBase_16, _2);
  # DEBUG flexcan_mb => flexcan_mb_21
  # DEBUG BEGIN_STMT
  flexcan_mb_config_22 ={v} *flexcan_mb_21;
  # DEBUG flexcan_mb_config => flexcan_mb_config_22
  # DEBUG BEGIN_STMT
  flexcan_mb_config_23 = flexcan_mb_config_22 & 4043309055;
  # DEBUG flexcan_mb_config => flexcan_mb_config_23
  # DEBUG BEGIN_STMT
  flexcan_mb_config_24 = flexcan_mb_config_23 | 150994944;
  # DEBUG flexcan_mb_config => flexcan_mb_config_24
  # DEBUG BEGIN_STMT
  *flexcan_mb_21 ={v} flexcan_mb_config_24;
  # DEBUG BEGIN_STMT
  uS2Ticks_27 = OsIf_MicrosToTicks (100, 0);
  # DEBUG uS2Ticks => uS2Ticks_27
  # DEBUG BEGIN_STMT
  _3 = OsIf_GetCounter (0);
  timeStart = _3;
  # DEBUG BEGIN_STMT
  goto <bb 4>; [100.00%]

  <bb 3> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _32 = OsIf_GetElapsed (&timeStart, 0);
  timeElapsed_33 = timeElapsed_11 + _32;
  # DEBUG timeElapsed => timeElapsed_33
  # DEBUG BEGIN_STMT
  if (uS2Ticks_27 <= timeElapsed_33)
    goto <bb 5>; [5.50%]
  else
    goto <bb 11>; [94.50%]

  <bb 11> [local count: 958878293]:

  <bb 4> [local count: 1073741824]:
  # timeElapsed_11 = PHI <0(2), timeElapsed_33(11)>
  # DEBUG timeElapsed => timeElapsed_11
  # DEBUG BEGIN_STMT
  _4 = FlexCAN_GetBuffStatusFlag (pBase_16, _2);
  if (_4 == 0)
    goto <bb 3>; [94.50%]
  else
    goto <bb 5>; [5.50%]

  <bb 5> [local count: 114863532]:
  # result_8 = PHI <3(3), 0(4)>
  # DEBUG result => result_8
  # DEBUG BEGIN_STMT
  if (result_8 != 3)
    goto <bb 6>; [66.00%]
  else
    goto <bb 10>; [34.00%]

  <bb 6> [local count: 75809931]:
  # DEBUG BEGIN_STMT
  flexcan_mb_config_34 ={v} *flexcan_mb_21;
  # DEBUG flexcan_mb_config => flexcan_mb_config_34
  # DEBUG BEGIN_STMT
  _5 = flexcan_mb_config_34 >> 24;
  _6 = _5 & 15;
  if (_6 == 8)
    goto <bb 7>; [34.00%]
  else
    goto <bb 8>; [66.00%]

  <bb 7> [local count: 25775377]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 5

  <bb 8> [local count: 75809931]:
  # result_9 = PHI <result_8(6), 5(7)>
  # DEBUG result => result_9
  # DEBUG BEGIN_STMT
  if (_6 == 9)
    goto <bb 9>; [34.00%]
  else
    goto <bb 10>; [66.00%]

  <bb 9> [local count: 25775377]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0

  <bb 10> [local count: 114863532]:
  # result_10 = PHI <result_8(5), result_9(8), 0(9)>
  # DEBUG result => result_10
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (pBase_16, _2);
  # DEBUG BEGIN_STMT
  _7 = (int) mb_idx_19(D);
  state_17->mbs[_7].state ={v} 0;
  # DEBUG BEGIN_STMT
  timeStart ={v} {CLOBBER};
  return result_10;

}


FlexCAN_IRQHandlerEnhancedRxFIFO (uint8 instance, uint32 intType)
{
  struct Flexcan_Ip_MsgBuffType data;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  int _1;
  <unnamed type> _2;
  struct Flexcan_Ip_MsgBuffType * _3;
  struct Flexcan_Ip_MsgBuffType * _4;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _5;
  <unnamed type> _6;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _7;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _8;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _9;
  long unsigned int _27;
  long unsigned int _28;
  long unsigned int _29;
  long unsigned int _30;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_13(D);
  base_15 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_15
  # DEBUG BEGIN_STMT
  state_16 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_16
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  switch (intType_17(D)) <default: <L20> [20.00%], case 28: <L0> [20.00%], case 29: <L21> [20.00%], case 30: <L22> [20.00%], case 31: <L23> [20.00%]>

  <bb 3> [local count: 214748365]:
<L0>:
  # DEBUG BEGIN_STMT
  _2 ={v} state_16->enhancedFifoOutput.state;
  if (_2 == 1)
    goto <bb 4>; [34.00%]
  else
    goto <bb 16>; [66.00%]

  <bb 4> [local count: 73014444]:
  # DEBUG BEGIN_STMT
  _3 = state_16->enhancedFifoOutput.pMBmessage;
  if (_3 == 0B)
    goto <bb 5>; [30.00%]
  else
    goto <bb 6>; [70.00%]

  <bb 5> [local count: 21904333]:
  # DEBUG BEGIN_STMT
  state_16->enhancedFifoOutput.pMBmessage = &data;

  <bb 6> [local count: 73014444]:
  # DEBUG BEGIN_STMT
  _4 = state_16->enhancedFifoOutput.pMBmessage;
  FlexCAN_ReadEnhancedRxFifo (base_15, _4);
  # DEBUG BEGIN_STMT
  # DEBUG base => base_15
  # DEBUG intFlag => intType_17(D)
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  _27 = 1 << intType_17(D);
  base_15->ERFSR ={v} _27;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG BEGIN_STMT
  # DEBUG base => base_15
  # DEBUG intFlag => 29
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  base_15->ERFSR ={v} 536870912;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG BEGIN_STMT
  # DEBUG base => base_15
  # DEBUG intFlag => 30
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  base_15->ERFSR ={v} 1073741824;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG BEGIN_STMT
  state_16->enhancedFifoOutput.state ={v} 0;
  # DEBUG BEGIN_STMT
  _5 = state_16->callback;
  if (_5 != 0B)
    goto <bb 7>; [70.00%]
  else
    goto <bb 8>; [30.00%]

  <bb 7> [local count: 51110111]:
  # DEBUG BEGIN_STMT
  _5 (instance_13(D), 5, 255, state_16);

  <bb 8> [local count: 73014444]:
  # DEBUG BEGIN_STMT
  _6 ={v} state_16->enhancedFifoOutput.state;
  if (_6 == 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 16>; [67.00%]

  <bb 9> [local count: 24094767]:
  # DEBUG BEGIN_STMT
  FlexCAN_CompleteRxMessageEnhancedFifoData (instance_13(D));
  goto <bb 16>; [100.00%]

  <bb 10> [local count: 214748365]:
<L21>:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_15
  # DEBUG intFlag => intType_17(D)
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  _28 = 1 << intType_17(D);
  base_15->ERFSR ={v} _28;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG BEGIN_STMT
  _7 = state_16->callback;
  if (_7 != 0B)
    goto <bb 11>; [70.00%]
  else
    goto <bb 16>; [30.00%]

  <bb 11> [local count: 150323855]:
  # DEBUG BEGIN_STMT
  _7 (instance_13(D), 6, 255, state_16);
  goto <bb 16>; [100.00%]

  <bb 12> [local count: 214748365]:
<L22>:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_15
  # DEBUG intFlag => intType_17(D)
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  _29 = 1 << intType_17(D);
  base_15->ERFSR ={v} _29;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG BEGIN_STMT
  _8 = state_16->callback;
  if (_8 != 0B)
    goto <bb 13>; [70.00%]
  else
    goto <bb 16>; [30.00%]

  <bb 13> [local count: 150323855]:
  # DEBUG BEGIN_STMT
  _8 (instance_13(D), 7, 255, state_16);
  goto <bb 16>; [100.00%]

  <bb 14> [local count: 214748365]:
<L23>:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_15
  # DEBUG intFlag => intType_17(D)
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  _30 = 1 << intType_17(D);
  base_15->ERFSR ={v} _30;
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG BEGIN_STMT
  _9 = state_16->callback;
  if (_9 != 0B)
    goto <bb 15>; [70.00%]
  else
    goto <bb 16>; [30.00%]

  <bb 15> [local count: 150323855]:
  # DEBUG BEGIN_STMT
  _9 (instance_13(D), 8, 255, state_16);

  <bb 16> [local count: 1073741824]:
<L20>:
  data ={v} {CLOBBER};
  return;

}


FlexCAN_ProcessIRQHandlerEnhancedRxFIFO (uint8 u8Instance, boolean bIsSpuriousIntPrevious)
{
  boolean bIsSpuriousInt;
  uint32 u32intType;
  const struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  int _1;
  unsigned char _3;
  unsigned char _4;
  _Bool _5;
  long unsigned int _20;

  <bb 2> [local count: 214748364]:
  # DEBUG BEGIN_STMT
  _1 = (int) u8Instance_11(D);
  base_13 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_13
  # DEBUG BEGIN_STMT
  state_14 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_14
  # DEBUG BEGIN_STMT
  # DEBUG u32intType => 0
  # DEBUG BEGIN_STMT
  # DEBUG bIsSpuriousInt => bIsSpuriousIntPrevious_15(D)
  # DEBUG BEGIN_STMT
  # DEBUG u32intType => 31
  goto <bb 10>; [100.00%]

  <bb 3> [local count: 858993459]:
  # DEBUG BEGIN_STMT
  _3 = FlexCAN_GetEnhancedRxFIFOStatusFlag (base_13, u32intType_6);
  if (_3 != 0)
    goto <bb 4>; [33.00%]
  else
    goto <bb 9>; [67.00%]

  <bb 4> [local count: 283467841]:
  # DEBUG BEGIN_STMT
  _4 = FlexCAN_GetEnhancedRxFIFOIntStatusFlag (base_13, u32intType_6);
  if (_4 != 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 93544388]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerEnhancedRxFIFO (u8Instance_11(D), u32intType_6);
  # DEBUG BEGIN_STMT
  # DEBUG bIsSpuriousInt => 0
  goto <bb 9>; [100.00%]

  <bb 6> [local count: 189923454]:
  # DEBUG BEGIN_STMT
  if (bIsSpuriousInt_8 != 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 7> [local count: 94961727]:
  _5 = state_14->enhancedFifoOutput.isPolling;
  if (_5 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 47480863]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_13
  # DEBUG intFlag => u32intType_6
  # DEBUG INLINE_ENTRY FlexCAN_ClearEnhancedRxFifoIntStatusFlag
  # DEBUG BEGIN_STMT
  _20 = 1 << u32intType_6;
  base_13->ERFSR ={v} _20;

  <bb 9> [local count: 858993459]:
  # bIsSpuriousInt_7 = PHI <bIsSpuriousInt_8(3), 0(5), bIsSpuriousInt_8(6), 1(7), 1(8)>
  # DEBUG base => NULL
  # DEBUG intFlag => NULL
  # DEBUG bIsSpuriousInt => bIsSpuriousInt_7
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  u32intType_19 = u32intType_6 + 4294967295;
  # DEBUG u32intType => u32intType_19

  <bb 10> [local count: 1073741824]:
  # u32intType_6 = PHI <31(2), u32intType_19(9)>
  # bIsSpuriousInt_8 = PHI <bIsSpuriousIntPrevious_15(D)(2), bIsSpuriousInt_7(9)>
  # DEBUG bIsSpuriousInt => bIsSpuriousInt_8
  # DEBUG u32intType => u32intType_6
  # DEBUG BEGIN_STMT
  if (u32intType_6 > 27)
    goto <bb 3>; [80.00%]
  else
    goto <bb 11>; [20.00%]

  <bb 11> [local count: 214748365]:
  # bIsSpuriousInt_2 = PHI <bIsSpuriousInt_8(10)>
  # DEBUG BEGIN_STMT
  return bIsSpuriousInt_2;

}


FlexCAN_ProcessSpuriousInterruptMB (uint8 instance, uint32 startMbIdx, uint32 endMbIdx)
{
  uint32 u32MbHandle;
  uint32 mb_idx;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  int _1;
  unsigned char _2;
  unsigned char _3;
  _Bool _4;
  _Bool _5;
  <unnamed type> _6;

  <bb 2> [local count: 118111602]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_11(D);
  base_13 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_13
  # DEBUG BEGIN_STMT
  state_14 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_14
  # DEBUG BEGIN_STMT
  # DEBUG mb_idx => 0
  # DEBUG BEGIN_STMT
  # DEBUG u32MbHandle => 0
  # DEBUG BEGIN_STMT
  # DEBUG mb_idx => startMbIdx_15(D)
  goto <bb 12>; [100.00%]

  <bb 3> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  _2 = FlexCAN_GetBuffStatusFlag (base_13, mb_idx_7);
  if (_2 != 0)
    goto <bb 4>; [33.00%]
  else
    goto <bb 11>; [67.00%]

  <bb 4> [local count: 315357973]:
  _3 = FlexCAN_GetBuffStatusImask (base_13, mb_idx_7);
  if (_3 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 5> [local count: 157678987]:
  # DEBUG BEGIN_STMT
  # DEBUG u32MbHandle => mb_idx_7
  # DEBUG BEGIN_STMT
  _4 = state_14->bIsLegacyFifoEn;
  if (_4 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 6> [local count: 78839493]:
  if (mb_idx_7 <= 7)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 39419747]:
  # DEBUG BEGIN_STMT
  # DEBUG u32MbHandle => 0

  <bb 8> [local count: 157678987]:
  # u32MbHandle_8 = PHI <mb_idx_7(5), mb_idx_7(6), 0(7)>
  # DEBUG u32MbHandle => u32MbHandle_8
  # DEBUG BEGIN_STMT
  _5 = state_14->mbs[u32MbHandle_8].isPolling;
  if (_5 != 0)
    goto <bb 11>; [67.00%]
  else
    goto <bb 9>; [33.00%]

  <bb 9> [local count: 52034066]:
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_13, mb_idx_7);
  # DEBUG BEGIN_STMT
  _6 ={v} state_14->mbs[u32MbHandle_8].state;
  if (_6 == 2)
    goto <bb 10>; [34.00%]
  else
    goto <bb 11>; [66.00%]

  <bb 10> [local count: 17691582]:
  # DEBUG BEGIN_STMT
  state_14->mbs[u32MbHandle_8].state ={v} 0;
  # DEBUG BEGIN_STMT
  state_14->mbs[u32MbHandle_8].isPolling = 1;

  <bb 11> [local count: 955630223]:
  # DEBUG BEGIN_STMT
  mb_idx_22 = mb_idx_7 + 1;
  # DEBUG mb_idx => mb_idx_22

  <bb 12> [local count: 1073741824]:
  # mb_idx_7 = PHI <startMbIdx_15(D)(2), mb_idx_22(11)>
  # DEBUG mb_idx => mb_idx_7
  # DEBUG BEGIN_STMT
  if (mb_idx_7 <= endMbIdx_16(D))
    goto <bb 3>; [89.00%]
  else
    goto <bb 13>; [11.00%]

  <bb 13> [local count: 118111601]:
  return;

}


FlexCAN_IRQHandlerRxFIFO (uint8 instance, uint32 mb_idx)
{
  struct Flexcan_Ip_MsgBuffType data;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  int _1;
  struct Flexcan_Ip_MsgBuffType * _2;
  <unnamed type> _3;
  struct Flexcan_Ip_MsgBuffType * _4;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _5;
  <unnamed type> _6;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _7;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _8;

  <bb 2> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_12(D);
  base_14 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_14
  # DEBUG BEGIN_STMT
  state_15 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_15
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _2 = state_15->mbs[0].pMBmessage;
  if (_2 == 0B)
    goto <bb 3>; [30.00%]
  else
    goto <bb 4>; [70.00%]

  <bb 3> [local count: 322122547]:
  # DEBUG BEGIN_STMT
  state_15->mbs[0].pMBmessage = &data;

  <bb 4> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  switch (mb_idx_17(D)) <default: <L17> [25.00%], case 5: <L2> [25.00%], case 6: <L9> [25.00%], case 7: <L12> [25.00%]>

  <bb 5> [local count: 268435456]:
<L2>:
  # DEBUG BEGIN_STMT
  _3 ={v} state_15->mbs[0].state;
  if (_3 == 1)
    goto <bb 6>; [20.24%]
  else
    goto <bb 14>; [79.76%]

  <bb 6> [local count: 54331336]:
  # DEBUG BEGIN_STMT
  _4 = state_15->mbs[0].pMBmessage;
  FlexCAN_ReadRxFifo (base_14, _4);
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_14, mb_idx_17(D));
  # DEBUG BEGIN_STMT
  state_15->mbs[0].state ={v} 0;
  # DEBUG BEGIN_STMT
  _5 = state_15->callback;
  if (_5 != 0B)
    goto <bb 7>; [70.00%]
  else
    goto <bb 8>; [30.00%]

  <bb 7> [local count: 38031935]:
  # DEBUG BEGIN_STMT
  _5 (instance_12(D), 1, 0, state_15);

  <bb 8> [local count: 54331336]:
  # DEBUG BEGIN_STMT
  _6 ={v} state_15->mbs[0].state;
  if (_6 == 0)
    goto <bb 9>; [33.00%]
  else
    goto <bb 14>; [67.00%]

  <bb 9> [local count: 17929341]:
  # DEBUG BEGIN_STMT
  state_15->mbs[0].isPolling = 1;
  # DEBUG BEGIN_STMT
  FlexCAN_CompleteRxMessageFifoData (instance_12(D));
  goto <bb 14>; [100.00%]

  <bb 10> [local count: 268435456]:
<L9>:
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_14, mb_idx_17(D));
  # DEBUG BEGIN_STMT
  _7 = state_15->callback;
  if (_7 != 0B)
    goto <bb 11>; [70.00%]
  else
    goto <bb 14>; [30.00%]

  <bb 11> [local count: 187904819]:
  # DEBUG BEGIN_STMT
  _7 (instance_12(D), 2, 0, state_15);
  goto <bb 14>; [100.00%]

  <bb 12> [local count: 268435456]:
<L12>:
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_14, mb_idx_17(D));
  # DEBUG BEGIN_STMT
  _8 = state_15->callback;
  if (_8 != 0B)
    goto <bb 13>; [70.00%]
  else
    goto <bb 14>; [30.00%]

  <bb 13> [local count: 187904819]:
  # DEBUG BEGIN_STMT
  _8 (instance_12(D), 3, 0, state_15);

  <bb 14> [local count: 1073741824]:
<L17>:
  data ={v} {CLOBBER};
  return;

}


FlexCAN_IRQHandlerTxMB (uint8 u8Instance, uint32 u32MbIdx)
{
  boolean bCurrentIntStat;
  struct Flexcan_Ip_MsgBuffType mb;
  struct Flexcan_Ip_StateType * pState;
  struct FLEXCAN_Type * pBase;
  int _1;
  _Bool _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _8;
  <unnamed type> _9;
  _Bool _10;
  _Bool _11;
  _Bool _12;
  _Bool _13;
  long unsigned int vol.5_36;
  long unsigned int vol.5_37;

  <bb 2> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  _1 = (int) u8Instance_17(D);
  pBase_19 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_19
  # DEBUG BEGIN_STMT
  pState_20 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG pState => pState_20
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG bCurrentIntStat => 0
  # DEBUG BEGIN_STMT
  _2 = pState_20->mbs[u32MbIdx_21(D)].isRemote;
  if (_2 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870911]:
  # DEBUG BEGIN_STMT
  FlexCAN_LockRxMsgBuff (pBase_19, u32MbIdx_21(D));
  # DEBUG BEGIN_STMT
  FlexCAN_GetMsgBuff (pBase_19, u32MbIdx_21(D), &mb);
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_19
  # DEBUG INLINE_ENTRY FlexCAN_UnlockRxMsgBuff
  # DEBUG BEGIN_STMT
  vol.5_36 ={v} MEM[(const struct FLEXCAN_Type *)pBase_19].TIMER;
  # DEBUG base => NULL
  # DEBUG BEGIN_STMT
  _3 = mb.time_stamp;
  pState_20->mbs[u32MbIdx_21(D)].time_stamp = _3;
  # DEBUG BEGIN_STMT
  _4 = mb.cs;
  _5 = _4 >> 24;
  _6 = _5 & 15;
  if (_6 == 4)
    goto <bb 4>; [20.24%]
  else
    goto <bb 6>; [79.76%]

  <bb 4> [local count: 108662672]:
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (pBase_19, u32MbIdx_21(D));
  goto <bb 6>; [100.00%]

  <bb 5> [local count: 536870911]:
  # DEBUG BEGIN_STMT
  _7 = FlexCAN_GetMsgBuffTimestamp (pBase_19, u32MbIdx_21(D));
  pState_20->mbs[u32MbIdx_21(D)].time_stamp = _7;
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_19
  # DEBUG INLINE_ENTRY FlexCAN_UnlockRxMsgBuff
  # DEBUG BEGIN_STMT
  vol.5_37 ={v} MEM[(const struct FLEXCAN_Type *)pBase_19].TIMER;
  # DEBUG base => NULL
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (pBase_19, u32MbIdx_21(D));

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  pState_20->mbs[u32MbIdx_21(D)].state ={v} 0;
  # DEBUG BEGIN_STMT
  bCurrentIntStat_30 = pState_20->mbs[u32MbIdx_21(D)].isPolling;
  # DEBUG bCurrentIntStat => bCurrentIntStat_30
  # DEBUG BEGIN_STMT
  _8 = pState_20->callback;
  if (_8 != 0B)
    goto <bb 7>; [70.00%]
  else
    goto <bb 8>; [30.00%]

  <bb 7> [local count: 751619278]:
  # DEBUG BEGIN_STMT
  _8 (u8Instance_17(D), 4, u32MbIdx_21(D), pState_20);

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _9 ={v} pState_20->mbs[u32MbIdx_21(D)].state;
  if (_9 == 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 9> [local count: 536870913]:
  _10 = pState_20->mbs[u32MbIdx_21(D)].isPolling;
  if (_10 != 0)
    goto <bb 11>; [67.00%]
  else
    goto <bb 10>; [33.00%]

  <bb 10> [local count: 177167401]:
  # DEBUG BEGIN_STMT
  pState_20->mbs[u32MbIdx_21(D)].isPolling = 1;
  # DEBUG BEGIN_STMT
  _11 = pState_20->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (pBase_19, u8Instance_17(D), u32MbIdx_21(D), 0, _11);
  goto <bb 14>; [100.00%]

  <bb 11> [local count: 896574424]:
  # DEBUG BEGIN_STMT
  if (bCurrentIntStat_30 != 0)
    goto <bb 14>; [50.00%]
  else
    goto <bb 12>; [50.00%]

  <bb 12> [local count: 448287211]:
  _12 = pState_20->mbs[u32MbIdx_21(D)].isPolling;
  if (_12 != 0)
    goto <bb 13>; [33.00%]
  else
    goto <bb 14>; [67.00%]

  <bb 13> [local count: 147934780]:
  # DEBUG BEGIN_STMT
  _13 = pState_20->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (pBase_19, u8Instance_17(D), u32MbIdx_21(D), 0, _13);

  <bb 14> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  mb ={v} {CLOBBER};
  return;

}


FlexCAN_IRQHandlerRxMB (uint8 instance, uint32 mb_idx)
{
  boolean bCurrentIntStat;
  struct Flexcan_Ip_MsgBuffType data;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  int _1;
  struct Flexcan_Ip_MsgBuffType * _2;
  struct Flexcan_Ip_MsgBuffType * _3;
  void (*<T33b>) (uint8, Flexcan_Ip_EventType, uint32, const struct FlexCANState *) _4;
  <unnamed type> _5;
  _Bool _6;
  _Bool _7;
  _Bool _8;
  _Bool _9;
  long unsigned int vol.5_29;

  <bb 2> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_13(D);
  base_15 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_15
  # DEBUG BEGIN_STMT
  state_16 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_16
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG bCurrentIntStat => 0
  # DEBUG BEGIN_STMT
  _2 = state_16->mbs[mb_idx_17(D)].pMBmessage;
  if (_2 == 0B)
    goto <bb 3>; [30.00%]
  else
    goto <bb 4>; [70.00%]

  <bb 3> [local count: 322122547]:
  # DEBUG BEGIN_STMT
  state_16->mbs[mb_idx_17(D)].pMBmessage = &data;

  <bb 4> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  FlexCAN_LockRxMsgBuff (base_15, mb_idx_17(D));
  # DEBUG BEGIN_STMT
  _3 = state_16->mbs[mb_idx_17(D)].pMBmessage;
  FlexCAN_GetMsgBuff (base_15, mb_idx_17(D), _3);
  # DEBUG BEGIN_STMT
  FlexCAN_ClearMsgBuffIntStatusFlag (base_15, mb_idx_17(D));
  # DEBUG BEGIN_STMT
  # DEBUG base => base_15
  # DEBUG INLINE_ENTRY FlexCAN_UnlockRxMsgBuff
  # DEBUG BEGIN_STMT
  vol.5_29 ={v} MEM[(const struct FLEXCAN_Type *)base_15].TIMER;
  # DEBUG base => NULL
  # DEBUG BEGIN_STMT
  state_16->mbs[mb_idx_17(D)].state ={v} 0;
  # DEBUG BEGIN_STMT
  bCurrentIntStat_23 = state_16->mbs[mb_idx_17(D)].isPolling;
  # DEBUG bCurrentIntStat => bCurrentIntStat_23
  # DEBUG BEGIN_STMT
  _4 = state_16->callback;
  if (_4 != 0B)
    goto <bb 5>; [70.00%]
  else
    goto <bb 6>; [30.00%]

  <bb 5> [local count: 751619277]:
  # DEBUG BEGIN_STMT
  _4 (instance_13(D), 0, mb_idx_17(D), state_16);

  <bb 6> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  _5 ={v} state_16->mbs[mb_idx_17(D)].state;
  if (_5 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 7> [local count: 536870911]:
  _6 = state_16->mbs[mb_idx_17(D)].isPolling;
  if (_6 != 0)
    goto <bb 9>; [67.00%]
  else
    goto <bb 8>; [33.00%]

  <bb 8> [local count: 177167401]:
  # DEBUG BEGIN_STMT
  state_16->mbs[mb_idx_17(D)].isPolling = 1;
  # DEBUG BEGIN_STMT
  _7 = state_16->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (base_15, instance_13(D), mb_idx_17(D), 0, _7);
  goto <bb 12>; [100.00%]

  <bb 9> [local count: 896574422]:
  # DEBUG BEGIN_STMT
  if (bCurrentIntStat_23 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 10> [local count: 448287211]:
  _8 = state_16->mbs[mb_idx_17(D)].isPolling;
  if (_8 != 0)
    goto <bb 11>; [33.00%]
  else
    goto <bb 12>; [67.00%]

  <bb 11> [local count: 147934780]:
  # DEBUG BEGIN_STMT
  _9 = state_16->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (base_15, instance_13(D), mb_idx_17(D), 0, _9);

  <bb 12> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  data ={v} {CLOBBER};
  return;

}


FlexCAN_StartRxMessageFifoData (uint8 instance, struct Flexcan_Ip_MsgBuffType * data)
{
  volatile boolean x;
  Flexcan_Ip_StatusType eResult;
  _Bool _1;
  _Bool x.0_7;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG base => 0B
  # DEBUG BEGIN_STMT
  # DEBUG state => 0B
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 0
  # DEBUG BEGIN_STMT
  _1 = instance_4(D) <= 5;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_7 ={v} x;
  if (x.0_7 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  eResult_3 = FlexCAN_StartRxMessageFifoData.part.0 (instance_4(D), data_6(D));
  # DEBUG eResult => eResult_3
  # DEBUG BEGIN_STMT
  return eResult_3;

}


FlexCAN_StartSendData (uint8 Flexcan_Ip_u8Instance, uint8 mb_idx, const struct Flexcan_Ip_DataInfoType * tx_info, uint32 msg_id, const uint8 * mb_data)
{
  volatile boolean x;
  volatile boolean x;
  struct FLEXCAN_Type * base;
  struct Flexcan_Ip_StateType * state;
  struct Flexcan_Ip_MsbuffCodeStatusType cs;
  Flexcan_Ip_StatusType eResult;
  int _1;
  _Bool _2;
  _Bool _3;
  _Bool _4;
  long unsigned int _5;
  _Bool _6;
  int _7;
  <unnamed type> _8;
  long unsigned int _9;
  _Bool _10;
  _Bool _11;
  long unsigned int _12;
  <unnamed type> _13;
  _Bool _14;
  unsigned char _15;
  _Bool _16;
  _Bool x.0_43;
  _Bool x.0_44;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = (int) Flexcan_Ip_u8Instance_20(D);
  state_22 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_22
  # DEBUG BEGIN_STMT
  base_23 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_23
  # DEBUG BEGIN_STMT
  _2 = Flexcan_Ip_u8Instance_20(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_44 ={v} x;
  if (x.0_44 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 14>; [50.00%]

  <bb 14> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 16> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = tx_info_24(D) != 0B;
  x ={v} _3;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_43 ={v} x;
  if (x.0_43 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 13> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 15> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _4 = state_22->bIsLegacyFifoEn;
  _5 = state_22->u32MaxMbNum;
  _6 = FlexCAN_IsMbOutOfRange (base_23, mb_idx_25(D), _4, _5);
  if (_6 != 0)
    goto <bb 12>; [35.00%]
  else
    goto <bb 7>; [65.00%]

  <bb 7> [local count: 34897]:
  # DEBUG BEGIN_STMT
  _7 = (int) mb_idx_25(D);
  _8 ={v} state_22->mbs[_7].state;
  if (_8 != 0)
    goto <bb 12>; [52.23%]
  else
    goto <bb 8>; [47.77%]

  <bb 8> [local count: 16670]:
  # DEBUG BEGIN_STMT
  _9 = (long unsigned int) mb_idx_25(D);
  FlexCAN_ClearMsgBuffIntStatusFlag (base_23, _9);
  # DEBUG BEGIN_STMT
  state_22->mbs[_7].state ={v} 2;
  # DEBUG BEGIN_STMT
  state_22->mbs[_7].time_stamp = 0;
  # DEBUG BEGIN_STMT
  _10 = tx_info_24(D)->is_polling;
  state_22->mbs[_7].isPolling = _10;
  # DEBUG BEGIN_STMT
  _11 = tx_info_24(D)->is_remote;
  state_22->mbs[_7].isRemote = _11;
  # DEBUG BEGIN_STMT
  _12 = tx_info_24(D)->data_length;
  cs.dataLen = _12;
  # DEBUG BEGIN_STMT
  _13 = tx_info_24(D)->msg_id_type;
  cs.msgIdType = _13;
  # DEBUG BEGIN_STMT
  _14 = tx_info_24(D)->fd_enable;
  cs.fd_enable = _14;
  # DEBUG BEGIN_STMT
  _15 = tx_info_24(D)->fd_padding;
  cs.fd_padding = _15;
  # DEBUG BEGIN_STMT
  _16 = tx_info_24(D)->enable_brs;
  cs.enable_brs = _16;
  # DEBUG BEGIN_STMT
  if (_11 != 0)
    goto <bb 9>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 9> [local count: 8335]:
  # DEBUG BEGIN_STMT
  cs.code = 28;
  goto <bb 11>; [100.00%]

  <bb 10> [local count: 8335]:
  # DEBUG BEGIN_STMT
  cs.code = 12;

  <bb 11> [local count: 16670]:
  # DEBUG BEGIN_STMT
  FlexCAN_SetTxMsgBuff (base_23, _9, &cs, msg_id_39(D), mb_data_40(D), 0);

  <bb 12> [local count: 53687]:
  # eResult_17 = PHI <4(6), 2(7), 0(11)>
  # DEBUG eResult => eResult_17
  # DEBUG BEGIN_STMT
  cs ={v} {CLOBBER};
  return eResult_17;

}


FlexCAN_StartRxMessageBufferData (uint8 instance, uint8 mb_idx, struct Flexcan_Ip_MsgBuffType * data, boolean isPolling)
{
  volatile boolean x;
  struct Flexcan_Ip_StateType * state;
  const struct FLEXCAN_Type * base;
  Flexcan_Ip_StatusType result;
  int _1;
  _Bool _2;
  _Bool _3;
  long unsigned int _4;
  _Bool _5;
  int _6;
  <unnamed type> _7;
  _Bool x.0_21;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  # DEBUG result => 0
  # DEBUG BEGIN_STMT
  _1 = (int) instance_10(D);
  base_12 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_12
  # DEBUG BEGIN_STMT
  state_13 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_13
  # DEBUG BEGIN_STMT
  _2 = instance_10(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_21 ={v} x;
  if (x.0_21 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 8> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 9> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = state_13->bIsLegacyFifoEn;
  _4 = state_13->u32MaxMbNum;
  _5 = FlexCAN_IsMbOutOfRange (base_12, mb_idx_14(D), _3, _4);
  if (_5 != 0)
    goto <bb 7>; [35.00%]
  else
    goto <bb 5>; [65.00%]

  <bb 5> [local count: 69793]:
  # DEBUG BEGIN_STMT
  _6 = (int) mb_idx_14(D);
  _7 ={v} state_13->mbs[_6].state;
  if (_7 != 0)
    goto <bb 7>; [35.00%]
  else
    goto <bb 6>; [65.00%]

  <bb 6> [local count: 45366]:
  # DEBUG BEGIN_STMT
  state_13->mbs[_6].state ={v} 1;
  # DEBUG BEGIN_STMT
  state_13->mbs[_6].pMBmessage = data_17(D);
  # DEBUG BEGIN_STMT
  state_13->mbs[_6].isPolling = isPolling_19(D);

  <bb 7> [local count: 107374]:
  # result_8 = PHI <4(4), 2(5), 0(6)>
  # DEBUG result => result_8
  # DEBUG BEGIN_STMT
  return result_8;

}


FlexCAN_ProccessLegacyRxFIFO (uint8 u8Instance, uint32 u32TimeoutMs)
{
  uint32 u32intType;
  uint32 mS2Ticks;
  uint32 timeElapsed;
  uint32 timeStart;
  struct FLEXCAN_Type * pBase;
  struct Flexcan_Ip_StateType * pState;
  Flexcan_Ip_StatusType eResult;
  int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  unsigned char _5;
  <unnamed type> _6;
  <unnamed type> _7;
  _Bool _8;
  _Bool _9;
  _Bool _10;
  <unnamed type> _11;
  long unsigned int _37;

  <bb 2> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 0
  # DEBUG BEGIN_STMT
  _1 = (int) u8Instance_23(D);
  pState_25 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG pState => pState_25
  # DEBUG BEGIN_STMT
  pBase_26 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_26
  # DEBUG BEGIN_STMT
  timeStart = 0;
  # DEBUG BEGIN_STMT
  # DEBUG timeElapsed => 0
  # DEBUG BEGIN_STMT
  _2 = u32TimeoutMs_28(D) * 1000;
  mS2Ticks_30 = OsIf_MicrosToTicks (_2, 0);
  # DEBUG mS2Ticks => mS2Ticks_30
  # DEBUG BEGIN_STMT
  # DEBUG u32intType => 0
  # DEBUG BEGIN_STMT
  _3 = OsIf_GetCounter (0);
  timeStart = _3;
  # DEBUG BEGIN_STMT
  goto <bb 9>; [100.00%]

  <bb 3> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _4 = pState_25->transferType;
  if (_4 == 1)
    goto <bb 17>; [16.00%]
  else
    goto <bb 8>; [84.00%]

  <bb 17> [local count: 162349764]:
  goto <bb 7>; [100.00%]

  <bb 4> [local count: 487049291]:
  # DEBUG BEGIN_STMT
  _5 = FlexCAN_GetBuffStatusFlag (pBase_26, u32intType_15);
  if (_5 != 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 160726266]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerRxFIFO (u8Instance_23(D), u32intType_15);

  <bb 6> [local count: 487049291]:
  # DEBUG BEGIN_STMT
  u32intType_35 = u32intType_15 + 4294967295;
  # DEBUG u32intType => u32intType_35

  <bb 7> [local count: 649399056]:
  # u32intType_15 = PHI <u32intType_35(6), 7(17)>
  # DEBUG u32intType => u32intType_15
  # DEBUG BEGIN_STMT
  if (u32intType_15 > 4)
    goto <bb 4>; [75.00%]
  else
    goto <bb 8>; [25.00%]

  <bb 8> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _37 = OsIf_GetElapsed (&timeStart, 0);
  timeElapsed_38 = timeElapsed_14 + _37;
  # DEBUG timeElapsed => timeElapsed_38
  # DEBUG BEGIN_STMT
  if (mS2Ticks_30 <= timeElapsed_38)
    goto <bb 10>; [5.50%]
  else
    goto <bb 18>; [94.50%]

  <bb 18> [local count: 958878293]:

  <bb 9> [local count: 1073741824]:
  # timeElapsed_14 = PHI <0(2), timeElapsed_38(18)>
  # DEBUG timeElapsed => timeElapsed_14
  # DEBUG BEGIN_STMT
  _6 ={v} pState_25->mbs[0].state;
  if (_6 == 1)
    goto <bb 3>; [94.50%]
  else
    goto <bb 10>; [5.50%]

  <bb 10> [local count: 114863532]:
  # eResult_12 = PHI <3(8), 0(9)>
  # DEBUG eResult => eResult_12
  # DEBUG BEGIN_STMT
  if (eResult_12 == 3)
    goto <bb 11>; [34.00%]
  else
    goto <bb 13>; [66.00%]

  <bb 11> [local count: 39053601]:
  _7 = pState_25->transferType;
  if (_7 != 1)
    goto <bb 12>; [48.88%]
  else
    goto <bb 13>; [51.12%]

  <bb 12> [local count: 19089400]:
  # DEBUG BEGIN_STMT
  _8 = pState_25->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (pBase_26, u8Instance_23(D), 5, 0, _8);
  # DEBUG BEGIN_STMT
  _9 = pState_25->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (pBase_26, u8Instance_23(D), 6, 0, _9);
  # DEBUG BEGIN_STMT
  _10 = pState_25->isIntActive;
  FlexCAN_SetMsgBuffIntCmd (pBase_26, u8Instance_23(D), 7, 0, _10);

  <bb 13> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  _11 ={v} pState_25->mbs[0].state;
  switch (_11) <default: <L18> [33.33%], case 0: <L22> [33.33%], case 1: <L16> [33.33%]>

  <bb 14> [local count: 38284015]:
<L16>:
  # DEBUG BEGIN_STMT
  pState_25->mbs[0].state ={v} 0;
  # DEBUG BEGIN_STMT
  goto <bb 16>; [100.00%]

  <bb 15> [local count: 38284015]:
<L18>:
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 1
  # DEBUG BEGIN_STMT

  <bb 16> [local count: 114852045]:
  # eResult_13 = PHI <eResult_12(14), 0(13), 1(15)>
<L22>:
  # DEBUG eResult => eResult_13
  # DEBUG BEGIN_STMT
  timeStart ={v} {CLOBBER};
  return eResult_13;

}


FlexCAN_ProccessEnhancedRxFifo (uint8 u8Instance, uint32 u32TimeoutMs)
{
  uint32 u32intType;
  uint32 mS2Ticks;
  uint32 timeElapsed;
  uint32 timeStart;
  struct FLEXCAN_Type * pBase;
  struct Flexcan_Ip_StateType * pState;
  Flexcan_Ip_StatusType eResult;
  int _1;
  long unsigned int _2;
  long unsigned int _3;
  <unnamed type> _4;
  unsigned char _5;
  <unnamed type> _6;
  <unnamed type> _7;
  <unnamed type> _8;
  long unsigned int _34;
  long unsigned int _38;
  long unsigned int _39;

  <bb 2> [local count: 114863532]:
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 0
  # DEBUG BEGIN_STMT
  _1 = (int) u8Instance_20(D);
  pState_22 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG pState => pState_22
  # DEBUG BEGIN_STMT
  pBase_23 = g_Flexcan_Ip_aBase[_1];
  # DEBUG pBase => pBase_23
  # DEBUG BEGIN_STMT
  timeStart = 0;
  # DEBUG BEGIN_STMT
  # DEBUG timeElapsed => 0
  # DEBUG BEGIN_STMT
  _2 = u32TimeoutMs_25(D) * 1000;
  mS2Ticks_27 = OsIf_MicrosToTicks (_2, 0);
  # DEBUG mS2Ticks => mS2Ticks_27
  # DEBUG BEGIN_STMT
  # DEBUG u32intType => 0
  # DEBUG BEGIN_STMT
  _3 = OsIf_GetCounter (0);
  timeStart = _3;
  # DEBUG BEGIN_STMT
  goto <bb 9>; [100.00%]

  <bb 3> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _4 = pState_22->transferType;
  if (_4 == 1)
    goto <bb 17>; [16.00%]
  else
    goto <bb 8>; [84.00%]

  <bb 17> [local count: 162349764]:
  goto <bb 7>; [100.00%]

  <bb 4> [local count: 649399059]:
  # DEBUG BEGIN_STMT
  _5 = FlexCAN_GetEnhancedRxFIFOStatusFlag (pBase_23, u32intType_12);
  if (_5 != 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 214301689]:
  # DEBUG BEGIN_STMT
  FlexCAN_IRQHandlerEnhancedRxFIFO (u8Instance_20(D), u32intType_12);

  <bb 6> [local count: 649399059]:
  # DEBUG BEGIN_STMT
  u32intType_32 = u32intType_12 + 4294967295;
  # DEBUG u32intType => u32intType_32

  <bb 7> [local count: 811748823]:
  # u32intType_12 = PHI <u32intType_32(6), 31(17)>
  # DEBUG u32intType => u32intType_12
  # DEBUG BEGIN_STMT
  if (u32intType_12 > 27)
    goto <bb 4>; [80.00%]
  else
    goto <bb 8>; [20.00%]

  <bb 8> [local count: 1014686025]:
  # DEBUG BEGIN_STMT
  _34 = OsIf_GetElapsed (&timeStart, 0);
  timeElapsed_35 = timeElapsed_11 + _34;
  # DEBUG timeElapsed => timeElapsed_35
  # DEBUG BEGIN_STMT
  if (mS2Ticks_27 <= timeElapsed_35)
    goto <bb 10>; [5.50%]
  else
    goto <bb 18>; [94.50%]

  <bb 18> [local count: 958878293]:

  <bb 9> [local count: 1073741824]:
  # timeElapsed_11 = PHI <0(2), timeElapsed_35(18)>
  # DEBUG timeElapsed => timeElapsed_11
  # DEBUG BEGIN_STMT
  _6 ={v} pState_22->enhancedFifoOutput.state;
  if (_6 == 1)
    goto <bb 3>; [94.50%]
  else
    goto <bb 10>; [5.50%]

  <bb 10> [local count: 114863532]:
  # eResult_9 = PHI <3(8), 0(9)>
  # DEBUG eResult => eResult_9
  # DEBUG BEGIN_STMT
  if (eResult_9 == 3)
    goto <bb 11>; [34.00%]
  else
    goto <bb 13>; [66.00%]

  <bb 11> [local count: 39053601]:
  _7 = pState_22->transferType;
  if (_7 != 1)
    goto <bb 12>; [66.00%]
  else
    goto <bb 13>; [34.00%]

  <bb 12> [local count: 25775377]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_23
  # DEBUG enable => 0
  # DEBUG INLINE_ENTRY FlexCAN_SetEnhancedRxFifoIntAll
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _38 ={v} pBase_23->ERFIER;
  _39 = _38 & 268435455;
  pBase_23->ERFIER ={v} _39;

  <bb 13> [local count: 114863532]:
  # DEBUG base => NULL
  # DEBUG enable => NULL
  # DEBUG BEGIN_STMT
  _8 ={v} pState_22->enhancedFifoOutput.state;
  switch (_8) <default: <L18> [33.33%], case 0: <L22> [33.33%], case 1: <L16> [33.33%]>

  <bb 14> [local count: 38284015]:
<L16>:
  # DEBUG BEGIN_STMT
  pState_22->enhancedFifoOutput.state ={v} 0;
  # DEBUG BEGIN_STMT
  goto <bb 16>; [100.00%]

  <bb 15> [local count: 38284015]:
<L18>:
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 1
  # DEBUG BEGIN_STMT

  <bb 16> [local count: 114852045]:
  # eResult_10 = PHI <eResult_9(14), 0(13), 1(15)>
<L22>:
  # DEBUG eResult => eResult_10
  # DEBUG BEGIN_STMT
  timeStart ={v} {CLOBBER};
  return eResult_10;

}


FlexCAN_StartRxMessageEnhancedFifoData (uint8 instance, struct Flexcan_Ip_MsgBuffType * data)
{
  volatile boolean x;
  Flexcan_Ip_StatusType eResult;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  <unnamed type> _3;
  <unnamed type> _4;
  _Bool _5;
  _Bool x.0_18;
  long unsigned int _19;
  long unsigned int _20;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_9(D);
  base_11 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_11
  # DEBUG BEGIN_STMT
  state_12 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_12
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 0
  # DEBUG BEGIN_STMT
  _2 = instance_9(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_18 ={v} x;
  if (x.0_18 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 11>; [50.00%]

  <bb 11> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 12> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 ={v} state_12->enhancedFifoOutput.state;
  if (_3 == 1)
    goto <bb 10>; [21.72%]
  else
    goto <bb 5>; [78.28%]

  <bb 5> [local count: 84052]:
  # DEBUG BEGIN_STMT
  state_12->enhancedFifoOutput.state ={v} 1;
  # DEBUG BEGIN_STMT
  state_12->enhancedFifoOutput.pMBmessage = data_14(D);
  # DEBUG BEGIN_STMT
  _4 = state_12->transferType;
  if (_4 == 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 6> [local count: 42026]:
  # DEBUG BEGIN_STMT
  state_12->enhancedFifoOutput.isPolling = 0;
  # DEBUG BEGIN_STMT
  _5 = state_12->isIntActive;
  if (_5 != 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 21013]:
  # DEBUG BEGIN_STMT
  # DEBUG base => base_11
  # DEBUG enable => 1
  # DEBUG INLINE_ENTRY FlexCAN_SetEnhancedRxFifoIntAll
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _19 ={v} base_11->ERFIER;
  _20 = _19 | 4026531840;
  base_11->ERFIER ={v} _20;

  <bb 8> [local count: 84052]:
  # DEBUG base => NULL
  # DEBUG enable => NULL
  # DEBUG BEGIN_STMT
  if (_4 == 1)
    goto <bb 9>; [34.00%]
  else
    goto <bb 10>; [66.00%]

  <bb 9> [local count: 28578]:
  # DEBUG BEGIN_STMT
  state_12->enhancedFifoOutput.isPolling = 1;

  <bb 10> [local count: 107374]:
  # eResult_6 = PHI <2(4), 0(8), 0(9)>
  # DEBUG eResult => eResult_6
  # DEBUG BEGIN_STMT
  return eResult_6;

}


FlexCAN_CompleteRxMessageEnhancedFifoData (uint8 instance)
{
  volatile boolean x;
  volatile boolean x;
  struct Flexcan_Ip_StateType * state;
  struct FLEXCAN_Type * base;
  int _1;
  _Bool _2;
  _Bool _3;
  _Bool _4;
  _Bool x.0_14;
  _Bool x.0_15;
  long unsigned int _16;
  long unsigned int _17;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = (int) instance_6(D);
  base_8 = g_Flexcan_Ip_aBase[_1];
  # DEBUG base => base_8
  # DEBUG BEGIN_STMT
  state_9 = g_flexcan_Ip_StatePtr[_1];
  # DEBUG state => state_9
  # DEBUG BEGIN_STMT
  _2 = instance_6(D) <= 5;
  x ={v} _2;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_15 ={v} x;
  if (x.0_15 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 10>; [50.00%]

  <bb 10> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 12> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _3 = FlexCAN_IsEnhancedRxFifoAvailable (base_8);
  x ={v} _3;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_14 ={v} x;
  if (x.0_14 != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 9> [local count: 53687]:

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 11> [local count: 536870913]:
  goto <bb 5>; [100.00%]

  <bb 6> [local count: 53687]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  _4 = state_9->enhancedFifoOutput.isPolling;
  if (_4 != 0)
    goto <bb 8>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 7> [local count: 26844]:
  # DEBUG BEGIN_STMT
  state_9->enhancedFifoOutput.isPolling = 1;
  # DEBUG BEGIN_STMT
  # DEBUG base => base_8
  # DEBUG enable => 0
  # DEBUG INLINE_ENTRY FlexCAN_SetEnhancedRxFifoIntAll
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _16 ={v} base_8->ERFIER;
  _17 = _16 & 268435455;
  base_8->ERFIER ={v} _17;

  <bb 8> [local count: 53687]:
  # DEBUG base => NULL
  # DEBUG enable => NULL
  # DEBUG BEGIN_STMT
  state_9->enhancedFifoOutput.pMBmessage = 0B;
  # DEBUG BEGIN_STMT
  state_9->enhancedFifoOutput.state ={v} 0;
  return;

}


FlexCAN_InitController (struct FLEXCAN_Type * pBase, const struct Flexcan_Ip_ConfigType * Flexcan_Ip_pData)
{
  Flexcan_Ip_StatusType eResult;
  long unsigned int _1;
  long unsigned int _2;
  _Bool _3;
  _Bool _4;
  long unsigned int _5;
  <unnamed type> _6;
  const struct Flexcan_Ip_PayloadSizeType * _7;
  long unsigned int _8;
  long unsigned int _40;
  signed int _41;
  long unsigned int _42;
  long unsigned int _43;
  long unsigned int _44;

  <bb 2> [local count: 1073741823]:
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 0
  # DEBUG BEGIN_STMT
  # DEBUG pBase => pBase_15(D)
  # DEBUG INLINE_ENTRY FlexCAN_IsEnabled
  # DEBUG BEGIN_STMT
  _40 ={v} MEM[(const struct FLEXCAN_Type *)pBase_15(D)].MCR;
  _41 = (signed int) _40;
  # DEBUG pBase => NULL
  if (_41 >= 0)
    goto <bb 4>; [59.00%]
  else
    goto <bb 7>; [41.00%]

  <bb 4> [local count: 633507676]:
  # DEBUG BEGIN_STMT
  eResult_17 = FlexCAN_EnterFreezeMode (pBase_15(D));
  # DEBUG eResult => eResult_17
  # DEBUG BEGIN_STMT
  if (eResult_17 == 0)
    goto <bb 5>; [33.00%]
  else
    goto <bb 6>; [67.00%]

  <bb 5> [local count: 209057533]:
  # DEBUG BEGIN_STMT
  eResult_19 = FlexCAN_Disable (pBase_15(D));
  # DEBUG eResult => eResult_19

  <bb 6> [local count: 633507676]:
  # eResult_9 = PHI <eResult_19(5), eResult_17(4)>
  # DEBUG eResult => eResult_9
  # DEBUG BEGIN_STMT
  if (eResult_9 == 0)
    goto <bb 7>; [50.00%]
  else
    goto <bb 15>; [50.00%]

  <bb 7> [local count: 756987986]:
  # DEBUG eResult => NULL
  # DEBUG BEGIN_STMT
  SchM_Enter_Can_CAN_EXCLUSIVE_AREA_00 ();
  # DEBUG BEGIN_STMT
  _1 ={v} pBase_15(D)->MCR;
  _2 = _1 & 2147483647;
  pBase_15(D)->MCR ={v} _2;
  # DEBUG BEGIN_STMT
  SchM_Exit_Can_CAN_EXCLUSIVE_AREA_00 ();
  # DEBUG BEGIN_STMT
  eResult_24 = FlexCAN_Init (pBase_15(D));
  # DEBUG eResult => eResult_24
  # DEBUG BEGIN_STMT
  if (eResult_24 != 0)
    goto <bb 8>; [50.00%]
  else
    goto <bb 9>; [50.00%]

  <bb 8> [local count: 378493993]:
  # DEBUG BEGIN_STMT
  FlexCAN_EnterFreezeMode (pBase_15(D));
  # DEBUG BEGIN_STMT
  FlexCAN_Disable (pBase_15(D));
  goto <bb 15>; [100.00%]

  <bb 9> [local count: 378493993]:
  # DEBUG BEGIN_STMT
  FlexCAN_DisableMemErrorDetection (pBase_15(D));
  # DEBUG BEGIN_STMT
  _3 = Flexcan_Ip_pData_26(D)->fd_enable;
  _4 = Flexcan_Ip_pData_26(D)->bitRateSwitch;
  FlexCAN_SetFDEnabled (pBase_15(D), _3, _4);
  # DEBUG BEGIN_STMT
  _5 = Flexcan_Ip_pData_26(D)->ctrlOptions;
  FlexCAN_ConfigCtrlOptions (pBase_15(D), _5);
  # DEBUG BEGIN_STMT
  _6 = Flexcan_Ip_pData_26(D)->flexcanMode;
  if (_6 != 2)
    goto <bb 10>; [66.00%]
  else
    goto <bb 11>; [34.00%]

  <bb 10> [local count: 249806035]:
  # DEBUG BEGIN_STMT
  # DEBUG base => pBase_15(D)
  # DEBUG enable => 0
  # DEBUG INLINE_ENTRY FlexCAN_SetSelfReception
  # DEBUG BEGIN_STMT
  _42 ={v} pBase_15(D)->MCR;
  _43 = _42 & 4294836223;
  _44 = _43 | 131072;
  pBase_15(D)->MCR ={v} _44;

  <bb 11> [local count: 378493993]:
  # DEBUG base => NULL
  # DEBUG enable => NULL
  # DEBUG BEGIN_STMT
  eResult_30 = FlexCAN_InitRxFifo (pBase_15(D), Flexcan_Ip_pData_26(D));
  # DEBUG eResult => eResult_30
  # DEBUG BEGIN_STMT
  if (eResult_30 != 0)
    goto <bb 12>; [50.00%]
  else
    goto <bb 13>; [50.00%]

  <bb 12> [local count: 189246996]:
  # DEBUG BEGIN_STMT
  FlexCAN_EnterFreezeMode (pBase_15(D));
  # DEBUG BEGIN_STMT
  FlexCAN_Disable (pBase_15(D));
  goto <bb 15>; [100.00%]

  <bb 13> [local count: 189246996]:
  # DEBUG BEGIN_STMT
  _7 = &Flexcan_Ip_pData_26(D)->payload;
  FlexCAN_SetPayloadSize (pBase_15(D), _7);
  # DEBUG BEGIN_STMT
  _8 = Flexcan_Ip_pData_26(D)->max_num_mb;
  eResult_33 = FlexCAN_SetMaxMsgBuffNum (pBase_15(D), _8);
  # DEBUG eResult => eResult_33
  # DEBUG BEGIN_STMT
  if (eResult_33 != 0)
    goto <bb 14>; [33.00%]
  else
    goto <bb 15>; [67.00%]

  <bb 14> [local count: 62451509]:
  # DEBUG BEGIN_STMT
  FlexCAN_EnterFreezeMode (pBase_15(D));
  # DEBUG BEGIN_STMT
  FlexCAN_Disable (pBase_15(D));

  <bb 15> [local count: 1073741824]:
  # eResult_10 = PHI <eResult_9(6), eResult_24(8), eResult_30(12), eResult_33(13), eResult_33(14)>
  # DEBUG eResult => eResult_10
  # DEBUG BEGIN_STMT
  return eResult_10;

}


FlexCAN_InitRxFifo (struct FLEXCAN_Type * pBase, const struct Flexcan_Ip_ConfigType * Flexcan_Ip_pData)
{
  Flexcan_Ip_StatusType eResult;
  _Bool _1;
  <unnamed type> _2;
  long unsigned int _3;
  _Bool _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG eResult => 0
  # DEBUG BEGIN_STMT
  _1 = Flexcan_Ip_pData_11(D)->is_rx_fifo_needed;
  if (_1 != 0)
    goto <bb 4>; [33.00%]
  else
    goto <bb 5>; [67.00%]

  <bb 4> [local count: 354334802]:
  # DEBUG BEGIN_STMT
  _2 = Flexcan_Ip_pData_11(D)->num_id_filters;
  _3 = (long unsigned int) _2;
  eResult_14 = FlexCAN_EnableRxFifo (pBase_12(D), _3);
  # DEBUG eResult => eResult_14
  # DEBUG BEGIN_STMT
  if (eResult_14 == 0)
    goto <bb 5>; [50.00%]
  else
    goto <bb 7>; [50.00%]

  <bb 5> [local count: 896574424]:
  # eResult_17 = PHI <eResult_14(4), 0(2)>
  # DEBUG eResult => NULL
  _4 = Flexcan_Ip_pData_11(D)->is_enhanced_rx_fifo_needed;
  if (_4 != 0)
    goto <bb 6>; [33.00%]
  else
    goto <bb 7>; [67.00%]

  <bb 6> [local count: 295869560]:
  # DEBUG BEGIN_STMT
  _5 = Flexcan_Ip_pData_11(D)->num_enhanced_std_id_filters;
  _6 = Flexcan_Ip_pData_11(D)->num_enhanced_ext_id_filters;
  _7 = Flexcan_Ip_pData_11(D)->num_enhanced_watermark;
  eResult_16 = FlexCAN_EnableEnhancedRxFifo (pBase_12(D), _5, _6, _7);
  # DEBUG eResult => eResult_16

  <bb 7> [local count: 1073741824]:
  # eResult_8 = PHI <eResult_14(4), eResult_17(5), eResult_16(6)>
  # DEBUG eResult => eResult_8
  # DEBUG BEGIN_STMT
  return eResult_8;

}


FlexCAN_SetRegDefaultVal (struct FLEXCAN_Type * base)
{
  _Bool _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = FlexCAN_IsEnhancedRxFifoAvailable (base_16(D));
  if (_1 != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  base_16(D)->ERFSR ={v} 4160749568;
  # DEBUG BEGIN_STMT
  base_16(D)->ERFIER ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->ERFCR ={v} 0;

  <bb 4> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  base_16(D)->FDCBT ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->FDCTRL ={v} 2147500288;
  # DEBUG BEGIN_STMT
  base_16(D)->ERRSR ={v} 851981;
  # DEBUG BEGIN_STMT
  base_16(D)->ERRIPPR ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->ERRIDPR ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->ERRIAR ={v} 0;
  # DEBUG BEGIN_STMT
  _2 ={v} base_16(D)->CTRL2;
  _3 = _2 | 536870912;
  base_16(D)->CTRL2 ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_16(D)->MECR;
  _5 = _4 & 2147483647;
  base_16(D)->MECR ={v} _5;
  # DEBUG BEGIN_STMT
  base_16(D)->MECR ={v} 786560;
  # DEBUG BEGIN_STMT
  _6 ={v} base_16(D)->MECR;
  _7 = _6 | 2147483648;
  base_16(D)->MECR ={v} _7;
  # DEBUG BEGIN_STMT
  _8 ={v} base_16(D)->CTRL2;
  _9 = _8 & 3758096383;
  base_16(D)->CTRL2 ={v} _9;
  # DEBUG BEGIN_STMT
  _10 = FlexCAN_GetMaxMbNum (base_16(D));
  if (_10 > 64)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  base_16(D)->IFLAG3 ={v} 4294967295;
  # DEBUG BEGIN_STMT
  base_16(D)->IMASK3 ={v} 0;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _11 = FlexCAN_GetMaxMbNum (base_16(D));
  if (_11 > 32)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  base_16(D)->IFLAG2 ={v} 4294967295;
  # DEBUG BEGIN_STMT
  base_16(D)->IMASK2 ={v} 0;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  base_16(D)->IFLAG1 ={v} 4294967295;
  # DEBUG BEGIN_STMT
  base_16(D)->IMASK1 ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->CBT ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->CTRL2 ={v} 1048576;
  # DEBUG BEGIN_STMT
  base_16(D)->ESR1 ={v} 241670;
  # DEBUG BEGIN_STMT
  base_16(D)->ECR ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->TIMER ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->CTRL1 ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->EPRS ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->ENCBT ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->EDCBT ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->ETDC ={v} 0;
  # DEBUG BEGIN_STMT
  base_16(D)->MCR ={v} 3633315855;
  return;

}


FlexCAN_GetEnhancedRxFIFOIntStatusFlag (const struct FLEXCAN_Type * base, uint32 intFlag)
{
  long unsigned int _1;
  int _2;
  int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  uint8 _10;
  long unsigned int _11;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_8(D)->ERFIER;
  _11 = intFlag_9(D) & 255;
  _2 = (int) _11;
  _3 = _2 & 31;
  _4 = 1 << _3;
  _5 = _1 & _4;
  _6 = _5 >> _3;
  _10 = (uint8) _6;
  return _10;

}


FlexCAN_GetEnhancedRxFIFOStatusFlag (const struct FLEXCAN_Type * base, uint32 intFlag)
{
  long unsigned int _1;
  int _2;
  int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  uint8 _10;
  long unsigned int _11;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_8(D)->ERFSR;
  _11 = intFlag_9(D) & 255;
  _2 = (int) _11;
  _3 = _2 & 31;
  _4 = 1 << _3;
  _5 = _1 & _4;
  _6 = _5 >> _3;
  _10 = (uint8) _6;
  return _10;

}


FlexCAN_SetRxMaskType (struct FLEXCAN_Type * base, Flexcan_Ip_RxMaskType type)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  if (type_6(D) == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_8(D)->MCR;
  _2 = _1 & 4294901759;
  base_8(D)->MCR ={v} _2;
  goto <bb 5>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _3 ={v} base_8(D)->MCR;
  _4 = _3 | 65536;
  base_8(D)->MCR ={v} _4;

  <bb 5> [local count: 1073741824]:
  return;

}


FlexCAN_SetTxArbitrationStartDelay (struct FLEXCAN_Type * base, uint8 tasd)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_8(D)->CTRL2;
  _2 = _1 & 4278714367;
  _3 = (long unsigned int) tasd_9(D);
  _4 = _3 << 19;
  _5 = _4 & 16252928;
  _6 = _2 | _5;
  base_8(D)->CTRL2 ={v} _6;
  return;

}


FlexCAN_GetMsgBuffIntStatusFlag (const struct FLEXCAN_Type * base, uint32 msgBuffIdx)
{
  uint32 mask;
  uint8 flag;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  unsigned char _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  unsigned char _10;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG flag => 0
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_13(D) <= 31)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  mask_18 ={v} base_15(D)->IMASK1;
  # DEBUG mask => mask_18
  # DEBUG BEGIN_STMT
  _1 ={v} base_15(D)->IFLAG1;
  _2 = _1 & mask_18;
  _3 = msgBuffIdx_13(D);
  _4 = _2 >> _3;
  _5 = (unsigned char) _4;
  flag_19 = _5 & 1;
  # DEBUG flag => flag_19
  goto <bb 8>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_13(D) <= 63)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  mask_16 ={v} base_15(D)->IMASK2;
  # DEBUG mask => mask_16
  # DEBUG BEGIN_STMT
  _6 ={v} base_15(D)->IFLAG2;
  _7 = _6 & mask_16;
  _8 = msgBuffIdx_13(D) & 31;
  _9 = _7 >> _8;
  _10 = (unsigned char) _9;
  flag_17 = _10 & 1;
  # DEBUG flag => flag_17
  goto <bb 8>; [100.00%]

  <bb 6> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_13(D) <= 95)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 134217728]:
  flag_20 = FlexCAN_GetMsgBuffIntStatusFlag.part.0 (base_15(D), msgBuffIdx_13(D));

  <bb 8> [local count: 1073741824]:
  # flag_11 = PHI <flag_19(3), flag_17(5), 0(6), flag_20(7)>
  # DEBUG flag => flag_11
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  return flag_11;

}


RxFifoOcuppiedLastMsgBuff (uint32 x)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  uint32 _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = x_4(D) + 1;
  _2 = _1 * 8;
  _3 = _2 >> 2;
  _5 = _3 + 5;
  return _5;

}


FlexCAN_EnhCbtEnable (struct FLEXCAN_Type * base, boolean enableCBT)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int iftmp.6_4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_6(D)->CTRL2;
  _2 = _1 & 4294959103;
  if (enableCBT_7(D) != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 536870913]:

  <bb 4> [local count: 1073741824]:
  # iftmp.6_4 = PHI <8192(2), 0(3)>
  _3 = _2 | iftmp.6_4;
  base_6(D)->CTRL2 ={v} _3;
  return;

}


FlexCAN_EnableExtCbt (struct FLEXCAN_Type * base, boolean enableCBT)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int iftmp.4_4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_6(D)->CBT;
  _2 = _1 & 2147483647;
  if (enableCBT_7(D) != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 536870913]:

  <bb 4> [local count: 1073741824]:
  # iftmp.4_4 = PHI <2147483648(2), 0(3)>
  _3 = _2 | iftmp.4_4;
  base_6(D)->CBT ={v} _3;
  return;

}


FlexCAN_GetFDTimeSegments (const struct FLEXCAN_Type * base, struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_16(D)->FDCBT;
  _2 = _1 >> 20;
  _3 = _2 & 1023;
  timeSeg_17(D)->preDivider = _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_16(D)->FDCBT;
  _5 = _4 >> 10;
  _6 = _5 & 31;
  timeSeg_17(D)->propSeg = _6;
  # DEBUG BEGIN_STMT
  _7 ={v} base_16(D)->FDCBT;
  _8 = _7 >> 5;
  _9 = _8 & 7;
  timeSeg_17(D)->phaseSeg1 = _9;
  # DEBUG BEGIN_STMT
  _10 ={v} base_16(D)->FDCBT;
  _11 = _10 & 7;
  timeSeg_17(D)->phaseSeg2 = _11;
  # DEBUG BEGIN_STMT
  _12 ={v} base_16(D)->FDCBT;
  _13 = _12 >> 16;
  _14 = _13 & 7;
  timeSeg_17(D)->rJumpwidth = _14;
  return;

}


FlexCAN_GetTimeSegments (const struct FLEXCAN_Type * base, struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_15(D)->CTRL1;
  _2 = _1 >> 24;
  timeSeg_16(D)->preDivider = _2;
  # DEBUG BEGIN_STMT
  _3 ={v} base_15(D)->CTRL1;
  _4 = _3 & 7;
  timeSeg_16(D)->propSeg = _4;
  # DEBUG BEGIN_STMT
  _5 ={v} base_15(D)->CTRL1;
  _6 = _5 >> 19;
  _7 = _6 & 7;
  timeSeg_16(D)->phaseSeg1 = _7;
  # DEBUG BEGIN_STMT
  _8 ={v} base_15(D)->CTRL1;
  _9 = _8 >> 16;
  _10 = _9 & 7;
  timeSeg_16(D)->phaseSeg2 = _10;
  # DEBUG BEGIN_STMT
  _11 ={v} base_15(D)->CTRL1;
  _12 = _11 >> 22;
  _13 = _12 & 3;
  timeSeg_16(D)->rJumpwidth = _13;
  return;

}


FlexCAN_GetExtendedTimeSegments (const struct FLEXCAN_Type * base, struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  long unsigned int _13;
  long unsigned int _14;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_16(D)->CBT;
  _2 = _1 >> 21;
  _3 = _2 & 1023;
  timeSeg_17(D)->preDivider = _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_16(D)->CBT;
  _5 = _4 >> 10;
  _6 = _5 & 63;
  timeSeg_17(D)->propSeg = _6;
  # DEBUG BEGIN_STMT
  _7 ={v} base_16(D)->CBT;
  _8 = _7 >> 5;
  _9 = _8 & 31;
  timeSeg_17(D)->phaseSeg1 = _9;
  # DEBUG BEGIN_STMT
  _10 ={v} base_16(D)->CBT;
  _11 = _10 & 31;
  timeSeg_17(D)->phaseSeg2 = _11;
  # DEBUG BEGIN_STMT
  _12 ={v} base_16(D)->CBT;
  _13 = _12 >> 16;
  _14 = _13 & 31;
  timeSeg_17(D)->rJumpwidth = _14;
  return;

}


FlexCAN_GetEnhancedDataTimeSegments (const struct FLEXCAN_Type * base, struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  _Bool _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  _Bool x.0_21;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = timeSeg_13(D) != 0B;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_21 ={v} x;
  if (x.0_21 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 5> [local count: 107374]:

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT

  <bb 6> [local count: 1073741824]:
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  # DEBUG BEGIN_STMT
  # DEBUG x => NULL
  # DEBUG BEGIN_STMT
  timeSeg_13(D)->propSeg = 0;
  # DEBUG BEGIN_STMT
  _2 ={v} base_16(D)->EDCBT;
  _3 = _2 & 31;
  timeSeg_13(D)->phaseSeg1 = _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_16(D)->EDCBT;
  _5 = _4 >> 12;
  _6 = _5 & 15;
  timeSeg_13(D)->phaseSeg2 = _6;
  # DEBUG BEGIN_STMT
  _7 ={v} base_16(D)->EDCBT;
  _8 = _7 >> 22;
  _9 = _8 & 15;
  timeSeg_13(D)->rJumpwidth = _9;
  # DEBUG BEGIN_STMT
  _10 ={v} base_16(D)->EPRS;
  _11 = _10 >> 16;
  _12 = _11 & 1023;
  timeSeg_13(D)->preDivider = _12;
  return;

}


FlexCAN_SetEnhancedDataTimeSegments (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  _Bool _1;
  _Bool x.0_6;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = timeSeg_2(D) != 0B;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_6 ={v} x;
  if (x.0_6 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  FlexCAN_SetEnhancedDataTimeSegments.part.0 (base_5(D), timeSeg_2(D));
  return;

}


FlexCAN_GetEnhancedNominalTimeSegments (const struct FLEXCAN_Type * base, struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  timeSeg_12(D)->propSeg = 0;
  # DEBUG BEGIN_STMT
  _1 ={v} base_14(D)->EPRS;
  _2 = _1 & 1023;
  timeSeg_12(D)->preDivider = _2;
  # DEBUG BEGIN_STMT
  _3 ={v} base_14(D)->ENCBT;
  _4 = _3 & 255;
  timeSeg_12(D)->phaseSeg1 = _4;
  # DEBUG BEGIN_STMT
  _5 ={v} base_14(D)->ENCBT;
  _6 = _5 >> 12;
  _7 = _6 & 127;
  timeSeg_12(D)->phaseSeg2 = _7;
  # DEBUG BEGIN_STMT
  _8 ={v} base_14(D)->ENCBT;
  _9 = _8 >> 22;
  _10 = _9 & 127;
  timeSeg_12(D)->rJumpwidth = _10;
  return;

}


FlexCAN_SetEnhancedNominalTimeSegments (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  _Bool _1;
  _Bool x.0_6;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = timeSeg_2(D) != 0B;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_6 ={v} x;
  if (x.0_6 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  FlexCAN_SetEnhancedNominalTimeSegments.part.0 (base_5(D), timeSeg_2(D));
  return;

}


FlexCAN_SetExtendedTimeSegments (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  _Bool _1;
  _Bool x.0_6;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = timeSeg_2(D) != 0B;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_6 ={v} x;
  if (x.0_6 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  FlexCAN_SetExtendedTimeSegments.part.0 (base_5(D), timeSeg_2(D));
  return;

}


FlexCAN_SetTimeSegments (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  _Bool _1;
  _Bool x.0_6;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = timeSeg_2(D) != 0B;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_6 ={v} x;
  if (x.0_6 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  FlexCAN_SetTimeSegments.part.0 (base_5(D), timeSeg_2(D));
  return;

}


FlexCAN_SetFDTimeSegments (struct FLEXCAN_Type * base, const struct Flexcan_Ip_TimeSegmentType * timeSeg)
{
  volatile boolean x;
  _Bool _1;
  _Bool x.0_6;

  <bb 2> [local count: 214748]:
  # DEBUG BEGIN_STMT
  _1 = timeSeg_2(D) != 0B;
  x ={v} _1;
  # DEBUG x => x
  # DEBUG INLINE_ENTRY DevAssert
  # DEBUG BEGIN_STMT
  x.0_6 ={v} x;
  if (x.0_6 != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  goto <bb 3>; [100.00%]

  <bb 4> [local count: 107374]:
  FlexCAN_SetFDTimeSegments.part.0 (base_5(D), timeSeg_2(D));
  return;

}


FlexCAN_GetBuffStatusImask (const struct FLEXCAN_Type * base, uint32 msgBuffIdx)
{
  uint32 u32Imask;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  uint8 _20;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG u32Imask => 0
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_14(D) <= 31)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_16(D)->IMASK1;
  _2 = msgBuffIdx_14(D);
  _3 = 1 << _2;
  _4 = _1 & _3;
  u32Imask_19 = _4 >> _2;
  # DEBUG u32Imask => u32Imask_19
  goto <bb 8>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_14(D) <= 63)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _5 ={v} base_16(D)->IMASK2;
  _6 = msgBuffIdx_14(D) & 31;
  _7 = 1 << _6;
  _8 = _5 & _7;
  u32Imask_18 = _8 >> _6;
  # DEBUG u32Imask => u32Imask_18
  goto <bb 8>; [100.00%]

  <bb 6> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_14(D) <= 95)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  _9 ={v} base_16(D)->IMASK3;
  _10 = msgBuffIdx_14(D) & 31;
  _11 = 1 << _10;
  _12 = _9 & _11;
  u32Imask_17 = _12 >> _10;
  # DEBUG u32Imask => u32Imask_17

  <bb 8> [local count: 1073741824]:
  # u32Imask_13 = PHI <u32Imask_19(3), u32Imask_18(5), 0(6), u32Imask_17(7)>
  # DEBUG u32Imask => u32Imask_13
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _20 = (uint8) u32Imask_13;
  return _20;

}


FlexCAN_GetBuffStatusFlag (const struct FLEXCAN_Type * base, uint32 msgBuffIdx)
{
  uint32 flag;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int _9;
  long unsigned int _10;
  long unsigned int _11;
  long unsigned int _12;
  uint8 _20;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG flag => 0
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_14(D) <= 31)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_16(D)->IFLAG1;
  _2 = msgBuffIdx_14(D);
  _3 = 1 << _2;
  _4 = _1 & _3;
  flag_19 = _4 >> _2;
  # DEBUG flag => flag_19
  goto <bb 8>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_14(D) <= 63)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  _5 ={v} base_16(D)->IFLAG2;
  _6 = msgBuffIdx_14(D) & 31;
  _7 = 1 << _6;
  _8 = _5 & _7;
  flag_18 = _8 >> _6;
  # DEBUG flag => flag_18
  goto <bb 8>; [100.00%]

  <bb 6> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_14(D) <= 95)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  _9 ={v} base_16(D)->IFLAG3;
  _10 = msgBuffIdx_14(D) & 31;
  _11 = 1 << _10;
  _12 = _9 & _11;
  flag_17 = _12 >> _10;
  # DEBUG flag => flag_17

  <bb 8> [local count: 1073741824]:
  # flag_13 = PHI <flag_19(3), flag_18(5), 0(6), flag_17(7)>
  # DEBUG flag => flag_13
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _20 = (uint8) flag_13;
  return _20;

}


FlexCAN_ClearMsgBuffIntStatusFlag (struct FLEXCAN_Type * base, uint32 msgBuffIdx)
{
  uint32 flag;
  long unsigned int _1;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = msgBuffIdx_3(D) & 31;
  flag_4 = 1 << _1;
  # DEBUG flag => flag_4
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_3(D) <= 31)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  base_6(D)->IFLAG1 ={v} flag_4;
  goto <bb 8>; [100.00%]

  <bb 4> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_3(D) <= 63)
    goto <bb 5>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 5> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  base_6(D)->IFLAG2 ={v} flag_4;
  goto <bb 8>; [100.00%]

  <bb 6> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  if (msgBuffIdx_3(D) <= 95)
    goto <bb 7>; [50.00%]
  else
    goto <bb 8>; [50.00%]

  <bb 7> [local count: 134217728]:
  # DEBUG BEGIN_STMT
  base_6(D)->IFLAG3 ={v} flag_4;

  <bb 8> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  return;

}


FlexCAN_SetListenOnlyMode (struct FLEXCAN_Type * base, boolean enableListenOnly)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int iftmp.7_4;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_6(D)->CTRL1;
  _2 = _1 & 4294967287;
  if (enableListenOnly_7(D) != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 536870913]:

  <bb 4> [local count: 1073741824]:
  # iftmp.7_4 = PHI <8(2), 0(3)>
  _3 = _2 | iftmp.7_4;
  base_6(D)->CTRL1 ={v} _3;
  return;

}


FlexCAN_SetFDEnabled (struct FLEXCAN_Type * base, boolean enableFD, boolean enableBRS)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;
  long unsigned int _7;
  long unsigned int _8;
  long unsigned int iftmp.1_9;
  long unsigned int iftmp.2_10;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_12(D)->MCR;
  _2 = _1 & 4294965247;
  if (enableFD_13(D) != 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 3>; [50.00%]

  <bb 3> [local count: 536870913]:

  <bb 4> [local count: 1073741824]:
  # iftmp.1_9 = PHI <2048(2), 0(3)>
  _3 = _2 | iftmp.1_9;
  base_12(D)->MCR ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} base_12(D)->FDCTRL;
  _5 = _4 & 2147483647;
  if (enableBRS_15(D) != 0)
    goto <bb 6>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 5> [local count: 536870913]:

  <bb 6> [local count: 1073741824]:
  # iftmp.2_10 = PHI <2147483648(4), 0(5)>
  _6 = _5 | iftmp.2_10;
  base_12(D)->FDCTRL ={v} _6;
  # DEBUG BEGIN_STMT
  _7 ={v} base_12(D)->FDCTRL;
  _8 = _7 & 4294926591;
  base_12(D)->FDCTRL ={v} _8;
  return;

}


FlexCAN_DisableMemErrorDetection (struct FLEXCAN_Type * base)
{
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 ={v} base_7(D)->CTRL2;
  _2 = _1 | 536870912;
  base_7(D)->CTRL2 ={v} _2;
  # DEBUG BEGIN_STMT
  base_7(D)->MECR ={v} 0;
  # DEBUG BEGIN_STMT
  base_7(D)->MECR ={v} 0;
  # DEBUG BEGIN_STMT
  _3 ={v} base_7(D)->MECR;
  _4 = _3 | 256;
  base_7(D)->MECR ={v} _4;
  # DEBUG BEGIN_STMT
  _5 ={v} base_7(D)->CTRL2;
  base_7(D)->CTRL2 ={v} _5;
  return;

}


FlexCAN_SetEnhancedTDCOffset (struct FLEXCAN_Type * base, boolean enable, uint8 offset)
{
  uint32 tmp;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  tmp_7 ={v} base_6(D)->ETDC;
  # DEBUG tmp => tmp_7
  # DEBUG BEGIN_STMT
  tmp_8 = tmp_7 & 2139160575;
  # DEBUG tmp => tmp_8
  # DEBUG BEGIN_STMT
  if (enable_9(D) != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  tmp_10 = tmp_8 | 2147483648;
  # DEBUG tmp => tmp_10
  # DEBUG BEGIN_STMT
  _1 = (long unsigned int) offset_11(D);
  _2 = _1 << 16;
  _3 = _2 & 8323072;
  tmp_12 = _3 | tmp_10;
  # DEBUG tmp => tmp_12

  <bb 4> [local count: 1073741824]:
  # tmp_4 = PHI <tmp_8(2), tmp_12(3)>
  # DEBUG tmp => tmp_4
  # DEBUG BEGIN_STMT
  base_6(D)->ETDC ={v} tmp_4;
  return;

}


FlexCAN_SetTDCOffset (struct FLEXCAN_Type * base, boolean enable, uint8 offset)
{
  uint32 tmp;
  long unsigned int _1;
  long unsigned int _2;
  long unsigned int _3;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  tmp_7 ={v} base_6(D)->FDCTRL;
  # DEBUG tmp => tmp_7
  # DEBUG BEGIN_STMT
  tmp_8 = tmp_7 & 4294926591;
  # DEBUG tmp => tmp_8
  # DEBUG BEGIN_STMT
  if (enable_9(D) != 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 4>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  tmp_10 = tmp_8 | 32768;
  # DEBUG tmp => tmp_10
  # DEBUG BEGIN_STMT
  _1 = (long unsigned int) offset_11(D);
  _2 = _1 << 8;
  _3 = _2 & 7936;
  tmp_12 = _3 | tmp_10;
  # DEBUG tmp => tmp_12

  <bb 4> [local count: 1073741824]:
  # tmp_4 = PHI <tmp_8(2), tmp_12(3)>
  # DEBUG tmp => tmp_4
  # DEBUG BEGIN_STMT
  base_6(D)->FDCTRL ={v} tmp_4;
  return;

}


