
Analyzing function: SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02/12
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2 3 4 5
;; 2 succs { 3 5 }
;; 3 succs { 4 5 }
;; 4 succs { 5 }
;; 5 succs { 1 }

Analyzing function body size: SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02

IPA function summary for SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02/12 inlinable
  global time:     21.750000
  self size:       16
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:11.000000, time:8.750000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Sys_GetCoreID/13 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11


Analyzing function: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02/11
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2 3 4 5
;; 2 succs { 3 5 }
;; 3 succs { 4 5 }
;; 4 succs { 5 }
;; 5 succs { 1 }

Analyzing function body size: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02

IPA function summary for SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02/11 inlinable
  global time:     22.250000
  self size:       18
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:13.000000, time:9.250000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Sys_GetCoreID/13 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11


Analyzing function: SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01/10
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2 3 4 5
;; 2 succs { 3 5 }
;; 3 succs { 4 5 }
;; 4 succs { 5 }
;; 5 succs { 1 }

Analyzing function body size: SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01

IPA function summary for SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01/10 inlinable
  global time:     21.750000
  self size:       16
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:11.000000, time:8.750000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Sys_GetCoreID/13 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11


Analyzing function: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01/9
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2 3 4 5
;; 2 succs { 3 5 }
;; 3 succs { 4 5 }
;; 4 succs { 5 }
;; 5 succs { 1 }

Analyzing function body size: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01

IPA function summary for SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01/9 inlinable
  global time:     22.250000
  self size:       18
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:13.000000, time:9.250000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Sys_GetCoreID/13 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11


Analyzing function: SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00/8
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2 3 4 5
;; 2 succs { 3 5 }
;; 3 succs { 4 5 }
;; 4 succs { 5 }
;; 5 succs { 1 }

Analyzing function body size: SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00

IPA function summary for SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00/8 inlinable
  global time:     21.750000
  self size:       16
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:11.000000, time:8.750000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Sys_GetCoreID/13 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11


Analyzing function: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00/7
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2 3 4 5
;; 2 succs { 3 5 }
;; 3 succs { 4 5 }
;; 4 succs { 5 }
;; 5 succs { 1 }

Analyzing function body size: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00

IPA function summary for SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00/7 inlinable
  global time:     22.250000
  self size:       18
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:13.000000, time:9.250000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:
    Sys_GetCoreID/13 function body not available
      loop depth: 0 freq:1.00 size: 2 time: 11


Analyzing function: Mcu_schm_read_msr/6
;; 1 loops found
;;
;; Loop 0
;;  header 0, latch 1
;;  depth 0, outer -1
;;  nodes: 0 1 2
;; 2 succs { 1 }

Analyzing function body size: Mcu_schm_read_msr

IPA function summary for Mcu_schm_read_msr/6 inlinable
  global time:     3.000000
  self size:       4
  global size:     0
  min size:       0
  self stack:      0
  global stack:    0
    size:1.000000, time:1.000000
    size:3.000000, time:2.000000,  executed if:(not inlined)
  calls:

Symbol table:

Sys_GetCoreID/13 (Sys_GetCoreID) @06caca80
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02/12 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02/11 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01/10 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01/9 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00/8 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00/7 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02/12 (SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02) @06cac540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_MCU_EXCLUSIVE_AREA_02/5 (read)reentry_guard_MCU_EXCLUSIVE_AREA_02/5 (write)msr_MCU_EXCLUSIVE_AREA_02/4 (read)reentry_guard_MCU_EXCLUSIVE_AREA_02/5 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/13 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02/11 (SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02) @06cac2a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_MCU_EXCLUSIVE_AREA_02/5 (read)msr_MCU_EXCLUSIVE_AREA_02/4 (write)msr_MCU_EXCLUSIVE_AREA_02/4 (read)reentry_guard_MCU_EXCLUSIVE_AREA_02/5 (read)reentry_guard_MCU_EXCLUSIVE_AREA_02/5 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/13 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01/10 (SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01) @06cac000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_MCU_EXCLUSIVE_AREA_01/3 (read)reentry_guard_MCU_EXCLUSIVE_AREA_01/3 (write)msr_MCU_EXCLUSIVE_AREA_01/2 (read)reentry_guard_MCU_EXCLUSIVE_AREA_01/3 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/13 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01/9 (SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01) @06b1ba80
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_MCU_EXCLUSIVE_AREA_01/3 (read)msr_MCU_EXCLUSIVE_AREA_01/2 (write)msr_MCU_EXCLUSIVE_AREA_01/2 (read)reentry_guard_MCU_EXCLUSIVE_AREA_01/3 (read)reentry_guard_MCU_EXCLUSIVE_AREA_01/3 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/13 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00/8 (SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00) @06b1bee0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_MCU_EXCLUSIVE_AREA_00/1 (read)reentry_guard_MCU_EXCLUSIVE_AREA_00/1 (write)msr_MCU_EXCLUSIVE_AREA_00/0 (read)reentry_guard_MCU_EXCLUSIVE_AREA_00/1 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/13 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00/7 (SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00) @06b1bc40
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_MCU_EXCLUSIVE_AREA_00/1 (read)msr_MCU_EXCLUSIVE_AREA_00/0 (write)msr_MCU_EXCLUSIVE_AREA_00/0 (read)reentry_guard_MCU_EXCLUSIVE_AREA_00/1 (read)reentry_guard_MCU_EXCLUSIVE_AREA_00/1 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/13 (1073741824 (estimated locally),1.00 per call) 
Mcu_schm_read_msr/6 (Mcu_schm_read_msr) @06b1b9a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
reentry_guard_MCU_EXCLUSIVE_AREA_02/5 (reentry_guard_MCU_EXCLUSIVE_AREA_02) @06b1a630
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02/11 (read)SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02/11 (read)SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02/11 (write)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02/12 (read)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02/12 (write)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02/12 (read)
  Availability: available
  Varpool flags:
msr_MCU_EXCLUSIVE_AREA_02/4 (msr_MCU_EXCLUSIVE_AREA_02) @06b1a5a0
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02/11 (read)SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02/11 (write)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02/12 (read)
  Availability: available
  Varpool flags:
reentry_guard_MCU_EXCLUSIVE_AREA_01/3 (reentry_guard_MCU_EXCLUSIVE_AREA_01) @06b1a510
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01/9 (read)SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01/9 (read)SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01/9 (write)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01/10 (read)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01/10 (write)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01/10 (read)
  Availability: available
  Varpool flags:
msr_MCU_EXCLUSIVE_AREA_01/2 (msr_MCU_EXCLUSIVE_AREA_01) @06b1a480
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01/9 (read)SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01/9 (write)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01/10 (read)
  Availability: available
  Varpool flags:
reentry_guard_MCU_EXCLUSIVE_AREA_00/1 (reentry_guard_MCU_EXCLUSIVE_AREA_00) @06b1a3f0
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00/7 (read)SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00/7 (read)SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00/7 (write)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00/8 (read)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00/8 (write)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00/8 (read)
  Availability: available
  Varpool flags:
msr_MCU_EXCLUSIVE_AREA_00/0 (msr_MCU_EXCLUSIVE_AREA_00) @06b1a360
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00/7 (read)SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00/7 (write)SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00/8 (read)
  Availability: available
  Varpool flags:
SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_02 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_02[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_MCU_EXCLUSIVE_AREA_02[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_MCU_EXCLUSIVE_AREA_02[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_02[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_02 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_02[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Mcu_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_MCU_EXCLUSIVE_AREA_02[u32CoreId_10] ={v} reg_tmp_14;
  # DEBUG BEGIN_STMT
  _3 ={v} msr_MCU_EXCLUSIVE_AREA_02[u32CoreId_10];
  _4 = _3 & 1;
  if (_4 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _5 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_02[u32CoreId_10];
  _6 = _5 + 1;
  reentry_guard_MCU_EXCLUSIVE_AREA_02[u32CoreId_10] ={v} _6;
  return;

}


SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_01 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_01[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_MCU_EXCLUSIVE_AREA_01[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_MCU_EXCLUSIVE_AREA_01[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_01[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_01 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_01[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Mcu_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_MCU_EXCLUSIVE_AREA_01[u32CoreId_10] ={v} reg_tmp_14;
  # DEBUG BEGIN_STMT
  _3 ={v} msr_MCU_EXCLUSIVE_AREA_01[u32CoreId_10];
  _4 = _3 & 1;
  if (_4 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _5 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_01[u32CoreId_10];
  _6 = _5 + 1;
  reentry_guard_MCU_EXCLUSIVE_AREA_01[u32CoreId_10] ={v} _6;
  return;

}


SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_00[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_MCU_EXCLUSIVE_AREA_00[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_MCU_EXCLUSIVE_AREA_00[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_00[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_00[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Mcu_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  msr_MCU_EXCLUSIVE_AREA_00[u32CoreId_10] ={v} reg_tmp_14;
  # DEBUG BEGIN_STMT
  _3 ={v} msr_MCU_EXCLUSIVE_AREA_00[u32CoreId_10];
  _4 = _3 & 1;
  if (_4 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _5 ={v} reentry_guard_MCU_EXCLUSIVE_AREA_00[u32CoreId_10];
  _6 = _5 + 1;
  reentry_guard_MCU_EXCLUSIVE_AREA_00[u32CoreId_10] ={v} _6;
  return;

}


Mcu_schm_read_msr ()
{
  register uint32 reg_tmp;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_1);
  # DEBUG reg_tmp => reg_tmp_1
  # DEBUG BEGIN_STMT
  return reg_tmp_1;

}


